{"text_format":"1","workbook":"xlsx","n_sheets":11,"sheets":["REMISE","SUN C250","Sun 3000","Pro C ","FeuilleproC","Outils accessoires","Accessoires et options","feuille PRO c250","Liste de prix","Feuille Power OPC","Mise à jour"],"not_rendered":{"charts":0,"images":19,"macros":1,"external_links":0,"defined_names":66,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"REMISE","index":0,"n_rows":9,"n_cols":6,"rows_kept":9,"cut":false,"hidden":true,"merged":[[2,1,2,3],[5,1,5,3],[8,1,8,3]]}
[]
[]
[null,"Remise feuille PRO C250",null,null,null,0]
[]
[]
[null,"Remise feuille POWER",null,null,null,0]
[]
[]
[null,"Remise feuille Accessoires et options",null,null,null,0]

{"sheet":"SUN C250","index":1,"n_rows":64,"n_cols":11,"rows_kept":64,"cut":false,"hidden":false,"merged":[[60,9,60,10],[56,4,56,5],[56,9,56,10],[58,4,58,5],[59,4,59,5],[58,9,58,10],[59,9,59,10],[52,9,52,10],[51,4,51,5],[52,4,52,5],[45,4,45,5],[47,4,47,5],[49,4,49,5],[51,9,51,10],[43,9,43,10],[44,9,44,10],[45,9,45,10],[28,9,28,10],[32,9,32,10],[33,9,33,10],[34,9,34,10],[2,4,2,8],[62,4,62,5],[62,6,62,8],[63,4,63,5],[63,6,63,8],[32,4,32,5],[28,4,28,5],[30,4,30,5],[36,4,36,5],[38,4,38,5],[34,4,34,5],[40,4,40,5],[43,4,43,5],[44,4,44,5],[60,4,60,5],[48,2,48,3],[10,2,10,3],[10,4,10,8],[11,4,11,8],[12,4,12,8],[14,2,14,3],[16,2,16,4],[18,7,18,8],[23,2,23,3],[33,4,33,5]]}
[null,null,null,null,null,null,null,null,null,null,"Version 01/2017"]
[]
[null,null,null,null,"Chiffrage des capteurs SUN C250 "]
[]
[null,null,null,null,null,null,null,null,null,null,{"$f":"TODAY()","v":"2017-01-31"}]
[]
[]
[]
[]
[]
[null,null," Référence     "]
[]
[]
[]
[null,null,"Montage",null,"Horizontal"]
[]
[null,null,"Attention ! Lorsque vous modifiez une des sélections, il faut toujours revalider les suivantes ! "]
[]
[]
[null,null,null,null,"DESIGNATION","COLIS            ","Prix unitaire HT en €","Nbre capt. par rangée       ","Nbre rangée     ","Qté","Prix total HT en €"]
[]
[null,null,null,null,"► CAPTEURS PLANS EMBALLES"]
[]
[null,null,null,null,{"$f":"IF(E15='feuille PRO c250'!P10,'feuille PRO c250'!B18,'feuille PRO c250'!H18)","v":"CAPTEUR PLAN MONTAGE HORIZONTAL PRO C250 H"},{"$f":"IF(E15='feuille PRO c250'!P10,'feuille PRO c250'!C18,'feuille PRO c250'!I18)","v":"ER241"},{"$f":"IF(E15='feuille PRO c250'!P10,'feuille PRO c250'!D18,'feuille PRO c250'!J18)","v":820},null,null,{"$f":"H24*I24","v":0},{"$f":"J24*(1-REMISE!$F$3)*G24","v":0}]
[null,null,null,null,{"$f":"IF(E15='feuille PRO c250'!P10,'feuille PRO c250'!B18,'feuille PRO c250'!H18)","v":"CAPTEUR PLAN MONTAGE HORIZONTAL PRO C250 H"},{"$f":"IF(E15='feuille PRO c250'!P10,'feuille PRO c250'!C18,'feuille PRO c250'!I18)","v":"ER241"},{"$f":"IF(E15='feuille PRO c250'!P10,'feuille PRO c250'!D18,'feuille PRO c250'!J18)","v":820},null,null,{"$f":"H25*I25","v":0},{"$f":"J25*(1-REMISE!$F$3)*G25","v":0}]
[null,null,null,null,{"$f":"IF(E15='feuille PRO c250'!P10,'feuille PRO c250'!B18,'feuille PRO c250'!H18)","v":"CAPTEUR PLAN MONTAGE HORIZONTAL PRO C250 H"},{"$f":"IF(E15='feuille PRO c250'!P10,'feuille PRO c250'!C18,'feuille PRO c250'!I18)","v":"ER241"},{"$f":"IF(E15='feuille PRO c250'!P10,'feuille PRO c250'!D18,'feuille PRO c250'!J18)","v":820},null,null,{"$f":"H26*I26","v":0},{"$f":"J26*(1-REMISE!$F$3)*G26","v":0}]
[null,null,null,null,null,null,null,null,"Soit une surface totale de :",{"$f":"(J24+J25+J26)*2.38","v":0},"m²"]
[]
[null,null,null,null,"Désignation",null,"Colis","Colis","Quantité","prix total HT"]
[]
[null,null,null,null,"► ACCESSOIRES POUR RACCORDEMENT HYDRAULIQUE"]
[]
[null,null,null,null,{"$f":"'feuille PRO c250'!H23","v":"KIT DE RACCORDEMENT CHAMP DE CAPTEURS"},null,{"$f":"'feuille PRO c250'!J23","v":120},{"$f":"'feuille PRO c250'!I23","v":"ER245"},{"$f":"'feuille PRO c250'!E23","v":0},{"$f":"G33*I33*(1-REMISE!$F$3)","v":0}]
[null,null,null,null,{"$f":"'feuille PRO c250'!H24","v":"KIT DE LIAISON HYDRAULIQUE ENTRE CAPTEURS"},null,{"$f":"'feuille PRO c250'!J24","v":41},{"$f":"'feuille PRO c250'!I24","v":"ER246"},{"$f":"'feuille PRO c250'!E24","v":0},{"$f":"G34*I34*(1-REMISE!$F$3)","v":0}]
[null,null,"Option :","NON",{"$f":"'feuille PRO c250'!H25","v":"KIT  FLEXIBLES CIRCUIT SOLAIRE CHAMP CAPTEURS"},null,{"$f":"'feuille PRO c250'!J25","v":77},{"$f":"'feuille PRO c250'!I25","v":"ER247"},{"$f":"IF(D35=\"NON\",0,'feuille PRO c250'!E25)","v":0},{"$f":"G35*I35*(1-REMISE!$F$3)","v":0}]
[]
[null,null,null,null,"► POSE"]
[]
[null,null,null,null,"sur toiture",null,null,{"$f":"IF(choix=\"en intégration de toiture\",\" Obligation de poser un film écran sous toiture!\",\"\")","v":""}]
[null,null,null,null,{"$f":"IF(AND(E15=\"horizontal\",choix=\"en intégration de toiture\"),\" Attention le nombre de capteur par rangée est limité à 4 en intégration horizontale\",\"\")","v":""}]
[null,null,null,null,"tuile canal 17°"]
[]
[]
[null,null,null,null,{"$f":"IF($E$15='feuille PRO c250'!$P$10,'feuille PRO c250'!B82,'feuille PRO c250'!H82)","v":"KIT DE BASE 17° D'INTEGRATION TUILE CANAL 2 C250 H "},null,{"$f":"IF($E$15='feuille PRO c250'!$P$10,'feuille PRO c250'!D82,'feuille PRO c250'!J82)","v":1325},{"$f":"IF($E$15='feuille PRO c250'!$P$10,'feuille PRO c250'!C82,'feuille PRO c250'!I82)","v":"ER644"},{"$f":"IF($E$15='feuille PRO c250'!$P$10,'feuille PRO c250'!E82,'feuille PRO c250'!K82)","v":0},{"$f":"G44*I44*(1-REMISE!$F$3)","v":0}]
[null,null,null,null,{"$f":"IF($E$15='feuille PRO c250'!$P$10,'feuille PRO c250'!B83,'feuille PRO c250'!H83)","v":"KIT EXTENSION 17° INTEGRATION TUILE CANAL C 250 H"},null,{"$f":"IF($E$15='feuille PRO c250'!$P$10,'feuille PRO c250'!D83,'feuille PRO c250'!J83)","v":478},{"$f":"IF($E$15='feuille PRO c250'!$P$10,'feuille PRO c250'!C83,'feuille PRO c250'!I83)","v":"ER645"},{"$f":"IF($E$15='feuille PRO c250'!$P$10,'feuille PRO c250'!E83,'feuille PRO c250'!K83)","v":0},{"$f":"IF(E45=\"\",0,G45*I45*(1-REMISE!$F$3))","v":0}]
[null,null,null,null,{"$f":"IF($E$15='feuille PRO c250'!$P$10,'feuille PRO c250'!B84,'feuille PRO c250'!H84)","v":""},null,{"$f":"IF($E$15='feuille PRO c250'!$P$10,'feuille PRO c250'!D84,'feuille PRO c250'!J84)","v":""},{"$f":"IF($E$15='feuille PRO c250'!$P$10,'feuille PRO c250'!C84,'feuille PRO c250'!I84)","v":""},{"$f":"IF($E$15='feuille PRO c250'!$P$10,'feuille PRO c250'!E84,'feuille PRO c250'!K84)","v":""},{"$f":"IF(E46=\"\",0,G46*I46*(1-REMISE!$F$3))","v":0}]
[]
[null,null,null,null,"► FERRURES D'ANCRAGE"]
[]
[null,null,null,null,"Tuiles mécaniques (alu)"]
[]
[null,null,null,null,{"$f":"IF(choix=\"sur toiture\",'feuille PRO c250'!B87,\"\")","v":"4 FERRURES D'ANCRAGE ALU POUR MONTAGE SUR TUILES MÉCANIQUES"},null,{"$f":"IF(choix=\"sur toiture\",'feuille PRO c250'!D87,\"\")","v":98},{"$f":"IF(choix=\"sur toiture\",'feuille PRO c250'!C87,\"\")","v":"EG311"},{"$f":"IF(choix=\"sur toiture\",'feuille PRO c250'!E87,\"\")","v":0},{"$f":"IF(E52=\"\",0,G52*I52*(1-REMISE!$F$3))","v":0}]
[null,null,null,null,{"$f":"IF(choix=\"sur toiture\",'feuille PRO c250'!B88,\"\")","v":"6 FERRURES D'ANCRAGE ALU POUR MONTAGE SUR TUILES MÉCANIQUES"},null,{"$f":"IF(choix=\"sur toiture\",'feuille PRO c250'!D88,\"\")","v":141},{"$f":"IF(choix=\"sur toiture\",'feuille PRO c250'!C88,\"\")","v":"EG312"},{"$f":"IF(choix=\"sur toiture\",'feuille PRO c250'!E88,\"\")","v":0},{"$f":"IF(E53=\"\",0,G53*I53*(1-REMISE!$F$3))","v":0}]
[]
[null,null,null,"Attention ! Lorsque vous modifiez une des sélections, il faut toujours revalider les suivantes ! "]
[]
[null,null,null,null,"Désignation",null,"Colis","Colis","Quantité","prix total HT"]
[]
[]
[]
[]
[]
[null,null,null,null,"Système PRO C250 complet",null,"Prix total HT"]
[null,null,null,null,"Ensemble capteurs, fixations, raccords hydrauliques ",null,{"$f":"SUM(J53+J52+J46+J45+J44+J35+J34+J33+K26+K25+K24+J59+J60+J61)","v":0}]

{"sheet":"Sun 3000","index":2,"n_rows":66,"n_cols":12,"rows_kept":66,"cut":false,"hidden":false,"merged":[[2,3,2,7],[63,8,63,9],[37,2,39,2],[58,2,59,2],[37,1,39,1],[49,3,49,5],[24,2,29,2],[43,3,43,10],[21,3,22,3],[24,1,29,1],[32,3,33,3],[67,4,67,6],[68,4,68,6],[7,2,7,8],[8,2,8,8],[9,2,9,8],[64,1,66,1],[56,1,59,1],[45,2,46,2],[55,3,55,5],[63,4,63,6],[64,4,64,6],[66,4,66,6],[65,4,65,6]]}
[null,null,null,null,null,null,null,null,null,null,{"$f":"'SUN C250'!K1","v":"Version 01/2017"}]
[]
[null,null,null,"Chiffrage des capteurs tubulaires SUN 3000"]
[]
[null,null,null,null,null,null,null,null,null,null,{"$f":"TODAY()","v":"2017-01-31"}]
[]
[]
[null," Référence     "]
[null,null,null,null,null,null,null,null,null,null,{"$f":"REMISE!F6","v":0}]
[]
[]
[]
[null,null,null,"DESIGNATION","Référence","COLIS","PRIX","Nbre capteur par rangée       ","Nbre rangée     ","Qté","Prix total    HT en €"]
[]
[null,null,null,"►MONTAGE"]
[null,null,null,"Sur toiture"]
[]
[null,null,null,"►CAPTEURS TUBULAIRES"]
[null,null,null,"Sun 3010",100012353,{"$f":"VLOOKUP(E19,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER40"},{"$f":"VLOOKUP(E19,'Liste de prix'!$1:$1048576,4,FALSE)","v":1656},null,null,{"$f":"H19*I19","v":0},{"$f":"L19*(1-K9)","v":0},{"$f":"J19*G19","v":0}]
[null,null,null,"Sun 3015",100012354,{"$f":"VLOOKUP(E20,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER41"},{"$f":"VLOOKUP(E20,'Liste de prix'!$1:$1048576,4,FALSE)","v":1974},null,null,{"$f":"H20*I20","v":0},{"$f":"L20*(1-K9)","v":0},{"$f":"J20*G20","v":0}]
[null,null,null,null,null,null,null,"Soit une surface totale de:",null,{"$f":"J19*1.14+J20*1.72","v":0},"m²"]
[null,null,null,"►ACCESSOIRES POUR RACCORDEMENT HYDRAULIQUE"]
[]
[]
[null,null,null,"• Raccordement des capteurs en montage   vertical  juxtaposés ou  horizontal  superposés "]
[]
[null,null,null,"Kit de raccordement hydraulique (extémité+bouchon) Tichelmann",100011397,{"$f":"VLOOKUP(E27,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG394"},{"$f":"VLOOKUP(E27,'Liste de prix'!$1:$1048576,4,FALSE)","v":112},null,null,{"$f":"'Feuille Power OPC'!F17","v":0},{"$f":"L27*(1-K9)","v":0},{"$f":"G27*J27","v":0}]
[null,null,null,"Kit de liaison entre 2 capteurs",100011396,{"$f":"VLOOKUP(E28,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG393"},{"$f":"VLOOKUP(E28,'Liste de prix'!$1:$1048576,4,FALSE)","v":150},null,null,{"$f":"'Feuille Power OPC'!F23","v":0},{"$f":"L28*(1-K$9)","v":0},{"$f":"G28*J28","v":0}]
[null,null,null,"Kit raccordement flexibles capteur tubulaire + sonde capteur",89807355,{"$f":"VLOOKUP(E29,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG355"},{"$f":"VLOOKUP(E29,'Liste de prix'!$1:$1048576,4,FALSE)","v":197},null,null,{"$f":"'Feuille Power OPC'!F29","v":0},{"$f":"L29*(1-K9)","v":0},{"$f":"G29*J29","v":0}]
[null,null,null,"Kit fixation 1 capteur tubulaire",100011395,{"$f":"VLOOKUP(E30,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG392"},{"$f":"VLOOKUP(E30,'Liste de prix'!$1:$1048576,4,FALSE)","v":78},null,null,{"$f":"'Feuille Power OPC'!F35","v":0},{"$f":"L30*(1-K9)","v":0},{"$f":"G30*J30","v":0}]
[]
[]
[null,null,null,"►ELEMENTS DE POSE SUR TOIT OU EN TERRASSE  "]
[]
[null,null,null,"A choisir parmi les types de montage suivants :"]
[null,null,null,"SUR TOIT OU EN TERRASSE"]
[]
[null,null,null,"Montage vertical  sur profilés de ER "]
[null,null,null,"Kit de montage 1 capteur POWER 10",100012019,{"$f":"VLOOKUP(E39,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER31"},{"$f":"VLOOKUP(E39,'Liste de prix'!$1:$1048576,4,FALSE)","v":158},null,null,{"$f":"'Feuille Power OPC'!F47","v":0},{"$f":"L39*(1-K$9)","v":0},{"$f":"IF(J39<>0,G39*J39,0)","v":0}]
[null,null,null,"Kit de montage 1 capteur POWER 15",100012020,{"$f":"VLOOKUP(E40,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER32"},{"$f":"VLOOKUP(E40,'Liste de prix'!$1:$1048576,4,FALSE)","v":166},null,null,{"$f":"'Feuille Power OPC'!F48","v":0},{"$f":"L40*(1-K$9)","v":0},{"$f":"IF(J40<>0,G40*J40,0)","v":0}]
[]
[]
[]
[null,null,null,"• Supports inclinables pour TERRASSE (ou au sol) pour les capteurs Power 10 et 15 uniquement "]
[null,null,null,"selon la disposition des capteurs en + des profilés"]
[null,null,null,"3 supports avec croix stabilisatrices pour 2 capt. Montage    vertical    ",89807358,{"$f":"VLOOKUP(E46,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG358"},{"$f":"VLOOKUP(E46,'Liste de prix'!$1:$1048576,4,FALSE)","v":287},null,null,{"$f":"'Feuille Power OPC'!F58","v":0},{"$f":"L46*(1-K$9)","v":0},{"$f":"G46*J46","v":0}]
[null,null,null,"3 supports (sans croix stabilisatrices) pour 2 capt. Montage    vertical",89807359,{"$f":"VLOOKUP(E47,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG359"},{"$f":"VLOOKUP(E47,'Liste de prix'!$1:$1048576,4,FALSE)","v":245},null,null,{"$f":"'Feuille Power OPC'!F65","v":0},{"$f":"L47*(1-K$9)","v":0},{"$f":"G47*J47","v":0}]
[]
[]
[null,null,null,"• Ferrures d’ancrage pour montage SUR TOITURE "]
[null,null,null," à choisir selon le type de couverture en + des profilés"]
[null,null,null,"montage indépendant des chevrons en alu pour tuiles mécaniques",{"$f":"'Feuille Power OPC'!H78","v":89807311},{"$f":"VLOOKUP(E52,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG311"},{"$f":"VLOOKUP(E52,'Liste de prix'!$1:$1048576,4,FALSE)","v":98},null,null,{"$f":"'Feuille Power OPC'!E70","v":0},{"$f":"L52*(1-K$9)","v":0},{"$f":"IF(J52<>0,G52*J52,0)","v":0}]
[null,null,null,null,{"$f":"'Feuille Power OPC'!H79","v":89807312},{"$f":"VLOOKUP(E53,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG312"},{"$f":"VLOOKUP(E53,'Liste de prix'!$1:$1048576,4,FALSE)","v":141},null,null,{"$f":"'Feuille Power OPC'!E71","v":0},{"$f":"L53*(1-K$9)","v":0},{"$f":"G53*J53","v":0}]
[]
[]
[null,null,null,"• Montage sur tuiles canal "]
[null,"chiffrage",null,"Ferrure d'ancrage pour montage sur tuiles canal",89807358,{"$f":"VLOOKUP(E57,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG358"},{"$f":"VLOOKUP(E57,'Liste de prix'!$1:$1048576,4,FALSE)","v":287},null,null,{"$f":"'Feuille Power OPC'!F93","v":0},{"$f":"L57*(1-K$9)","v":0},{"$f":"G57*J57","v":0}]
[null,null,null,null,89807359,{"$f":"VLOOKUP(E58,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG359"},{"$f":"VLOOKUP(E58,'Liste de prix'!$1:$1048576,4,FALSE)","v":245},null,null,{"$f":"'Feuille Power OPC'!F94","v":0},{"$f":"L58*(1-K$9)","v":0},{"$f":"G58*J58","v":0}]
[]
[]
[]
[]
[]
[null,null,null,"Système","Prix total HT en €"]
[null," \"Capteurs, fixations et raccords hydrauliques \""]
[null,null,null,{"$f":"D16","v":"Sur toiture"},{"$f":"IF(D16='Outils accessoires'!A74,K19+K20+K27+K28+K29+K30+K39+K40+K52+K53,IF(D16='Outils accessoires'!A75,K19+K20+K27+K28+K29+K30+K39+K40+K46+K47,IF(D16='Outils accessoires'!A76,K19+K20+K27+K28+K29+K30+K39+K40+K57+K58,\"\")))","v":0}]

{"sheet":"Pro C ","index":3,"n_rows":66,"n_cols":11,"rows_kept":66,"cut":false,"hidden":true,"merged":[[1,3,1,8],[11,1,11,2],[22,3,24,3],[33,3,34,3],[15,6,15,7],[31,1,31,3],[7,1,7,2],[13,1,13,3],[19,1,19,2],[7,3,7,7],[66,1,68,2],[40,1,48,1],[3,8,3,9],[60,4,60,5],[8,3,8,7],[9,3,9,7],[25,1,30,1],[25,2,30,2],[55,1,55,3],[65,3,65,4],[65,5,65,7],[64,3,64,4],[61,1,61,2],[40,2,46,2],[59,4,59,5],[64,5,64,7]]}
[]
[null,null,null,"Chiffrage colis installation solaire COLLECTIVE capteurs PRO C250"]
[]
[null,null,null,null,null,null,null,null,"Version 09/2010"]
[null,"Identification de l'étude ",null,null,null,null,null,null,null,{"$f":"TODAY()","v":"2017-01-31"}]
[]
[]
[null," Référence     "]
[null,null,null,null,null,null,null,null,null,{"$f":"REMISE!F3","v":0}]
[]
[]
[null,"Montage",null,"vertical",{"$f":"IF(D12=\"horizontal\",\" Attention le nombre de capteur par rangée est limité à 4\",\"\")","v":""}]
[]
[null,"Attention ! Lorsque vous modifiez une des sélections, il faut toujours revalider les suivantes ! "]
[]
[]
[null,null,null,"DESIGNATION","COLIS            ","Prix untaire HT en €","Nbre capt. par rangée       ","Nbre rangée     ","Qté","Prix total HT en €"]
[null,null,null,"►CAPTEURS PLANS EMBALLES"]
[]
[null,null,null,{"$f":"FeuilleproC!$C$129","v":{"$error":"#N/A"}},{"$f":"FeuilleproC!$D$129","v":{"$error":"#N/A"}},{"$f":"FeuilleproC!$E$129","v":{"$error":"#N/A"}},0,0,{"$f":"G20*H20","v":0},{"$f":"K20*(1-J$9)","v":{"$error":"#N/A"}},{"$f":"F20*I20","v":{"$error":"#N/A"}}]
[null,null,null,{"$f":"FeuilleproC!$C$129","v":{"$error":"#N/A"}},{"$f":"FeuilleproC!$D$129","v":{"$error":"#N/A"}},{"$f":"FeuilleproC!$E$129","v":{"$error":"#N/A"}},0,0,{"$f":"G21*H21","v":0},{"$f":"K21*(1-J$9)","v":{"$error":"#N/A"}},{"$f":"F21*I21","v":{"$error":"#N/A"}}]
[null,null,null,{"$f":"FeuilleproC!$C$129","v":{"$error":"#N/A"}},{"$f":"FeuilleproC!$D$129","v":{"$error":"#N/A"}},{"$f":"FeuilleproC!$E$129","v":{"$error":"#N/A"}},null,null,{"$f":"G22*H22","v":0},{"$f":"K22*(1-J$9)","v":{"$error":"#N/A"}},{"$f":"F22*I22","v":{"$error":"#N/A"}}]
[null,null,null,"►ACCESSOIRES POUR RACCORDEMENT HYDRAULIQUE",null,null,"Soit une surface totale de :",null,{"$f":"(I20+I21+I22)*2.5","v":0},"m²"]
[]
[]
[null,null,null,{"$f":"FeuilleproC!B27","v":{"$error":"#REF!"}},{"$f":"FeuilleproC!C27","v":{"$error":"#REF!"}},{"$f":"FeuilleproC!D27","v":{"$error":"#REF!"}},null,null,{"$f":"FeuilleproC!AV27","v":{"$error":"#REF!"}},{"$f":"K26*(1-J$9)","v":{"$error":"#REF!"}},{"$f":"F26*I26","v":{"$error":"#REF!"}}]
[null,null,null,{"$f":"FeuilleproC!B28","v":{"$error":"#REF!"}},{"$f":"FeuilleproC!C28","v":{"$error":"#REF!"}},{"$f":"FeuilleproC!D28","v":{"$error":"#REF!"}},null,null,{"$f":"FeuilleproC!AV28","v":{"$error":"#REF!"}},{"$f":"K27*(1-J$9)","v":{"$error":"#REF!"}},{"$f":"F27*I27","v":{"$error":"#REF!"}}]
[null,null,null,{"$f":"FeuilleproC!B29","v":{"$error":"#REF!"}},{"$f":"FeuilleproC!C29","v":{"$error":"#REF!"}},{"$f":"FeuilleproC!D29","v":{"$error":"#REF!"}},null,null,{"$f":"FeuilleproC!AV29","v":{"$error":"#REF!"}},{"$f":"K28*(1-J$9)","v":{"$error":"#REF!"}},{"$f":"F28*I28","v":{"$error":"#REF!"}}]
[null,null,null,{"$f":"FeuilleproC!B30","v":{"$error":"#REF!"}},{"$f":"FeuilleproC!C30","v":{"$error":"#REF!"}},{"$f":"FeuilleproC!D30","v":{"$error":"#REF!"}},null,null,{"$f":"FeuilleproC!AV30","v":{"$error":"#REF!"}},{"$f":"K29*(1-J$9)","v":{"$error":"#REF!"}},{"$f":"IF(I29=0,0,F29*I29)","v":{"$error":"#REF!"}}]
[]
[]
[null,"Attention ! Lorsque vous modifiez une des sélections, il faut toujours revalider les suivantes ! "]
[]
[null,null,null,"►ELEMENTS DE POSE SUR TOIT OU TERRASSE  "]
[]
[null,null,"Montage ","sur toiture"]
[]
[]
[]
[null,null,null,"• Profilés à choisir en fonction du montage capteurs souhaité"]
[null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m",{"$f":"IF(AND(G20>4,D41=\"Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m \"),\"Type de profilé incompatible avec le nombre de capteur !\",\"\")","v":""}]
[]
[null,null,null,{"$f":"FeuilleproC!B77","v":{"$error":"#N/A"}},{"$f":"FeuilleproC!C77","v":{"$error":"#N/A"}},{"$f":"FeuilleproC!D77","v":{"$error":"#N/A"}},null,null,{"$f":"FeuilleproC!AV77","v":0},{"$f":"K43*(1-J$9)","v":{"$error":"#N/A"}},{"$f":"IF(I43<>\"IMPOSSIBLE\",F43*I43,\"\")","v":{"$error":"#N/A"}}]
[null,null,null,{"$f":"FeuilleproC!B78","v":"KIT COUPLEURS (2 PCES) POUR PROFILES (FIXATION PROFILES JUXTAPOSÉS)"},{"$f":"FeuilleproC!C78","v":"EG307"},{"$f":"FeuilleproC!D78","v":31},null,null,{"$f":"FeuilleproC!AV78","v":0},{"$f":"K44*(1-J$9)","v":0},{"$f":"F44*I44","v":0}]
[null,null,null,{"$f":"FeuilleproC!B79","v":{"$error":"#N/A"}},{"$f":"FeuilleproC!C79","v":{"$error":"#N/A"}},{"$f":"FeuilleproC!D79","v":{"$error":"#N/A"}},null,null,{"$f":"FeuilleproC!AV79","v":0},{"$f":"K45*(1-J$9)","v":{"$error":"#N/A"}},{"$f":"F45*I45","v":{"$error":"#N/A"}}]
[null,null,null,{"$f":"FeuilleproC!B80","v":{"$error":"#N/A"}},{"$f":"FeuilleproC!C80","v":{"$error":"#N/A"}},{"$f":"FeuilleproC!D80","v":{"$error":"#N/A"}},null,null,{"$f":"FeuilleproC!AV80","v":0},{"$f":"K46*(1-J$9)","v":0},{"$f":"IF(I46=0,0,F46*I46)","v":0}]
[null,null,null,{"$f":"FeuilleproC!B81","v":" -"},{"$f":"FeuilleproC!C81","v":" -"},{"$f":"FeuilleproC!D81","v":" -"},null,null,{"$f":"FeuilleproC!AV81","v":0},{"$f":"K47*(1-J$9)","v":0},{"$f":"IF(I47<>0,F47*I47,0)","v":0}]
[]
[]
[null,null,null,"• Supports inclinables pour montage sur TERRASSE (ou au sol) "]
[null,null,null,"à choisir selon la disposition des capteurs en + des profilés"]
[]
[null,null,null,{"$f":"IF(D36=\"sur toiture\",\"\",FeuilleproC!B104)","v":""},{"$f":"IF(D36=\"sur toiture\",\"\",FeuilleproC!C104)","v":""},{"$f":"IF(D36=\"sur toiture\",\"\",FeuilleproC!D104)","v":""},null,null,{"$f":"IF(E53=\"\",\"\",FeuilleproC!AV104)","v":""},{"$f":"K53*(1-J$9)","v":0},{"$f":"IF(I53=\"\",0,F53*I53)","v":0}]
[null,null,null,{"$f":"IF(D36=\"sur toiture\",\"\",FeuilleproC!B105)","v":""},{"$f":"IF(D36=\"sur toiture\",\"\",FeuilleproC!C105)","v":""},{"$f":"IF(D36=\"sur toiture\",\"\",FeuilleproC!D105)","v":""},null,null,{"$f":"IF(E54=\"\",\"\",FeuilleproC!AV105)","v":""},{"$f":"K54*(1-J$9)","v":0},{"$f":"IF(OR(I54=\"\",I54=\" - \"),0,F54*I54)","v":0}]
[]
[null,"Attention ! Lorsque vous modifiez une des sélections, il faut toujours revalider les suivantes ! "]
[]
[null,null,null,"• Ferrures d’ancrage pour montage sur TOITURE  "]
[null,null,null," à choisir selon le type de couverture en + des profilés"]
[null,null,null,"montage sur chevrons en inox sur toit éternit",{"$f":"FeuilleproC!D122","v":"4 pces EG 317"},null,{"$f":"IF(D60<>\"\",76.5,\"\")","v":76.5},null,{"$f":"IF(E60=\"\",\"\",FeuilleproC!AV122)","v":0},{"$f":"K60*(1-J$9)","v":0},{"$f":"IF(I60=\"\",0,G60*I60)","v":0}]
[null,null,null,null,{"$f":"FeuilleproC!D123","v":"6 pces EG 318"},null,{"$f":"IF(D60<>\"\",110.2,\"\")","v":110.2},null,{"$f":"IF(E61=\"\",\"\",FeuilleproC!AV123)","v":0},{"$f":"K61*(1-J$9)","v":0},{"$f":"IF(I61=\"\",0,G61*I61)","v":0}]
[null,"Chiffrage"]
[]
[]
[null,null,null,"Système PRO C complet",null,"Prix total HT"]
[null,null,null,"Ensemble capteurs, fixations, raccords hydrauliques ",null,{"$f":"J20+J21+J22+J26+J27+J28+J29+J43+J44+J45+J46+J47+J53+J54+J60+J61","v":{"$error":"#N/A"}}]

{"sheet":"FeuilleproC","index":4,"n_rows":129,"n_cols":48,"rows_kept":129,"cut":false,"hidden":true,"merged":[[0,0,1,0],[0,15,1,15],[0,31,1,31],[34,33,35,33],[34,1,35,1],[34,17,35,17]]}
["1ere ligne",null,null,"nbr capteur par rangée","nbre rangée","nbre colis","nbre colis final","nbre colis arrondi",null,null,null,null,null,null,null,"2eme ligne",null,null,null,"nbr capteur par rangée","nbre rangée","nbre colis","nbre colis final","nbre colis arrondi",null,null,null,null,null,null,null,"3eme ligne",null,null,null,"nbr capteur par rangée","nbre rangée","nbre colis","nbre colis final","nbre colis arrondi"]
[null,null,null,{"$f":"'Pro C '!G20","v":0},{"$f":"'Pro C '!H20","v":0},{"$f":"'Pro C '!I20","v":0},null,{"$f":"ROUND(F2,0)","v":0},null,null,null,"liste vertical",0,null,null,null,null,null,null,{"$f":"'Pro C '!G21","v":0},{"$f":"'Pro C '!H21","v":0},{"$f":"'Pro C '!I21","v":0},null,{"$f":"ROUND(V2,0)","v":0},null,null,null,"liste vertical",1,null,null,null,null,null,null,{"$f":"'Pro C '!G22","v":0},{"$f":"'Pro C '!H22","v":0},{"$f":"'Pro C '!I22","v":0},null,null,null,null,null,"liste vertical",1]
[null,"montage",{"$f":"'Pro C '!D12","v":"vertical"},null,null,null,null,null,null,null,null,null,1,null,null,null,null,"montage",{"$f":"'Pro C '!T12","v":0},null,null,null,null,null,null,null,null,null,2,null,null,null,null,"montage",{"$f":"'Pro C '!AJ12","v":0},null,null,null,null,null,null,null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3]
[null,"►ACCESSOIRES POUR RACCORDEMENT HYDRAULIQUE",null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,"►ACCESSOIRES POUR RACCORDEMENT HYDRAULIQUE",null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,"►ACCESSOIRES POUR RACCORDEMENT HYDRAULIQUE",null,null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5]
["liste validation","Raccordement des capteurs en montage vertical juxtaposés ou horizontal superposés",null,null,null,null,null,null,null,null,null,null,5,null,null,null,"liste validation","Raccordement des capteurs en montage vertical juxtaposés ou horizontal superposés",null,null,null,null,null,null,null,null,null,null,6,null,null,null,"liste validation","Raccordement des capteurs en montage vertical juxtaposés ou horizontal superposés",null,null,null,null,null,null,null,null,null,null,6]
["\"accessoireshydrau\"","Raccordement des capteurs en montage horizontal juxtaposés",null,null,null,null,null,null,null,null,null,null,6,null,null,null,"\"accessoireshydrau\"","Raccordement des capteurs en montage horizontal juxtaposés",null,null,null,null,null,null,null,null,null,null,7,null,null,null,"\"accessoireshydrau\"","Raccordement des capteurs en montage horizontal juxtaposés",null,null,null,null,null,null,null,null,null,null,7]
[null,null,null,null,null,null,null,null,null,null,null,null,7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8]
[null,null,null,null,null,null,null,"nbre colis arrondi",null,"REF",null,null,8,null,null,null,null,null,null,null,null,null,null,"nbre colis arrondi",null,"REF",null,null,null,null,null,null,null,null,null,null,null,null,null,"nbre colis arrondi",null,"REF"]
["1ere ligne","Raccordement des capteurs en montage vertical juxtaposés ou horizontal superposés",{"$f":"VLOOKUP(J11,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J11,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J11,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},1,{"$f":"F11*E2","v":0},{"$f":"ROUNDUP(G11,0)","v":0},null,89807345,null,null,null,null,null,null,"1ere ligne","Raccordement des capteurs en montage vertical juxtaposés ou horizontal superposés",{"$f":"VLOOKUP(Z11,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z11,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z11,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},1,{"$f":"V11*U2","v":0},{"$f":"ROUNDUP(W11,0)","v":0},null,89807345,null,null,null,null,null,null,"1ere ligne","Raccordement des capteurs en montage vertical juxtaposés ou horizontal superposés",{"$f":"VLOOKUP(AP11,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP11,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP11,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},1,{"$f":"AL11*AK2","v":0},{"$f":"ROUNDUP(AM11,0)","v":0},null,89807345]
[null,"Raccordement des capteurs en montage horizontal juxtaposés",{"$f":"VLOOKUP(J12,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J12,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J12,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},1,{"$f":"F12*E2","v":0},{"$f":"ROUNDUP(G12,0)","v":0},null,89807345,null,"liste horizontal",0,null,null,null,null,"Raccordement des capteurs en montage horizontal juxtaposés",{"$f":"VLOOKUP(Z12,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z12,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z12,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},1,{"$f":"V12*U2","v":0},{"$f":"ROUNDUP(W12,0)","v":0},null,89807345,null,"liste horizontal",1,null,null,null,null,"Raccordement des capteurs en montage horizontal juxtaposés",{"$f":"VLOOKUP(AP12,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP12,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP12,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},1,{"$f":"AL12*AK2","v":0},{"$f":"ROUNDUP(AM12,0)","v":0},null,89807345,null,"liste horizontal",1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2]
["2em ligne","Raccordement des capteurs en montage vertical juxtaposés ou horizontal superposés",{"$f":"VLOOKUP(J14,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J14,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J14,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},0.2,{"$f":"F14*E2","v":0},0,null,89807347,null,null,2,null,null,null,"2em ligne","Raccordement des capteurs en montage vertical juxtaposés ou horizontal superposés",{"$f":"VLOOKUP(Z14,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z14,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z14,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},0.2,{"$f":"V14*U2","v":0},0,null,89807347,null,null,3,null,null,null,"2em ligne","Raccordement des capteurs en montage vertical juxtaposés ou horizontal superposés",{"$f":"VLOOKUP(AP14,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP14,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP14,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},0.2,{"$f":"AL14*AK2","v":0},0,null,89807347,null,null,3]
[null,"Raccordement des capteurs en montage horizontal juxtaposés",{"$f":"VLOOKUP(J15,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J15,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J15,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"D2-1","v":-1},{"$f":"F15*E2","v":0},0,null,89807366,null,null,3,null,null,null,null,"Raccordement des capteurs en montage horizontal juxtaposés",{"$f":"VLOOKUP(Z15,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z15,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z15,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"T2-1","v":-1},{"$f":"V15*U2","v":0},0,null,89807366,null,null,4,null,null,null,null,"Raccordement des capteurs en montage horizontal juxtaposés",{"$f":"VLOOKUP(AP15,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP15,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP15,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"AJ2-1","v":-1},{"$f":"AL15*AK2","v":0},0,null,89807366,null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5]
["3eme ligne","Raccordement des capteurs en montage vertical juxtaposés ou horizontal superposés",{"$f":"VLOOKUP(J17,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J17,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J17,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(D2=1,0,IF(D2=2,0.2,IF(D2=3,0.4,IF(D2=4,0.6,IF(D2=5,0.6,IF(D2=6,0.8,IF(D2=7,1,IF(D2=8,1.2))))))))","v":false},{"$f":"F17*E2","v":0},0,null,89807346,null,null,null,null,null,null,"3eme ligne","Raccordement des capteurs en montage vertical juxtaposés ou horizontal superposés",{"$f":"VLOOKUP(Z17,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z17,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z17,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(T2=1,0,IF(T2=2,0.2,IF(T2=3,0.4,IF(T2=4,0.6,IF(T2=5,0.6,IF(T2=6,0.8,IF(T2=7,1,IF(T2=8,1.2))))))))","v":false},{"$f":"V17*U2","v":0},0,null,89807346,null,null,6,null,null,null,"3eme ligne","Raccordement des capteurs en montage vertical juxtaposés ou horizontal superposés",{"$f":"VLOOKUP(AP17,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP17,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP17,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(AJ2=1,0,IF(AJ2=2,0.2,IF(AJ2=3,0.4,IF(AJ2=4,0.6,IF(AJ2=5,0.6,IF(AJ2=6,0.8,IF(AJ2=7,1,IF(AJ2=8,1.2))))))))","v":false},{"$f":"AL17*AK2","v":0},0,null,89807346,null,null,6]
[null,"Raccordement des capteurs en montage horizontal juxtaposés",{"$f":"VLOOKUP(J18,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J18,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J18,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"D2*0.2","v":0},{"$f":"F18*E2","v":0},0,null,89807347,null,null,null,null,null,null,null,"Raccordement des capteurs en montage horizontal juxtaposés",{"$f":"VLOOKUP(Z18,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z18,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z18,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"T2*0.2","v":0},{"$f":"V18*U2","v":0},0,null,89807347,null,null,null,null,null,null,null,"Raccordement des capteurs en montage horizontal juxtaposés",{"$f":"VLOOKUP(AP18,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP18,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP18,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"AJ2*0.2","v":0},{"$f":"AL18*AK2","v":0},0,null,89807347]
[]
["4 eme ligne","Raccordement des capteurs en montage vertical juxtaposés ou horizontal superposés",{"$f":"VLOOKUP(J20,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J20,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J20,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(D2>=5,1,0)","v":0},{"$f":"F20*E2","v":0},0,null,89807372,null,null,null,null,null,null,"4 eme ligne","Raccordement des capteurs en montage vertical juxtaposés ou horizontal superposés",{"$f":"VLOOKUP(Z20,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z20,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z20,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(T2>=5,1,0)","v":0},{"$f":"V20*U2","v":0},0,null,89807372,null,null,null,null,null,null,"4 eme ligne","Raccordement des capteurs en montage vertical juxtaposés ou horizontal superposés",{"$f":"VLOOKUP(AP20,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP20,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP20,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(AJ2>=5,1,0)","v":0},{"$f":"AL20*AK2","v":0},0,null,89807372]
[null,"Raccordement des capteurs en montage horizontal juxtaposés"," - "," - "," - ","-","-",0,null,null,null,null,null,null,null,null,null,"Raccordement des capteurs en montage horizontal juxtaposés"," - "," - "," - ","-","-",0,null,null,null,null,null,null,null,null,null,"Raccordement des capteurs en montage horizontal juxtaposés"," - "," - ",0,"-","-",0]
[]
[]
["RECAPITULATION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RECAPITULATION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RECAPITULATION"]
["choix",{"$f":"'Pro C '!#REF!","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"choix",{"$f":"'Pro C '!#REF!","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"choix",{"$f":"'Pro C '!#REF!","v":{"$error":"#REF!"}}]
[null,null,null,null,"nbre colis arronndi",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"nbre colis arronndi",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"nbre colis arronndi"]
["1ere ligne",{"$f":"VLOOKUP(B25,B11:C12,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(B27,C11:D15,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(C27,D11:E15,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(B25,B11:H12,7,FALSE)","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,null,"1ere ligne",{"$f":"VLOOKUP(R25,R11:S12,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(R27,S11:T15,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(S27,T11:U15,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(R25,R11:X12,7,FALSE)","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,null,"1ere ligne",{"$f":"VLOOKUP(AH25,AH11:AI12,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(AH27,AI11:AJ15,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(AI27,AJ11:AK15,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(AH25,AH11:AN12,7,FALSE)","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,{"$f":"AK27+U27+E27","v":{"$error":"#REF!"}}]
["2em ligne",{"$f":"VLOOKUP(B25,B14:C15,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(B28,C14:D18,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(C28,D14:E18,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(B25,B14:H15,7,FALSE)","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,null,"2em ligne",{"$f":"VLOOKUP(R25,R14:S15,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(R28,S14:T18,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(S28,T14:U18,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(R25,R14:X15,7,FALSE)","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,null,"2em ligne",{"$f":"VLOOKUP(AH25,AH14:AI15,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(AH28,AI14:AJ18,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(AI28,AJ14:AK18,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(AH25,AH14:AN15,7,FALSE)","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,{"$f":"AK28+U28+E28","v":{"$error":"#REF!"}}]
["3eme ligne",{"$f":"VLOOKUP(B25,B17:C18,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(B29,C17:D18,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(C29,D17:E18,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(B25,B17:H18,7,FALSE)","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,null,"3eme ligne",{"$f":"VLOOKUP(R25,R17:S18,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(R29,S17:T18,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(S29,T17:U18,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(R25,R17:X18,7,FALSE)","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,null,"3eme ligne",{"$f":"VLOOKUP(AH25,AH17:AI18,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(AH29,AI17:AJ18,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(AI29,AJ17:AK18,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(AH25,AH17:AN18,7,FALSE)","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,{"$f":"AK29+U29+E29","v":{"$error":"#REF!"}}]
["4 eme ligne",{"$f":"VLOOKUP(B25,B20:C21,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(B30,C20:D21,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(C30,D20:E21,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(B25,B20:H21,7,FALSE)","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,null,"4 eme ligne",{"$f":"VLOOKUP(R25,R20:S21,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(R30,S20:T21,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(S30,T20:U21,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(R25,R20:X21,7,FALSE)","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,null,"4 eme ligne",{"$f":"VLOOKUP(AH25,AH20:AI21,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(AH30,AI20:AJ21,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(AI30,AJ20:AK21,2,FALSE)","v":{"$error":"#REF!"}},{"$f":"VLOOKUP(AH25,AH20:AN21,7,FALSE)","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,{"$f":"AK30+U30+E30","v":{"$error":"#REF!"}}]
[]
[]
[]
[]
[null,"►ELEMENTS DE POSE SUR TOIT OU TERRASSE  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"►ELEMENTS DE POSE SUR TOIT OU TERRASSE  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"►ELEMENTS DE POSE SUR TOIT OU TERRASSE  "]
[]
[]
["liste validation","Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"liste validation","Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"liste validation","Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m "]
["\"montagevertihori\"","Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"\"montagevertihori\"","Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"\"montagevertihori\"","Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m"]
[null,"Montage vertical juxt. ou horizontal superposés sur profilés de 2,6 m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 2,6 m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 2,6 m"]
[]
[]
[]
["liste validation","Montage HORIZONTAL juxtaposés ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"liste validation","Montage HORIZONTAL juxtaposés ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"liste validation","Montage HORIZONTAL juxtaposés "]
["\"montagehori\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"\"montagehori\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"\"montagehori\""]
[]
[null,null,null,null,null,null,"nbre colis final","nbre colis arrondi",null,"Ref",null,null,null,null,null,null,null,null,null,null,null,null,"nbre colis final","nbre colis arrondi",null,"Ref",null,null,null,null,null,null,null,null,null,null,null,null,"nbre colis final","nbre colis arrondi",null,"Ref"]
["1ere ligne","Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m ",{"$f":"VLOOKUP(J48,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J48,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J48,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(D2<=4,D2,\"faux\")","v":0},{"$f":"IF(F48<>\"faux\",F48*E2,\"IMPOSSIBLE\")","v":0},{"$f":"G48","v":0},null,100008015,null,null,null,null,null,null,"1ere ligne","Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m ",{"$f":"VLOOKUP(Z48,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z48,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z48,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(T2<=4,T2,\"faux\")","v":0},{"$f":"IF(V48<>\"faux\",V48*U2,\"IMPOSSIBLE\")","v":0},{"$f":"W48","v":0},null,100008015,null,null,null,null,null,null,"1ere ligne","Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m ",{"$f":"VLOOKUP(AP48,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP48,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP48,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(AJ2<=4,AJ2,\"faux\")","v":0},{"$f":"IF(AL48<>\"faux\",AL48*AK2,\"IMPOSSIBLE\")","v":0},{"$f":"AM48","v":0},null,100008015]
[null,"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m",{"$f":"VLOOKUP(J49,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J49,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J49,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(D2=2,0.2,IF(D2=3,0.4,IF(D2=4,0.5,IF(D2=5,0.6,IF(D2=6,0.8,IF(D2=7,0.9,IF(D2=8,1,\"faux\")))))))","v":"faux"},{"$f":"IF(F49=\"faux\",0,F49*E2)","v":0},{"$f":"ROUNDUP(G49,0)","v":0},null,89807357,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m",{"$f":"VLOOKUP(Z49,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z49,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z49,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(T2=2,0.2,IF(T2=3,0.4,IF(T2=4,0.5,IF(T2=5,0.6,IF(T2=6,0.8,IF(T2=7,0.9,IF(T2=8,1,\"faux\")))))))","v":"faux"},{"$f":"IF(V49=\"faux\",0,V49*U2)","v":0},{"$f":"ROUNDUP(W49,0)","v":0},null,89807357,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m",{"$f":"VLOOKUP(AP49,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP49,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP49,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(AJ2=2,0.2,IF(AJ2=3,0.4,IF(AJ2=4,0.5,IF(AJ2=5,0.6,IF(AJ2=6,0.8,IF(AJ2=7,0.9,IF(AJ2=8,1,\"faux\")))))))","v":"faux"},{"$f":"IF(AL49=\"faux\",0,AL49*AK2)","v":0},{"$f":"ROUNDUP(AM49,0)","v":0},null,89807357]
[null,"Montage vertical juxt. ou horizontal superposés sur profilés de 2,6 m",{"$f":"VLOOKUP(J50,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J50,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J50,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(D2=2,0.5,IF(D2=3,0.75,IF(D2=4,1,IF(D2=5,1.25,IF(D2=6,1.5,IF(D2=7,1.75,IF(D2=8,2)))))))","v":false},{"$f":"F50*E2","v":0},0,null,89807356,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 2,6 m",{"$f":"VLOOKUP(Z50,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z50,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z50,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(T2=2,0.5,IF(T2=3,0.75,IF(T2=4,1,IF(T2=5,1.25,IF(T2=6,1.5,IF(T2=7,1.75,IF(T2=8,2)))))))","v":false},{"$f":"V50*U2","v":0},0,null,89807356,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 2,6 m",{"$f":"VLOOKUP(AP50,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP50,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP50,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(AJ2=2,0.5,IF(AJ2=3,0.75,IF(AJ2=4,1,IF(AJ2=5,1.25,IF(AJ2=6,1.5,IF(AJ2=7,1.75,IF(AJ2=8,2)))))))","v":false},{"$f":"AL50*AK2","v":0},0,null,89807356]
[null,"Montage HORIZONTAL juxtaposés ",{"$f":"VLOOKUP(J51,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J51,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J51,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(D2<4,1,2)","v":1},{"$f":"F51*E2","v":0},0,null,89807357,null,null,null,null,null,null,null,"Montage HORIZONTAL juxtaposés ",{"$f":"VLOOKUP(Z51,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z51,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z51,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(T2<4,1,2)","v":1},{"$f":"V51*U2","v":0},0,null,89807357,null,null,null,null,null,null,null,"Montage HORIZONTAL juxtaposés ",{"$f":"VLOOKUP(AP51,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP51,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP51,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(AJ2<4,1,2)","v":1},{"$f":"AL51*AK2","v":0},0,null,89807357]
[]
["2eme ligne","Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m ",{"$f":"VLOOKUP(J53,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J53,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J53,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"D2*0.2","v":0},{"$f":"IF(F53<>\"faux\",F53*E2,0)","v":0},0,null,89807348,null,null,null,null,null,null,"2eme ligne","Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m ",{"$f":"VLOOKUP(Z53,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z53,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z53,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"T2*0.2","v":0},{"$f":"IF(V53<>\"faux\",V53*U2,0)","v":0},0,null,89807348,null,null,null,null,null,null,"2eme ligne","Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m ",{"$f":"VLOOKUP(AP53,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP53,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP53,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"AJ2*0.2","v":0},{"$f":"IF(AL53<>\"faux\",AL53*AK2,0)","v":0},0,null,89807348]
[null,"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m",{"$f":"VLOOKUP(J54,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT COUPLEURS (2 PCES) POUR PROFILES (FIXATION PROFILES JUXTAPOSÉS)"},{"$f":"VLOOKUP(J54,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG307"},{"$f":"VLOOKUP(J54,'Liste de prix'!$1:$1048576,4,FALSE)","v":31},{"$f":"IF(D2<5,\"faux\",1)","v":"faux"},{"$f":"IF(F54<>\"faux\",F54*E2,0)","v":0},0,null,89807307,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m",{"$f":"VLOOKUP(Z54,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT COUPLEURS (2 PCES) POUR PROFILES (FIXATION PROFILES JUXTAPOSÉS)"},{"$f":"VLOOKUP(Z54,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG307"},{"$f":"VLOOKUP(Z54,'Liste de prix'!$1:$1048576,4,FALSE)","v":31},{"$f":"IF(T2<5,\"faux\",1)","v":"faux"},{"$f":"IF(V54<>\"faux\",V54*U2,0)","v":0},0,null,89807307,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m",{"$f":"VLOOKUP(AP54,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT COUPLEURS (2 PCES) POUR PROFILES (FIXATION PROFILES JUXTAPOSÉS)"},{"$f":"VLOOKUP(AP54,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG307"},{"$f":"VLOOKUP(AP54,'Liste de prix'!$1:$1048576,4,FALSE)","v":31},{"$f":"IF(AJ2<5,\"faux\",1)","v":"faux"},{"$f":"IF(AL54<>\"faux\",AL54*AK2,0)","v":0},0,null,89807307]
[null,"Montage vertical juxt. ou horizontal superposés sur profilés de 2,6 m",{"$f":"VLOOKUP(J55,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT COUPLEURS (2 PCES) POUR PROFILES (FIXATION PROFILES JUXTAPOSÉS)"},{"$f":"VLOOKUP(J55,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG307"},{"$f":"VLOOKUP(J55,'Liste de prix'!$1:$1048576,4,FALSE)","v":31},{"$f":"IF(D2=2,0,IF(D2=3,1,IF(D2=4,1,IF(D2=5,2,IF(D2=6,2,IF(D2=7,3,IF(D2=8,3)))))))","v":false},{"$f":"F55*E2","v":0},0,null,89807307,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 2,6 m",{"$f":"VLOOKUP(Z55,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT COUPLEURS (2 PCES) POUR PROFILES (FIXATION PROFILES JUXTAPOSÉS)"},{"$f":"VLOOKUP(Z55,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG307"},{"$f":"VLOOKUP(Z55,'Liste de prix'!$1:$1048576,4,FALSE)","v":31},{"$f":"IF(T2=2,0,IF(T2=3,1,IF(T2=4,1,IF(T2=5,2,IF(T2=6,2,IF(T2=7,3,IF(T2=8,3)))))))","v":false},{"$f":"V55*U2","v":0},0,null,89807307,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 2,6 m",{"$f":"VLOOKUP(AP55,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT COUPLEURS (2 PCES) POUR PROFILES (FIXATION PROFILES JUXTAPOSÉS)"},{"$f":"VLOOKUP(AP55,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG307"},{"$f":"VLOOKUP(AP55,'Liste de prix'!$1:$1048576,4,FALSE)","v":31},{"$f":"IF(AJ2=2,0,IF(AJ2=3,1,IF(AJ2=4,1,IF(AJ2=5,2,IF(AJ2=6,2,IF(AJ2=7,3,IF(AJ2=8,3)))))))","v":false},{"$f":"AL55*AK2","v":0},0,null,89807307]
[null,"Montage HORIZONTAL juxtaposés ",{"$f":"VLOOKUP(J56,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J56,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J56,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(D2=3,1,FALSE)","v":false},{"$f":"F56*E2","v":0},0,null,89807356,null,null,null,null,null,null,null,"Montage HORIZONTAL juxtaposés ",{"$f":"VLOOKUP(Z56,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z56,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z56,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(T2=3,1,FALSE)","v":false},{"$f":"V56*U2","v":0},0,null,89807356,null,null,null,null,null,null,null,"Montage HORIZONTAL juxtaposés ",{"$f":"VLOOKUP(AP56,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP56,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP56,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(AJ2=3,1,FALSE)","v":false},{"$f":"AL56*AK2","v":0},0,null,89807356]
[]
["3eme ligne","Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m ",{"$f":"VLOOKUP(J58,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J58,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J58,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"D2*0.2","v":0},{"$f":"IF(F58<>\"faux\",F58*E2,0)","v":0},0,null,89807365,null,null,null,null,null,null,"3eme ligne","Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m ",{"$f":"VLOOKUP(Z58,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z58,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z58,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"T2*0.2","v":0},{"$f":"IF(V58<>\"faux\",V58*U2,0)","v":0},0,null,89807365,null,null,null,null,null,null,"3eme ligne","Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m ",{"$f":"VLOOKUP(AP58,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP58,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP58,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"AJ2*0.2","v":0},{"$f":"IF(AL58<>\"faux\",AL58*AK2,0)","v":0},0,null,89807365]
[null,"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m",{"$f":"VLOOKUP(J59,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J59,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J59,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"D2*0.2","v":0},{"$f":"F59*E2","v":0},0,null,89807348,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m",{"$f":"VLOOKUP(Z59,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z59,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z59,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"T2*0.2","v":0},{"$f":"V59*U2","v":0},0,null,89807348,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m",{"$f":"VLOOKUP(AP59,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP59,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP59,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"AJ2*0.2","v":0},{"$f":"AL59*AK2","v":0},0,null,89807348]
[null,"Montage vertical juxt. ou horizontal superposés sur profilés de 2,6 m",{"$f":"VLOOKUP(J60,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J60,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J60,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"0.2*D2","v":0},{"$f":"F60*E2","v":0},0,null,89807348,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 2,6 m",{"$f":"VLOOKUP(Z60,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z60,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z60,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"0.2*T2","v":0},{"$f":"V60*U2","v":0},0,null,89807348,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 2,6 m",{"$f":"VLOOKUP(AP60,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP60,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP60,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"0.2*AJ2","v":0},{"$f":"AL60*AK2","v":0},0,null,89807348]
[null,"Montage HORIZONTAL juxtaposés ",{"$f":"VLOOKUP(J61,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT COUPLEURS (2 PCES) POUR PROFILES (FIXATION PROFILES JUXTAPOSÉS)"},{"$f":"VLOOKUP(J61,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG307"},{"$f":"VLOOKUP(J61,'Liste de prix'!$1:$1048576,4,FALSE)","v":31},{"$f":"IF(D2=3,1,IF(D2=4,1,0))","v":0},{"$f":"F61*E2","v":0},0,null,89807307,null,null,null,null,null,null,null,"Montage HORIZONTAL juxtaposés ",{"$f":"VLOOKUP(Z61,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT COUPLEURS (2 PCES) POUR PROFILES (FIXATION PROFILES JUXTAPOSÉS)"},{"$f":"VLOOKUP(Z61,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG307"},{"$f":"VLOOKUP(Z61,'Liste de prix'!$1:$1048576,4,FALSE)","v":31},{"$f":"IF(T2=3,1,IF(T2=4,1,0))","v":0},{"$f":"V61*U2","v":0},0,null,89807307,null,null,null,null,null,null,null,"Montage HORIZONTAL juxtaposés ",{"$f":"VLOOKUP(AP61,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT COUPLEURS (2 PCES) POUR PROFILES (FIXATION PROFILES JUXTAPOSÉS)"},{"$f":"VLOOKUP(AP61,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG307"},{"$f":"VLOOKUP(AP61,'Liste de prix'!$1:$1048576,4,FALSE)","v":31},{"$f":"IF(AJ2=3,1,IF(AJ2=4,1,0))","v":0},{"$f":"AL61*AK2","v":0},0,null,89807307]
[]
["4eme ligne","Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m "," - "," -"," -","-",0,0,null,null,null,null,null,null,null,null,"4eme ligne","Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m "," - "," -"," -","-","-",0,null,null,null,null,null,null,null,null,"4eme ligne","Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m "," - "," -"," -","-",0,0]
[null,"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m",{"$f":"VLOOKUP(J64,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J64,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J64,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"D2*0.2","v":0},{"$f":"F64*E2","v":0},0,null,89807365,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m",{"$f":"VLOOKUP(Z64,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z64,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z64,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"T2*0.2","v":0},{"$f":"V64*U2","v":0},0,null,89807365,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m",{"$f":"VLOOKUP(AP64,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP64,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP64,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"AJ2*0.2","v":0},{"$f":"AL64*AK2","v":0},0,null,89807365]
[null,"Montage vertical juxt. ou horizontal superposés sur profilés de 2,6 m",{"$f":"VLOOKUP(J65,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J65,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J65,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"0.2*D2","v":0},{"$f":"F65*E2","v":0},0,null,89807365,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 2,6 m",{"$f":"VLOOKUP(Z65,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z65,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z65,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"0.2*T2","v":0},{"$f":"V65*U2","v":0},0,null,89807365,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 2,6 m",{"$f":"VLOOKUP(AP65,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP65,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP65,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"0.2*AJ2","v":0},{"$f":"AL65*AK2","v":0},0,null,89807365]
[null,"Montage HORIZONTAL juxtaposés ",{"$f":"VLOOKUP(J66,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J66,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J66,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"D2*0.2","v":0},{"$f":"F66*E2","v":0},0,null,89807348,null,null,null,null,null,null,null,"Montage HORIZONTAL juxtaposés ",{"$f":"VLOOKUP(Z66,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z66,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z66,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"T2*0.2","v":0},{"$f":"V66*U2","v":0},0,null,89807348,null,null,null,null,null,null,null,"Montage HORIZONTAL juxtaposés ",{"$f":"VLOOKUP(AP66,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP66,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP66,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"AJ2*0.2","v":0},{"$f":"AL66*AK2","v":0},0,null,89807348]
[null,null,null,null," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["5eme ligne","Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m "," -"," -"," -",null,0,0,null,null,null,null,null,null,null,null,"5eme ligne","Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m "," -"," -"," -",null,0,0,null,null,null,null,null,null,null,null,"5eme ligne","Montage vertical juxt. ou horizontal superposés sur profilés de 1,3 m "," -"," -"," -",null,0,0]
[null,"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m"," -"," -"," -",null,0,0,null,null,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m"," -"," -"," -",null,0,0,null,null,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m"," -"," -"," -",null,0,0]
[null,"Montage vertical juxt. ou horizontal superposés sur profilés de 2,6 m"," -"," -"," - ",null,0,0,null,null,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 2,6 m"," -"," -"," - ",null,0,0,null,null,null,null,null,null,null,null,null,"Montage vertical juxt. ou horizontal superposés sur profilés de 2,6 m"," -"," -"," - ",null,0,0]
[null,"Montage HORIZONTAL juxtaposés ",{"$f":"VLOOKUP(J71,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J71,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J71,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"0.2*D2","v":0},{"$f":"F71*E2","v":0},0,null,89807365,null,null,null,null,null,null,null,"Montage HORIZONTAL juxtaposés ",{"$f":"VLOOKUP(Z71,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z71,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Z71,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"0.2*T2","v":0},{"$f":"V71*U2","v":0},0,null,89807365,null,null,null,null,null,null,null,"Montage HORIZONTAL juxtaposés ",{"$f":"VLOOKUP(AP71,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP71,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AP71,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"0.2*AJ2","v":0},{"$f":"AL71*AK2","v":0},0,null,89807365]
[]
[]
["RECAPITULATION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RECAPITULATION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RECAPITULATION"]
["choix",{"$f":"'Pro C '!D41","v":"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"choix",{"$f":"'Pro C '!D41","v":"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"choix",{"$f":"'Pro C '!D41","v":"Montage vertical juxt. ou horizontal superposés sur profilés de 5,2 m"}]
[null,null,null,null,"nbre colis arrondi",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"nbre colis arrondi",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"nbre colis arrondi"]
["1er ligne",{"$f":"VLOOKUP(B75,B48:C51,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(B77,C48:D51,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(C77,D48:E51,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(B75,B48:H51,7,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,"1er ligne",{"$f":"VLOOKUP(R75,R48:S51,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(R77,S48:T51,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(S77,T48:U51,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(R75,R48:X51,7,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,"1er ligne",{"$f":"VLOOKUP(AH75,AH48:AI51,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AH77,AI48:AJ51,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AI77,AJ48:AK51,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AH75,AH48:AN51,7,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,{"$f":"AK77+U77+E77","v":0}]
["2eme ligne",{"$f":"VLOOKUP(B75,B53:C56,2,FALSE)","v":"KIT COUPLEURS (2 PCES) POUR PROFILES (FIXATION PROFILES JUXTAPOSÉS)"},{"$f":"VLOOKUP(B78,C53:D56,2,FALSE)","v":"EG307"},{"$f":"VLOOKUP(C78,D53:E56,2,FALSE)","v":31},{"$f":"VLOOKUP(B75,B53:H56,7,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,"2eme ligne",{"$f":"VLOOKUP(R75,R53:S56,2,FALSE)","v":"KIT COUPLEURS (2 PCES) POUR PROFILES (FIXATION PROFILES JUXTAPOSÉS)"},{"$f":"VLOOKUP(R78,S53:T56,2,FALSE)","v":"EG307"},{"$f":"VLOOKUP(S78,T53:U56,2,FALSE)","v":31},{"$f":"VLOOKUP(R75,R53:X56,7,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,"2eme ligne",{"$f":"VLOOKUP(AH75,AH53:AI56,2,FALSE)","v":"KIT COUPLEURS (2 PCES) POUR PROFILES (FIXATION PROFILES JUXTAPOSÉS)"},{"$f":"VLOOKUP(AH78,AI53:AJ56,2,FALSE)","v":"EG307"},{"$f":"VLOOKUP(AI78,AJ53:AK56,2,FALSE)","v":31},{"$f":"VLOOKUP(AH75,AH53:AN56,7,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,{"$f":"AK78+U78+E78","v":0}]
["3eme",{"$f":"VLOOKUP(B75,B58:C61,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(B79,C58:D61,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(C79,D58:E61,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(B75,B58:H61,7,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,"3eme",{"$f":"VLOOKUP(R75,R58:S61,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(R79,S58:T61,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(S79,T58:U61,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(R75,R58:X61,7,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,"3eme",{"$f":"VLOOKUP(AH75,AH58:AI61,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AH79,AI58:AJ61,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AI79,AJ58:AK61,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AH75,AH58:AN61,7,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,{"$f":"AK79+U79+E79","v":0}]
["4eme",{"$f":"VLOOKUP(B75,B63:C66,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(B80,C63:D66,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(C80,D63:E66,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(B75,B63:H66,7,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,"4eme",{"$f":"VLOOKUP(R75,R63:S66,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(R80,S63:T66,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(S80,T63:U66,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(R75,R63:X66,7,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,"4eme",{"$f":"VLOOKUP(AH75,AH63:AI66,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AH80,AI63:AJ66,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AI80,AJ63:AK66,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AH75,AH63:AN66,7,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,{"$f":"AK80+U80+E80","v":0}]
["5eme",{"$f":"VLOOKUP(B75,B68:C71,2,FALSE)","v":" -"},{"$f":"VLOOKUP(B81,C68:D71,2,FALSE)","v":" -"},{"$f":"VLOOKUP(C81,D68:E71,2,FALSE)","v":" -"},{"$f":"VLOOKUP(B75,B68:H71,7,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,"5eme",{"$f":"VLOOKUP(R75,R68:S71,2,FALSE)","v":" -"},{"$f":"VLOOKUP(R81,S68:T71,2,FALSE)","v":" -"},{"$f":"VLOOKUP(S81,T68:U71,2,FALSE)","v":" -"},{"$f":"VLOOKUP(R75,R68:X71,7,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,"5eme",{"$f":"VLOOKUP(AH75,AH68:AI71,2,FALSE)","v":" -"},{"$f":"VLOOKUP(AH81,AI68:AJ71,2,FALSE)","v":" -"},{"$f":"VLOOKUP(AI81,AJ68:AK71,2,FALSE)","v":" -"},{"$f":"VLOOKUP(AH75,AH68:AN71,7,FALSE)","v":0}]
[]
[]
["terrasse",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"terrasse",null,"vertical",null,null,null,null,null,null,null,null,null,null,null,null,null,"terrasse",null,"vertical"]
["sur toiture",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sur toiture",null,"horizontal",null,null,null,null,null,null,null,null,null,null,null,null,null,"sur toiture",null,"horizontal"]
[]
["choix",{"$f":"'Pro C '!D36","v":"sur toiture"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"choix",{"$f":"'Pro C '!D36","v":"sur toiture"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"choix",{"$f":"'Pro C '!D36","v":"sur toiture"}]
["verti ou hori",{"$f":"'SUN C250'!E39","v":"sur toiture"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"verti ou hori",{"$f":"'SUN C250'!E39","v":"sur toiture"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"verti ou hori",{"$f":"'SUN C250'!E39","v":"sur toiture"}]
[]
[]
[]
[]
[]
[null,"• Supports inclinables pour TERRASSE (ou au sol) ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"• Supports inclinables pour TERRASSE (ou au sol) ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"• Supports inclinables pour TERRASSE (ou au sol) "]
[null,"à choisir selon la disposition des capteurs en + des profilés",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"à choisir selon la disposition des capteurs en + des profilés",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"à choisir selon la disposition des capteurs en + des profilés"]
[null,null,null,null,null,"nbre colis final","nbre colis arrondi","Ref",null,null,null,null,null,null,null,null,null,null,null,null,null,"nbre colis final","nbre colis arrondi","Ref",null,null,null,null,null,null,null,null,null,null,null,null,null,"nbre colis final","nbre colis arrondi","Ref"]
["terrasse et vertical","3 supports avec croix stabilisatrices pour 2 capt. montage vertical",{"$f":"VLOOKUP(H97,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG358"},{"$f":"VLOOKUP(H97,'Liste de prix'!$1:$1048576,4,FALSE)","v":287},{"$f":"IF(D2=0,0,IF(D2<5,1,2))","v":0},{"$f":"E97*E2","v":0},{"$f":"ROUNDUP(F97,0)","v":0},89807358,null,null,null,null,null,null,null,null,"terrasse et vertical","3 supports avec croix stabilisatrices pour 2 capt. montage vertical",{"$f":"VLOOKUP(X97,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG358"},{"$f":"VLOOKUP(X97,'Liste de prix'!$1:$1048576,4,FALSE)","v":287},{"$f":"IF(T2=0,0,IF(T2<5,1,2))","v":0},{"$f":"U97*U2","v":0},{"$f":"ROUNDUP(V97,0)","v":0},89807358,null,null,null,null,null,null,null,null,"terrasse et vertical","3 supports avec croix stabilisatrices pour 2 capt. montage vertical",{"$f":"VLOOKUP(AN97,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG358"},{"$f":"VLOOKUP(AN97,'Liste de prix'!$1:$1048576,4,FALSE)","v":287},{"$f":"IF(AJ2=0,0,IF(AJ2<5,1,2))","v":0},{"$f":"AK97*AK2","v":0},{"$f":"ROUNDUP(AL97,0)","v":0},89807358]
[null,"3 supports (sans croix stabilisatrices) pour 2 capt. montage vertical",{"$f":"VLOOKUP(H98,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG359"},{"$f":"VLOOKUP(H98,'Liste de prix'!$1:$1048576,4,FALSE)","v":245},{"$f":"IF(D2=2,0,IF(D2=3,1,IF(D2=4,1,IF(D2=5,1,IF(D2=6,1,IF(D2=7,1,IF(D2=8,2,0)))))))","v":0},{"$f":"E98*E2","v":0},{"$f":"ROUNDUP(F98,0)","v":0},89807359,null,null,null,null,null,null,null,null,null,"3 supports (sans croix stabilisatrices) pour 2 capt. montage vertical",{"$f":"VLOOKUP(X98,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG359"},{"$f":"VLOOKUP(X98,'Liste de prix'!$1:$1048576,4,FALSE)","v":245},{"$f":"IF(T2=2,0,IF(T2=3,1,IF(T2=4,1,IF(T2=5,1,IF(T2=6,1,IF(T2=7,1,IF(T2=8,2,0)))))))","v":0},{"$f":"U98*U2","v":0},{"$f":"ROUNDUP(V98,0)","v":0},89807359,null,null,null,null,null,null,null,null,null,"3 supports (sans croix stabilisatrices) pour 2 capt. montage vertical",{"$f":"VLOOKUP(AN98,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG359"},{"$f":"VLOOKUP(AN98,'Liste de prix'!$1:$1048576,4,FALSE)","v":245},{"$f":"IF(AJ2=2,0,IF(AJ2=3,1,IF(AJ2=4,1,IF(AJ2=5,1,IF(AJ2=6,1,IF(AJ2=7,1,IF(AJ2=8,2,0)))))))","v":0},{"$f":"AK98*AK2","v":0},{"$f":"ROUNDUP(AL98,0)","v":0},89807359]
[]
["terrasse et hori","2 supports avec croix stabilisatrice pour 1 capt. montage horizontal",{"$f":"VLOOKUP(H100,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG325"},{"$f":"VLOOKUP(H100,'Liste de prix'!$1:$1048576,4,FALSE)","v":161},{"$f":"IF(D2=2,2,IF(D2=3,3,IF(D2=4,4,FALSE)))","v":false},{"$f":"E100*E2","v":0},{"$f":"ROUNDUP(F100,0)","v":0},89807325,null,null,null,null,null,null,null,null,"terrasse et hori","2 supports avec croix stabilisatrice pour 1 capt. montage horizontal",{"$f":"VLOOKUP(X100,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG325"},{"$f":"VLOOKUP(X100,'Liste de prix'!$1:$1048576,4,FALSE)","v":161},{"$f":"IF(T2=2,2,IF(T2=3,3,IF(T2=4,4,FALSE)))","v":false},{"$f":"U100*U2","v":0},{"$f":"ROUNDUP(V100,0)","v":0},89807325,null,null,null,null,null,null,null,null,"terrasse et hori","2 supports avec croix stabilisatrice pour 1 capt. montage horizontal",{"$f":"VLOOKUP(AN100,'Liste de prix'!$1:$1048576,3,FALSE)","v":"EG325"},{"$f":"VLOOKUP(AN100,'Liste de prix'!$1:$1048576,4,FALSE)","v":161},{"$f":"IF(AJ2=2,2,IF(AJ2=3,3,IF(AJ2=4,4,FALSE)))","v":false},{"$f":"AK100*AK2","v":0},{"$f":"ROUNDUP(AL100,0)","v":0},89807325]
[null,"-","-",0,"-",0,0,null,null,null,null,null,null,null,null,null,null,"-","-",0,"-",0,0,null,null,null,null,null,null,null,null,null,null,"-","-",0,null,0,0]
[]
[]
["Récapitulation terrasse",{"$f":"IF(AND(B87=\"terrasse\",B88=\"vertical\"),B97,B100)","v":"2 supports avec croix stabilisatrice pour 1 capt. montage horizontal"},{"$f":"VLOOKUP(B104,B97:C101,2,FALSE)","v":"EG325"},{"$f":"VLOOKUP(C104,C97:D101,2,FALSE)","v":161},{"$f":"VLOOKUP(B104,B97:G101,6,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,"Récapitulation terrasse",{"$f":"IF(AND(R87=\"terrasse\",R88=\"vertical\"),R97,R100)","v":"2 supports avec croix stabilisatrice pour 1 capt. montage horizontal"},{"$f":"VLOOKUP(R104,R97:S101,2,FALSE)","v":"EG325"},{"$f":"VLOOKUP(S104,S97:T101,2,FALSE)","v":161},{"$f":"VLOOKUP(R104,R97:W101,6,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,"Récapitulation terrasse",{"$f":"IF(AND(AH87=\"terrasse\",AH88=\"vertical\"),AH97,AH100)","v":"2 supports avec croix stabilisatrice pour 1 capt. montage horizontal"},{"$f":"VLOOKUP(AH104,AH97:AI101,2,FALSE)","v":"EG325"},{"$f":"VLOOKUP(AI104,AI97:AJ101,2,FALSE)","v":161},{"$f":"VLOOKUP(AH104,AH97:AM101,6,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,{"$f":"AK104+U104+E104","v":0}]
[null,{"$f":"IF(AND(B87=\"terrasse\",B88=\"vertical\"),B98,B101)","v":"-"},{"$f":"VLOOKUP(B105,B97:C101,2,FALSE)","v":"-"},{"$f":"VLOOKUP(C105,C97:D101,2,FALSE)","v":0},{"$f":"VLOOKUP(B105,B97:G101,6,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(R87=\"terrasse\",R88=\"vertical\"),R98,R101)","v":"-"},{"$f":"VLOOKUP(R105,R97:S101,2,FALSE)","v":"-"},{"$f":"VLOOKUP(S105,S97:T101,2,FALSE)","v":0},{"$f":"VLOOKUP(R105,R97:W101,6,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AH87=\"terrasse\",AH88=\"vertical\"),AH98,AH101)","v":"-"},{"$f":"VLOOKUP(AH105,AH97:AI101,2,FALSE)","v":"-"},{"$f":"VLOOKUP(AI105,AI97:AJ101,2,FALSE)","v":0},{"$f":"VLOOKUP(AH105,AH97:AM101,6,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,{"$f":"AK105+U105+E105","v":0}]
[]
[]
[]
[]
[null,"• Ferrures d’ancrage pour montage SUR TOITURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"• Ferrures d’ancrage pour montage SUR TOITURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"• Ferrures d’ancrage pour montage SUR TOITURE"]
[null," à choisir selon le type de couverture en + des profilés",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," à choisir selon le type de couverture en + des profilés",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," à choisir selon le type de couverture en + des profilés"]
[null,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0]
["liste validation \"surtoiture\"","montage indépendant des chevrons en alu pour tuiles mécaniques",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"liste validation \"surtoiture\"","montage indépendant des chevrons en alu pour tuiles mécaniques",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"liste validation \"surtoiture\"","montage indépendant des chevrons en alu pour tuiles mécaniques",1]
[null,"montage sur chevrons en inox pour tuiles mécaniques",2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"montage sur chevrons en inox pour tuiles mécaniques",2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"montage sur chevrons en inox pour tuiles mécaniques",2]
[null,"montage sur chevrons en inox pour tuiles plates",3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"montage sur chevrons en inox pour tuiles plates",3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"montage sur chevrons en inox pour tuiles plates",3]
[null,"montage sur chevrons en inox sur toit éternit",4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"montage sur chevrons en inox sur toit éternit",4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"montage sur chevrons en inox sur toit éternit",4]
[null,"montage sur chevrons en inox sur toit d'ardoises",5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"montage sur chevrons en inox sur toit d'ardoises",5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"montage sur chevrons en inox sur toit d'ardoises",5]
[]
[]
[]
[null,null,null,null,"nbre colis par rangée","nbre colis final",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"nbre colis par rangée","nbre colis final",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"nbre colis par rangée","nbre colis final"]
["choix ",{"$f":"'Pro C '!D60","v":"montage sur chevrons en inox sur toit éternit"},{"$f":"VLOOKUP(B122,B112:C117,2,FALSE)","v":4},{"$f":"IF(C122=1,\"4 pces EG 311\",IF(C122=2,\"4 pces EG 313\",IF(C122=3,\"4 pces EG 315\",IF(C122=4,\"4 pces EG 317\",IF(C122=5,\"4 pces EG 319\",\"\")))))","v":"4 pces EG 317"},{"$f":"IF(D2=3,2,IF(D2=6,2,IF(D2=7,1,0)))","v":0},{"$f":"E122*E2","v":0},null,null,null,null,null,null,null,null,null,null,"choix ",{"$f":"'Pro C '!D60","v":"montage sur chevrons en inox sur toit éternit"},{"$f":"VLOOKUP(R122,R112:S117,2,FALSE)","v":4},{"$f":"IF(S122=1,\"4 pces EG 311\",IF(S122=2,\"4 pces EG 313\",IF(S122=3,\"4 pces EG 315\",IF(S122=4,\"4 pces EG 317\",IF(S122=5,\"4 pces EG 319\",\"\")))))","v":"4 pces EG 317"},{"$f":"IF(T2=3,2,IF(T2=6,2,IF(T2=7,1,0)))","v":0},{"$f":"U122*U2","v":0},null,null,null,null,null,null,null,null,null,null,"choix ",{"$f":"'Pro C '!D60","v":"montage sur chevrons en inox sur toit éternit"},{"$f":"VLOOKUP(AH122,AH112:AI117,2,FALSE)","v":4},{"$f":"IF(AI122=1,\"4 pces EG 311\",IF(AI122=2,\"4 pces EG 313\",IF(AI122=3,\"4 pces EG 315\",IF(AI122=4,\"4 pces EG 317\",IF(AI122=5,\"4 pces EG 319\",\"\")))))","v":"4 pces EG 317"},{"$f":"IF(AJ2=3,2,IF(AJ2=6,2,IF(AJ2=7,1,0)))","v":0},{"$f":"AK122*AK2","v":0},null,null,null,null,null,null,null,null,null,{"$f":"F122+V122+AL122","v":0}]
[null,null,null,{"$f":"IF(C122=1,\"6 pces EG 312\",IF(C122=2,\"6 pces EG 314\",IF(C122=3,\"6 pces EG 316\",IF(C122=4,\"6 pces EG 318\",IF(C122=5,\"6 pces EG 320\",\"\")))))","v":"6 pces EG 318"},{"$f":"IF(D2=2,1,IF(D2=4,2,IF(D2=5,2,IF(D2=6,1,IF(D2=7,2,IF(D2=8,3,0))))))","v":0},{"$f":"E123*E2","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(S122=1,\"6 pces EG 312\",IF(S122=2,\"6 pces EG 314\",IF(S122=3,\"6 pces EG 316\",IF(S122=4,\"6 pces EG 318\",IF(S122=5,\"6 pces EG 320\",\"\")))))","v":"6 pces EG 318"},{"$f":"IF(T2=2,1,IF(T2=4,2,IF(T2=5,2,IF(T2=6,1,IF(T2=7,2,IF(T2=8,3,0))))))","v":0},{"$f":"U123*U2","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AI122=1,\"6 pces EG 312\",IF(AI122=2,\"6 pces EG 314\",IF(AI122=3,\"6 pces EG 316\",IF(AI122=4,\"6 pces EG 318\",IF(AI122=5,\"6 pces EG 320\",\"\")))))","v":"6 pces EG 318"},{"$f":"IF(AJ2=2,1,IF(AJ2=4,2,IF(AJ2=5,2,IF(AJ2=6,1,IF(AJ2=7,2,IF(AJ2=8,3,0))))))","v":0},{"$f":"AK123*AK2","v":0},null,null,null,null,null,null,null,null,null,{"$f":"F123+V123+AL123","v":0}]
[]
[]
[]
[]
[]
[null,100008010,{"$f":"VLOOKUP(B129,'Liste de prix'!1:1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(B129,'Liste de prix'!1:1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(B129,'Liste de prix'!1:1048576,4,FALSE)","v":{"$error":"#N/A"}},null,null,null,null,null,null,null,null,null,null,null,null,100008010,{"$f":"VLOOKUP(R129,'Liste de prix'!1:1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(R129,'Liste de prix'!1:1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(R129,'Liste de prix'!1:1048576,4,FALSE)","v":{"$error":"#N/A"}},null,null,null,null,null,null,null,null,null,null,null,null,100008010,{"$f":"VLOOKUP(AH129,'Liste de prix'!1:1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AH129,'Liste de prix'!1:1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(AH129,'Liste de prix'!1:1048576,4,FALSE)","v":{"$error":"#N/A"}}]

{"sheet":"Outils accessoires","index":5,"n_rows":76,"n_cols":7,"rows_kept":76,"cut":false,"hidden":true,"merged":[]}
[null,{"$f":"\"\"","v":""},0]
["…","-",0,null,null,0]
[{"$f":"VLOOKUP(D3,liste,2,FALSE)","v":"VASE D'EXPANSION 100 l"},{"$f":"VLOOKUP(D3,liste,3,FALSE)","v":"EG120"},{"$f":"VLOOKUP(D3,liste,4,FALSE)","v":402},100008733,null,1]
[{"$f":"VLOOKUP(D4,liste,2,FALSE)","v":"VASE D'EXPANSION 200 l"},{"$f":"VLOOKUP(D4,liste,3,FALSE)","v":"EG122"},{"$f":"VLOOKUP(D4,liste,4,FALSE)","v":637},100008735,null,2]
[{"$f":"VLOOKUP(D5,liste,2,FALSE)","v":"VASE D'EXPANSION 300 l"},{"$f":"VLOOKUP(D5,liste,3,FALSE)","v":"EG123"},{"$f":"VLOOKUP(D5,liste,4,FALSE)","v":1142},100008736,null,3]
[{"$f":"VLOOKUP(D6,liste,2,FALSE)","v":"VASE D'EXPANSION SOLAIRE 35 L"},{"$f":"VLOOKUP(D6,liste,3,FALSE)","v":"EG83"},{"$f":"VLOOKUP(D6,liste,4,FALSE)","v":181},89807772,null,4]
[{"$f":"VLOOKUP(D7,liste,2,FALSE)","v":"VASE D'EXPANSION SOLAIRE 50 L"},{"$f":"VLOOKUP(D7,liste,3,FALSE)","v":"EG84"},{"$f":"VLOOKUP(D7,liste,4,FALSE)","v":348},89807773,null,5]
["OPTION",null,null,null,null,6]
["…","-",0,0,null,7]
[{"$f":"VLOOKUP(D10,liste,2,FALSE)","v":"ANODE ACI CORREX UP BALLON > 300 LITRES"},{"$f":"VLOOKUP(D10,liste,3,FALSE)","v":"AM7"},{"$f":"VLOOKUP(D10,liste,4,FALSE)","v":532},89608920,null,8]
["RESISTANCE BLINDEE 6 KW/400V A VISSER 1''1/2 + THERMOSTAT DE REGLAGE","AJ36",628,89757750,null,9]
["KIT ELECTRIQUE 9 KW/400V 1 1/2 ( POUR RSB 1000 A 3000 )","AJ47",650,100019313,null,10]
["RESISTANCE BLINDEE 6 KW/400V A VISSER 1''1/2 + THERMOSTAT DE REGLAGE","ER335",728,100019314]
["RESISTANCE BLINDEE 6 KW/400V A VISSER 1''1/2 + THERMOSTAT DE REGLAGE","ER131",295,100014590]
["CENTRALE DE MESURE D'ENERGIE CME","ER313",1675,100017498]
["DATALOGGER DL2 POUR GRS","ER55",460,100013514]
["MODULE REPORT DE PANNE OETROSOL AM1","ER314",180,100017499]
["REGULATION POMPE DE CHARGE SLA 2","EC320",208,100007832]
["THERMOMETRE","AJ32",51,89757746]
["VANNE 3 VOIES 3/4\" POUR 2 CIRCUITS","EC164",237,89804803]
["PREPARATEUR"]
["…","-",0,0]
[{"$f":"VLOOKUP(D23,liste,2,FALSE)","v":"PREPARATEUR SOLAIRE OBS 200 N"},{"$f":"VLOOKUP(D23,liste,3,FALSE)","v":"ER424"},{"$f":"VLOOKUP(D23,liste,4,FALSE)","v":902},100019529]
["PREPARATEUR SOLAIRE OBS 300 N","ER425",913,100019522]
["PREPARATEUR SOLAIRE OBS 400 N","ER426",1957,100019526]
["PREPARATEUR SOLAIRE OBS 500 N","ER341",2284,100019068,null,"COLIS",{"$f":"VLOOKUP('Accessoires et options'!I34,A22:D44,2,FALSE)","v":"-"}]
[{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},100011343,null,"PRIX",{"$f":"VLOOKUP('Accessoires et options'!I34,A22:D44,3,FALSE)","v":0}]
[{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"VLOOKUP(D28,liste,4,FALSE)","v":{"$error":"#N/A"}},125549]
[{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},125550]
[{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},126758,null,"CHOIX 2",{"$f":"'Accessoires et options'!I41","v":"…"}]
[{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},126757,null,"COLIS",{"$f":"VLOOKUP(G30,A22:D44,2,FALSE)","v":"-"}]
["PREPARATEUR ECS INSTANTANEE FWS 750","EC546",4808,100008019,null,"PRIX",{"$f":"VLOOKUP(G30,A22:D44,3,FALSE)","v":0}]
[{"$f":"VLOOKUP(D33,liste,2,FALSE)","v":"PREPARATEUR SOLAIRE FWS 1500 COMPLET"},{"$f":"VLOOKUP(D33,liste,3,FALSE)","v":0},{"$f":"VLOOKUP(D33,liste,4,FALSE)","v":7103},100017466]
[{"$f":"VLOOKUP(D34,liste,2,FALSE)","v":"BALLON TAMPON PSB 750"},{"$f":"VLOOKUP(D34,liste,3,FALSE)","v":"EC129"},{"$f":"VLOOKUP(D34,liste,4,FALSE)","v":1645},100005010]
[{"$f":"VLOOKUP(D35,liste,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(D35,liste,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(D35,liste,4,FALSE)","v":{"$error":"#N/A"}},126975]
[{"$f":"VLOOKUP(D36,liste,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(D36,liste,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(D36,liste,4,FALSE)","v":{"$error":"#N/A"}},126976]
[{"$f":"VLOOKUP(D37,liste,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(D37,liste,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(D37,liste,4,FALSE)","v":{"$error":"#N/A"}},126977]
[{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},126978]
[{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},100017469]
[{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},100017472]
[{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},100017475]
[{"$f":"VLOOKUP(D42,liste,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(D42,liste,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(D42,liste,4,FALSE)","v":{"$error":"#N/A"}},100017476]
[{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},100017477]
[{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},100017478]
["REGULATION",null,null,null,"CHOIX",{"$f":"'Accessoires et options'!I18","v":"…"}]
["…"," - ",0," - "]
[{"$f":"VLOOKUP(D47,liste,2,FALSE)","v":"REGULATION SOL COLLECTIF SC5 "},{"$f":"VLOOKUP(D47,liste,3,FALSE)","v":"ER672"},{"$f":"VLOOKUP(D47,liste,4,FALSE)","v":609},7619972,"COLIS",{"$f":"VLOOKUP(F45,A46:D52,2,FALSE)","v":" - "}]
[{"$f":"VLOOKUP(D48,liste,2,FALSE)","v":"REGULATION OETROSOL-AEL"},{"$f":"VLOOKUP(D48,liste,3,FALSE)","v":"ER708"},{"$f":"VLOOKUP(D48,liste,4,FALSE)","v":291},7630421,"Prix",{"$f":"VLOOKUP(F45,A46:D52,3,FALSE)","v":0}]
[{"$f":"VLOOKUP(D49,liste,2,FALSE)","v":"REGULATION OETROSOL-PLUS"},{"$f":"VLOOKUP(D49,liste,3,FALSE)","v":"ER709"},{"$f":"VLOOKUP(D49,liste,4,FALSE)","v":260},7630422,"Ref",{"$f":"VLOOKUP(F45,A46:D52,4,FALSE)","v":" - "}]
[{"$f":"VLOOKUP(D50,liste,2,FALSE)","v":"RÉGULATION \"DELTASOL E\" POUR STATION TRANSFERT SOLAIRE"},{"$f":"VLOOKUP(D50,liste,3,FALSE)","v":"ER315"},{"$f":"VLOOKUP(D50,liste,4,FALSE)","v":717},100017500]
[{"$f":"VLOOKUP(D51,liste,2,FALSE)","v":"REGULATION \"MCDB\" POUR CHARGE/DECHARGE BALLON "},{"$f":"VLOOKUP(D51,liste,3,FALSE)","v":"EC162"},{"$f":"VLOOKUP(D51,liste,4,FALSE)","v":270},100004650]
[]
["STATION SOLAIRE"]
["…"," - ",0," - "]
[{"$f":"VLOOKUP(D55,liste,2,FALSE)","v":"STATION SOLAIRE SKS 13-45"},{"$f":"VLOOKUP(D55,liste,3,FALSE)","v":"ER665"},{"$f":"VLOOKUP(D55,liste,4,FALSE)","v":676},7619964]
["STATION SOLAIRE SKP 7-8","ER655",447,7624853]
["STATION SOLAIRE STS 14-30 CME","ER667",2705,7619966,0,"CHOIX",{"$f":"'Accessoires et options'!I25","v":"…"}]
["STATION SOLAIRE STS 14-50 CME","ER668",3121,7619967,1,"COLIS",{"$f":"VLOOKUP(G57,A54:D61,2,FALSE)","v":" - "}]
["STATION SOLAIRE STS 14-100 CME","ER669",6242,7619968,1,"PRIX",{"$f":"VLOOKUP(G57,A54:D61,3,FALSE)","v":0}]
["MODULE TRANSFERT SOLAIRE DRAIN BACK DB-20","ER301",2772,100017486,1]
["STATION TRANSFERT DMCDB ","ER468",1037,7604939,1]
[null,null,null,null,0]
[null,null,null,null,0]
["Fluide"]
["…","-",0]
["FLUIDE CALOPORTEUR HAUTES PERFORMANCES BIO  (-26°C) 20 LITRES",{"$f":"VLOOKUP(D66,liste,3,FALSE)","v":"ER316"},{"$f":"VLOOKUP('Outils accessoires'!D66,'Liste de prix'!$1:$1048576,4,FALSE)","v":134},100017611]
["FLUIDE CALOPORTEUR TYPE L (-21°C) 20 LITRES. ",{"$f":"VLOOKUP(D67,liste,3,FALSE)","v":"EG101"},{"$f":"VLOOKUP('Outils accessoires'!D67,'Liste de prix'!$1:$1048576,4,FALSE)","v":78},89807794]
["FLUIDE CALOPORTEUR HAUTES PERFORMANCES TYPE LS (-26°C) 20 LITRES",{"$f":"VLOOKUP(D68,liste,3,FALSE)","v":"EG100"},{"$f":"VLOOKUP('Outils accessoires'!D68,'Liste de prix'!$1:$1048576,4,FALSE)","v":154},89807792]
[]
[]
["Devis capteurs SUN C250"]
["Devis capteurs SUN 3000"]
[]
["Sur toiture"]
["Terrasse (Vertical juxtaposé)"]
["Sur tuiles canal"]

{"sheet":"Accessoires et options","index":6,"n_rows":95,"n_cols":18,"rows_kept":95,"cut":false,"hidden":false,"merged":[[0,13,0,15],[58,6,58,10],[5,13,5,14],[72,6,72,10],[14,12,14,13],[21,6,21,10],[30,6,30,10],[44,6,44,10],[51,6,51,10],[2,7,2,12],[9,7,9,11],[10,7,10,11],[11,7,11,11],[37,6,37,10],[94,7,94,8],[79,6,79,8],[92,7,92,8],[94,9,94,11],[91,9,91,11],[91,7,91,8],[84,6,84,13],[85,6,85,13],[82,6,82,10],[87,6,87,10],[93,9,93,11],[93,7,93,8],[80,6,80,8],[81,6,81,8],[92,9,92,11],[77,6,77,8],[78,6,78,8],[83,6,83,13],[76,6,76,8],[65,6,65,10],[75,6,75,8]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'SUN C250'!K1","v":"Version 01/2017"}]
[]
[null,null,null,null,null,null,null,"Chiffrage des accessoires avec capteurs SUN C250 et/ou SUN 3000"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"TODAY()","v":"2017-01-31"}]
[]
[]
[]
[null,null,null,null,null,null," Référence     "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"REMISE!F9","v":0}]
[]
[]
[]
[null,null,null,null,null,null,"REGULATION",null,"Désignation","Colis","Prix unitaire HT en €","Qté","Prix total HT en €"]
[]
[null,null,null,null,null,null,null,null,"Régulation"]
[null,null,null,null,null,null,null,null,"…",{"$f":"IF(I18=\"\",\"\",'Outils accessoires'!F47)","v":" - "},{"$f":"'Outils accessoires'!F48","v":0},null,{"$f":"K18*L18","v":0},{"$f":"M18*(1-N$11)","v":0}]
[]
[]
[]
[null,null,null,null,null,null,"STATION SOLAIRE"]
[]
[null,null,null,null,null,null,null,null,"Station"]
[null,null,null,null,null,null,null,null,"…",{"$f":"IF(I25=\"\",\"\",'Outils accessoires'!G58)","v":" - "},{"$f":"'Outils accessoires'!G59","v":0},null,{"$f":"K25*L25","v":0},{"$f":"M25*(1-N$11)","v":0}]
[null,null,null,null,null,null,null,null,{"$f":"IF(J25=\" - \",\"\",IF(VLOOKUP(J25,mamadou,4,FALSE)=1,\"Régulation intégrée\",\"\"))","v":""}]
[]
[]
[]
[]
[null,null,null,null,null,null,"PREPARATEUR 1"]
[]
[null,null,null,null,null,null,null,null,"Préparateur",null,null,null,null,{"$f":"IF(I34=\"PREPARATEUR  BESC 300 I\",\"Nous consulter\",\"\")","v":""}]
[null,null,null,null,null,null,null,null,"…",{"$f":"IF(I34=\"\",\"\",'Outils accessoires'!G26)","v":"-"},{"$f":"'Outils accessoires'!G27","v":0},null,{"$f":"K34*L34","v":0},{"$f":"IF(I34=\"PREPARATEUR  BESC 300 I\",0,M34*(1-N$11))","v":0}]
[]
[]
[]
[null,null,null,null,null,null,"PREPARATEUR 2"]
[]
[null,null,null,null,null,null,null,null,"Préparateur",null,null,null,null,{"$f":"IF(I41=\"PREPARATEUR  BESC 300 I\",\"Nous consulter\",\"\")","v":""}]
[null,null,null,null,null,null,null,null,"…",{"$f":"IF(I41=\"\",\"\",'Outils accessoires'!G31)","v":"-"},{"$f":"'Outils accessoires'!G32","v":0},null,{"$f":"K41*L41","v":0},{"$f":"IF(I41=\"PREPARATEUR  BESC 300 I\",0,M41*(1-N$11))","v":0}]
[]
[]
[]
[null,null,null,null,null,null,"OPTION 1"]
[]
[null,null,null,null,null,null,null,null,"Option"]
[null,null,null,null,null,null,null,null,"…",{"$f":"IF(I48=\"\",\"\",VLOOKUP(I48,'Outils accessoires'!A9:D20,2,FALSE))","v":"-"},{"$f":"VLOOKUP(I48,'Outils accessoires'!A9:D20,3,FALSE)","v":0},null,{"$f":"K48*L48","v":0},{"$f":"M48*(1-N$11)","v":0}]
[]
[]
[]
[null,null,null,null,null,null,"OPTION 2"]
[]
[null,null,null,null,null,null,null,null,"Option"]
[null,null,null,null,null,null,null,null,"…",{"$f":"IF(I55=\"\",\"\",VLOOKUP(I55,'Outils accessoires'!A9:D20,2,FALSE))","v":"-"},{"$f":"VLOOKUP(I55,'Outils accessoires'!A9:D20,3,FALSE)","v":0},null,{"$f":"K55*L55","v":0},{"$f":"M55*(1-N$11)","v":0}]
[]
[]
[]
[null,null,null,null,null,null,"FLUIDE CALOPORTEUR (donné à titre indicatif – à calculer en fonction de l'installation)"]
[]
[null,null,null,null,null,null,null,null,"Type"]
[null,null,null,null,null,null,null,null,"…",{"$f":"IF(I62=\"\",\"\",VLOOKUP(I62,'Outils accessoires'!A65:D68,2,FALSE))","v":"-"},{"$f":"VLOOKUP(I62,'Outils accessoires'!A65:D68,3,FALSE)","v":0},null,{"$f":"K62*L62","v":0},{"$f":"M62*(1-N$11)","v":0}]
[]
[]
[]
[null,null,null,null,null,null,"VASE EXPANSION SOLAIRE (donné à titre indicatif – à calculer en fonction de l'installation)"]
[]
[null,null,null,null,null,null,null,null,"Vase"]
[null,null,null,null,null,null,null,null,"…",{"$f":"IF(I69=\"\",\"\",VLOOKUP(I69,'Outils accessoires'!A2:D7,2,FALSE))","v":"-"},{"$f":"VLOOKUP(I69,'Outils accessoires'!A2:D7,3,FALSE)","v":0},null,{"$f":"K69*L69","v":0},{"$f":"M69*(1-N$11)","v":0}]
[]
[]
[]
[null,null,null,null,null,null,"AUTRE"]
[]
[null,null,null,null,null,null,null,null,"Désignation","N° Colis",null,"PU ","Qté","Prix total"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M76<>0,O76*(1-N$11),0)","v":0},{"$f":"PRODUCT(L76,M76)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0]
[null,null,null,null,null,null,"NOTE"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oui"]
[null,null,null,null,null,null,"MISE EN SERVICE (Prix NET)",null,null,null,null,null,"Oui",{"$f":"IF(M88=\"Oui\",440,0)","v":440},null,null,null,"Non"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRODUCT(L89,M89)","v":0}]
[]
[]
[null,null,null,null,null,null,null,"Système",null,"Prix total HT en €"]
[null,null,null,null,null,null,null,"Devis capteurs SUN C250",null,{"$f":"IF(H93='Outils accessoires'!A71,'SUN C250'!G64,'Sun 3000'!E66)","v":0}]
[null,null,null,null,null,null,null,"Devis ACCESSOIRES",null,{"$f":"N18+N25+N34+N41+N48+N55+N62+N69+N76+N77+N78+N79+N80+N81+N82+N88","v":440}]
[null,null,null,null,null,null,null,"Devis TOTAL",null,{"$f":"J93+J94","v":440}]

{"sheet":"feuille PRO c250","index":7,"n_rows":99,"n_cols":20,"rows_kept":99,"cut":false,"hidden":true,"merged":[]}
["Choix:",{"$f":"'Pro C '!D12","v":"vertical"},null,null,null,null,null,null,null,null,null,null,"charges de neige et vent importantes",null,null,"en terrasse (ou au sol)","Table A"]
[null,null,null,null,null,null,null,null,null,null,null,null,"charges de neige et vent standards",null,null,{"$f":"IF(OR('SUN C250'!H24>4,'SUN C250'!H25>4,'SUN C250'!H26>4),\"\",\"en intégration de toiture\")","v":"en intégration de toiture"},0,0,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sur toiture",2,1,null,2]
["Nombre capteurs/séries",{"$f":"'SUN C250'!H24","v":0},{"$f":"'SUN C250'!I24","v":0},{"$f":"B4*C4","v":0},null,null,null,null,null,null,null,null," ",null,null,null,3,1,null,3]
[null,{"$f":"'SUN C250'!H25","v":0},{"$f":"'SUN C250'!I25","v":0},{"$f":"B5*C5","v":0},null,null,null,null,null,null,null,null,null,null,null,null,4,1,null,4]
[null,{"$f":"'SUN C250'!H26","v":0},{"$f":"'SUN C250'!I26","v":0},{"$f":"B6*C6","v":0},null,null,null,null,null,null,null,null,"tuile mécanique 22°",null,null,{"$f":"IF(choix=$P$1,M1,IF(choix=$P$2,M6,IF(choix=$P$3,M10)))","v":"clipper"},5,1,null,5]
[null,{"$f":"SUM(B4:B6)","v":0},{"$f":"SUM(C4:C6)","v":0},{"$f":"SUM(D4:D6)","v":0},null,null,null,null,null,null,null,null,"tuile canal 17°",null,null,{"$f":"IF(choix=$P$1,M2,IF(choix=$P$2,M7,IF(choix=$P$3,\"\")))","v":""},6,1,null,6]
[null,null,null,null,null,null,null,null,null,null,null,null,"tuile plate 21°",null,null,{"$f":"IF(choix=$P$1,M4,IF(choix=$P$2,\"\",IF(choix=$P$3,\" \")))","v":" "},7,1,null,7]
[null,null,"A",{"$f":"C4*VLOOKUP(B4,TA,2,FALSE)+C5*VLOOKUP(B5,TA,2,FALSE)+C6*VLOOKUP(B6,TA,2,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,8,1,null,8]
[null,null,"B",{"$f":"C4*VLOOKUP(B4,TB,2,FALSE)+C5*VLOOKUP(B5,TB,2,FALSE)+C6*VLOOKUP(B6,TB,2,FALSE)","v":0},null,null,null,null,null,null,null,null,"clipper",null,null,"Vertical",9,1,null,9]
[null,null,"C",{"$f":"C4*VLOOKUP(B4,TC,2,FALSE)+C5*VLOOKUP(B5,TC,2,FALSE)+C6*VLOOKUP(B6,TC,2,FALSE)","v":0},null,null,null,null,null,null,null,null,"visser",null,null,"Horizontal",10,1,null,10]
[null,"ferrures","Chevron 4",{"$f":"C4*VLOOKUP(B4,chevrons,2,FALSE)+C5*VLOOKUP(B5,chevrons,2,FALSE)+C6*VLOOKUP(B6,chevrons,2,FALSE)","v":0},"ALU 4",{"$f":"C4*VLOOKUP(B4,alu,3,FALSE)+C5*VLOOKUP(B5,alu,3,FALSE)+C6*VLOOKUP(B6,alu,3,FALSE)","v":0},"Tire-fond 6",{"$f":"C4*VLOOKUP(B4,TF,2,FALSE)+C5*VLOOKUP(B5,TF,2,FALSE)+C6*VLOOKUP(B6,TF,2,FALSE)","v":0}]
[null,null,6,{"$f":"C4*VLOOKUP(B4,chevrons,3,FALSE)+C5*VLOOKUP(B5,chevrons,3,FALSE)+C6*VLOOKUP(B6,chevrons,3,FALSE)","v":0},2,{"$f":"C4*VLOOKUP(B4,alu,2,FALSE)+C5*VLOOKUP(B5,alu,2,FALSE)+C6*VLOOKUP(B6,alu,2,FALSE)","v":0},8,{"$f":"C4*VLOOKUP(B4,TF,3,FALSE)+C5*VLOOKUP(B5,TF,3,FALSE)+C6*VLOOKUP(B6,TF,3,FALSE)","v":0},null,null,null,null,null,null,null,null,"Table B"]
["Vertical",null,null,null,null,null,"Horizontal",null,null,null,null,null,null,null,null,null,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,2]
["Réf","Désignation","Colis","Prix",null,null,"Réf","Désignation","Colis","Prix",null,null,null,null,null,null,4,3]
[100016502,{"$f":"VLOOKUP(A18,'Liste de prix'!$1:$1048576,2,FALSE)","v":"CAPTEUR PLAN MONTAGE VERTICAL PRO C250 V"},{"$f":"VLOOKUP(A18,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER240"},{"$f":"VLOOKUP(A18,'Liste de prix'!$1:$1048576,4,FALSE)","v":797},null,null,100016503,{"$f":"VLOOKUP(G18,'Liste de prix'!$1:$1048576,2,FALSE)","v":"CAPTEUR PLAN MONTAGE HORIZONTAL PRO C250 H"},{"$f":"VLOOKUP(G18,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER241"},{"$f":"VLOOKUP(G18,'Liste de prix'!$1:$1048576,4,FALSE)","v":820},null,null,null,null,null,null,5,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,6]
["Accessoires pour le raccordement hydraulique du capteur pro C250V",null,null,null,null,null,"Accessoires pour le raccordement hydraulique du capteur pro C250V",null,null,null,null,null,null,null,null,null,8,7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,8]
[100016506,{"$f":"VLOOKUP(A23,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT DE RACCORDEMENT CHAMP DE CAPTEURS"},{"$f":"VLOOKUP(A23,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER245"},{"$f":"VLOOKUP(A23,'Liste de prix'!$1:$1048576,4,FALSE)","v":120},{"$f":"TAA","v":0},null,100016506,{"$f":"VLOOKUP(G23,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT DE RACCORDEMENT CHAMP DE CAPTEURS"},{"$f":"VLOOKUP(G23,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER245"},{"$f":"VLOOKUP(G23,'Liste de prix'!$1:$1048576,4,FALSE)","v":120},null,null,null,null,null,null,10,9]
[100016507,{"$f":"VLOOKUP(A24,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT DE LIAISON HYDRAULIQUE ENTRE CAPTEURS"},{"$f":"VLOOKUP(A24,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER246"},{"$f":"VLOOKUP(A24,'Liste de prix'!$1:$1048576,4,FALSE)","v":41},{"$f":"TBB","v":0},null,100016507,{"$f":"VLOOKUP(G24,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT DE LIAISON HYDRAULIQUE ENTRE CAPTEURS"},{"$f":"VLOOKUP(G24,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER246"},{"$f":"VLOOKUP(G24,'Liste de prix'!$1:$1048576,4,FALSE)","v":41}]
[100016508,{"$f":"VLOOKUP(A25,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT  FLEXIBLES CIRCUIT SOLAIRE CHAMP CAPTEURS"},{"$f":"VLOOKUP(A25,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER247"},{"$f":"VLOOKUP(A25,'Liste de prix'!$1:$1048576,4,FALSE)","v":77},{"$f":"TAA","v":0},null,100016508,{"$f":"VLOOKUP(G25,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT  FLEXIBLES CIRCUIT SOLAIRE CHAMP CAPTEURS"},{"$f":"VLOOKUP(G25,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER247"},{"$f":"VLOOKUP(G25,'Liste de prix'!$1:$1048576,4,FALSE)","v":77},null,null,null,null,null,null,"Table C"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,3]
["Dispositif de montage en terrasse (ou ausol)",null,null,null,null,null,"Dispositif de montage en terrasse (ou ausol)",null,null,null,null,null,null,null,null,null,4,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,5]
["High load",null,null,null,null,null,"High load",null,null,null,null,null,null,null,null,null,6,6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,7]
[100016509,{"$f":"VLOOKUP(A33,'Liste de prix'!$1:$1048576,2,FALSE)","v":"2 SUPPORTS HL AVEC CROIX  MONTAGE VERTICAL 1 C250 SANS PROFILES"},{"$f":"VLOOKUP(A33,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER250"},{"$f":"VLOOKUP(A33,'Liste de prix'!$1:$1048576,4,FALSE)","v":312},{"$f":"TAA","v":0},null,100016511,{"$f":"VLOOKUP(G33,'Liste de prix'!$1:$1048576,2,FALSE)","v":"2 SUPPORTS HL AVEC CROIX  MONTAGE HORIZONTAL 1 C250 SANS PROFILES"},{"$f":"VLOOKUP(G33,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER252"},{"$f":"VLOOKUP(G33,'Liste de prix'!$1:$1048576,4,FALSE)","v":255},null,null,null,null,null,null,8,8]
[100016510,{"$f":"VLOOKUP(A34,'Liste de prix'!$1:$1048576,2,FALSE)","v":"1 SUPPORT HL VERTICAL POUR EXTENSION 1 C250 "},{"$f":"VLOOKUP(A34,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER251"},{"$f":"VLOOKUP(A34,'Liste de prix'!$1:$1048576,4,FALSE)","v":161},{"$f":"TBB","v":0},null,100016512,{"$f":"VLOOKUP(G34,'Liste de prix'!$1:$1048576,2,FALSE)","v":"1 SUPPORT HL HORIZONTAL POUR EXTENSION 1 C250 "},{"$f":"VLOOKUP(G34,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER253"},{"$f":"VLOOKUP(G34,'Liste de prix'!$1:$1048576,4,FALSE)","v":145},null,null,null,null,null,null,9,9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,10]
["Standard",null,null,null,null,null,"Standard"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ferrures","4 pces","6 pces"]
[7217038,{"$f":"VLOOKUP(A38,'Liste de prix'!$1:$1048576,2,FALSE)","v":"2 SUPPORTS SL MONTAGE VERTICAL 1 CAPTEUR"},{"$f":"VLOOKUP(A38,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER658"},{"$f":"VLOOKUP(A38,'Liste de prix'!$1:$1048576,4,FALSE)","v":196},{"$f":"TAA","v":0},null,7217041,{"$f":"VLOOKUP(G38,'Liste de prix'!$1:$1048576,2,FALSE)","v":"2 SUPPORTS SL HL MONTAGE HORIZONTAL 1 CAPTEUR"},{"$f":"VLOOKUP(G38,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER656"},{"$f":"VLOOKUP(G38,'Liste de prix'!$1:$1048576,4,FALSE)","v":156},null,null,null,null,null,null,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,0,1]
[7217039,{"$f":"VLOOKUP(A40,'Liste de prix'!$1:$1048576,2,FALSE)","v":"1 SUPPORT SL VERTICAL POUR EXTENSION 1 CAPTEUR "},{"$f":"VLOOKUP(A40,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER659"},{"$f":"VLOOKUP(A40,'Liste de prix'!$1:$1048576,4,FALSE)","v":91},{"$f":"TBB","v":0},null,100017620,{"$f":"VLOOKUP(G40,'Liste de prix'!$1:$1048576,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(G40,'Liste de prix'!$1:$1048576,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(G40,'Liste de prix'!$1:$1048576,4,FALSE)","v":{"$error":"#N/A"}},null,null,null,null,null,null,3,2,0]
[7217044,{"$f":"VLOOKUP(A41,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT PROFILES 45 MTGE VT "},{"$f":"VLOOKUP(A41,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER664"},{"$f":"VLOOKUP(A41,'Liste de prix'!$1:$1048576,4,FALSE)","v":80},{"$f":"TCC","v":0},null,7217048,{"$f":"VLOOKUP(G41,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT PROFILES 45 2,5M2 HZ "},{"$f":"VLOOKUP(G41,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER662"},{"$f":"VLOOKUP(G41,'Liste de prix'!$1:$1048576,4,FALSE)","v":98},null,null,null,null,null,null,4,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,0,2]
["Dispositif de montage en intégration toiture",null,null,null,null,null,"Dispositif de montage en intégration toiture",null,null,null,null,null,null,null,null,null,6,2,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,1,2]
[7212864,{"$f":"VLOOKUP(A45,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT DE BASE 22° D'INTEGRATION TUILE MECANIQUE 1 C250 V"},{"$f":"VLOOKUP(A45,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER634"},{"$f":"VLOOKUP(A45,'Liste de prix'!$1:$1048576,4,FALSE)","v":551},0,null,7212866,{"$f":"VLOOKUP(G45,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT DE BASE 22° D'INTEGRATION TUILE MECANIQUE 1 C250 H"},{"$f":"VLOOKUP(G45,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER637"},{"$f":"VLOOKUP(G45,'Liste de prix'!$1:$1048576,4,FALSE)","v":583},null,null,null,null,null,null,8,0,3]
[7212869,{"$f":"VLOOKUP(A46,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT DE BASE 22° D'INTEGRATION TUILE MECANIQUE 2 C250 V"},{"$f":"VLOOKUP(A46,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER635"},{"$f":"VLOOKUP(A46,'Liste de prix'!$1:$1048576,4,FALSE)","v":795},{"$f":"IF(AND(B4<>2,B4<>3,B4<>4),0,1)*C4+IF(AND(B5<>2,B5<>3,B5<>4),0,1)*C5+IF(AND(B6<>2,B6<>3,B6<>4),0,1)*C6","v":0},null,7212870,{"$f":"VLOOKUP(G46,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT DE BASE 22° D'INTEGRATION TUILE MECANIQUE 2 C250 H"},{"$f":"VLOOKUP(G46,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER638"},{"$f":"VLOOKUP(G46,'Liste de prix'!$1:$1048576,4,FALSE)","v":954},null,null,null,null,null,null,9,2,2]
[7212867,{"$f":"VLOOKUP(A47,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT EXTENSION 22° INTEGRATION TUILE MECANIQUE 1 C 250 V"},{"$f":"VLOOKUP(A47,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER636"},{"$f":"VLOOKUP(A47,'Liste de prix'!$1:$1048576,4,FALSE)","v":329},{"$f":"IF(B4=3,1,IF(B4=4,2,0))*C4+IF(B5=3,1,IF(B5=4,2,0))*C5+IF(B6=3,1,IF(B6=4,2,0))*C6","v":0},null,7212868,{"$f":"VLOOKUP(G47,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT EXTENSION 22° INTEGRATION TUILE MECANIQUE C 250 H"},{"$f":"VLOOKUP(G47,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER639"},{"$f":"VLOOKUP(G47,'Liste de prix'!$1:$1048576,4,FALSE)","v":425},null,null,null,null,null,null,10,1,3]
[7212872,{"$f":"VLOOKUP(A48,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT DE BASE 17° D'INTEGRATION TUILE CANAL 1 C250 V "},{"$f":"VLOOKUP(A48,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER640"},{"$f":"VLOOKUP(A48,'Liste de prix'!$1:$1048576,4,FALSE)","v":721},0,null,7212873,{"$f":"VLOOKUP(G48,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT DE BASE 17° D'INTEGRATION TUILE CANAL 1 C250 H "},{"$f":"VLOOKUP(G48,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER643"},{"$f":"VLOOKUP(G48,'Liste de prix'!$1:$1048576,4,FALSE)","v":806}]
[7503821,{"$f":"VLOOKUP(A49,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT DE BASE 17° D'INTEGRATION TUILE CANAL 2 C250 V "},{"$f":"VLOOKUP(A49,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER641"},{"$f":"VLOOKUP(A49,'Liste de prix'!$1:$1048576,4,FALSE)","v":1113},{"$f":"IF(AND(B4<>2,B4<>3,B4<>4),0,1)*C4+IF(AND(B5<>2,B5<>3,B5<>4),0,1)*C5+IF(AND(B6<>2,B6<>3,B6<>4),0,1)*C6","v":0},null,7212880,{"$f":"VLOOKUP(G49,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT DE BASE 17° D'INTEGRATION TUILE CANAL 2 C250 H "},{"$f":"VLOOKUP(G49,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER644"},{"$f":"VLOOKUP(G49,'Liste de prix'!$1:$1048576,4,FALSE)","v":1325},null,null,null,null,null,null,"Ferrures alu pour profilés","2pces","4pces"]
[7212875,{"$f":"VLOOKUP(A50,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT EXTENSION 17° INTEGRATION TUILE CANAL C 250 V "},{"$f":"VLOOKUP(A50,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER642"},{"$f":"VLOOKUP(A50,'Liste de prix'!$1:$1048576,4,FALSE)","v":425},{"$f":"IF(B4=3,1,IF(B4=4,2,0))*C4+IF(B5=3,1,IF(B5=4,2,0))*C5+IF(B6=3,1,IF(B6=4,2,0))*C6","v":0},null,7212877,{"$f":"VLOOKUP(G50,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT EXTENSION 17° INTEGRATION TUILE CANAL C 250 H"},{"$f":"VLOOKUP(G50,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER645"},{"$f":"VLOOKUP(G50,'Liste de prix'!$1:$1048576,4,FALSE)","v":478},null,null,null,null,null,null,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,0,2]
["Dispositif de montage sur toiture (kit profilé et ferrures d'ancrage)",null,null,null,null,null,"Dispositif de montage sur toiture (kit profilé et ferrures d'ancrage)",null,null,null,null,null,null,null,null,null,4,1,2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,0,3]
[100016513,{"$f":"VLOOKUP(A55,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT PROFILES A CLIPER POUR 1 C250 V"},{"$f":"VLOOKUP(A55,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER260"},{"$f":"VLOOKUP(A55,'Liste de prix'!$1:$1048576,4,FALSE)","v":139},{"$f":"TCC","v":0},null,100016514,{"$f":"VLOOKUP(G55,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT PROFILES A CLIPER POUR 1 C250 H"},{"$f":"VLOOKUP(G55,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER261"},{"$f":"VLOOKUP(G55,'Liste de prix'!$1:$1048576,4,FALSE)","v":173},null,null,null,null,null,null,6,1,3]
[7217044,{"$f":"VLOOKUP(A56,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT PROFILES 45 MTGE VT "},{"$f":"VLOOKUP(A56,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER664"},{"$f":"VLOOKUP(A56,'Liste de prix'!$1:$1048576,4,FALSE)","v":80},{"$f":"TCC","v":0},null,7217048,{"$f":"VLOOKUP(G56,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT PROFILES 45 2,5M2 HZ "},{"$f":"VLOOKUP(G56,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER662"},{"$f":"VLOOKUP(G56,'Liste de prix'!$1:$1048576,4,FALSE)","v":98},null,null,null,null,null,null,7,0,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,1,4]
[89807311,"4 FERRURES D'ANCRAGE ALU POUR MONTAGE SUR TUILES MÉCANIQUES","EG311",{"$f":"VLOOKUP(A58,'Liste de prix'!$1:$1048576,4,FALSE)","v":98},{"$f":"D12","v":0},null,89807311,"4 FERRURES D'ANCRAGE ALU POUR MONTAGE SUR TUILES MÉCANIQUES","EG311",85,null,null,null,null,null,null,9,0,5]
[89807312,"6 FERRURES D'ANCRAGE ALU POUR MONTAGE SUR TUILES MÉCANIQUES","EG312",{"$f":"VLOOKUP(A59,'Liste de prix'!$1:$1048576,4,FALSE)","v":141},{"$f":"D13","v":0},null,89807312,"6 FERRURES D'ANCRAGE ALU POUR MONTAGE SUR TUILES MÉCANIQUES","EG312",122,null,null,null,null,null,null,10,1,5]
[89807313,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES MÉCANIQUES","EG313",{"$f":"VLOOKUP(A60,'Liste de prix'!$1:$1048576,4,FALSE)","v":98},{"$f":"D12","v":0},null,89807313,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES MÉCANIQUES","EG313",85]
[89807314,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES MÉCANIQUES","EG314",{"$f":"VLOOKUP(A61,'Liste de prix'!$1:$1048576,4,FALSE)","v":141},{"$f":"D13","v":0},null,89807314,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES MÉCANIQUES","EG314",122,null,null,null,null,null,null,"Tire fonds",6,8]
[89807315,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES PLATES","EG315",{"$f":"VLOOKUP(A62,'Liste de prix'!$1:$1048576,4,FALSE)","v":98},{"$f":"D16","v":0},null,89807315,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES PLATES","EG315",85,null,null,null,null,null,null,0,0,0]
[89807316,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES PLATES","EG316",{"$f":"VLOOKUP(A63,'Liste de prix'!$1:$1048576,4,FALSE)","v":141},{"$f":"D13","v":0},null,89807316,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES PLATES","EG316",122,null,null,null,null,null,null,2,0,1]
[100015315,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES CANAL","ER137",{"$f":"VLOOKUP(A64,'Liste de prix'!$1:$1048576,4,FALSE)","v":141},{"$f":"D13","v":0},null,null,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES CANAL","ER137",122,null,null,null,null,null,null,3,2,0]
[89807317,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT ETERNIT","EG317",{"$f":"VLOOKUP(A65,'Liste de prix'!$1:$1048576,4,FALSE)","v":98},{"$f":"D12","v":0},null,89807317,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT ETERNIT","EG317",85,null,null,null,null,null,null,4,0,2]
[89807318,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT ETERNIT","EG318",{"$f":"VLOOKUP(A66,'Liste de prix'!$1:$1048576,4,FALSE)","v":141},{"$f":"D13","v":0},null,89807318,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT ETERNIT","EG318",122,null,null,null,null,null,null,5,1,2]
[89807319,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT D'ARDOISES","EG319",{"$f":"VLOOKUP(A67,'Liste de prix'!$1:$1048576,4,FALSE)","v":98},{"$f":"D12","v":0},null,89807319,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT D'ARDOISES","EG319",85,null,null,null,null,null,null,6,4,0]
[89807320,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT D'ARDOISES","EG320",{"$f":"VLOOKUP(A68,'Liste de prix'!$1:$1048576,4,FALSE)","v":141},{"$f":"D13","v":0},null,89807320,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT D'ARDOISES","EG320",122,null,null,null,null,null,null,7,2,2]
[100015314,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES CANAL","ER136",{"$f":"VLOOKUP(A69,'Liste de prix'!$1:$1048576,4,FALSE)","v":97},{"$f":"D12","v":0},null,null,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES CANAL","ER136",85,null,null,null,null,null,null,8,0,4]
[100016517,"4 FERRURES D'ANCRAGE ALU  A CRANS MTGE SUR CHEVRON","ER264",{"$f":"VLOOKUP(A70,'Liste de prix'!$1:$1048576,4,FALSE)","v":131},{"$f":"F12","v":0},null,100016517,"4 FERRURES D'ANCRAGE ALU  A CRANS MTGE SUR CHEVRON","ER264",115,null,null,null,null,null,null,9,6,0]
[100016518,"2 FERRURES D'ANCRAGE ALU  A CRANS MTGE SUR CHEVRON","ER265",{"$f":"VLOOKUP(A71,'Liste de prix'!$1:$1048576,4,FALSE)","v":79},{"$f":"F13","v":0},null,100016518,"2 FERRURES D'ANCRAGE ALU  A CRANS MTGE SUR CHEVRON","ER265",70,null,null,null,null,null,null,10,5,0]
[89807782,"KIT TIRE-FONDS POUR MONTAGE 2 CAPTEURS","EG94",{"$f":"VLOOKUP(A72,'Liste de prix'!$1:$1048576,4,FALSE)","v":247},{"$f":"H12","v":0},null,89807782,"KIT TIRE-FONDS POUR MONTAGE 2 CAPTEURS","EG94",219]
[89807783,"KIT TIRE-FONDS POUR MONTAGE 3 CAPTEURS","EG95",{"$f":"VLOOKUP(A73,'Liste de prix'!$1:$1048576,4,FALSE)","v":310},{"$f":"H13","v":0},null,89807783,"KIT TIRE-FONDS POUR MONTAGE 3 CAPTEURS","EG95",268]
[]
[]
[]
[]
[]
[]
[]
[]
[{"$f":"IF('SUN C250'!E41='feuille PRO c250'!M1,'feuille PRO c250'!A33,IF('SUN C250'!E41='feuille PRO c250'!M2,'feuille PRO c250'!A38,IF('SUN C250'!E41=M6,A46,IF('SUN C250'!E41=M7,A49,IF('SUN C250'!E41='feuille PRO c250'!M10,'feuille PRO c250'!A56)))))","v":7503821},{"$f":"VLOOKUP(A82,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT DE BASE 17° D'INTEGRATION TUILE CANAL 2 C250 V "},{"$f":"VLOOKUP(A82,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER641"},{"$f":"VLOOKUP(A82,'Liste de prix'!$1:$1048576,4,FALSE)","v":1113},{"$f":"IF('SUN C250'!E41='feuille PRO c250'!M1,'feuille PRO c250'!E33,IF('SUN C250'!E41='feuille PRO c250'!M2,'feuille PRO c250'!E38,IF('SUN C250'!E41='feuille PRO c250'!M6,'feuille PRO c250'!E46,IF('SUN C250'!E41='feuille PRO c250'!M7,'feuille PRO c250'!E49,IF('SUN C250'!E41='feuille PRO c250'!M10,'feuille PRO c250'!E55,IF('SUN C250'!E41='feuille PRO c250'!M11,'feuille PRO c250'!E56))))))","v":0},null,{"$f":"IF('SUN C250'!E41='feuille PRO c250'!M1,'feuille PRO c250'!G33,IF('SUN C250'!E41='feuille PRO c250'!M2,'feuille PRO c250'!G38,IF('SUN C250'!E41='feuille PRO c250'!M6,'feuille PRO c250'!G46,IF('SUN C250'!E41='feuille PRO c250'!M7,'feuille PRO c250'!G49,IF('SUN C250'!E41='feuille PRO c250'!M10,'feuille PRO c250'!G55,IF('SUN C250'!E41='feuille PRO c250'!M11,'feuille PRO c250'!G56))))))","v":7212880},{"$f":"VLOOKUP('feuille PRO c250'!G82,'Liste de prix'!$1:$1048576,2,FALSE)","v":"KIT DE BASE 17° D'INTEGRATION TUILE CANAL 2 C250 H "},{"$f":"VLOOKUP('feuille PRO c250'!G82,'Liste de prix'!$1:$1048576,3,FALSE)","v":"ER644"},{"$f":"VLOOKUP('feuille PRO c250'!G82,'Liste de prix'!$1:$1048576,4,FALSE)","v":1325},{"$f":"E82","v":0}]
[{"$f":"IF('SUN C250'!E41='feuille PRO c250'!M1,A34,IF('SUN C250'!E41='feuille PRO c250'!M2,A40,IF('SUN C250'!E41='feuille PRO c250'!M6,A47,IF('SUN C250'!E41='feuille PRO c250'!M7,'feuille PRO c250'!A50,\"\"))))","v":7212875},{"$f":"IF(A83=\"\",\"\",VLOOKUP(A83,'Liste de prix'!$1:$1048576,2,FALSE))","v":"KIT EXTENSION 17° INTEGRATION TUILE CANAL C 250 V "},{"$f":"IF(A83=\"\",\"\",VLOOKUP(A83,'Liste de prix'!$1:$1048576,3,FALSE))","v":"ER642"},{"$f":"IF(A83=\"\",\"\",VLOOKUP(A83,'Liste de prix'!$1:$1048576,4,FALSE))","v":425},{"$f":"IF('SUN C250'!E41='feuille PRO c250'!M1,E34,IF('SUN C250'!E41='feuille PRO c250'!M2,E40,IF('SUN C250'!E41='feuille PRO c250'!M6,E47,IF('SUN C250'!E41='feuille PRO c250'!M7,'feuille PRO c250'!E50,\"\"))))","v":0},null,{"$f":"IF('SUN C250'!E41='feuille PRO c250'!M1,G34,IF('SUN C250'!E41='feuille PRO c250'!M2,G40,IF('SUN C250'!E41='feuille PRO c250'!M6,G47,IF('SUN C250'!E41='feuille PRO c250'!M7,'feuille PRO c250'!G50,\"\"))))","v":7212877},{"$f":"IF(G83=\"\",\"\",VLOOKUP('feuille PRO c250'!G83,'Liste de prix'!$1:$1048576,2,FALSE))","v":"KIT EXTENSION 17° INTEGRATION TUILE CANAL C 250 H"},{"$f":"IF(G83=\"\",\"\",VLOOKUP('feuille PRO c250'!G83,'Liste de prix'!$1:$1048576,3,FALSE))","v":"ER645"},{"$f":"IF(G83=\"\",\"\",VLOOKUP('feuille PRO c250'!G83,'Liste de prix'!$1:$1048576,4,FALSE))","v":478},{"$f":"E83","v":0}]
[{"$f":"IF('SUN C250'!E41='feuille PRO c250'!M2,A41,\"\")","v":""},{"$f":"IF('SUN C250'!E41='feuille PRO c250'!M2,B41,\"\")","v":""},{"$f":"IF('SUN C250'!E41='feuille PRO c250'!M2,C41,\"\")","v":""},{"$f":"IF('SUN C250'!E41='feuille PRO c250'!M2,D41,\"\")","v":""},{"$f":"IF('SUN C250'!E41='feuille PRO c250'!M2,E41,\"\")","v":""},null,{"$f":"IF('SUN C250'!E41='feuille PRO c250'!M2,G41,\"\")","v":""},{"$f":"IF('SUN C250'!E41='feuille PRO c250'!M2,H41,\"\")","v":""},{"$f":"IF('SUN C250'!E41='feuille PRO c250'!M2,I41,\"\")","v":""},{"$f":"IF('SUN C250'!E41='feuille PRO c250'!M2,J41,\"\")","v":""},{"$f":"E84","v":""}]
[]
[]
[{"$f":"VLOOKUP('SUN C250'!E50,'feuille PRO c250'!A92:B99,2,FALSE)","v":89807311},{"$f":"VLOOKUP(A87,A58:E73,2,FALSE)","v":"4 FERRURES D'ANCRAGE ALU POUR MONTAGE SUR TUILES MÉCANIQUES"},{"$f":"VLOOKUP(A87,A58:E73,3,FALSE)","v":"EG311"},{"$f":"VLOOKUP(A87,A58:E73,4,FALSE)","v":98},{"$f":"VLOOKUP(A87,A58:E73,5,FALSE)","v":0}]
[{"$f":"A87+1","v":89807312},{"$f":"VLOOKUP(A88,A58:E73,2,FALSE)","v":"6 FERRURES D'ANCRAGE ALU POUR MONTAGE SUR TUILES MÉCANIQUES"},{"$f":"VLOOKUP(A88,A58:E73,3,FALSE)","v":"EG312"},{"$f":"VLOOKUP(A88,A58:E73,4,FALSE)","v":141},{"$f":"VLOOKUP(A88,A58:E73,5,FALSE)","v":0}]
[]
[]
[]
["Tuiles mécaniques (alu)",89807311]
["Tuiles mécaniques (inox)",89807313]
["Tuiles plates",89807315]
["Tuiles canal",100015314]
["Tuiles éternit",89807317]
["Tuiles ardoises",89807319]
[]
["kit tire-fonds",89807782]

{"sheet":"Liste de prix","index":8,"n_rows":5660,"n_cols":15,"rows_kept":5660,"cut":false,"hidden":true,"merged":[[5185,7,5185,8],[1118,6,1118,8],[5184,7,5184,8]]}
["N°Article","Désignation","Colis","Tarif HT au 01/01/2017","Eco Participation HT","code eco taxe  2017","Classe Energétique Chauffage","Classe Ener-\ngétique ECS","Profil de puisage ECS","Code EAN","Poids ","Long mm","Larg mm","Haut mm","Groupe article"]
[]
["LA LEGISLATION IMPOSE UNE ECO-PARTICIPATION  AFIN D'ORGANISER SUR LE TERRITOIRE NATIONAL LA COLLECTE ET"]
["LE RECYCLAGE DE CERTAINS PRODUITS ELECTRIQUES ET ELECTRONIQUES D'EQUIPEMENTS DE LA MAISON . CELA SIGNIFIE QUE LE"]
["CONSOMMATEUR POURRA DEMANDER AU PROFESSIONNEL LA REPRISE DE L'ANCIEN MATERIEL CONTRE L'ACHAT D'UN NOUVEL"]
["EQUIPEMENT DE MEME NATURE , SELON LE PRINCIPE DE << UN >> POUR << UN  >> . "]
["LES PRODUITS ELIGIBLES SONT REPERTORIES SUR LE SITE OFFICIEL : www.eco-systemes.fr "]
["ET  APPARAISSENT DANS NOTRE TARIF AVEC UN MONTANT HT D'ECO-PARTICIPATION "]
["* TOUT MONTANT D'ECO PARTICIPATION EST SUSCEPTIBLE D'EVOLUER EN CAS DE MODIFICATION DU BAREME PAR NOTRE ORGANISME COLLECTEUR"]
[]
["FAMILLE:","POMPE A CHALEUR"]
[]
[null,"VERSIONS POUR CHAUFFAGE ET RAFRAICHISSEMENT"]
[7610054,"OENOVIAPAC-2 4 MR-3/H",null,{"$f":"D30+D37+D42","v":4068},null,null,"A+++","/","/",366123859383,83.7,null,null,null,"C9"]
[7610055,"OENOVIAPAC-2 4 MR-3/EM",null,{"$f":"D30+D39+D42","v":4068},null,null,"A+++","/","/",366123859384,83.7,null,null,null,"C9"]
[7610056,"OENOVIAPAC-2 6 MR-3/H",null,{"$f":"D31+D37+D42","v":4157},null,null,"A++","/","/",366123859385,82.7,null,null,null,"C9"]
[7610057,"OENOVIAPAC-2 6 MR-3/EM",null,{"$f":"D31+D39+D42","v":4157},null,null,"A++","/","/",366123859386,82.7,null,null,null,"C9"]
[7610058,"OENOVIAPAC-2 8 MR-3/H",null,{"$f":"D32+D37","v":4850},null,null,"A++","/","/",366123859387,112.2,null,null,null,"C9"]
[7610059,"OENOVIAPAC-2 8 MR-3/EM",null,{"$f":"D32+D39","v":4850},null,null,"A++","/","/",366123859388,112.2,null,null,null,"C9"]
[7610060,"OENOVIAPAC-2 11 MR-3/H",null,{"$f":"D33+D38","v":6238},null,null,"A++","/","/",366123859389,168.7,null,null,null,"C9"]
[7610061,"OENOVIAPAC-2 11 MR-3/EM",null,{"$f":"D33+D40","v":6238},null,null,"A++","/","/",366123859390,168.7,null,null,null,"C9"]
[7610062,"OENOVIAPAC-2 11 TR-3/H",null,{"$f":"D34+D38","v":6542},null,null,"A++","/","/",366123859391,182.7,null,null,null,"C9"]
[7610063,"OENOVIAPAC-2 11 TR-3/ET",null,{"$f":"D34+D41","v":6542},null,null,"A++","/","/",366123859392,182.7,null,null,null,"C9"]
[7610064,"OENOVIAPAC-2 16 MR-3/H",null,{"$f":"D35+D38","v":7331},null,null,"A++","/","/",366123859393,168.7,null,null,null,"C9"]
[7610065,"OENOVIAPAC-2 16 MR-3/EM",null,{"$f":"D35+D40","v":7331},null,null,"A++","/","/",366123859394,168.7,null,null,null,"C9"]
[7610066,"OENOVIAPAC-2 16 TR-3/H",null,{"$f":"D36+D38","v":7756},null,null,"A++","/","/",366123859395,182.7,null,null,null,"C9"]
[7610067,"OENOVIAPAC-2 16 TR-3/ET",null,{"$f":"D36+D41","v":7756},null,null,"A++","/","/",366123859396,182.7,null,null,null,"C9"]
[]
["COMPOSANTS"]
[7603571,"AWHP 4 MR","EH336",1837,6.67,11050," /"," /"," /",3661238581012,48,450,950,690,"C9"]
[7609925,"AWHP 6 MR-2 ","EH380",1926,6.67,11050," /"," /"," /",3661238589513,47,450,950,690,"C9"]
[7609926,"AWHP 8 MR-2 ","EH381",2677,6.67,11050," /"," /"," /",3661238589520,77,450,1040,1030,"C9"]
[7609927,"AWHP 11 MR-2 ","EH382",3529,6.67,11050," /"," /"," /",3661238589537,131,450,1040,1440,"C9"]
[7609928,"AWHP 11 TR-2 ","EH383",3833,6.67,11050," /"," /"," /",3661238589544,145,450,1040,1440,"C9"]
[7609929,"AWHP 16 MR-2 ","EH384",4622,6.67,11050," /"," /"," /",3661238589551,131,450,1040,1440,"C9"]
[7609930,"AWHP 16 TR-2 ","EH385",5047,6.67,11050," /"," /"," /",3661238589568,145,450,1040,1440,"C9"]
[7609961,"MHX-3/H 4-8 ","EH413",2173,null,null," /"," /"," /",3661238589841,35.200000000000003,465,465,800,"C9"]
[7609962,"MHX-3/H 11-16 ","EH414",2709,null,null," /"," /"," /",3661238589858,37.700000000000003,465,465,800,"C9"]
[7609963,"MHX-3/EM 4-8 ","EH415",2173,null,null," /"," /"," /",3661238589865,35.200000000000003,465,465,800,"C9"]
[7609964,"MHX-3/EM 11-16 ","EH416",2709,null,null," /"," /"," /",3661238589872,37.700000000000003,465,465,800,"C9"]
[7609965,"MHX-3/ET 11-16 ","EH417",2709,null,null," /"," /"," /",3661238589889,37.700000000000003,465,465,800,"C9"]
[100015480,"RACCORD D'ADAPTATION FRIGO POUR 4 kW ET 6 kW","EH146",58,null,null," /"," /"," /",3661238381612,0.5,150,80,30,"C9"]
[]
[null,"VERSIONS POUR CLIMATISATION"]
[7610068,"OENOVIAPAC-2 4 MR-3/HI",null,{"$f":"D61+D68+D73+D75","v":5122},null,null,"A+++","/","/",366123859397,87.8,null,null,null,"C9"]
[7610069,"OENOVIAPAC-2 4 MR-3/EMI",null,{"$f":"D61+D70+D73+D74","v":5028},null,null,"A+++","/","/",366123859398,86.7,null,null,null,"C9"]
[7610070,"OENOVIAPAC-2 6 MR-3/HI",null,{"$f":"D62+D68+D73+D75","v":5211},null,null,"A++","/","/",366123859399,86.8,null,null,null,"C9"]
[7610071,"OENOVIAPAC-2 6 MR-3/EMI",null,{"$f":"D62+D70+D73+D74","v":5117},null,null,"A++","/","/",366123859400,85.7,null,null,null,"C9"]
[7610072,"OENOVIAPAC-2 8 MR-3/HI",null,{"$f":"D63+D68+D75","v":5904},null,null,"A++","/","/",366123859401,116.3,null,null,null,"C9"]
[7610073,"OENOVIAPAC-2 8 MR-3/EMI",null,{"$f":"D63+D70+D74","v":5810},null,null,"A++","/","/",366123859402,115.2,null,null,null,"C9"]
[7610074,"OENOVIAPAC-2 11 MR-3/HI",null,{"$f":"D64+D69+D75","v":7487},null,null,"A++","/","/",366123859403,172.79999999999998,null,null,null,"C9"]
[7610075,"OENOVIAPAC-2 11 MR-3/EMI",null,{"$f":"D64+D71+D74","v":7393},null,null,"A++","/","/",366123859404,171.7,null,null,null,"C9"]
[7610076,"OENOVIAPAC-2 11 TR-3/HI",null,{"$f":"D65+D69+D75","v":7791},null,null,"A++","/","/",366123859405,186.79999999999998,null,null,null,"C9"]
[7610077,"OENOVIAPAC-2 11 TR-3/ETI",null,{"$f":"D65+D72+D74","v":7697},null,null,"A++","/","/",366123859406,185.7,null,null,null,"C9"]
[7610078,"OENOVIAPAC-2 16 MR-3/HI",null,{"$f":"D66+D69+D75","v":8580},null,null,"A++","/","/",366123859407,172.79999999999998,null,null,null,"C9"]
[7610079,"OENOVIAPAC-2 16 MR-3/EMI",null,{"$f":"D66+D71+D74","v":8486},null,null,"A++","/","/",366123859408,171.7,null,null,null,"C9"]
[7610080,"OENOVIAPAC-2 16 TR-3/HI",null,{"$f":"D67+D69+D75","v":9005},null,null,"A++","/","/",366123859409,186.79999999999998,null,null,null,"C9"]
[7610081,"OENOVIAPAC-2 16 TR-3/ETI",null,{"$f":"D67+D72+D74","v":8911},null,null,"A++","/","/",366123859410,185.7,null,null,null,"C9"]
[]
["COMPOSANTS"]
[7603571,"AWHP 4 MR","EH336",1837,6.67,11050,"/","/","/",3661238581012,48,450,950,690,"C9"]
[7609925,"AWHP 6 MR-2 ","EH380",1926,6.67,11050,"/","/","/",3661238589513,47,450,950,690,"C9"]
[7609926,"AWHP 8 MR-2 ","EH381",2677,6.67,11050,"/","/","/",3661238589520,77,450,1040,1030,"C9"]
[7609927,"AWHP 11 MR-2 ","EH382",3529,6.67,11050,"/","/","/",3661238589537,131,450,1040,1440,"C9"]
[7609928,"AWHP 11 TR-2 ","EH383",3833,6.67,11050,"/","/","/",3661238589544,145,450,1040,1440,"C9"]
[7609929,"AWHP 16 MR-2 ","EH384",4622,6.67,11050,"/","/","/",3661238589551,131,450,1040,1440,"C9"]
[7609930,"AWHP 16 TR-2 ","EH385",5047,6.67,11050,"/","/","/",3661238589568,145,450,1040,1440,"C9"]
[7609966,"MHX-3/HI 4-8 ","EH418",2958,null,null,"/","/","/",3661238589896,35.200000000000003,465,465,800,"C9"]
[7609967,"MHX-3/HI 11-16 ","EH419",3689,null,null,"/","/","/",3661238589902,37.700000000000003,465,465,800,"C9"]
[7609968,"MHX-3/EMI 4-8 ","EH420",2958,null,null,"/","/","/",3661238589919,35.200000000000003,465,465,800,"C9"]
[7609969,"MHX-3/EMI 11-16 ","EH421",3689,null,null,"/","/","/",3661238589926,37.700000000000003,465,465,800,"C9"]
[7609970,"MHX-3/ETI 11-16 ","EH422",3689,null,null,"/","/","/",3661238589933,37.700000000000003,465,465,800,"C9"]
[100015480,"RACCORD D'ADAPTATION FRIGO POUR 4 kW ET 6 kW","EH146",58,null,null,"/","/","/",3661238381612,0.5,150,80,30,"C9"]
[100015481,"DOSSERET DE MONTAGE VERSION E","EH147",175,null,null,"/","/","/",3661238381629,3,715,420,115,"C9"]
[100015482,"DOSSERET DE MONTAGE VERSION H","EH148",269,null,null,"/","/","/",3661238381636,4.0999999999999996,715,420,115,"C9"]
[]
["OPTIONS"]
[100004417,"FILTRE 400UM + VANNE D'ISOLEMENT PAC ROE 6-10 ET ROE+","EH61",105,null,null,"/","/","/",3661238003415,0.85,175,90,130,"C6"]
[100011222,"SUPPORT MURALE & PLOTS ANTIVIBRATILES POUR  ROE-II AWHP 6-8","EH95",162,null,null,"/","/","/",3661238339927,5.4,820,90,90,"C6"]
[100012532,"BAC DE RECUPERATION CONDENSATS POUR SUPPORT MURAL","EH111",142,null,null,"/","/","/",3661238361553,2,960,440,80,"C6"]
[100012534,"CORDON CHAUFFANT ELECTRIQUE","EH113",150,null,null,"/","/","/",3661238361577,0.2,200,200,10,"C6"]
[100012533,"SUPPORT POSE AU SOL AWHP","EH112",45,null,null,"/","/","/",3661238361560,1.2,450,140,80,"C6"]
[100015476,"LIAISON FRIGORIFIQUE PE 1/2\" 1/4\" - LG 10 m","EH142",233,null,null,"/","/","/",3661238381575,7.9,600,650,150,"C6"]
[100012535,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 5m","EH114",233,null,null,"/","/","/",3661238361522,4.5999999999999996,600,600,150,"C6"]
[100012536,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 10m","EH115",416,null,null,"/","/","/",3661238361539,7.2,600,600,200,"C6"]
[100012537,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 20m","EH116",751,null,null,"/","/","/",3661238361546,14.3,750,750,230,"C6"]
[100008841,"BALLON TAMPON 80L B 80 T","EH85",521,null,null,"/","/","/",3661238166325,44.5,510,510,920,"C6"]
[100004415,"BALLON TAMPON 160L B 150 T","EH60",781,null,null,"/","/","/",3661238003422,63.2,825,690,1120,"C6"]
[100002276,"VANNE D'INVERSION CHAUFFAGE SANITAIRE MC 35E MC 45 ET 65","HC135",352,null,null,"/","/","/",3661238007734,1,195,155,130,"C0"]
[100003301,"KIT CABLAGE PLANCHER CHAUFFANT DIRECT","HA249",39,0.02,95020,"/","/","/",3661238005570,0.1,210,140,20,"C0"]
[88017904,"THERMOSTAT AMBIANCE PROGRAMMABLE (FILAIRE)","AD191",161,0.12,95010,"/","/","/",3661238102415,0.25,135,90,55,"C0"]
[88017010,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (SANS FILS)","AD192",286,0.12,95010,"/","/","/",3661238102439,0.42499999999999999,180,150,90,"C0"]
[100015479,"VANNE D'INVERSION CHAUFFAGE-SANITAIRE+SONDE ECS ","EH145",335,null,null,"/","/","/",3661238381605,4.2,410,210,125,"C6"]
[100015468,"KIT RAC HYDRAULIQUE PAC - BALLON ECS","EH149",99,null,null,"/","/","/",3661238413818,1.2,575,505,145,"C6"]
[100015481,"DOSSERET DE MONTAGE VERSION E","EH147",175,null,null,"/","/","/",3661238381629,6,715,420,115,"C6"]
[]
[]
[7638440,"OENOVIAPAC-2C 4 MR-4/H V200",null,{"$f":"SUM(D115+D123+D127)","v":5997},null,null,"A++","A","L",3661238640337,null,null,null,null,"C9"]
[7638441,"OENOVIAPAC-2C 4 MR-4/E V200",null,{"$f":"SUM(D115+D125+D127)","v":6111},null,null,"A++","A","L",3661238640344,null,null,null,null,"C9"]
[7649701,"OENOVIAPAC 2C 4.5 MR 4/E V200",null,{"$f":"D116+D125+D127","v":6158},null,null,"A++","A","L",3661238659629,null,null,null,null,"C9"]
[7638442,"OENOVIAPAC-2C 6 MR-4/H V200",null,{"$f":"SUM(D117+D123+D127)","v":6086},null,null,"A++","A","L",3661238640351,null,null,null,null,"C9"]
[7638443,"OENOVIAPAC-2C 6 MR-4/E V200",null,{"$f":"SUM(D117+D125+D127)","v":6200},null,null,"A++","A","L",3661238640368,null,null,null,null,"C9"]
[7638444,"OENOVIAPAC-2C 8 MR-4/H V200",null,{"$f":"SUM(D118+D123)","v":6779},null,null,"A++","A","L",3661238640375,null,null,null,null,"C9"]
[7638445,"OENOVIAPAC-2C 8 MR-4/E V200",null,{"$f":"SUM(D118+D125)","v":6893},null,null,"A++","A","L",3661238640382,null,null,null,null,"C9"]
[7638446,"OENOVIAPAC-2C 11 MR-4/H V200",null,{"$f":"SUM(D119+D124)","v":8846},null,null,"A++","A","L",3661238640399,null,null,null,null,"C9"]
[7638447,"OENOVIAPAC-2C 11 MR-4/E V200",null,{"$f":"SUM(D119+D126)","v":8971},null,null,"A++","A","L",3661238640405,null,null,null,null,"C9"]
[7638448,"OENOVIAPAC-2C 11 TR-4/H V200",null,{"$f":"SUM(D120+D124)","v":9150},null,null,"A++","A","L",3661238640412,null,null,null,null,"C9"]
[7638449,"OENOVIAPAC-2C 11 TR-4/E V200",null,{"$f":"SUM(D120+D126)","v":9275},null,null,"A++","A","L",3661238640429,null,null,null,null,"C9"]
[7638450,"OENOVIAPAC-2C 16 MR-4/H V200",null,{"$f":"SUM(D121+D124)","v":9939},null,null,"A++","A","L",3661238640436,null,null,null,null,"C9"]
[7638451,"OENOVIAPAC-2C 16 MR-4/E V200",null,{"$f":"SUM(D121+D126)","v":10064},null,null,"A++","A","L",3661238640443,null,null,null,null,"C9"]
[7638452,"OENOVIAPAC-2C 16 TR-4/H V200",null,{"$f":"SUM(D122+D124)","v":10364},null,null,"A++","A","L",3661238640450,null,null,null,null,"C9"]
[7638453,"OENOVIAPAC-2C 16 TR-4/E V200",null,{"$f":"SUM(D122+D126)","v":10489},null,null,"A++","A","L",3661238640467,null,null,null,null,"C9"]
[]
["COMPOSANTS"]
[7603571,"AWHP 4 MR","EH336",1837,6.67,11050,"/","/","/",3661238581012,48,450,950,690,"C9"]
[7656794,"AWHP 4.5 MR-4","EH616",1884,6.67,11050,"/","/","/",3661238665613,54,1000,430,1050,"C9"]
[7609925,"AWHP 6 MR-2 ","EH380",1926,6.67,11050,"/","/","/",3661238589513,47,450,950,690,"C9"]
[7609926,"AWHP 8 MR-2 ","EH381",2677,6.67,11050,"/","/","/",3661238589520,77,450,1040,1030,"C9"]
[7609927,"AWHP 11 MR-2 ","EH382",3529,6.67,11050,"/","/","/",3661238589537,131,450,1040,1440,"C9"]
[7609928,"AWHP 11 TR-2 ","EH383",3833,6.67,11050,"/","/","/",3661238589544,145,450,1040,1440,"C9"]
[7609929,"AWHP 16 MR-2 ","EH384",4622,6.67,11050,"/","/","/",3661238589551,131,450,1040,1440,"C9"]
[7609930,"AWHP 16 TR-2 ","EH385",5047,6.67,11050,"/","/","/",3661238589568,145,450,1040,1440,"C9"]
[7625406,"MHX-4/H 4-8 V200 ","EH546",4102,null,null,"/","/","/",3661238622968,143,970,675,1435,"C9"]
[7625407,"MHX-4/H 11-16 V200 ","EH547",5317,null,null,"/","/","/",3661238622975,145,970,675,1435,"C9"]
[7625408,"MHX-4/E 4-8 V200 ","EH548",4216,null,null,"/","/","/",3661238622982,146,970,675,1435,"C9"]
[7625421,"MHX-4/E 11-16 V200 ","EH549",5442,null,null,"/","/","/",3661238622999,148,970,675,1435,"C9"]
[100015480,"RACCORD D'ADAPTATION FRIGO POUR 4 kW ET 6 kW","EH146",58,null,null,"/","/","/",3661238381612,0.5,150,80,30,"C9"]
[]
["OPTIONS"]
[100004417,"FILTRE 400UM + VANNE D'ISOLEMENT PAC ROE 6-10 ET ROE+","EH61",105,null,null,"/","/","/",3661238003415,0.85,175,90,130,"C6"]
[100011222,"SUPPORT MURALE & PLOTS ANTIVIBRATILES POUR  ROE-II AWHP 6-8","EH95",162,null,null,"/","/","/",3661238339927,5.4,820,90,90,"C6"]
[100018409,"SUPPORT MURAL AWHP 11à 27 kW","EH250",166,null,null,"/","/","/",3661238543874,5,820,90,90,"C6"]
[100012532,"BAC DE RECUPERATION CONDENSATS POUR SUPPORT MURAL","EH111",142,null,null,"/","/","/",3661238361553,2,960,440,80,"C6"]
[100012534,"CORDON CHAUFFANT ELECTRIQUE","EH113",150,null,null,"/","/","/",3661238361577,0.2,200,200,10,"C6"]
[100012533,"SUPPORT POSE AU SOL AWHP","EH112",45,null,null,"/","/","/",3661238361560,1.2,450,140,80,"C6"]
[100015476,"LIAISON FRIGORIFIQUE PE 1/2\" 1/4\" - LG 10 m","EH142",233,null,null,"/","/","/",3661238381575,7.9,600,650,150,"C6"]
[100012535,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 5m","EH114",233,null,null,"/","/","/",3661238361522,4.5999999999999996,600,600,150,"C6"]
[100012536,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 10m","EH115",416,null,null,"/","/","/",3661238361539,7.2,600,600,200,"C6"]
[100012537,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 20m","EH116",751,null,null,"/","/","/",3661238361546,14.3,750,750,230,"C6"]
[100015468,"KIT RAC HYDRAULIQUE PAC - BALLON ECS","EH149",99,null,null,"/","/","/",3661238413818,1.2,575,505,145,"C6"]
[100008841,"BALLON TAMPON 80L B 80 T","EH85",521,null,null,"/","/","/",3661238166325,44.5,510,510,920,"C6"]
[100004415,"BALLON TAMPON 160L B 150 T","EH60",781,null,null,"/","/","/",3661238003422,63.2,825,690,1120,"C6"]
[100003301,"KIT CABLAGE PLANCHER CHAUFFANT DIRECT","HA249",39,0.02,95020,"/","/","/",3661238005570,0.1,210,140,20,"C0"]
[7624902,"KIT CABLAGE PLANCHER CHAUFFANT DIRECT","HA255",37,0.02,95020,"/","/","/",3661238618176,0.1,210,140,20,"C0"]
[88017904,"THERMOSTAT AMBIANCE PROGRAMMABLE (FILAIRE)","AD191",161,0.12,95010,"/","/","/",3661238102415,0.25,135,90,55,"C0"]
[88017010,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (SANS FILS)","AD192",286,0.12,95010,"/","/","/",3661238102439,0.42499999999999999,180,150,90,"C0"]
[100019114,"KIT DETECTEUR DE CONDENSATION","HK27",212,0.12,95010,"/","/","/",3661238569119,0.7,185,130,105,"C0"]
[7619010,"KIT VANNE 3 VOIES","EH528",576,0.12,95010,"/","/","/",3661238618152,17.7,750,300,150,"C0"]
[7622273,"CARTE DE REGULATION 2 CIRCUITS","EH527",199,0.12,95010,"/","/","/",3661238618145,0.3,185,130,105,"C6"]
[7626737,"KIT ISOLATION MODE FROID","EH567",208,null,null,"/","/","/",3661238624115,0.64,615,280,80,"C0"]
[7636899,"KIT SILENCIEUX MODULE EXTERIEUR","EH572",60,0.02,95020,"/","/","/",3661238644335,0.2,170,210,20,"C0"]
[7622433,"KIT SONDE CONDENSATION 0-10V HZ64","HZ64",383,0.02,95020,"/","/","/",3661238614123,0.3,185,130,105,"C6"]
[]
["OPTIONS ECS"]
[7631121,"KIT CONNEXION BASE ","EH590",458,null,null,null,null,null,3661238631229,10.9,1187,397,181,"C6"]
[7631133,"KIT CONNEXION SECOND CIRCUIT","EH591",132,null,null,null,null,null,3661238631311,2.4500000000000002,600,150,100,"C6"]
[7631134,"KIT CONNEXION CHAUDIERE APPOIN","EH592",132,null,null,null,null,null,3661238631328,2.1,795,160,160,"C6"]
[7631764,"KIT CONNEXION RECIRCULATIO","EH593",77,null,null,null,null,null,3661238632349,1.55,600,150,100,"C6"]
[]
[]
[7609994,"OENOVIAPAC-2 CONFORT 4 MR-2/H",null,{"$f":"D181+D190+D196","v":5089},null,null,"A++","/","/",366123859365,110.1,null,null,null,"C6"]
[7609995,"OENOVIAPAC-2 CONFORT 4 MR-2/EM",null,{"$f":"D181+D192+D196","v":5579},null,null,"A++","/","/",366123859366,116.2,null,null,null,"C6"]
[7609996,"OENOVIAPAC-2 CONFORT 6 MR-2/H",null,{"$f":"D182+D190+D196","v":5178},null,null,"A++","/","/",366123859367,109.1,null,null,null,"C6"]
[7609997,"OENOVIAPAC-2 CONFORT 6 MR-2/EM",null,{"$f":"D182+D192+D196","v":5668},null,null,"A++","/","/",366123859368,115.2,null,null,null,"C6"]
[7609998,"OENOVIAPAC-2 CONFORT 8 MR-2/H",null,{"$f":"D183+D190","v":5871},null,null,"A++","/","/",366123859369,138.6,null,null,null,"C6"]
[7609999,"OENOVIAPAC-2 CONFORT 8 MR-2/EM",null,{"$f":"D183+D192","v":6361},null,null,"A++","/","/",366123859370,144.69999999999999,null,null,null,"C6"]
[7610000,"OENOVIAPAC-2 CONFORT 11 MR-2/H",null,{"$f":"D184+D191","v":7398},null,null,"A++","/","/",366123859371,195.2,null,null,null,"C6"]
[7610001,"OENOVIAPAC-2 CONFORT 11 MR-2/EM",null,{"$f":"D184+D193","v":7975},null,null,"A++","/","/",366123859372,205.5,null,null,null,"C6"]
[7610002,"OENOVIAPAC-2 CONFORT 11 TR-2/H",null,{"$f":"D185+D191","v":7702},null,null,"A++","/","/",366123859373,209.2,null,null,null,"C6"]
[7610003,"OENOVIAPAC-2 CONFORT 11 TR-2/ET",null,{"$f":"D185+D193","v":8279},null,null,"A++","/","/",366123859374,219.5,null,null,null,"C6"]
[7610004,"OENOVIAPAC-2 CONFORT 16 MR-2/H",null,{"$f":"D186+D191","v":8491},null,null,"A++","/","/",366123859375,195.2,null,null,null,"C6"]
[7610005,"OENOVIAPAC-2 CONFORT 16 MR-2/EM",null,{"$f":"D186+D193","v":9068},null,null,"A++","/","/",366123859376,205.5,null,null,null,"C6"]
[7610006,"OENOVIAPAC-2 CONFORT 16 TR-2/H",null,{"$f":"D187+D191","v":8916},null,null,"A++","/","/",366123859377,209.2,null,null,null,"C6"]
[7610007,"OENOVIAPAC-2 CONFORT 16 TR-2/ET",null,{"$f":"D187+D193","v":9493},null,null,"A++","/","/",366123859378,219.5,null,null,null,"C6"]
[7610008,"OENOVIAPAC-2 CONFORT 22 TR-2/H",null,{"$f":"D188+D194+D197","v":11380},null,null,"A++","/","/",366123859379,211.2,null,null,null,"C6"]
[7610009,"OENOVIAPAC-2 CONFORT 22 TR-2/ET",null,{"$f":"D188+D195+D197","v":12196},null,null,"A++","/","/",366123859380,217.29999999999998,null,null,null,"C6"]
[7610010,"OENOVIAPAC-2 CONFORT 27 TR-2/H",null,{"$f":"D189+D194","v":12613},null,null,"A+","/","/",366123859381,216.2,null,null,null,"C6"]
[7610011,"OENOVIAPAC-2 CONFORT 27 TR-2/ET",null,{"$f":"D189+D195","v":13429},null,null,"A+","/","/",366123859382,222.29999999999998,null,null,null,"C6"]
[]
["COMPOSANTS"]
[7603571,"AWHP 4 MR","EH336",1837,6.67,11050,"/","/","/",3661238581012,48,450,950,690,"C9"]
[7609925,"AWHP 6 MR-2 ","EH380",1926,6.67,11050,"/","/","/",3661238589513,47,450,950,690,"C9"]
[7609926,"AWHP 8 MR-2 ","EH381",2677,6.67,11050,"/","/","/",3661238589520,77,450,1040,1030,"C9"]
[7609927,"AWHP 11 MR-2 ","EH382",3529,6.67,11050,"/","/","/",3661238589537,131,450,1040,1440,"C9"]
[7609928,"AWHP 11 TR-2 ","EH383",3833,6.67,11050,"/","/","/",3661238589544,145,450,1040,1440,"C9"]
[7609929,"AWHP 16 MR-2 ","EH384",4622,6.67,11050,"/","/","/",3661238589551,131,450,1040,1440,"C9"]
[7609930,"AWHP 16 TR-2","EH385",5047,6.67,11050,"/","/","/",3661238589568,145,450,1040,1440,"C9"]
[7655104,"AWHP 22 TR","EH614",5900,6.67,11050,"/","/","/",3661238663817,143,450,1100,1430,"C9"]
[7655105,"AWHP 27 TR","EH615",7169,6.67,11050,"/","/","/",3661238663824,148,450,1100,1430,"C9"]
[7609940,"MHR-IN-2/H 4-8 OE-TRO ","EH392",3194,null,null,"/","/","/",3661238589636,61.6,670,1135,650,"C6"]
[7609941,"MHR-IN-2/H 11-16 OE-TRO ","EH393",3869,null,null,"/","/","/",3661238589643,64.2,670,1135,650,"C6"]
[7609942,"MHR-IN-2/E 4-8 OE-TRO ","EH394",3684,null,null,"/","/","/",3661238589650,68.2,670,1135,650,"C6"]
[7609943,"MHR-IN-2/E 11-16 OE-TRO ","EH395",4446,null,null,"/","/","/",3661238589667,67.7,670,1135,650,"C6"]
[7609944,"MHR-IN-2/H 22-27 OE-TRO ","EH396",5444,null,null,"/","/","/",3661238589674,74.5,670,1135,650,"C6"]
[7609945,"MHR-IN-2/E 22-27 OE-TRO ","EH397",6260,null,null,"/","/","/",3661238589681,74.2,670,1135,650,"C6"]
[100015480,"RACCORD D'ADAPTATION FRIGO POUR 4 kW ET 6 kW","EH146",58,null,null,"/","/","/",3661238381612,0.5,150,80,30,"C9"]
[100018428,"RACCORD D'ADAPTATION FRIGO POUR 22 kW","HK26",36,null,null,"/","/","/",3661238544635,0.1,140,70,25,"C9"]
[]
["OPTIONS"]
[100011222,"SUPPORT MURALE & PLOTS ANTIVIBRATILES POUR  ROE-II AWHP 6-8","EH95",162,null,null,"/","/","/",3661238339927,5.4,820,90,90,"C6"]
[100018409,"SUPPORT MURAL AWHP 11à 27 kW","EH250",166,null,null,"/","/","/",3661238543874,5,820,90,90,"C6"]
[100012532,"BAC DE RECUPERATION CONDENSATS POUR SUPPORT MURAL","EH111",142,null,null,"/","/","/",3661238361553,2,960,440,80,"C6"]
[100012534,"CORDON CHAUFFANT ELECTRIQUE","EH113",150,null,null,"/","/","/",3661238361577,0.2,200,200,10,"C6"]
[100012533,"SUPPORT POSE AU SOL AWHP","EH112",45,null,null,"/","/","/",3661238361560,1.2,450,140,80,"C6"]
[100012535,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 5m","EH114",233,null,null,"/","/","/",3661238361522,4.5999999999999996,600,600,150,"C6"]
[100012536,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 10m","EH115",416,null,null,"/","/","/",3661238361539,7.2,600,600,200,"C6"]
[100012537,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 20m","EH116",751,null,null,"/","/","/",3661238361546,14.2,750,750,230,"C6"]
[100015476,"LIAISON FRIGORIFIQUE PE 1/2\" 1/4\" - LG 10 m","EH142",233,null,null,"/","/","/",3661238381575,7.9,600,650,150,"C6"]
[100018410,"KIT ISOLATION MODE FROID MIT-IN iSYSTEM","HK24",271,null,null,"/","/","/",3661238543881,0.87,360,340,180,"C6"]
[100018411,"KIT ISOLATION MODE FROID KIT VANNE 3 VOIES (CIRCUIT B)","HK25",153,null,null,"/","/","/",3661238543898,0.26,310,210,130,"C6"]
[100008841,"BALLON TAMPON 80L B 80 T","EH85",521,null,null,"/","/","/",3661238166325,44.5,510,510,920,"C6"]
[100003301,"KIT CABLAGE PLANCHER CHAUFFANT DIRECT","HA249",39,0.02,95020,"/","/","/",3661238005570,0.1,210,140,20,"C0"]
[100017830,"KIT VANNE 3 VOIES (CIRCUIT B)","HK21",667,null,null,"/","/","/",3661238544727,5.9,880,270,150,"C6"]
[100017832,"KIT TUBULURES 2 CIRCUITS","HK22",142,null,null,"/","/","/",3661238544710,1.6,880,270,150,"C6"]
[100017833,"VANNE D'INVERSION CHAUFFAGE-SANITAIRE","HK23",198,null,null,"/","/","/",3661238544734,1.4,310,230,130,"C6"]
[100015468,"KIT RAC HYDRAULIQUE PAC - BALLON ECS","EH149",99,null,null,"/","/","/",3661238413818,1.2,575,505,145,"C6"]
[100020164,"COLLECTEUR 2/3 CIRCUITS ","EA140",348,null,null,"/","/","/",3661238575011,6.6,660,180,200,"C0"]
[100020165,"CONSOLE MUR COLLECTEUR ","EA141",44,null,null,"/","/","/",3661238575028,1.2,220,125,70,"C0"]
[100020166,"CONSOLE MUR 1 MODULE ","EA142",116,null,null,"/","/","/",3661238575035,1.6,220,125,70,"C0"]
[100020167,"CIRCUIT DIRECT P.ELEC CLASSE A  ","EA143",644,0.83,14050,"/","/","/",3661238575042,5.0999999999999996,460,270,235,"C0"]
[100020169,"MODULE HYDR COMPACT 2 CIRCUITS HEE","EA145",1146,0.83,14050,"/","/","/",3661238575059,9,525,415,210,"C0"]
[100020294,"KIT COMPTAGE D'ENERGIE","HK29",190,0.12,95010,"/","/","/",3661238576513,0.34,190,145,124,"C6"]
[]
["OPTIONS REGULATIONS"]
[100013304,"OPTION V3V ","AD249",158,0.12,95010,"/","/","/",3661238363519,0.4,260,170,130,"C0"]
[100013305,"SONDE SYSTÈME ECS","AD250",46,0.02,95020,"/","/","/",3661238363588,0.13400000000000001,150,210,25,"C0"]
[100013306,"SONDE EXTERIEURE RADIO ","AD251",77,0.12,95010,"/","/","/",3661238363595,0.15,150,210,40,"C0"]
[100013307,"MODULE CHAUDIERE RADIO (EMETTEUR)","AD252",123,0.12,95010,"/","/","/",3661238363601,0.32,260,160,130,"C0"]
[100018923,"CDE À DIST RADIO CDR 2/CD","AD284",237,0.12,95010,"/","/","/",3661238544932,0.253,175,122,60,"C0"]
[100013477,"COMMANDE A DISTANCE RS 400","AD257",177,0.12,95010,"/","/","/",3661238364257,0.253,175,122,60,"C0"]
[100013472,"CDE A DISTANCE RADIO RS 400R     ","AD255",238,0.12,95010,"/","/","/",3661238364233,0.253,175,122,60,"C0"]
[88017851,"CABLE DE LIAISON BUS LG 12 M","AD134",110,0.02,95020,"/","/","/",3661238048850,0.4,350,260,30,"C0"]
[88017878,"MODULE DE TELESURVEILLANCE VOCAL TELCOM 2","AD152",704,0.12,95010,"/","/","/",3661238048751,1.1000000000000001,210,190,105,"C0"]
[88017017,"SONDE DEPART v3v","AD199",80,0.02,95020,"/","/","/",3661238049185,0.21,150,200,40,"C0"]
[100002803,"COMMANDE A DISTANCE SIMPLIFIEE AD208","AD208",104,0.12,95010,"/","/","/",3661238554931,0.2,120,85,40,"C0"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.2,200,150,30,"C0"]
[7623159,"KIT DE REGULATION 2 CIRCUITS ","EH493",655,0.12,95010,"/","/","/",3661238619517,2.2200000000000002,325,280,90,"C0"]
[]
[]
[7617624,"OEnoviaPAC-GS 5 MR","HZ38",6866,6.67,11050,"A++","/","/",3661238603561,149.69999999999999,970,675,1135,"C6"]
[7617626,"OEnoviaPAC-GS 5 TR","HZ39",6866,6.67,11050,"A++","/","/",3661238603578,149.69999999999999,970,675,1135,"C6"]
[7618122,"OEnoviaPAC-GS 9 MR","HZ40",7595,6.67,11050,"A++","/","/",3661238614437,166,970,675,1135,"C6"]
[7618123,"OEnoviaPAC-GS 9 TR","HZ41",7595,6.67,11050,"A++","/","/",3661238614444,166,970,675,1135,"C6"]
[7618124,"OEnoviaPAC-GS 12 MR","HZ42",8177,6.67,11050,"A++","/","/",3661238603585,168,970,675,1135,"C6"]
[7615884,"OEnoviaPAC-GS 12 TR","HZ43",8177,6.67,11050,"A++","/","/",3661238603592,168,970,675,1135,"C6"]
[7618125,"OEnoviaPAC-GS 15 TR","HZ44",8781,6.67,11050,"A++","/","/",3661238603608,182.9,970,675,1135,"C6"]
[7618126,"OEnoviaPAC-GS 19 TR","HZ45",9488,6.67,11050,"A++","/","/",3661238603615,173.4,970,675,1135,"C6"]
[7618127,"OEnoviaPAC-GS 27 TR","HZ46",11142,6.67,11050,"A++","/","/",3661238603622,208.5,970,675,1135,"C6"]
[]
["OPTIONS "]
[7616429,"VANNE INVERSION + SONDE ECS GSHP 19 – 27 kW ","HZ17",425,0.17,14060,"/","/","/",3661238600812,4.0999999999999996,410,210,110,"C6"]
[7616680,"KIT APPOINT ELECTRIQUE 9 kW GSHP 05 à 15 kW","HZ20",655,0.17,14060,"/","/","/",3661238639829,4.7,420,280,190,"C6"]
[7616643,"KIT APPOINT ELECTRIQUE 9 kW GSHP 19 - 27 kW","HZ19",708,0.17,14060,"/","/","/",3661238603226,4.8,420,280,190,"C6"]
[7618061,"KIT ECHANGEUR DE BARRAGE GSHP 05 – 09 kW","HZ24",957,null,null,"/","/","/",3661238603264,16.2,660,220,325,"C6"]
[7618063,"KIT ECHANGEUR DE BARRAGE GSHP 12 – 15 kW","HZ26",1165,null,null,"/","/","/",3661238603288,19.5,660,220,325,"C6"]
[7618065,"KIT ECHANGEUR DE BARRAGE GSHP 19 – 27 kW","HZ28",1519,null,null,"/","/","/",3661238603301,25.4,660,220,325,"C6"]
[7622431,"KIT CABLAGE THERMOSTAT DE SECURITE PCBT","HZ29",75,0.02,95020,"/","/","/",3661238614116,0.3,210,150,40,"C6"]
[7622062,"KIT POMPE WILO PARA 25/1-8 pour GSHP 19","HZ63",666,0.83,14050,"/","/","/",3661238613041,5,360,235,285,"C6"]
[7610411,"KIT CIRCUIT PLANCHER CHAUFFANT ","ER604",728,0.83,14050,"/","/","/",3661238600669,5.3,815,415,250,"C0"]
[7620436,"KIT ISOLATION MODE FROID","ER581",183,null,null,"/","/","/",3661238621572,3.5,615,205,205,"C0"]
[7610412,"KIT CIRCUIT RADIATEUR","ER605",479,0.83,14050,"/","/","/",3661238600645,6.8,815,415,250,"C0"]
[7610667,"KIT DE RACCORDEMENT BALLON TAMPON - GSHP","ER606",198,null,null,"/","/","/",3661238600652,3.2,860,250,135,"C0"]
[7607396,"COLIS BALLON TAMPON GSHP 200L","ER602",894,null,null,"/","/","/",3661238600034,85,790,675,1330,"C0"]
[]
["OPTIONS REGULATION"]
[100013304,"OPTION V3V ","AD249",158,0.12,95010,"/","/","/",3661238363519,0.4,260,170,130,"C0"]
[100013305,"SONDE SYSTÈME ECS","AD250",46,0.02,95020,"/","/","/",3661238363588,0.13400000000000001,150,210,25,"C0"]
[100013306,"SONDE EXTERIEURE RADIO ","AD251",77,0.12,95010,"/","/","/",3661238363595,0.15,150,210,40,"C0"]
[100013307,"MODULE CHAUDIERE RADIO (EMETTEUR)","AD252",123,0.12,95010,"/","/","/",3661238363601,0.32,260,160,130,"C0"]
[100018923,"CDE À DIST RADIO CDR 2/CD","AD284",237,0.12,95010,"/","/","/",3661238544932,0.253,175,122,60,"C0"]
[100013477,"COMMANDE A DISTANCE RS 400","AD257",177,0.12,95010,"/","/","/",3661238364257,0.253,175,122,60,"C0"]
[100013472," CDE A DISTANCE RADIO RS 400R     ","AD255",238,0.12,95010,"/","/","/",3661238364233,0.253,175,122,60,"C0"]
[88017851,"CABLE DE LIAISON BUS LG 12 M","AD134",110,0.02,95020,"/","/","/",3661238048850,0.4,350,260,30,"C0"]
[88017017,"SONDE DEPART v3v","AD199",80,0.02,95020,"/","/","/",3661238049185,0.21,150,200,40,"C0"]
[100002803,"COMMANDE A DISTANCE SIMPLIFIEE AD208","AD208",104,0.12,95010,"/","/","/",3661238554931,0.2,120,85,40,"C0"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.2,200,150,30,"C0"]
[100020294,"KIT COMPTAGE D'ENERGIE","HK29",190,0.12,95010,"/","/","/",3661238576513,0.34,190,145,124,"C6"]
[100019114,"KIT SONDE HYGRO RAFRAICHISSEMENT","HK27",212,0.12,95010,"/","/","/",3661238569119,0.2,185,130,105,"C0"]
[]
[]
[7638403,"OEnoviaPAC-GS 5 MR/B200GHL",null,{"$f":"SUM(D297+D304+D305)","v":8957},null,null,"A++","A","L",3661238640474,null,null,null,null,"C6"]
[7638404,"OEnoviaPAC-GS 5 MR/V200GHL",null,{"$f":"SUM(D297+D304+D306)","v":8844},null,null,"A++","A","L",3661238640481,null,null,null,null,"C6"]
[7638405,"OEnoviaPAC-GS 5 TR/B200GHL",null,{"$f":"SUM(D298+D304+D305)","v":8957},null,null,"A++","A","L",3661238640498,null,null,null,null,"C6"]
[7638406,"OEnoviaPAC-GS 5 TR/V200GHL",null,{"$f":"SUM(D298+D304+D306)","v":8844},null,null,"A++","A","L",3661238640504,null,null,null,null,"C6"]
[7638407,"OEnoviaPAC-GS 9 MR/B200GHL",null,{"$f":"SUM(D299+D304+D305)","v":9686},null,null,"A++","A","L",3661238640511,null,null,null,null,"C6"]
[7638408,"OEnoviaPAC-GS 9 MR/V200GHL",null,{"$f":"SUM(D299+D304+D306)","v":9573},null,null,"A++","A","L",3661238640528,null,null,null,null,"C6"]
[7638409,"OEnoviaPAC-GS 9 TR/B200GHL",null,{"$f":"SUM(D300+D304+D305)","v":9686},null,null,"A++","A","L",3661238640535,null,null,null,null,"C6"]
[7638410,"OEnoviaPAC-GS 9 TR/V200GHL",null,{"$f":"SUM(D300+D304+D306)","v":9573},null,null,"A++","A","L",3661238640542,null,null,null,null,"C6"]
[7638411,"OEnoviaPAC-GS 12 MR/B200GHL",null,{"$f":"SUM(D301+D304+D305)","v":10268},null,null,"A++","A","L",3661238640559,null,null,null,null,"C6"]
[7638412,"OEnoviaPAC-GS 12 MR/V200GHL",null,{"$f":"SUM(D301+D304+D306)","v":10155},null,null,"A++","A","L",3661238640566,null,null,null,null,"C6"]
[7638413,"OEnoviaPAC-GS 12 TR/B200GHL",null,{"$f":"SUM(D302+D304+D305)","v":10268},null,null,"A++","A","L",3661238640573,null,null,null,null,"C6"]
[7638414,"OEnoviaPAC-GS 12 TR/V200GHL",null,{"$f":"SUM(D302+D304+D306)","v":10155},null,null,"A++","A","L",3661238640580,null,null,null,null,"C6"]
[7638415,"OEnoviaPAC-GS 15 TR/B200GHL",null,{"$f":"SUM(D303+D304+D305)","v":10872},null,null,"A++","A","L",3661238640597,null,null,null,null,"C6"]
[7638416,"OEnoviaPAC-GS 15 TR/V200GHL",null,{"$f":"SUM(D303+D304+D306)","v":10759},null,null,"A++","A","L",3661238640603,null,null,null,null,"C6"]
[]
["COMPOSANTS"]
[7617624,"OEnoviaPAC-GS 5 MR","HZ38",6866,6.67,11050,"A++","/","/",3661238603561,149.69999999999999,970,675,1135,"C6"]
[7617626,"OEnoviaPAC-GS 5 TR","HZ39",6866,6.67,11050,"A++","/","/",3661238603578,149.69999999999999,970,675,1135,"C6"]
[7618122,"OEnoviaPAC-GS 9 MR","HZ40",7595,6.67,11050,"A++","/","/",3661238614437,166,970,675,1135,"C6"]
[7618123,"OEnoviaPAC-GS 9 TR","HZ41",7595,6.67,11050,"A++","/","/",3661238614444,166,970,675,1135,"C6"]
[7618124,"OEnoviaPAC-GS 12 MR","HZ42",8177,6.67,11050,"A++","/","/",3661238603585,168,970,675,1135,"C6"]
[7615884,"OEnoviaPAC-GS 12 TR","HZ43",8177,6.67,11050,"A++","/","/",3661238603592,168,970,675,1135,"C6"]
[7618125,"OEnoviaPAC-GS 15 TR","HZ44",8781,6.67,11050,"A++","/","/",3661238603608,182.9,970,675,1135,"C6"]
[7613947,"BALLON 200 GHL","ER600",1820,null,null,"/","/","/",3661238600621,90,790,675,1330,"C6"]
[7611489,"KIT DE LIAISON PAC-BALLON B200","ER611",271,null,null,"/","/","/",3661238590618,6,860,670,220,"C6"]
[7611488,"KIT DE LIAISON PAC-BALLON V200","ER610",158,null,null,"/","/","/",3661238590717,3,510,460,175,"C6"]
[]
["OPTIONS"]
[7616429,"VANNE INVERSION + SONDE ECS GSHP 19 – 27 kW ","HZ17",425,0.17,14060,"/","/","/",3661238600812,4.0999999999999996,410,210,110,"C6"]
[7616680,"KIT APPOINT ELECTRIQUE 9 kW GSHP 05 à 15 kW","HZ20",655,0.17,14060,"/","/","/",3661238639829,4.7,420,280,190,"C6"]
[7616643,"KIT APPOINT ELECTRIQUE 9 kW GSHP 19 - 27 kW","HZ19",708,0.17,14060,"/","/","/",3661238603226,4.8,420,280,190,"C6"]
[7618061,"KIT ECHANGEUR DE BARRAGE GSHP 05 – 09 kW","HZ24",957,null,null,"/","/","/",3661238603264,16.2,660,220,325,"C6"]
[7618063,"KIT ECHANGEUR DE BARRAGE GSHP 12 – 15 kW","HZ26",1165,null,null,"/","/","/",3661238603288,19.5,660,220,325,"C6"]
[7618065,"KIT ECHANGEUR DE BARRAGE GSHP 19 – 27 kW","HZ28",1519,null,null,"/","/","/",3661238603301,25.4,660,220,325,"C6"]
[7622431,"KIT CABLAGE THERMOSTAT DE SECURITE PCBT","HZ29",75,0.02,95020,"/","/","/",3661238614116,0.3,210,150,40,"C6"]
[7622062,"KIT POMPE WILO PARA 25/1-8 pour GSHP 19","HZ63",666,0.83,14050,"/","/","/",3661238613041,5,360,235,285,"C6"]
[7610411,"KIT CIRCUIT PLANCHER CHAUFFANT ","ER604",728,0.83,14050,"/","/","/",3661238600669,5.3,815,415,250,"C6"]
[7620436,"KIT ISOLATION MODE FROID","ER581",183,null,null,"/","/","/",3661238621572,3.5,615,205,205,"C6"]
[7610412,"KIT CIRCUIT RADIATEUR","ER605",479,0.83,14050,"/","/","/",3661238600645,6.8,815,415,250,"C6"]
[7610667,"KIT DE RACCORDEMENT BALLON TAMPON - GSHP","ER606",198,null,null,"/","/","/",3661238600652,3.2,860,250,135,"C6"]
[7607396,"COLIS BALLON TAMPON GSHP 200L","ER602",894,null,null,"/","/","/",3661238600034,85,790,675,1330,"C6"]
[]
["OPTIONS REGULATIONS"]
[100013304,"OPTION V3V ","AD249",158,0.12,95010,"/","/","/",3661238363519,0.4,260,170,130,"C0"]
[100013305,"SONDE SYSTÈME ECS","AD250",46,0.02,95020,"/","/","/",3661238363588,0.13400000000000001,150,210,25,"C0"]
[100013306,"SONDE EXTERIEURE RADIO ","AD251",77,0.12,95010,"/","/","/",3661238363595,0.15,150,210,40,"C0"]
[100013307,"MODULE CHAUDIERE RADIO (EMETTEUR)","AD252",123,0.12,95010,"/","/","/",3661238363601,0.32,260,160,130,"C0"]
[100018923,"CDE À DIST RADIO CDR 2/CD","AD284",237,0.12,95010,"/","/","/",3661238544932,0.253,175,122,60,"C0"]
[100013477,"COMMANDE A DISTANCE RS 400","AD257",177,0.12,95010,"/","/","/",3661238364257,0.253,175,122,60,"C0"]
[100013472," CDE A DISTANCE RADIO RS 400R     ","AD255",238,0.12,95010,"/","/","/",3661238364233,0.253,175,122,60,"C0"]
[88017851,"CABLE DE LIAISON BUS LG 12 M","AD134",110,0.02,95020,"/","/","/",3661238048850,0.4,350,260,30,"C0"]
[88017017,"SONDE DEPART v3v","AD199",80,0.02,95020,"/","/","/",3661238049185,0.21,150,200,40,"C0"]
[100002803,"COMMANDE A DISTANCE SIMPLIFIEE AD208","AD208",104,0.12,95010,"/","/","/",3661238554931,0.2,120,85,40,"C0"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.2,200,150,30,"C0"]
[100020294,"KIT COMPTAGE D'ENERGIE","HK29",190,0.12,95010,"/","/","/",3661238576513,0.34,190,145,124,"C6"]
[100019114,"KIT SONDE HYGRO RAFRAICHISSEMENT","HK27",212,0.12,95010,"/","/","/",3661238569119,0.2,185,130,105,"C0"]
[]
[]
[7638417,"OEnoviaPAC-GS 5 MR/B200GSHL",null,{"$f":"SUM(D355+D362+D363)","v":9208},null,null,"A++","A","L",3661238640610,null,null,null,null,"C6"]
[7638418,"OEnoviaPAC-GS 5 MR/V200GSHL",null,{"$f":"SUM(D355+D362+D364)","v":9095},null,null,"A++","A","L",3661238640627,null,null,null,null,"C6"]
[7638419,"OEnoviaPAC-GS 5 TR/B200GSHL",null,{"$f":"SUM(D356+D362+D363)","v":9208},null,null,"A++","A","L",3661238640634,null,null,null,null,"C6"]
[7638420,"OEnoviaPAC-GS 5 TR/V200GSHL",null,{"$f":"SUM(D356+D362+D364)","v":9095},null,null,"A++","A","L",3661238640641,null,null,null,null,"C6"]
[7638421,"OEnoviaPAC-GS 9 MR/B200GSHL",null,{"$f":"SUM(D357+D362+D363)","v":9937},null,null,"A++","A","L",3661238640658,null,null,null,null,"C6"]
[7638422,"OEnoviaPAC-GS 9 MR/V200GSHL",null,{"$f":"SUM(D357+D362+D364)","v":9824},null,null,"A++","A","L",3661238640665,null,null,null,null,"C6"]
[7638423,"OEnoviaPAC-GS 9 TR/B200GSHL",null,{"$f":"SUM(D358+D362+D363)","v":9937},null,null,"A++","A","L",3661238640672,null,null,null,null,"C6"]
[7638424,"OEnoviaPAC-GS 9 TR/V200GSHL",null,{"$f":"SUM(D358+D362+D364)","v":9824},null,null,"A++","A","L",3661238640689,null,null,null,null,"C6"]
[7638425,"OEnoviaPAC-GS 12 MR/B200GSHL",null,{"$f":"SUM(D359+D362+D363)","v":10519},null,null,"A++","A","L",3661238640696,null,null,null,null,"C6"]
[7638426,"OEnoviaPAC-GS 12 MR/V200GSHL",null,{"$f":"SUM(D359+D362+D364)","v":10406},null,null,"A++","A","L",3661238640702,null,null,null,null,"C6"]
[7638427,"OEnoviaPAC-GS 12 TR/B200GSHL",null,{"$f":"SUM(D360+D362+D363)","v":10519},null,null,"A++","A","L",3661238640719,null,null,null,null,"C6"]
[7638428,"OEnoviaPAC-GS 12 TR/V200GSHL",null,{"$f":"SUM(D360+D362+D364)","v":10406},null,null,"A++","A","L",3661238640726,null,null,null,null,"C6"]
[7638429,"OEnoviaPAC-GS 15 TR/B200GSHL",null,{"$f":"SUM(D361+D362+D363)","v":11123},null,null,"A++","A","L",3661238640733,null,null,null,null,"C6"]
[7638430,"OEnoviaPAC-GS 15 TR/V200GSHL",null,{"$f":"SUM(D361+D362+D364)","v":11010},null,null,"A++","A","L",3661238640740,null,null,null,null,"C6"]
[]
["COMPOSANTS"]
[7617624,"OEnoviaPAC-GS 5 MR","HZ38",6866,6.67,11050,"A++","/","/",3661238603561,149.69999999999999,970,675,1135,"C6"]
[7617626,"OEnoviaPAC-GS 5 TR","HZ39",6866,6.67,11050,"A++","/","/",3661238603578,149.69999999999999,970,675,1135,"C6"]
[7618122,"OEnoviaPAC-GS 9 MR","HZ40",7595,6.67,11050,"A++","/","/",3661238614437,166,970,675,1135,"C6"]
[7618123,"OEnoviaPAC-GS 9 TR","HZ41",7595,6.67,11050,"A++","/","/",3661238614444,166,970,675,1135,"C6"]
[7618124,"OEnoviaPAC-GS 12 MR","HZ42",8177,6.67,11050,"A++","/","/",3661238603585,168,970,675,1135,"C6"]
[7615884,"OEnoviaPAC-GS 12 TR","HZ43",8177,6.67,11050,"A++","/","/",3661238603592,168,970,675,1135,"C6"]
[7618125,"OEnoviaPAC-GS 15 TR","HZ44",8781,6.67,11050,"A++","/","/",3661238603608,182.9,970,675,1135,"C6"]
[7607389,"BALLON 200 GSHL","ER601",2071,null,null,"/","/","/",3661238590311,105,790,675,1330,"C6"]
[7611489,"KIT DE LIAISON PAC-BALLON B200","ER611",271,null,null,"/","/","/",3661238590618,6,860,670,220,"C6"]
[7611488,"KIT DE LIAISON PAC-BALLON V200","ER610",158,null,null,"/","/","/",3661238590717,3,510,460,175,"C6"]
[]
["OPTIONS"]
[7616429,"VANNE INVERSION + SONDE ECS GSHP 19 – 27 kW ","HZ17",425,0.17,14060,"/","/","/",3661238600812,4.0999999999999996,410,210,110,"C6"]
[7616680,"KIT APPOINT ELECTRIQUE 9 kW GSHP 05 à 15 kW","HZ20",655,0.17,14060,"/","/","/",3661238639829,4.7,420,280,190,"C6"]
[7616643,"KIT APPOINT ELECTRIQUE 9 kW GSHP 19 - 27 kW","HZ19",708,0.17,14060,"/","/","/",3661238603226,4.8,420,280,190,"C6"]
[7618061,"KIT ECHANGEUR DE BARRAGE GSHP 05 – 09 kW","HZ24",957,null,null,"/","/","/",3661238603264,16.2,660,220,325,"C6"]
[7618063,"KIT ECHANGEUR DE BARRAGE GSHP 12 – 15 kW","HZ26",1165,null,null,"/","/","/",3661238603288,19.5,660,220,325,"C6"]
[7618065,"KIT ECHANGEUR DE BARRAGE GSHP 19 – 27 kW","HZ28",1519,null,null,"/","/","/",3661238603301,25.4,660,220,325,"C6"]
[7622431,"KIT CABLAGE THERMOSTAT DE SECURITE PCBT","HZ29",75,0.02,95020,"/","/","/",3661238614116,0.3,210,150,40,"C6"]
[7622062,"KIT POMPE WILO PARA 25/1-8 pour GSHP 19","HZ63",666,0.83,14050,"/","/","/",3661238613041,5,360,235,285,"C6"]
[7610411,"KIT CIRCUIT PLANCHER CHAUFFANT ","ER604",728,0.83,14050,"/","/","/",3661238600669,5.3,815,415,250,"C6"]
[7620436,"KIT ISOLATION MODE FROID","ER581",183,null,null,"/","/","/",3661238621572,3.5,615,205,205,"C6"]
[7610412,"KIT CIRCUIT RADIATEUR","ER605",479,0.83,14050,"/","/","/",3661238600645,6.8,815,415,250,"C6"]
[7610667,"KIT DE RACCORDEMENT BALLON TAMPON - GSHP","ER606",198,null,null,"/","/","/",3661238600652,3.2,860,250,135,"C6"]
[7607396,"COLIS BALLON TAMPON GSHP 200L","ER602",894,null,null,"/","/","/",3661238600034,85,790,675,1330,"C6"]
[]
["OPTIONS REGULATIONS"]
[100013304,"OPTION V3V ","AD249",158,0.12,95010,"/","/","/",3661238363519,0.4,260,170,130,"C0"]
[100013305,"SONDE SYSTÈME ECS","AD250",46,0.02,95020,"/","/","/",3661238363588,0.13400000000000001,150,210,25,"C0"]
[100013306,"SONDE EXTERIEURE RADIO ","AD251",77,0.12,95010,"/","/","/",3661238363595,0.15,150,210,40,"C0"]
[100013307,"MODULE CHAUDIERE RADIO (EMETTEUR)","AD252",123,0.12,95010,"/","/","/",3661238363601,0.32,260,160,130,"C0"]
[100018923,"CDE À DIST RADIO CDR 2/CD","AD284",237,0.12,95010,"/","/","/",3661238544932,0.253,175,122,60,"C0"]
[100013477,"COMMANDE A DISTANCE RS 400","AD257",177,0.12,95010,"/","/","/",3661238364257,0.253,175,122,60,"C0"]
[100013472,"CDE A DISTANCE RADIO RS 400R     ","AD255",238,0.12,95010,"/","/","/",3661238364233,0.253,175,122,60,"C0"]
[88017851,"CABLE DE LIAISON BUS LG 12 M","AD134",110,0.02,95020,"/","/","/",3661238048850,0.4,350,260,30,"C0"]
[88017017,"SONDE DEPART v3v","AD199",80,0.02,95020,"/","/","/",3661238049185,0.21,150,200,40,"C0"]
[100002803,"COMMANDE A DISTANCE SIMPLIFIEE AD208","AD208",104,0.12,95010,"/","/","/",3661238554931,0.2,120,85,40,"C0"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.2,200,150,30,"C0"]
[100020294,"KIT COMPTAGE D'ENERGIE","HK29",190,0.12,95010,"/","/","/",3661238576513,0.34,190,145,124,"C6"]
[100019114,"KIT SONDE HYGRO RAFRAICHISSEMENT","HK27",212,0.12,95010,"/","/","/",3661238569119,0.2,185,130,105,"C0"]
[]
[]
[7625561,"AWHP 4-GMX-M 2024 COMBI HYBRID",null,{"$f":"SUM(D403+D406+D407+D402)","v":6087},{"$f":"SUM(E403+E406+E407+E402)","v":11.67},null,"A++","A","XL",3661238647121,106.8,null,null,null,"C9"]
[7625562,"AWHP 6-GMX-M 2024 COMBI HYBRID",null,{"$f":"SUM(D402+D404+D406+D407)","v":6176},{"$f":"SUM(E402+E404+E406+E407)","v":11.67},null,"A++","A","XL",3661238647138,104,null,null,null,"C9"]
[7625563,"AWHP 8-GMX-M 2024 COMBI HYBRID",null,{"$f":"SUM(D405+D402+D406+D407)","v":6927},{"$f":"SUM(E405+E402+E406+E407)","v":11.67},null,"A++","A","XL",3661238647145,141,null,null,null,"C9"]
[]
["COMPOSANTS"]
[7622151,"GMX-M 2024 COMBI CONDENS HYBRID","EH598",2029,5,null,"/","/","/",null,27.8,600,400,520,"C9"]
[7603571,"AWHP 4 MR","EH336",1837,6.67,11050,"/","/","/",3661238581012,48,450,950,690,"C9"]
[7609925,"AWHP 6 MR-2","EH380",1926,6.67,11050,"/","/","/",3661238589513,45.2,445,950,680,"C9"]
[7609926,"AWHP 8 MR-2","EH381",2677,6.67,11050,"/","/","/",3661238589520,82.2,460,1090,1100,"C9"]
[7625043,"KIT HYDRAULIQUE + HABILLAGE","EH519",244,null,null,"/","/","/",3661238618596,7.5,750,450,260,"C9"]
[7627623,"KIT HYBRIDE MURAL","EH568",1977,null,null,"/","/","/",3661238626492,23.5,404,341,1180,"C9"]
[]
["OPTIONS"]
[100008296,"TERMINAL HORIZONTAL PPS Ø 60/100 MM LG=800 MM","DY871",116,null,null,"/","/","/",3661238168022,2.8,1200,200,200,"C0"]
["S101688","ADAPTATEUR AIR/FUMEES D80/125","HR68",25,null,null,"/","/","/",8713809243722,0.2,175,180,130,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[100004417,"FILTRE 400UM + VANNE D'ISOLEMENT 1''","EH61",105,null,null,"/","/","/",3661238003415,0.9,175,90,130,"C6"]
[100011222,"SUPPORT FIXATION MURALE & PLOTS ANTIVIBRATILES POUR ROE-II 6 à 10 - AWHP","EH95",162,null,null,"/","/","/",3661238339927,5.4,820,90,90,"C6"]
[100012532,"BAC DE RECUPERATION CONDENSATS POUR SUPPORT MURAL","EH111",142,null,null,"/","/","/",3661238361553,2,960,430,80,"C6"]
[100012534,"KIT DE TRACAGE ELECTRIQUE POUR AWHP","EH113",150,null,null,"/","/","/",3661238361577,0.2,200,200,10,"C6"]
[100012533,"SUPPORT POSE AU SOL AWHP","EH112",45,null,null,"/","/","/",3661238361560,1.2,450,140,80,"C6"]
[100012535,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 5m","EH114",233,null,null,"/","/","/",3661238361522,4.5999999999999996,600,600,150,"C6"]
[100012536,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 10m","EH115",416,null,null,"/","/","/",3661238361539,7.2,600,600,200,"C6"]
[100012537,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 20m","EH116",751,null,null,"/","/","/",3661238361546,14.3,750,750,230,"C6"]
[100015476,"LIAISON FRIGORIFIQUE PE 1/2\" 1/4\" - LG 10 m","EH142",233,null,null,"/","/","/",3661238381575,7.9,600,650,150,"C6"]
[100008841,"COLIS BALLON TAMPON 80L","EH85",521,null,null,"/","/","/",3661238166325,44.5,510,510,920,"C6"]
[100004415,"COLIS BALLON TAMPON 160L","EH60",781,null,null,"/","/","/",3661238003422,63.2,825,690,1120,"C6"]
[88017904,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (FILAIRE)","AD191",161,0.12,95010,"/","/","/",3661238048836,0.2,130,90,55,"C0"]
[88017010,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (SANS FILS)","AD192",286,0.12,95010,"/","/","/",3661238049178,0.4,175,150,90,"C0"]
[7618227,"KIT VANNE 3 VOIES","EH517",463,0.12,95010,"/","/","/",3661238616240,3.9,404,274,152,"C6"]
[7622273,"CARTE DE REGULATION 2 CIRCUITS","EH527",199,0.12,95010,"/","/","/",3661238618145,0.3,185,130,105,"C6"]
[7624902,"KIT CABLAGE PLANCHER CHAUFFANT DIRECT","HA255",37,0.02,95020,"/","/","/",3661238618176,0.23,340,240,40,"C6"]
[7626700,"KIT ISOLATION MODE CLIMATISATION","EH566",208,null,null,"/","/","/",3661238622739,0.5,315,225,120,"C6"]
[7636899,"KIT SILENCIEUX MODULE EXTERIEUR","EH572",60,0.02,95020,"/","/","/",3661238644335,0.2,170,210,20,"C6"]
[]
[]
[7642831,"AWHP 4 MR-GSCR 15 HYBRID V200",null,{"$f":"SUM(D471+D474+D481+D484+D482)","v":7747},{"$f":"SUM(E471+E474+E481+E484+E482)","v":11.67},null,"A++","A","L",3661238647213,246.7,null,null,null,"C6"]
[7642832,"AWHP 4 MR-GSCR 15 HYBRID B200",null,{"$f":"SUM(D471+D474+D481+D482+D485)","v":7851},{"$f":"SUM(E471+E474+E481+E482+E485)","v":11.67},null,"A++","A","L",3661238647220,252.8,null,null,null,"C6"]
[7642833,"AWHP 6 MR-GSCR 15 HYBRID V200",null,{"$f":"SUM(D471+D475+D481+D482+D484)","v":7836},{"$f":"SUM(E471+E475+E481+E482+E484)","v":11.67},null,"A++","A","L",3661238647237,243.9,null,null,null,"C6"]
[7642834,"AWHP 6 MR-GSCR 15 HYBRID B200",null,{"$f":"SUM(D471+D475+D481+D482+D485)","v":7940},{"$f":"SUM(E471+E475+E481+E482+E485)","v":11.67},null,"A++","A","L",3661238647244,250,null,null,null,"C6"]
[7642835,"AWHP 8 MR-GSCR 15 HYBRID V200",null,{"$f":"SUM(D471+D476+D482+D484)","v":8529},{"$f":"SUM(E471+E476+E482+E484)","v":11.67},null,"A++","A","L",3661238647251,280.39999999999998,null,null,null,"C6"]
[7642836,"AWHP 8 MR-GSCR 15 HYBRID B200",null,{"$f":"SUM(D471+D476+D482+D485)","v":8633},{"$f":"SUM(E471+E476+E482+E485)","v":11.67},null,"A++","A","L",3661238647268,286.5,null,null,null,"C6"]
[7642837,"AWHP 11 MR-GSCR 15 HYBRID V200",null,{"$f":"SUM(D471+D477+D483+D484)","v":9797},{"$f":"SUM(E471+E477+E483+E484)","v":11.67},null,"A++","A","L",3661238647275,324.8,null,null,null,"C6"]
[7642839,"AWHP 11 MR-GSCR 15 HYBRIDE B200",null,{"$f":"SUM(D471+D477+D483+D485)","v":9901},{"$f":"SUM(E471+E477+E483+E485)","v":11.67},null,"A++","A","L",3661238647282,330.9,null,null,null,"C6"]
[7642840,"AWHP 11 TR-GSCR 15 HYBRID V200",null,{"$f":"SUM(D471+D478+D483+D484)","v":10101},{"$f":"SUM(E471+E478+E483+E484)","v":11.67},null,"A++","A","L",3661238647299,337.8,null,null,null,"C6"]
[7642841,"AWHP 11 TR-GSCR 15 HYBRID B200",null,{"$f":"SUM(D471+D478+D483+D485)","v":10205},{"$f":"SUM(E471+E478+E483+E485)","v":11.67},null,"A++","A","L",3661238647305,343.9,null,null,null,"C6"]
[7642842,"AWHP 16 MR-GSCR 15 HYBRID V200",null,{"$f":"SUM(D471+D479+D483+D484)","v":10890},{"$f":"SUM(E471+E479+E483+E484)","v":11.67},null,"A++","A","L",3661238647312,324.60000000000002,null,null,null,"C6"]
[7642843,"AWHP 16 MR-GSCR 15 HYBRID B200",null,{"$f":"SUM(D471+D479+D483+D485)","v":10994},{"$f":"SUM(E471+E479+E483+E485)","v":11.67},null,"A++","A","L",3661238647329,330.7,null,null,null,"C6"]
[7642844,"AWHP 16 TR-GSCR 15 HYBRID V200",null,{"$f":"SUM(D471+D480+D483+D484)","v":11315},{"$f":"SUM(E471+E480+E483+E484)","v":11.67},null,"A++","A","L",3661238647336,336.8,null,null,null,"C6"]
[7642845,"AWHP 16 TR-GSCR 15 HYBRID B200",null,{"$f":"SUM(D471+D480+D483+D485)","v":11419},{"$f":"SUM(E471+E480+E483+E485)","v":11.67},null,"A++","A","L",3661238647343,342.9,null,null,null,"C6"]
[7642846,"AWHHP 6 MR-GSCR 25 HYBRID V200",null,{"$f":"SUM(D472+D475+D481+D482+D484)","v":8000},{"$f":"SUM(E472+E475+E481+E482+E484)","v":11.67},null,"A++","A","L",3661238647350,246.9,null,null,null,"C6"]
[7642847,"AWHP 6 MR-GSCR 25 HYBRID B200",null,{"$f":"SUM(D472+D475+D481+D482+D485)","v":8104},{"$f":"SUM(E472+E475+E481+E482+E485)","v":11.67},null,"A++","A","L",3661238647367,253,null,null,null,"C6"]
[7642848,"AWHP 8 MR-GSCR 25 HYBRID V200",null,{"$f":"SUM(D472+D476+D482+D484)","v":8693},{"$f":"SUM(E472+E476+E482+E484)","v":11.67},null,"A++","A","L",3661238647374,283.39999999999998,null,null,null,"C6"]
[7642849,"AWHP 8 MR-GSCR 25 HYBRID B200",null,{"$f":"SUM(D472+D476+D482+D485)","v":8797},{"$f":"SUM(E472+E476+E482+E485)","v":11.67},null,"A++","A","L",3661238647381,289.5,null,null,null,"C6"]
[7642850,"AWHP 11 MR-GSCR 25 HYBRID V200",null,{"$f":"SUM(D472+D477+D483+D484)","v":9961},{"$f":"SUM(E472+E477+E483+E484)","v":11.67},null,"A++","A","L",3661238647398,327.8,null,null,null,"C6"]
[7642851,"AWHP 11 MR-GSCR 25 HYBRID B200",null,{"$f":"SUM(D472+D477+D483+D485)","v":10065},{"$f":"SUM(E472+E477+E483+E485)","v":11.67},null,"A++","A","L",3661238647404,333.9,null,null,null,"C6"]
[7642852,"AWHP 11 TR-GSCR 25 HYBRID V200",null,{"$f":"SUM(D472+D478+D483+D484)","v":10265},{"$f":"SUM(E472+E478+E483+E484)","v":11.67},null,"A++","A","L",3661238647411,340.8,null,null,null,"C6"]
[7642853,"AWHP 11 TR-GSCR 25 HYBRID B200",null,{"$f":"SUM(D472+D478+D483+D485)","v":10369},{"$f":"SUM(E472+E478+E483+E485)","v":11.67},null,"A++","A","L",3661238647428,346.9,null,null,null,"C6"]
[7642854,"AWHP 16 MR-GSCR 25 HYBRID V200",null,{"$f":"SUM(D472+D479+D483+D484)","v":11054},{"$f":"SUM(E472+E479+E483+E484)","v":11.67},null,"A++","A","L",3661238647435,327.60000000000002,null,null,null,"C6"]
[7642855,"AWHP 16 MR-GSCR 25 HYBRID B200",null,{"$f":"SUM(D472+D479+D483+D485)","v":11158},{"$f":"SUM(E472+E479+E483+E485)","v":11.67},null,"A++","A","L",3661238647442,333.7,null,null,null,"C6"]
[7642856,"AWHP 16 TR-GSCR 25 HYBRID V200",null,{"$f":"SUM(D472+D480+D483+D484)","v":11479},{"$f":"SUM(E472+E480+E483+E484)","v":11.67},null,"A++","A","L",3661238647459,339.8,null,null,null,"C6"]
[7642857,"AWHP 16 TR-GSCR 25 HYBRID B200",null,{"$f":"SUM(D472+D480+D483+D485)","v":11583},{"$f":"SUM(E472+E480+E483+E485)","v":11.67},null,"A++","A","L",3661238647466,345.9,null,null,null,"C6"]
[7642858,"AWHP 8 MR-GSCR 35 HYBRID V200",null,{"$f":"SUM(D473+D476+D482+D484)","v":9010},{"$f":"SUM(E473+E476+E482+E484)","v":11.67},null,"A++","A","L",3661238647473,283.39999999999998,null,null,null,"C6"]
[7642859,"AWHP 8 MR-GSCR 35 HYBRID B200",null,{"$f":"SUM(D473+D476+D482+D485)","v":9114},{"$f":"SUM(E473+E476+E482+E485)","v":11.67},null,"A++","A","L",3661238647480,289.5,null,null,null,"C6"]
[7642860,"AWHP 11 MR-GSCR 35 HYBRID V200",null,{"$f":"SUM(D473+D477+D483+D484)","v":10278},{"$f":"SUM(E473+E477+E483+E484)","v":11.67},null,"A++","A","L",3661238647497,327.8,null,null,null,"C6"]
[7642861,"AWHP 11 MR-GSCR 35 HYBRID B200",null,{"$f":"SUM(D473+D477+D483+D485)","v":10382},{"$f":"SUM(E473+E477+E483+E485)","v":11.67},null,"A++","A","L",3661238647503,333.9,null,null,null,"C6"]
[7642862,"AWHP 11 TR-GSCR 35 HYBRID V200",null,{"$f":"SUM(D473+D478+D483+D484)","v":10582},{"$f":"SUM(E473+E478+E483+E484)","v":11.67},null,"A++","A","L",3661238647510,340.8,null,null,null,"C6"]
[7642863,"AWHP 11 TR-GSCR 35 HYBRID B200",null,{"$f":"SUM(D473+D478+D483+D485)","v":10686},{"$f":"SUM(E473+E478+E483+E485)","v":11.67},null,"A++","A","L",3661238647527,346.9,null,null,null,"C6"]
[7642864,"AWHP 16 MR-GSCR 35 HYBRID V200",null,{"$f":"SUM(D473+D479+D483+D484)","v":11371},{"$f":"SUM(E473+E479+E483+E484)","v":11.67},null,"A++","A","L",3661238647534,327.60000000000002,null,null,null,"C6"]
[7642865,"AWHP 16 MR-GSCR 35 HYBRID B200",null,{"$f":"SUM(D473+D479+D483+D485)","v":11475},{"$f":"SUM(E473+E479+E483+E485)","v":11.67},null,"A++","A","L",3661238647541,333.7,null,null,null,"C6"]
[7642866,"AWHP 16 TR-GSCR 35 HYBRID V200",null,{"$f":"SUM(D473+D480+D483+D484)","v":11796},{"$f":"SUM(E473+E480+E483+E484)","v":11.67},null,"A++","A","L",3661238647558,339.8,null,null,null,"C6"]
[7642867,"AWHP 16 TR-GSCR 35 HYBRID B200",null,{"$f":"SUM(D473+D480+D483+D485)","v":11900},{"$f":"SUM(E473+E480+E483+E485)","v":11.67},null,"A++","A","L",3661238647565,345.9,null,null,null,"C6"]
[]
["COMPOSANTS"]
[100017756,"GSCR 15","JA21",3241,5,14070,"A","/","/",3661238505971,67,780,680,1070,"C0"]
[100017757,"GSCR 25","JA22",3405,5,14070,"A","/","/",3661238505988,70,780,680,1070,"C0"]
[100017758,"GSCR 35","JA23",3722,5,14070,"A","/","/",3661238505995,70,780,680,1070,"C0"]
[7603571,"AWHP 4 MR","EH336",1837,6.67,11050,"/","/","/",3661238581012,48,450,950,690,"C9"]
[7609925,"AWHP 6 MR-2","EH380",1926,6.67,11050,"/","/","/",3661238589513,45.2,445,950,680,"C9"]
[7609926,"AWHP 8 MR-2","EH381",2677,6.67,11050,"/","/","/",3661238589520,82.2,460,1090,1100,"C9"]
[7609927,"AWHP 11 MR-2","EH382",3529,6.67,11050,"/","/","/",3661238589537,131,450,1040,1440,"C9"]
[7609928,"AWHP 11 TR-2","EH383",3833,6.67,11050,"/","/","/",3661238589544,137.6,460,1090,1490,"C9"]
[7609929,"AWHP 16 MR-2","EH384",4622,6.67,11050,"/","/","/",3661238589551,124.4,460,1090,1490,"C9"]
[7609930,"AWHP 16 TR-2","EH385",5047,6.67,11050,"/","/","/",3661238589568,136.6,460,1090,1490,"C9"]
[100015480,"RACCORD D'ADAPTATION FRIGO POUR 4 kW ET 6 kW","EH146",58,null,null,"/","/","/",3661238381612,0.5,150,80,30,"C9"]
[7623217,"BALLON 200 CSL HYBRID 4-8","EH509",2497,null,null,"/","/","/",3661238621312,130,970,675,1435,"C6"]
[7623229,"BALLON 200 CSL HYBRID 11-16","EH513",2913,null,null,"/","/","/",3661238621329,132,970,675,1435,"C6"]
[7621386,"KIT DE MONTAGE BALLON VERSION V","EH524",114,null,null,"/","/","/",3661238618114,1.2,860,250,135,"C6"]
[7621387,"KIT DE MONTAGE BALLON VERSION B","EH525",218,null,null,"/","/","/",3661238618121,7.3,860,670,220,"C6"]
[]
["OPTIONS FUMISTERIE"]
[100013756,"TERMINAL HORIZONTAL Ø 60/100 MM AVEC COUDE DE VISITE","HR48",187,null,null,"/","/","/",3661238370883,3.4,1200,200,200,"C0"]
[100011365,"KIT VENTOUSE HOR PPS/ALU Ø 80/125mm","DY882",208,null,null,"/","/","/",3661238374768,0.3,1210,265,250,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 mm NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
["OPTIONS"]
[100004417,"FILTRE 400UM + VANNE D'ISOLEMENT 1''","EH61",105,null,null,"/","/","/",3661238003415,0.9,175,90,130,"C6"]
[100011222,"SUPPORT FIXATION MURALE & PLOTS ANTIVIBRATILES POUR ROE-II 6 à 10 - AWHP","EH95",162,null,null,"/","/","/",3661238339927,5.4,820,90,90,"C6"]
[100018409,"SUPPORT MURAL AWHP 11à 27 kW","EH250",166,null,null,"/","/","/",3661238543874,5,820,90,90,"C6"]
[100012532,"BAC DE RECUPERATION CONDENSATS POUR SUPPORT MURAL","EH111",142,null,null,"/","/","/",3661238361553,2,960,430,80,"C6"]
[100012534,"KIT DE TRACAGE ELECTRIQUE POUR AWHP","EH113",150,null,null,"/","/","/",3661238361577,0.2,200,200,10,"C6"]
[100012533,"SUPPORT POSE AU SOL AWHP","EH112",45,null,null,"/","/","/",3661238361560,1.2,450,140,80,"C6"]
[100012535,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 5m","EH114",233,null,null,"/","/","/",3661238361522,4.5999999999999996,600,600,150,"C6"]
[100012536,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 10m","EH115",416,null,null,"/","/","/",3661238361539,7.2,600,600,200,"C6"]
[100012537,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 20m","EH116",751,null,null,"/","/","/",3661238361546,14.3,750,750,230,"C6"]
[100015476,"LIAISON FRIGORIFIQUE PE 1/2\" 1/4\" - LG 10 m","EH142",233,null,null,"/","/","/",3661238381575,7.9,600,650,150,"C6"]
[100008841,"COLIS BALLON TAMPON 80L","EH85",521,null,null,"/","/","/",3661238166325,44.5,510,510,920,"C6"]
[100004415,"COLIS BALLON TAMPON 160L","EH60",781,null,null,"/","/","/",3661238003422,63.2,825,690,1120,"C6"]
[7624902,"KIT CABLAGE PLANCHER CHAUFFANT DIRECT","HA255",37,0.02,95020,"/","/","/",3661238618176,0.23,340,240,40,"C6"]
[7619010,"KIT VANNE 3 VOIES","EH528",576,0.12,95010,"/","/","/",3661238618152,17.7,750,300,150,"C6"]
[7626737,"KIT ISOLATION MODE CLIMATISATION","EH567",208,null,null,"/","/","/",3661238624115,0.64,615,280,80,"C6"]
[100019114,"KIT SONDE HYGRO RAFRAICHISSEMENT","HK27",212,0.12,95010,"/","/","/",3661238569119,0.2,185,130,105,"C0"]
[7636899,"KIT SILENCIEUX MODULE EXTERIEUR","EH572",60,0.02,95020,"/","/","/",3661238644335,0.2,170,210,20,"C6"]
[]
["OPTIONS REGULATION"]
[100013304,"OPTION V3V DIEMATIC iSystem","AD249",158,0.12,95010,"/","/","/",3661238363519,0.4,260,170,130,"C0"]
[100013305,"SONDE SYSTÈME ECS","AD250",46,0.02,95020,"/","/","/",3661238363588,0.1,150,210,25,"C0"]
[100013306,"SONDE EXTERIEURE RADIO DIEMATIC iSystem","AD251",77,0.12,95010,"/","/","/",3661238363595,0.2,150,210,40,"C0"]
[100013307,"MODULE CHAUDIERE RADIO DIEMATIC iSystem","AD252",123,0.12,95010,"/","/","/",3661238363601,0.3,260,160,130,"C0"]
[100018923,"COMMANDE A DISTANCE RADIO CDR iSystem","AD284",237,0.12,95010,"/","/","/",3661238544932,0.3,175,122,60,"C0"]
[100013477,"COMMANDE A DISTANCE RS 400","AD257",177,0.12,95010,"/","/","/",3661238364257,0.253,175,122,60,"C0"]
[100013472,"CDE A DISTANCE RADIO RS 400R     ","AD255",238,0.12,95010,"/","/","/",3661238364233,0.3,175,122,60,"C0"]
[88017017,"SONDE DEPART V3V","AD199",80,0.02,95020,"/","/","/",3661238049185,0.2,150,200,40,"C0"]
[100002803,"COMMANDE A DISTANCE SIMPLIFIEE AD208","AD208",104,0.12,95010,"/","/","/",3661238554931,0.1,120,85,40,"C0"]
[]
[]
[null,"Avec chaudière fioul basse température"]
[7642876,"AWHP 4MR-FSBR 22P HYBRID V200",null,{"$f":"D552+D556+D557+D564+D565+D567","v":8735},{"$f":"E552+E556+E557+E564+E565+E567","v":12.5},null," A++","A","L",3661238644717,null,null,null,null,"C9"]
[7642878,"AWHP 6MR-FSBR 22P HYBRID V200",null,{"$f":"D552+D556+D558+D564+D565+D567","v":8824},{"$f":"E552+E556+E558+E564+E565+E567","v":12.5},null," A++","A","L",3661238644731,null,null,null,null,"C9"]
[7642881,"AWHP 8MR-FSBR 22P HYBRID V200",null,{"$f":"D552+D556+D559+D565+D567","v":9517},{"$f":"E552+E556+E559+E565+E567","v":12.5},null," A++","A","L",3661238644755,null,null,null,null,"C9"]
[7642883,"AWHP 11MR-FSBR 22P HYBRID V200",null,{"$f":"D552+D556+D560+D566+D567","v":10837},{"$f":"E552+E556+E560+E566+E567","v":12.5},null," A++","A","L",3661238644779,null,null,null,null,"C9"]
[7642885,"AWHP 11TR-FSBR 22P HYBRID V200",null,{"$f":"D552+D556+D561+D566+D567","v":11141},{"$f":"E552+E556+E561+E566+E567","v":12.5},null," A++","A","L",3661238644793,null,null,null,null,"C9"]
[7642887,"AWHP 16MR-FSBR 22P HYBRID V200",null,{"$f":"D552+D556+D562+D566+D567","v":11930},{"$f":"E552+E556+E562+E566+E567","v":12.5},null," A++","A","L",3661238646018,null,null,null,null,"C9"]
[7642889,"AWHP 16TR-FSBR 22P HYBRID V200",null,{"$f":"D552+D556+D563+D566+D567","v":12355},{"$f":"E552+E556+E563+E566+E567","v":12.5},null," A++","A","L",3661238646032,null,null,null,null,"C9"]
[7642891,"AWHP 8MR-FSBR 29P HYBRID V200",null,{"$f":"D553+D556+D559+D565+D567","v":9670},{"$f":"E553+E556+E559+E565+E567","v":12.5},null," A++","A","L",3661238644854,null,null,null,null,"C9"]
[7642893,"AWHP 11MR-FSBR 29P HYBRID V200",null,{"$f":"D553+D556+D560+D566+D567","v":10990},{"$f":"E553+E556+E560+E566+E567","v":12.5},null," A++","A","L",3661238644878,null,null,null,null,"C9"]
[7642895,"AWHP 11TR-FSBR 29P HYBRID V200",null,{"$f":"D553+D556+D561+D566+D567","v":11294},{"$f":"E553+E556+E561+E566+E567","v":12.5},null," A++","A","L",3661238644892,null,null,null,null,"C9"]
[7642898,"AWHP 16MR-FSBR 29P HYBRID V200",null,{"$f":"D553+D556+D562+D566+D567","v":12083},{"$f":"E553+E556+E562+E566+E567","v":12.5},null," A++","A","L",3661238646117,null,null,null,null,"C9"]
[7642900,"AWHP 16TR-FSBR 29P HYBRID V200",null,{"$f":"D553+D556+D563+D566+D567","v":12508},{"$f":"E553+E556+E563+E566+E567","v":12.5},null," A++","A","L",3661238646131,null,null,null,null,"C9"]
[]
[null,"Avec chaudière fioul basse température ventouse"]
[7642903,"AWHP 4MR-FSBR 22PF HYBRID V200",null,{"$f":"D554+D556+D557+D564+D565+D567","v":8921},{"$f":"E554+E556+E557+E564+E565+E567","v":12.5},null," A++","A","L",3661238644953,null,null,null,null,"C9"]
[7642906,"AWHP 6MR-FSBR 22PF HYBRID V200",null,{"$f":"D554+D556+D558+D564+D565+D567","v":9010},{"$f":"E554+E556+E558+E564+E565+E567","v":12.5},null," A++","A","L",3661238644977,null,null,null,null,"C9"]
[7642908,"AWHP 8MR-FSBR 22PF HYBRID V200",null,{"$f":"D554+D556+D559+D565+D567","v":9703},{"$f":"E554+E556+E559+E565+E567","v":12.5},null," A++","A","L",3661238644991,null,null,null,null,"C9"]
[7642910,"AWHP 11MR-FSBR 22PF HYBRID V200",null,{"$f":"D554+D556+D560+D566+D567","v":11023},{"$f":"E554+E556+E560+E566+E567","v":12.5},null," A++","A","L",3661238645011,null,null,null,null,"C9"]
[7642912,"AWHP 11TR-FSBR 22PF HYBRID V200",null,{"$f":"D554+D556+D561+D566+D567","v":11327},{"$f":"E554+E556+E561+E566+E567","v":12.5},null," A++","A","L",3661238645035,null,null,null,null,"C9"]
[7642914,"AWHP 16MR-FSBR 22PF HYBRID V200",null,{"$f":"D554+D556+D562+D566+D567","v":12116},{"$f":"E554+E556+E562+E566+E567","v":12.5},null," A++","A","L",3661238646254,null,null,null,null,"C9"]
[7642916,"AWHP 16TR-FSBR 22PF HYBRID V200",null,{"$f":"D554+D556+D563+D566+D567","v":12541},{"$f":"E554+E556+E563+E566+E567","v":12.5},null," A++","A","L",3661238646278,null,null,null,null,"C9"]
[7642918,"AWHP 8MR-FSBR 29PF HYBRID V200",null,{"$f":"D555+D556+D559+D565+D567","v":9854},{"$f":"E555+E556+E559+E565+E567","v":12.5},null," A++","A","L",3661238645097,null,null,null,null,"C9"]
[7642920,"AWHP 11MR-FSBR 29PF HYBRID V200",null,{"$f":"D555+D556+D560+D566+D567","v":11174},{"$f":"E555+E556+E560+E566+E567","v":12.5},null," A++","A","L",3661238645110,null,null,null,null,"C9"]
[7642922,"AWHP 11TR-FSBR 29PF HYBRID V200",null,{"$f":"D555+D556+D561+D566+D567","v":11478},{"$f":"E555+E556+E561+E566+E567","v":12.5},null," A++","A","L",3661238645127,null,null,null,null,"C9"]
[7642924,"AWHP 16MR-FSBR 29PF HYBRID V200",null,{"$f":"D555+D556+D562+D566+D567","v":12267},{"$f":"E555+E556+E562+E566+E567","v":12.5},null," A++","A","L",3661238646353,null,null,null,null,"C9"]
[7642926,"AWHP 16TR-FSBR 29PF HYBRID V200",null,{"$f":"D555+D556+D563+D566+D567","v":12692},{"$f":"E555+E556+E563+E566+E567","v":12.5},null," A++","A","L",3661238646377,null,null,null,null,"C9"]
[]
["COMPOSANTS"]
[7624149,"FSB. 22  ","MY125",3229,5,14070,null,null,null,3661238616158,204,1220,750,1050,"D6"]
[7624151,"FSB. 29  ","MY135",3382,5,14070,null,null,null,3661238616189,232,1220,750,1050,"D6"]
[7627332,"FSB. 22 FF","MY122",3415,5,14070,null,null,null,3661238630222,214,1220,750,1050,"D6"]
[7627333,"FSB. 29 FF","MY132",3566,5,14070,null,null,null,3661238630239,242,1220,750,1050,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,15,675,485,180,"D6"]
[7603571,"AWHP 4 MR","EH336",1837,6.67,11050,"/","/","/",3661238581012,48,450,950,690,"C9"]
[7609925,"AWHP 6 MR-2 ","EH380",1926,6.67,11050,"/","/","/",3661238589513,45.2,445,950,680,"C9"]
[7609926,"AWHP 8 MR-2 ","EH381",2677,6.67,11050,null,null,null,3661238589520,82.2,460,1090,1100,"C9"]
[7609927,"AWHP 11 MR-2 ","EH382",3529,6.67,11050,null,null,null,3661238589537,131,450,1040,1440,"C9"]
[7609928,"AWHP 11 TR-2 ","EH383",3833,6.67,11050,"/","/","/",3661238589544,137.6,460,1090,1490,"C9"]
[7609929,"AWHP 16 MR-2 ","EH384",4622,6.67,11050," /"," /"," /",3661238589551,131,450,1040,1440,"C9"]
[7609930,"AWHP 16 TR-2 ","EH385",5047,6.67,11050," /"," /"," /",3661238589568,145,450,1040,1440,"C9"]
[100015480,"RACCORD D'ADAPTATION FRIGO POUR 4 kW ET 6 kW","EH146",58,null,null,"/","/","/",3661238381612,0.5,150,80,30,"C9"]
[7623191,"BALLON 200 PSL HYBRIDE 4-8","EH501",3017,null,null,null,null,null,3661238621299,130,970,645,1435,"C9"]
[7623204,"BALLON 200 PSL HYBRIDE 11-16","EH505",3485,null,null,null,null,null,3661238621305,132,970,645,1435,"C9"]
[7621386,"KIT DE MONTAGE BALLON VERSION V","EH524",114,null,null,null,null,null,3661238618114,1.1499999999999999,860,250,134,"C9"]
[7621387,"KIT DE MONTAGE BALLON VERSION B","EH525",218,null,null,null,null,null,3661238618121,7.3,860,670,220,"C9"]
[]
["OPTIONS"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,null,null,null,3661238157972,2,1025,170,170,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[81998533,"TERMINAL HORIZONTAL STANDARD","DB90",232,null,null,"/","/","/",3661238001329,2.9,1015,150,145,"C0"]
[81998534,"TERMINAL VERTICAL NOIR","DB91",206,null,null,"/","/","/",3661238001312,4.9000000000000004,1150,260,270,"C0"]
[81998539,"COUDE A 90 °","DB96",114,null,null,"/","/","/",3661238001268,0.9,325,240,150,"C0"]
[100004417,"FILTRE 400UM + VANNE D'ISOLEMENT PAC ROE 6-10 ET ROE+","EH61",105,null,null,"/","/","/",3661238003415,0.9,175,90,130,"C6"]
[100011222,"SUPPORT MURALE & PLOTS ANTIVIBRATILES POUR  ROE-II AWHP 6-8","EH95",162,null,null,"/","/","/",3661238339927,5.4,820,90,90,"C6"]
[100018409,"SUPPORT MURAL AWHP 11à 27 kW","EH250",166,null,null,"/","/","/",3661238543874,5,820,90,90,"C6"]
[100012532,"BAC DE RECUPERATION CONDENSATS POUR SUPPORT MURAL","EH111",142,null,null,"/","/","/",3661238361553,2,960,430,80,"C6"]
[100012534,"CORDON CHAUFFANT ELECTRIQUE","EH113",150,null,null,"/","/","/",3661238361577,0.2,200,200,10,"C6"]
[100012533,"SUPPORT POSE AU SOL AWHP","EH112",45,null,null,"/","/","/",3661238361560,1.2,450,140,80,"C6"]
[100015476,"LIAISON FRIGORIFIQUE PE 1/2\" 1/4\" - LG 10 m","EH142",233,null,null,"/","/","/",3661238381575,7.9,600,650,150,"C6"]
[100012535,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 5m","EH114",233,null,null,"/","/","/",3661238361522,4.5999999999999996,600,600,150,"C6"]
[100012536,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 10m","EH115",416,null,null,"/","/","/",3661238361539,7.2,600,600,200,"C6"]
[100012537,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 20m","EH116",751,null,null,"/","/","/",3661238361546,14.3,750,750,230,"C6"]
[100008841,"BALLON TAMPON 80L B 80 T","EH85",521,null,null,"/","/","/",3661238166325,44.5,510,510,920,"C6"]
[100004415,"BALLON TAMPON 160L B 150 T","EH60",781,null,null,"/","/","/",3661238003422,63.2,825,690,1120,"C6"]
[88017904,"THERMOSTAT AMBIANCE PROGRAMMABLE (FILAIRE)","AD191",161,0.12,95010,"/","/","/",3661238048836,0.2,130,90,55,"C0"]
[88017010,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (SANS FILS)","AD192",286,0.12,95010,"/","/","/",3661238049178,0.4,175,150,90,"C0"]
[7624902,"KIT CABLAGE PLANCHER CHAUFFANT DIRECT","HA255",37,0.02,95020,"/","/","/",3661238618176,0.23,340,240,40,"C6"]
[7619010,"KIT VANNE 3 VOIES","EH528",576,0.12,95010,"/","/","/",3661238618152,17.7,750,300,150,"C6"]
[7622273,"CARTE DE REGULATION 2 CIRCUITS","EH527",199,0.12,95010,"/","/","/",3661238618145,0.3,185,130,105,"C6"]
[7626737,"KIT ISOLATION MODE FROID","EH567",208,null,null,"/","/","/",3661238624115,0.64,615,280,80,"C6"]
[100019114,"KIT DETECTEUR DE CONDENSATION","HK27",212,0.12,95010,"/","/","/",3661238569119,0.2,185,130,105,"C0"]
[7636899,"KIT SILENCIEUX MODULE EXTERIEUR","EH572",60,0.02,95020,"/","/","/",3661238644335,0.2,170,210,20,"C0"]
[]
[null,"Avec chaudière fioul à condensation"]
[7642928,"AWHP 4MR-FSCR 19P HYBRID V200",null,{"$f":"D639+D642+D644+D651+D652+D654","v":9392},{"$f":"E639+E642+E644+E651+E652+E654","v":12.5},null," A++"," A","L",3661238645189,null,null,null,null,"C9"]
[7642930,"AWHP 6MR-FSCR 19P HYBRID V200",null,{"$f":"D639+D642+D645+D651+D652+D654","v":9481},{"$f":"E639+E642+E645+E651+E652+E654","v":12.5},null," A++"," A","L",3661238645202,null,null,null,null,"C9"]
[7642932,"AWHP 8MR-FSCR 19P HYBRID V200",null,{"$f":"D639+D642+D646+D652+D654","v":10174},{"$f":"E639+E642+E646+E652+E654","v":12.5},null," A++"," A","L",3661238645226,null,null,null,null,"C9"]
[7642934,"AWHP 11MR-FSCR 19P HYBRID V200",null,{"$f":"D639+D642+D647+D653+D654","v":11494},{"$f":"E639+E642+E647+E653+E654","v":12.5},null," A++"," A","L",3661238645240,null,null,null,null,"C9"]
[7642936,"AWHP 11TR-FSCR 19P HYBRID V200",null,{"$f":"D639+D642+D648+D653+D654","v":11798},{"$f":"E639+E642+E648+E653+E654","v":12.5},null," A++"," A","L",3661238645264,null,null,null,null,"C9"]
[7642938,"AWHP 16MR-FSCR 19P HYBRID V200",null,{"$f":"D639+D642+D649+D653+D654","v":12587},{"$f":"E639+E642+E649+E653+E654","v":12.5},null," A++"," A","L",3661238646490,null,null,null,null,"C9"]
[7642940,"AWHP 16TR-FSCR 19P HYBRID V200",null,{"$f":"D639+D642+D650+D653+D654","v":13012},{"$f":"E639+E642+E650+E653+E654","v":12.5},null," A++"," A","L",3661238646513,null,null,null,null,"C9"]
[7642942,"AWHP 6MR-FSCR 24P HYBRID V200",null,{"$f":"D640+D642+D645+D651+D652+D654","v":9683},{"$f":"E640+E642+E645+E651+E652+E654","v":12.5},null," A++"," A","L",3661238645325,null,null,null,null,"C9"]
[7642944,"AWHP 8MR-FSCR 24P HYBRID V200",null,{"$f":"D640+D642+D646+D652+D654","v":10376},{"$f":"E640+E642+E646+E652+E654","v":12.5},null," A++"," A","L",3661238645349,null,null,null,null,"C9"]
[7642946,"AWHP 11MR-FSCR 24P HYBRID V200",null,{"$f":"D640+D642+D647+D653+D654","v":11696},{"$f":"E640+E642+E647+E653+E654","v":12.5},null," A++"," A","L",3661238645363,null,null,null,null,"C9"]
[7642948,"AWHP 11TR-FSCR 24P HYBRID V200",null,{"$f":"D640+D642+D648+D653+D654","v":12000},{"$f":"E640+E642+E648+E653+E654","v":12.5},null," A++"," A","L",3661238645387,null,null,null,null,"C9"]
[7642950,"AWHP 16MR-FSCR 24P HYBRID V200",null,{"$f":"D640+D642+D649+D653+D654","v":12789},{"$f":"E640+E642+E649+E653+E654","v":12.5},null," A++"," A","L",3661238646612,null,null,null,null,"C9"]
[7642952,"AWHP 16TR-FSCR 24P HYBRID V200",null,{"$f":"D640+D642+D650+D653+D654","v":13214},{"$f":"E640+E642+E650+E653+E654","v":12.5},null," A++"," A","L",3661238646636,null,null,null,null,"C9"]
[7642954,"AWHP 8MR-FSCR 32P HYBRID V200",null,{"$f":"D641+D642+D646+D652+D654","v":10728},{"$f":"E641+E642+E646+E652+E654","v":12.5},null," A++"," A","L",3661238645448,null,null,null,null,"C9"]
[7642956,"AWHP 11MR-FSCR 32P HYBRID V200",null,{"$f":"D641+D642+D647+D653+D654","v":12048},{"$f":"E641+E642+E647+E653+E654","v":12.5},null," A++"," A","L",3661238645462,null,null,null,null,"C9"]
[7642958,"AWHP 11TR-FSCR 32P HYBRID V200",null,{"$f":"D641+D642+D648+D653+D654","v":12352},{"$f":"E641+E642+E648+E653+E654","v":12.5},null," A++"," A","L",3661238645486,null,null,null,null,"C9"]
[7642960,"AWHP 16MR-FSCR 32P HYBRID V200",null,{"$f":"D641+D642+D649+D653+D654","v":13141},{"$f":"E641+E642+E649+E653+E654","v":12.5},null," A++"," A","L",3661238646711,null,null,null,null,"C9"]
[7642962,"AWHP 16TR-FSCR 32P HYBRID V200",null,{"$f":"D641+D642+D650+D653+D654","v":13566},{"$f":"E641+E642+E650+E653+E654","v":12.5},null," A++"," A","L",3661238646735,null,null,null,null,"C9"]
[]
[null,"Avec chaudière fioul à condensation ventouse"]
[7642964,"AWHP 4MR-FSCR 19PF HYBRID V200",null,{"$f":"D639+D642+D643+D644+D651+D652+D654","v":9493},{"$f":"E639+E642+E643+E644+E651+E652+E654","v":12.5},null," A++"," A","L",3661238645547,null,null,null,null,"C9"]
[7642966,"AWHP 6MR-FSCR 19PF HYBRID V200",null,{"$f":"D639+D642+D643+D645+D651+D652+D654","v":9582},{"$f":"E639+E642+E643+E645+E651+E652+E654","v":12.5},null," A++"," A","L",3661238645561,null,null,null,null,"C9"]
[7642968,"AWHP 8MR-FSCR 19PF HYBRID V200",null,{"$f":"D639+D642+D643+D646+D652+D654","v":10275},{"$f":"E639+E642+E643+E646+E652+E654","v":12.5},null," A++"," A","L",3661238645585,null,null,null,null,"C9"]
[7642970,"AWHP 11MR-FSCR 19PF HYBRID V200",null,{"$f":"D639+D642+D643+D647+D653+D654","v":11595},{"$f":"E639+E642+E643+E647+E653+E654","v":12.5},null," A++"," A","L",3661238645615,null,null,null,null,"C9"]
[7642972,"AWHP 11TR-FSCR 19PF HYBRID V200",null,{"$f":"D639+D642+D643+D648+D653+D654","v":11899},{"$f":"E639+E642+E643+E648+E653+E654","v":12.5},null," A++"," A","L",3661238645639,null,null,null,null,"C9"]
[7642975,"AWHP 16MR-FSCR 19PF HYBRID V200",null,{"$f":"D639+D642+D643+D649+D653+D654","v":12688},{"$f":"E639+E642+E643+E649+E653+E654","v":12.5},null," A++"," A","L",3661238646858,null,null,null,null,"C9"]
[7642977,"AWHP 16TR-FSCR 19PF HYBRID V200",null,{"$f":"D639+D642+D643+D650+D653+D654","v":13113},{"$f":"E639+E642+E643+E650+E653+E654","v":12.5},null," A++"," A","L",3661238646872,null,null,null,null,"C9"]
[7642979,"AWHP 6MR-FSCR 24PF HYBRID V200",null,{"$f":"D640+D642+D643+D645+D651+D652+D654","v":9784},{"$f":"E640+E642+E643+E645+E651+E652+E654","v":12.5},null," A++"," A","L",3661238645691,null,null,null,null,"C9"]
[7642981,"AWHP 8MR-FSCR 24PF HYBRID V200",null,{"$f":"D640+D642+D643+D646+D652+D654","v":10477},{"$f":"E640+E642+E643+E646+E652+E654","v":12.5},null," A++"," A","L",3661238645714,null,null,null,null,"C9"]
[7642983,"AWHP 11MR-FSCR 24PF HYBRID V200",null,{"$f":"D640+D642+D643+D647+D653+D654","v":11797},{"$f":"E640+E642+E643+E647+E653+E654","v":12.5},null," A++"," A","L",3661238645738,null,null,null,null,"C9"]
[7642985,"AWHP 11TR-FSCR 24PF HYBRID V200",null,{"$f":"D640+D642+D643+D648+D653+D654","v":12101},{"$f":"E640+E642+E643+E648+E653+E654","v":12.5},null," A++"," A","L",3661238645752,null,null,null,null,"C9"]
[7642987,"AWHP 16MR-FSCR 24PF HYBRID V200",null,{"$f":"D640+D642+D643+D649+D653+D654","v":12890},{"$f":"E640+E642+E643+E649+E653+E654","v":12.5},null," A++"," A","L",3661238646971,null,null,null,null,"C9"]
[7642989,"AWHP 16TR-FSCR 24PF HYBRID V200",null,{"$f":"D640+D642+D643+D650+D653+D654","v":13315},{"$f":"E640+E642+E643+E650+E653+E654","v":12.5},null," A++"," A","L",3661238646995,null,null,null,null,"C9"]
[7642991,"AWHP 8MR-FSCR 32PF HYBRID V200",null,{"$f":"D641+D642+D643+D646+D652+D654","v":10829},{"$f":"E641+E642+E643+E646+E652+E654","v":12.5},null," A++"," A","L",3661238645813,null,null,null,null,"C9"]
[7642993,"AWHP 11MR-FSCR 32PF HYBRID V200",null,{"$f":"D641+D642+D643+D647+D653+D654","v":12149},{"$f":"E641+E642+E643+E647+E653+E654","v":12.5},null," A++"," A","L",3661238645837,null,null,null,null,"C9"]
[7642995,"AWHP 11TR-FSCR 32PF HYBRID V200",null,{"$f":"D641+D642+D643+D648+D653+D654","v":12453},{"$f":"E641+E642+E643+E648+E653+E654","v":12.5},null," A++"," A","L",3661238645851,null,null,null,null,"C9"]
[7642997,"AWHP 16MR-FSCR 32PF HYBRID V200",null,{"$f":"D641+D642+D643+D649+D653+D654","v":13242},{"$f":"E641+E642+E643+E649+E653+E654","v":12.5},null," A++"," A","L",3661238647084,null,null,null,null,"C9"]
[7642999,"AWHP 16TR-FSCR 32PF HYBRID V200",null,{"$f":"D641+D642+D643+D650+D653+D654","v":13667},{"$f":"E641+E642+E643+E650+E653+E654","v":12.5},null," A++"," A","L",3661238647107,null,null,null,null,"C9"]
[]
["COMPOSANTS"]
[7624096,"FSC. 19","MY103",3886,5,14070,null,null,null,3661238617315,209,1220,750,1050,"D6"]
[7624118,"FSC. 24","MY108",4088,5,14070,null,null,null,3661238617322,237,1220,750,1050,"D6"]
[7624125,"FSC. 32","MY113",4440,5,14070,null,null,null,3661238617339,265,1220,750,1050,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,15,675,485,180,"D6"]
[7605520,"KIT FLUX FORCE FSC.","MY405",101,null,null,null,null,null,3661238627048,2,510,460,175,"D6"]
[7603571,"AWHP 4 MR","EH336",1837,6.67,11050,"/","/","/",3661238581012,48,450,950,690,"C9"]
[7609925,"AWHP 6 MR-2 ","EH380",1926,6.67,11050,"/","/","/",3661238589513,45.2,445,950,680,"C9"]
[7609926,"AWHP 8 MR-2 ","EH381",2677,6.67,11050,null,null,null,3661238589520,82.2,460,1090,1100,"C9"]
[7609927,"AWHP 11 MR-2 ","EH382",3529,6.67,11050,null,null,null,3661238589537,131,450,1040,1440,"C9"]
[7609928,"AWHP 11 TR-2 ","EH383",3833,6.67,11050,"/","/","/",3661238589544,137.6,460,1090,1490,"C9"]
[7609929,"AWHP 16 MR-2 ","EH384",4622,6.67,11050," /"," /"," /",3661238589551,131,450,1040,1440,"C9"]
[7609930,"AWHP 16 TR-2 ","EH385",5047,6.67,11050," /"," /"," /",3661238589568,145,450,1040,1440,"C9"]
[100015480,"RACCORD D'ADAPTATION FRIGO POUR 4 kW ET 6 kW","EH146",58,null,null,"/","/","/",3661238381612,0.5,150,80,30,"C9"]
[7623191,"BALLON 200 PSL HYBRIDE 4-8","EH501",3017,null,null,null,null,null,3661238621299,130,970,645,1435,"C9"]
[7623204,"BALLON 200 PSL HYBRIDE 11-16","EH505",3485,null,null,null,null,null,3661238621305,132,970,645,1435,"C9"]
[7621386,"KIT DE MONTAGE BALLON VERSION V","EH524",114,null,null,null,null,null,3661238618114,1.1499999999999999,860,250,135,"C9"]
[7621387,"KIT DE MONTAGE BALLON VERSION B","EH525",218,null,null,null,null,null,3661238618121,7.3,860,670,220,"C9"]
[]
["OPTIONS"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,null,null,null,3661238157972,2,1025,170,170,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[100004417,"FILTRE 400UM + VANNE D'ISOLEMENT PAC ROE 6-10 ET ROE+","EH61",105,null,null,"/","/","/",3661238003415,0.9,175,90,130,"C6"]
[100011222,"SUPPORT MURALE & PLOTS ANTIVIBRATILES POUR  ROE-II AWHP 6-8","EH95",162,null,null,"/","/","/",3661238339927,5.4,820,90,90,"C6"]
[100018409,"SUPPORT MURAL AWHP 11à 27 kW","EH250",166,null,null,"/","/","/",3661238543874,5,820,90,90,"C6"]
[100012532,"BAC DE RECUPERATION CONDENSATS POUR SUPPORT MURAL","EH111",142,null,null,"/","/","/",3661238361553,2,960,430,80,"C6"]
[100012534,"CORDON CHAUFFANT ELECTRIQUE","EH113",150,null,null,"/","/","/",3661238361577,0.2,200,200,10,"C6"]
[100012533,"SUPPORT POSE AU SOL AWHP","EH112",45,null,null,"/","/","/",3661238361560,1.2,450,140,80,"C6"]
[100012535,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 5m","EH114",233,null,null,"/","/","/",3661238361522,4.5999999999999996,600,600,150,"C6"]
[100012536,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 10m","EH115",416,null,null,"/","/","/",3661238361539,7.2,600,600,200,"C6"]
[100012537,"LIAISON FRIGORIFIQUE PE 5/8'' 3/8'' - LG 20m","EH116",751,null,null,"/","/","/",3661238361546,14.3,750,750,230,"C6"]
[100015476,"LIAISON FRIGORIFIQUE PE 1/2\" 1/4\" - LG 10 m","EH142",233,null,null,"/","/","/",3661238381575,7.9,600,650,150,"C6"]
[100008841,"BALLON TAMPON 80L B 80 T","EH85",521,null,null,"/","/","/",3661238166325,44.5,510,510,920,"C6"]
[100004415,"BALLON TAMPON 160L B 150 T","EH60",781,null,null,"/","/","/",3661238003422,63.2,825,690,1120,"C6"]
[88017904,"THERMOSTAT AMBIANCE PROGRAMMABLE (FILAIRE)","AD191",161,0.12,95010,"/","/","/",3661238048836,0.2,130,90,55,"C0"]
[88017010,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (SANS FILS)","AD192",286,0.12,95010,"/","/","/",3661238049178,0.4,175,150,90,"C0"]
[7624902,"KIT CABLAGE PLANCHER CHAUFFANT DIRECT","HA255",37,0.02,95020,"/","/","/",3661238618176,0.23,340,240,40,"C6"]
[7619010,"KIT VANNE 3 VOIES","EH528",576,0.12,95010,"/","/","/",3661238618152,17.7,750,300,150,"C6"]
[7622273,"CARTE DE REGULATION 2 CIRCUITS","EH527",199,0.12,95010,"/","/","/",3661238618145,0.3,185,130,105,"C6"]
[7626737,"KIT ISOLATION MODE FROID","EH567",208,null,null,"/","/","/",3661238624115,0.64,615,280,80,"C6"]
[100019114,"KIT DETECTEUR DE CONDENSATION","HK27",212,0.12,95010,"/","/","/",3661238569119,0.2,185,130,105,"C0"]
[7636899,"KIT SILENCIEUX MODULE EXTERIEUR","EH572",60,0.02,95020,"/","/","/",3661238644335,0.2,170,210,20,"C0"]
[7621387,"KIT DE MONTAGE BALLON VERSION B","EH525",218,null,null,null,null,null,3661238618121,null,860,670,220,"C0"]
[]
[]
[100017618,"OTWH 300 E","EH196",2311,6.67,11050,"/","A","XL",3661238497023,127,780,800,2165,"D7"]
[100017619,"OTWH 300 EH","EH197",2742,6.67,11050,"/","A","XL",3661238497016,143,780,800,2165,"D7"]
[100017617,"OTWH 200 E","EH195",2205,6.67,11050,"/","A","L",3661238497030,112,780,800,1810,"D7"]
[7603139,"OTWH 200 EV","EH282",3089,6.67,11050,"/","A","L",3661238583337,96,800,780,1800,"D7"]
[7629072,"OTWH 180 E","EH583",1766,6.67,11050,"/","A","L",3661238625235,128,730,700,1865,"D7"]
[7629074,"OTWH 230 E","EH584",1867,6.67,11050,"/","A","XL",3661238625242,144,730,700,2185,"D7"]
[]
[]
[7629721,"OTWH SPLIT FS 200 E",null,{"$f":"D696+D698","v":2112},null,null,"/","A","L",3661238626584,null,null,null,null,"D7"]
[7629722,"OTWH SPLIT FS 270 E",null,{"$f":"D697+D698","v":2215},null,null,"/","A","XL",3661238626591,null,null,null,null,"D7"]
[]
["COMPOSANTS"]
[7629505,"BALLON OSFS 200 E ","ER688",1509,null,null,"/","/","/",3661238626560,81.5,900,800,1450,"D7"]
[7629506,"BALLON OSFS 270 E ","ER689",1612,null,null,"/","/","/",3661238626577,93,900,800,1850,"D7"]
[7626223,"UNITE EXTERIEURE SPLIT TD","EH571",603,6.67,11050,"/","/","/",3588691513148,39.4,915,385,715,"D7"]
[]
["ACCESSOIRES HYDRAULIQUES"]
[100019424,"KIT DE RACCORDEMENT GROUPE DE SECURITE ","ER208",24,null,null,"/","/","/",3661238571723,0.5,250,150,100,"C6"]
[]
["OPTIONS"]
[100011222,"SUPPORT MURALE & PLOTS ANTIVIBRATILES POUR  ROE-II AWHP 6-8","EH95",162,null,null,"/","/","/",3661238339927,5.4,820,90,90,"C6"]
[100012533,"SUPPORT POSE AU SOL AWHP","EH112",45,null,null,"/","/","/",3661238361560,1.2,450,140,80,"C6"]
[7627741,"TUBE CU ISOLE 1/4 3/8 L5M","EH569",129,null,null,"/","/","/",3661238626539,3,600,600,100,"C6"]
[7627742,"TUBE CU ISOLE 1/4 3/8 L10M","EH570",224,null,null,"/","/","/",3661238626546,4.5,600,600,150,"C6"]
[7629725,"TUBE CU ISOLE 1/4 3/8 L20","EH589",330,null,null,"/","/","/",3661238626553,8,800,800,100,"C6"]
[]
["ACCESSOIRES HYDRAULIQUES"]
[100019424,"KIT DE RACCORDEMENT GROUPE DE SECURITE ","ER208",24,null,null,"/","/","/",3661238571723,0.5,250,150,100,"C6"]
[]
["OPTIONS"]
[100007557,"COUDE A 90° D160","EH77",62,null,null,"/","/","/",3661238158498,1.26,420,290,195,"C6"]
[100017621,"MANCHON D'ADAPTATION D200 x D160","EH205",77,null,null,"/","/","/",3661238497047,0.65,220,205,150,"C6"]
[100017622,"GAINE SOUPLE ISOLEE  Ø 160 LONGUEUR 3 M","EH206",286,null,null,"/","/","/",3661238497054,5.3,3040,210,210,"C6"]
[100017623,"JEU DE 2 COLLIERS DE FIXATION Ø 160","EH207",32,null,null,"/","/","/",3661238497061,0.09,125,125,15,"C6"]
[7625587,"GRILLE PRISE ET REJET AIR D160 ","EH558",329,null,null,"/","/","/",3661238619302,3.1,510,330,245,"C6"]
[100017624,"TRAVERSEE DE MUR Ø 160 AVEC GRILLE","EH208",158,null,null,"/","/","/",3661238497078,1.6,225,205,295,"C6"]
[100017625,"GRILLE EXTERIEURE Ø 160 EN ALUMINIUM","EH209",227,null,null,"/","/","/",3661238497085,0.46,215,215,85,"C6"]
[100019964,"CONDUIT PPE Ø 160 mm 2 x 1 m + 2 MANCHONS","EH272",106,null,null,"/","/","/",3661238571310,1.6,400,310,1020,"C6"]
[100019965,"JEU DE 2  COUDES 90°  PPE  Ø 160 mm + 2 MANCHONS","EH273",77,null,null,"/","/","/",3661238571327,0.9,440,340,510,"C6"]
[100019966,"JEU DE 2 MANCHONS PPE Ø  160 mm","EH274",24,null,null,"/","/","/",3661238571334,0.6,250,180,260,"C6"]
[100019967,"TERMINAL VERTICAL NOIR Ø 160 mm","EH275",176,null,null,"/","/","/",3661238571341,2.84,1030,320,320,"C6"]
[100019968,"EMBASE D'ETANCHEITE TOIT PLAT Ø  160mm","EH276",37,null,null,"/","/","/",3661238571358,0.88,560,430,260,"C6"]
[100019969,"EMBASE D'ETANCHEITE TOIT PENTE DEN 25 à 45°","EH277",147,null,null,"/","/","/",3661238571365,3,null,null,null,"C6"]
[7613626,"COUDE CONDUIT","EH434",53,null,null,"/","/","/",3661238592414,1,565,370,235,"C6"]
[7603277,"BOUCHE EXTRACTION HYGRO CUISINE A PILES 6/40/90 m3/h   (1)","EH291",119,0.12,95010,"/","/","/",3661238581159,0.6,310,220,100,"C6"]
[7603278,"BOUCHE EXTRACTION HYGRO CUISINE A PILES 10/45/120 m3/h   (1)","EH292",119,0.12,95010,"/","/","/",3661238581142,0.6,310,220,100,"C6"]
[7603279,"BOUCHE EXTRACTION HYGRO CUISINE A PILES 10/45/135 m3/h    (1)","EH293",119,0.12,95010,"/","/","/",3661238581135,0.6,310,220,100,"C6"]
[7618711,"BOUCHE EXTRACTION HYGRO CUISINE A PILES 12/45/105 m3/h    (1)","EH487",119,0.12,95010,"/","/","/",3661238604438,0.65,310,220,110,"C6"]
[7603280,"BOUCHE EXTRACTION HYGRO CUISINE A PILES 12/45/135 m3/h    (1)","EH294",119,0.12,95010,"/","/","/",3661238581128,0.6,310,220,100,"C6"]
[7603281,"BOUCHE EXTRACTION HYGRO CUISINE A CORDON 6/40/90 m3/h ","EH295",102,null,null,"/","/","/",3661238581104,0.5,310,220,100,"C6"]
[7603282,"BOUCHE EXTRACTION HYGRO CUISINE A CORDON 10/45/120 m3/h ","EH296",102,null,null,"/","/","/",3661238581081,0.5,310,220,100,"C6"]
[7603283,"BOUCHE EXTRACTION HYGRO CUISINE A CORDON 10/45/135 m3/h ","EH297",102,null,null,"/","/","/",3661238581074,0.5,310,220,100,"C6"]
[7618714,"BOUCHE EXTRACTION HYGRO CUISINE A CORDON 12/45/105 m3/h ","EH488",102,null,null,"/","/","/",3661238604445,0.5,310,220,110,"C6"]
[7603284,"BOUCHE EXTRACTION HYGRO CUISINE A CORDON 12/45/135 m3/h ","EH298",102,null,null,"/","/","/",3661238581050,0.5,310,220,100,"C6"]
[7603286,"BOUCHE EXTRACTION HYGRO BAINS A PILES 5/40 m3/h ","EH299",71,0.12,95010,"/","/","/",3661238581043,0.3,310,220,100,"C6"]
[7603287,"BOUCHE EXTRACTION HYGRO BAINS A PILES 5/45 m3/h ","EH300",71,0.12,95010,"/","/","/",3661238581029,0.3,310,220,100,"C6"]
[7603288,"BOUCHE EXTRACTION HYGRO BAINS A PILES 10/40 m3/h ","EH301",71,0.12,95010,"/","/","/",3661238581173,0.3,310,220,100,"C6"]
[7603289,"BOUCHE EXTRACTION HYGRO BAINS A PILES 10/45 m3/h ","EH302",71,0.12,95010,"/","/","/",3661238581319,0.3,310,220,100,"C6"]
[7618715,"BOUCHE EXTRACTION HYGRO MANCHON PLACO 3 GRIFFES - BAINS A PILES 10/45/45 m3/h","EH489",75,0.12,95010,"/","/","/",3661238604452,0.5,310,220,110,"C6"]
[7603290,"BOUCHE EXTRACTION HYGRO WC A PILES 5/30 m3/h   (2)","EH303",78,0.12,95010,"/","/","/",3661238581296,0.4,310,220,100,"C6"]
[7604607,"KIT T3-T4 AVEC BOUCHES EXTRACTION HYGRO POUR CUISINE - BAINS - WC  (2)","EH338",251,0.83,14050,"/","/","/",3661238588127,1.4,405,310,205,"C6"]
[7604608,"KIT T5-T7 AVEC BOUCHES EXTRACTION HYGRO POUR CUISINE - BAINS - WC   (2)","EH339",251,0.83,14050,"/","/","/",3661238588134,1.4,405,310,205,"C6"]
[7603291,"KIT ENTREE D'AIR HYGRO 6/45 m3/h","EH304",35,null,null,"/","/","/",3661238581289,0.2,435,320,280,"C6"]
[7603296,"MANCHETTE PLASTIQUE D 125 POUR BOUCHE EXTRACTION","EH307",3,null,null,"/","/","/",3661238581241,0.2,210,200,120,"C6"]
[7603297,"MANCHETTE PLAST D80 BOUCHE EXTR","EH308",3,null,null,"/","/","/",3661238581234,0.4,450,325,55,"C6"]
[7603298,"CHAPEAU DE TOITURE COULEUR TUILE D 160","EH309",62,null,null,"/","/","/",3661238581210,2.6,420,255,310,"C6"]
[7608997,"CHAPEAU DE TOITURE COULEUR ARDOISE D 160","EH370",62,null,null,"/","/","/",3661238588141,2.6,420,255,310,"C6"]
[7603304,"CONDUIT FLEXIBLE ISOLE D 160 LONGUEUR 6 M","EH314",98,null,null,"/","/","/",3661238581418,5.5,1150,390,390,"C6"]
[7603303,"CONDUIT FLEXIBLE ISOLE D 125 LONGUEUR 6 M","EH313",62,null,null,"/","/","/",3661238581425,4.2,1150,260,260,"C6"]
[7603302,"CONDUIT FLEXIBLE ISOLE D 80 LONGUEUR 6 M","EH312",51,null,null,"/","/","/",3661238581340,3,1150,190,190,"C6"]
[7603305,"CAISSON COLLECTEUR  2 PIQUAGES D 125 ET 6 PIQUAGES D 80","EH315",142,null,null,"/","/","/",3661238581401,1,610,520,165,"C6"]
[7603306,"CONDUIT PPE D125 - LONGUEUR 2 x 1 M + 2 MANCHONS","EH316",76,null,null,"/","/","/",3661238581395,1.5,1000,400,300,"C6"]
[7603307,"TUBE PPE D125 L=1M ","EH317",76,null,null,"/","/","/",3661238581388,1.5,1000,400,300,"C6"]
[7603310,"2 COUDES 90° PPE D125 + 2 MANCHONS","EH319",70,null,null,"/","/","/",3661238581364,1,500,400,300,"C6"]
[7603312,"2 MANCHONS PPE D125","EH321",14,null,null,"/","/","/",3661238581432,0.5,240,180,250,"C6"]
[7603313,"TE DROIT GALVA 90° A JOINT D 125","EH322",22,null,null,"/","/","/",3661238581555,7,600,400,400,"C6"]
[7603314,"TE DROIT GALVA 90° A JOINT D 160","EH323",31,null,null,"/","/","/",3661238581548,50,1203,803,800,"C6"]
[7603315,"TE DROIT GALVA 90° A JOINT D 125 X 80","EH324",27,null,null,"/","/","/",3661238581531,10,400,400,800,"C6"]
[7603316,"TE DROIT GALVA 90° A JOINT D 160 X 125 ","EH325",26,null,null,"/","/","/",3661238581524,35,1203,803,800,"C6"]
[7603317,"REDUCTION GALVA  A JOINT  D 125 X 80","EH326",25,null,null,"/","/","/",3661238581517,13,400,400,400,"C6"]
[7603318,"REDUCTION GALVA  A Ø 160 X 80","EH327",30,null,null,"/","/","/",3661238581500,12,400,400,400,"C6"]
[7603319,"REDUCTION GALVA  A JOINT D 160 X 125 ","EH328",25,null,null,"/","/","/",3661238581494,7,400,400,400,"C6"]
[7603320,"MANCHON GALVA D 125","EH329",4,null,null,"/","/","/",3661238581487,1,250,180,140,"C6"]
[7603321,"MANCHON GALVA D 160","EH330",4,null,null,"/","/","/",3661238581470,1,300,180,140,"C6"]
[7603322,"JEU DE 10 COLLIERS DE FIXATION Ø 80 à Ø 125","EH331",49,null,null,"/","/","/",3661238581463,0.6,250,185,155,"C6"]
[7603325,"FILTRE DE RECHANGE ","EH334",35,null,null,"/","/","/",3661238581562,0.2,330,290,30,"C6"]
[7602875,"ENJOLIVEUR POUR MONTAGE REGULATEUR SUR OTWH 200 EV","EH286",79,null,null,"/","/","/",3661238587717,0.7,350,320,150,"C6"]
[100019890,"KIT POIGNEES DE PREHENSION","ER239",33,null,null,"/","/","/",3661238570634,1.2,250,150,100,"C6"]
[null,null,null,null,null,null,"/","/","/"]
["PREPARATEUR ECS MIXTE POUR PAC"]
[7622063,"PREPARATEUR MIXTE OBEPB 300 POUR PAC","ER616",2049,null,null,"/","C","XL",3661238613010,125,900,800,1970,"C6"]
["OPTIONS"]
[100009229,"VANNE 3 VOIES D'INVERSION POUR ECS AVEC KIT CABLAGE","EH84",334,null,null,"/","/","/",3661238337916,4.3499999999999996,410,210,115,"C6"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.16,200,150,30,"C0"]
[89757753,"ANODE ACI CORREX UP BALLON > 300 LITRES","AJ39",391,0.02,95020,"/","/","/",3661238046832,0.4,425,100,55,"C0"]
[]
["FAMILLE:","SOLAIRE - OERTLISOL    "]
[]
["CAPTEUR SOLAIRE PLAN DH 200SL "]
[7652623,"PACK TOIT 1 DH 200 SL- 2m² CROCHET UNIVERSEL TUILES MECANIQUES","ER771",1072,null,null,"/","/","/",3661238662117,70,1330,770,1944,"C7"]
[7652638,"PACK TOIT 2 DH 200 SL- 4m² CROCHET UNIVERSEL TUILES MECANIQUES","ER772",1787,null,null,"/","/","/",3661238662124,105,1330,770,1944,"C7"]
[7652640,"PACK TOIT 3 DH 200 SL- 6m² CROCHET UNIVERSEL TUILES MECANIQUES","ER773",2767,null,null,"/","/","/",3661238662131,128,1330,770,1944,"C7"]
[7652652,"PACK TOIT 1 DH 200 SL- 2m² SUR TOITURE ARDOISES","ER774",1072,null,null,"/","/","/",3661238662148,70,1330,770,1944,"C7"]
[7652653,"PACK TOIT 2 DH 200 SL- 4m² SUR TOITURE ARDOISES","ER775",1787,null,null,"/","/","/",3661238662162,105,1330,770,1944,"C7"]
[7652654,"PACK TOIT 3 DH 200 SL- 6m² SUR TOITURE ARDOISES","ER776",2767,null,null,"/","/","/",3661238662155,128,1330,770,1944,"C7"]
[7652656,"PACK TOIT 1 DH 200 SL- 2m² MONTAGE VERTICAL SUR TERRASSE ","ER777",1144,null,null,"/","/","/",3661238662179,72,1330,770,2086,"C7"]
[7652657,"PACK TOIT 2 DH 200 SL- 4m² MONTAGE VERTICAL SUR TERRASSE ","ER778",1909,null,null,"/","/","/",3661238662186,108,1330,770,2086,"C7"]
[7652658,"PACK TOIT 3 DH 200 SL- 6m² MONTAGE VERTICAL SUR TERRASSE ","ER779",2981,null,null,"/","/","/",3661238662193,132,1330,770,2086,"C7"]
[]
["PANNEAU SOLAIRE SLIM LINE DH 200 SL"]
[7219377,"CAPTEUR SOLAIRE  INISOL DH 200 SL","ER719",684,null,null,"/","/","/",3661238632936,35,2265,1230,105,"C7"]
[]
["ACCESSOIRES DE RACCORDEMENT HYDRAULIQUE"]
[null,"Pour système sous pression"]
[7221972,"KIT RACCORDS O RING 2 CAPTEURS SL ","ER726",184,null,null,"/","/","/",3661238633056,2.2999999999999998,1040,165,60,"C7"]
[7221975,"SET 2 RACCORDS O RING EXTENSION  SL","ER727",41,null,null,"/","/","/",3661238633070,0.2,175,115,35,"C7"]
[null,"Pour système auto vidangeable",null,null,null,null,"/","/","/"]
[7222026,"KIT RACCORDS BICONE 2 CAPTEURS SL ","ER720",112,null,null,"/","/","/",3661238632943,1.3,300,105,70,"C7"]
[7222029,"SET 2 RACCORDS BI CONES EXTENSION  SL","ER721",26,null,null,"/","/","/",3661238632974,0.3,175,115,35,"C7"]
[100016508,"KIT  FLEXIBLES CIRCUIT SOLAIRE CHAMP CAPTEURS","ER247",77,null,null,"/","/","/",3661238492349,1065,175,645,1.3,"C7"]
[]
["DISPOSITIF DE MONTAGE EN TERRASSE (OU AU SOL)"]
[7217045,"KIT PROFILES A KLIPPER (LONG)  POUR 1 CAPTEUR VERTICAL","ER732",82,null,null,"/","/","/",3661238639836,2.5,1350,145,80,"C7"]
[7217038,"2 SUPPORTS SL MONTAGE VERTICAL 1 CAPTEUR","ER658",196,null,null,"/","/","/","3661238630710",3.5,2267,145,80,"C7"]
[7217039,"1 SUPPORT SL VERTICAL POUR EXTENSION 1 CAPTEUR ","ER659",91,null,null,"/","/","/","3661238630277",1.7,1945,110,95,"C7"]
[]
["FERRURES D'ANCRAGE POUR MONTAGE SUR TOITURE"]
[89807311,"4 CROCHETS ALU UNIVERSEL POUR TUILES MÉCANIQUES","EG311",98,null,null,"/","/","/",3661238045903,2.34,365,120,140,"C7"]
[89807312,"6 CROCHETS ALU UNIVERSEL POUR TUILES MÉCANIQUES","EG312",141,null,null,"/","/","/",3661238045897,3.46,365,115,140,"C7"]
[89807313,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES MÉCANIQUES","EG313",98,null,null,"/","/","/",3661238045880,3.37,320,220,135,"C7"]
[89807314,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES MÉCANIQUES","EG314",141,null,null,"/","/","/",3661238045873,4.93,325,225,135,"C7"]
[89807315,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES PLATES","EG315",98,null,null,"/","/","/",3661238045866,2.4,300,135,95,"C7"]
[89807316,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES PLATES","EG316",141,null,null,"/","/","/",3661238045859,3.5,310,140,95,"C7"]
[100015314,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES CANAL","ER136",97,null,null,"/","/","/",3661238415539,4,325,260,120,"C7"]
[100015315,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES CANAL","ER137",141,null,null,"/","/","/",3661238415546,6.5,410,305,115,"C7"]
[89807317,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT ETERNIT","EG317",98,null,null,"/","/","/",3661238045842,3.56,260,215,75,"C7"]
[89807318,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT ETERNIT","EG318",141,null,null,"/","/","/",3661238045835,5.3,260,220,75,"C7"]
[89807319,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT D'ARDOISES","EG319",98,null,null,"/","/","/",3661238045828,2.21,280,120,80,"C7"]
[89807320,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT D'ARDOISES","EG320",141,null,null,"/","/","/",3661238045811,3.3,305,140,95,"C7"]
[89807782,"KIT TIRE-FONDS POUR MONTAGE 2 CAPTEURS","EG94",247,null,null,"/","/","/",3661238045057,2.8,400,135,175,"C7"]
[89807783,"KIT TIRE-FONDS POUR MONTAGE 3 CAPTEURS","EG95",310,null,null,"/","/","/",3661238045040,3.6,400,135,175,"C7"]
[]
["SUPPORTS INCLINABLES POUR MONTAGE EN TERRASSE (OU AU SOL)"]
[7217041,"2 SUPPORTS SL HL MONTAGE HORIZONTAL 1 CAPTEUR","ER656",156,null,null,"/","/","/",3661238630253,5.5,1250,145,80,"C7"]
[7217042,"1 SUPPORT SL HL HORIZONTAL POUR EXTENSION 1 CAPTEUR","ER657",79,null,null,"/","/","/",3661238630260,3,1250,145,80,"C7"]
[7502583,"2 SUPPORTS SL MONTAGE VERTICAL 1 CAPTEUR","ER547",196,null,null,"/","/","/",3661238588417,8.1999999999999993,1945,110,95,"C7"]
[7502951,"1 SUPPORT SL VERTICAL POUR EXTENSION 1 CAPTEUR ","ER548",92,null,null,"/","/","/",3661238586512,4.5,1945,110,95,"C7"]
[]
["FLUIDE CALOPORTEUR"]
[89807794,"FLUIDE CALOPORTEUR TYPE L (-21°C) 20 LITRES. ","EG101",78,null,null,"/","/","/",3661238045019,21.72,240,290,370,"C7"]
[100017611,"FLUIDE CALOPORTEUR HAUTE PREFORMANCE BIO (-26°C) 20 LITRES","ER316",134,null,null,"/","/","/",3661238496606,21.53,340,290,370,"C7"]
[89807792,"FLUIDE CALOPORTEUR HAUTE PREFORMANCE TYPE LS (-26°C) 20 LITRES","EG100",154,null,null,"/","/","/",3661238045033,21.53,340,290,370,"C7"]
[89807710,"CONCENTRE TYPE L, 10 LITRES","EG11",99,null,null,"/","/","/",3661238045316,10.95,220,190,295,"C7"]
[]
["PRÉPARATEURS SOLAIRES NON ÉQUIPÉS POUR APPOINT EXTERIEUR"]
[7606302,"BALLON OBS 150N ","ER337",846,null,null,"/","C stockage \nECS","/",3661238585959,null,null,null,null,"C7"]
[]
["Options"]
[7630415,"STATION SOLAIRE DKSC 6-8 MSB","ER711",479,0.83,14090,"/","/","/",3661238631014,7.3,620,240,450,"C7"]
[100020297,"DUO TUBE DN10 ","ER319",360,null,null,"/","/","/",3661238576612,11,780,770,160,"C7"]
["S102991","KIT SOLAIRE AVEC MITIGEUR DIAM 15","HR84",223,null,null,"/","/","/",8713809259983,1.3,145,140,120,"C7"]
[7603940,"KIT CONNECTION SOLAIRE ","ER417",163,0.12,95010,"/","/","/",3661238599376,0.4,185,130,105,"C7"]
[100020290,"KIT TUBULURES COURTES POUR MONTAGE DKS 6 MSB SUR BSL 150N","ER286",109,null,null,"/","/","/",3661238576384,3,280,280,250,"C7"]
[100019427,"VASE D'EXPANSION  18 L","EG117",97,null,null,"/","/","/",3661238563025,4.2,400,285,290,"C7"]
[7630422,"REGULATION OETROSOL-PLUS","ER709",260,0.12,95010,"/","/","/",3661238631045,0.69,227,194,85,"C7"]
[7630421,"REGULATION OETROSOL-AEL","ER708",291,0.12,95010,"/","/","/",3661238631038,0.88,290,205,92,"C7"]
[100019425,"MITIGEUR THERMOSTATIQUE","EC60",140,null,null,"/","/","/",3661238563018,0.65,125,105,90,"C7"]
[100019322,"KIT DE RACCORDEMENT EAU FROIDE","ER404",112,null,null,"/","/","/",3661238553408,2.2999999999999998,870,260,150,"C7"]
[]
["OECOSUN CONFORT"]
[7651949,"OECOSUN CONFORT 400 (QUADRO)",null,{"$f":"D858+D860+D861+D862+D863+D864+D865++D866+D867","v":4247},null,null,null,null,null,3661238659926,null,null,null,null,"C7"]
[7651946,"OECOSUN CONFORT 700 (QUADRO)",null,{"$f":"D859+D860+D861+D862+D863+D864+D865+D866+D867","v":4808},null,null,null,null,null,3661238659919,null,null,null,null,"C7"]
[]
["COMPOSANTS"]
[7650888,"CUVE QUADRO 400 ET HABILLAGE E","EC67",2910,null,null,null,null,null,3661238658899,125,1200,1200,2170,"C7"]
[7650884,"CUVE QUADRO 700 ET HABILLAGE E","EC66",3471,null,null,null,null,null,3661238658868,229,1200,1200,2150,"C7"]
[7630417,"STATION SOLAIRE DKSL 6-8 MSB E","ER710",562,0.83,14090,null,null,null,3661238631021,8,935,225,445,"C7"]
[100019423,"COLIS EQUIPEMENT SOLAIRE ER414","ER414",134,null,null,"/","/","/",3661238562912,5,470,310,290,"C7"]
[7630422,"SOLAR CONTROLER SOL PLUS ER709","ER709",260,0.12,95010,null,null,null,3661238631045,0.7,227,164,85,"C7"]
[7630424,"KIT CABLE DE LIAISON ModBUS (3m) OETROSOL-PLUS","ER713",32,0.02,95020,"/","/","/",3661238631069,0.11,null,null,null,"C7"]
[100019427,"VASE D'EXPANSION  18 L","EG117",97,null,null,"/","/","/",3661238563025,4.2,400,285,290,"C7"]
[100019322,"KIT DE RACCORDEMENT EAU FROIDE","ER404",112,null,null,"/","/","/",3661238553408,2.2999999999999998,870,260,150,"C7"]
[100019425,"MITIGEUR THERMOSTATIQUE","EC60",140,null,null,"/","/","/",3661238563018,0.65,125,105,90,"C7"]
[200023618,"DOCUMENTATION TECHNIQUE GEN ER",null,null,null,null,null,null,null,null,null,null,null,null,"C7"]
[]
["OPTIONS"]
[100020164,"COLLECTEUR 2/3 CIRCUITS ","EA140",348,null,null,"/","/","/",3661238575011,6.6,660,180,200,"C0"]
[100020165,"CONSOLE MUR COLLECTEUR ","EA141",44,null,null,"/","/","/",3661238575028,1.2,220,125,70,"C0"]
[100020166,"CONSOLE MUR 1 MODULE ","EA142",116,null,null,"/","/","/",3661238575035,1.6,220,125,70,"C0"]
[100020167,"CIRCUIT DIRECT P.ELEC CLASSE A  ","EA143",644,0.83,14050,"/","/","/",3661238575042,5.0999999999999996,460,270,235,"C0"]
[100020168,"CIRCUIT V3V P.ELEC","EA144",916,0.83,14050,"/","/","/",3661238575059,6,460,270,235,"C0"]
[7616233,"MODULE HYDRAULIQUE COMPACT POUR 2 CIRCUITS","MT12",1686,0.83,14050,"/","/","/",3661238600614,12.2,530,415,215,"C3"]
[]
["OECOSUN BASIC"]
[7651950,"OECUSUN BASIC 400 (QUADRO)",null,{"$f":"D882+D884+D885+D886+D887+D888+D889+D890+D891","v":4402},null,null,null,null,null,3661238659933,null,null,null,null,"C7"]
[7651951,"OECUSUN BASIC 700 (QUADRO)",null,{"$f":"D883+D884+D885+D886+D887+D888+D889+D890+D891","v":4963},null,null,null,null,null,3661238659940,null,null,null,null,"C7"]
[]
["COMPOSANTS"]
[7650888,"CUVE QUADRO 400 ET HABILLAGE E","EC67",2910,null,null,null,null,null,3661238658899,125,1200,1200,2170,"C7"]
[7650884,"CUVE QUADRO 700 ET HABILLAGE E","EC66",3471,null,null,null,null,null,3661238658868,229,1200,1200,2150,"C7"]
[7630417,"STATION SOLAIRE DKSL 6-8 MSB E","ER710",562,0.83,14090,null,null,null,3661238631021,8,935,225,445,"C7"]
[100019423,"COLIS EQUIPEMENT SOLAIRE ER414","ER414",134,null,null,"/","/","/",3661238562912,5,470,310,290,"C7"]
[7630422,"SOLAR CONTROLER SOL PLUS ER709","ER709",260,0.12,95010,null,null,null,3661238631045,0.7,227,164,85,"C7"]
[100019427,"VASE D'EXPANSION SOLAIRE 18L E","EG117",97,null,null,"/","/","/",3661238563025,4.2,400,285,290,"C7"]
[89804803,"VANNE 3 VOIES 3/4\" POUR 2 CIRCUITS","EC164",237,null,null,"/","/","/",3661238046528,1.05,205,125,90,"C7"]
[100003690,"SONDE A APPLIQUE PT1000","EC171",62,0.02,95020,"/","/","/",3661238005303,0.1,180,140,30,"C0"]
[100019425,"MITIGEUR T-STATIQ MMF1\" EC60","EC60",140,null,null,"/","/","/",3661238563018,0.65,125,105,90,"C7"]
[200023618,"DOCUMENTATION TECHNIQUE GEN ER",null,null,null,null,null,null,null,null,null,null,null,null,"C7"]
[]
["OPTIONS"]
[100020167,"CIRCUIT DIRECT P.ELEC CLASSE A  ","EA143",644,0.83,14050,"/","/","/",3661238575042,5.0999999999999996,460,270,235,"C0"]
[100019322,"KIT DE RACCORDEMENT EAU FROIDE","ER404",112,null,null,"/","/","/",3661238553408,2.2999999999999998,870,260,150,"C7"]
[89807767,"MITIGEUR THERMOSTATIQUE 1\"","EG78",136,null,null,"/","/","/",3661238045149,0.65,125,105,90,"C7"]
[]
["OECOSUN B0IS"]
[7651952,"OECOSUN BOIS 700 (QUADRO)",null,{"$f":"SUM(D902:D909)","v":4920},null,null,null,null,null,3661238659957,null,null,null,null,"C7"]
[]
["COMPOSANTS"]
[7650884,"CUVE QUADRO 700 ET HABILLAGE E","EC66",3471,null,null,null,null,null,3661238658868,229,1200,1200,2150,"C7"]
[7630417,"STATION SOLAIRE DKSL 6-8 MSB E","ER710",562,0.83,14090,null,null,null,3661238631021,8,935,225,445,"C7"]
[100019423,"COLIS EQUIPEMENT SOLAIRE ER414","ER414",134,null,null,"/","/","/",3661238562912,5,470,310,290,"C7"]
[100019427,"VASE D'EXPANSION SOLAIRE 18L E","EG117",97,null,null,"/","/","/",3661238563025,4.2,400,285,290,"C7"]
[7630421,"REGULATION OETROSOL-AEL","ER708",291,0.12,95010,"/","/","/",3661238631038,0.88,290,205,92,"C7"]
[100019165,"R. ELECTRIQUE 3 kW AVEC SONDE","ER394",225,null,null,"/","/","/",3661238551312,1.3,770,105,105,"C7"]
[100019425,"MITIGEUR T-STATIQ MMF1\" EC60","EC60",140,null,null,"/","/","/",3661238563018,0.65,125,105,90,"C7"]
[200023566,"DOCUMENTATION TECHNIQUE GEN ER",null,null,null,null,null,null,null,null,null,null,null,null,"C7"]
[]
["OPTIONS"]
[100020164,"COLLECTEUR 2/3 CIRCUITS ","EA140",348,null,null,"/","/","/",3661238575011,6.6,660,180,200,"C0"]
[100020165,"CONSOLE MUR COLLECTEUR ","EA141",44,null,null,"/","/","/",3661238575028,1.2,220,125,70,"C0"]
[100020166,"CONSOLE MUR 1 MODULE ","EA142",116,null,null,"/","/","/",3661238575035,1.6,220,125,70,"C0"]
[100020167,"CIRCUIT DIRECT P.ELEC CLASSE A  ","EA143",644,0.83,14050,"/","/","/",3661238575042,5.0999999999999996,460,270,235,"C0"]
[100020168,"CIRCUIT V3V P.ELEC","EA144",916,0.83,14050,"/","/","/",3661238575059,6,460,270,235,"C0"]
[7616233,"MODULE HYDRAULIQUE COMPACT POUR 2 CIRCUITS","MT12",1686,0.83,14050,"/","/","/",3661238600614,12.2,530,415,215,"C3"]
[100018255,"OE-TRONIC 4 MR","AD282",1053,0.12,95010,"/","/","/",3661238514454,2,360,280,140,"C0"]
[88017010,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (SANS FILS)","AD192",286,0.12,95010,"/","/","/",3661238102439,0.42499999999999999,180,150,90,"C0"]
[]
["PRÉPARATEURS SOLAIRES DOUBLE-SERPENTIN NON ÉQUIPÉS OBS"]
[100019529,"PREPARATEUR SOLAIRE OBS 200 N","ER424",902,null,null,"/","C stockage \nECS","/",3661238564428,110,900,800,1600,"C7"]
[100019522,"PREPARATEUR SOLAIRE OBS 300 N","ER425",913,null,null,"/","C stockage \nECS","/",3661238564459,121,900,800,1960,"C7"]
[100019526,"PREPARATEUR SOLAIRE OBS 400 N","ER426",1957,null,null,"/","C stockage \nECS","/",3661238564329,155,900,850,1795,"C7"]
[100019068,"PREPARATEUR SOLAIRE OBS 500 N","ER341",2284,null,null,"/","C stockage \nECS","/",3661238548527,177,890,850,1950,"C7"]
[]
["PRÉPARATEURS ELECTRO-SOLAIRES BASICSUN ÉQUIPÉS OBES"]
[100019143,"BALLON OBES 200","ER375",1604,5,14070,"/","C","XL",3661238551268,110,1200,850,1640,"C7"]
[100019144,"BALLON OBES 300","ER376",1713,5,14070,"/","C","XL",3661238551275,126,1200,850,2020,"C7"]
[100019145,"BALLON OBES 400","ER377",2692,5,14070,"/","C","XL",3661238551282,166,1200,850,1794,"C7"]
[]
["PRÉPARATEURS SOLAIRES  BASICSUN DOUBLE-SERPENTIN ÉQUIPÉS OBS"]
[100019137,"BALLON OBS 200","ER362",1604,null,null,"/","C stockage \nECS","/",3661238551206,119,1200,850,1650,"C7"]
[100019138,"BALLON OBS 300","ER363",1713,null,null,"/","C stockage \nECS","/",3661238551213,136,1200,850,2020,"C7"]
[100019139,"BALLON OBS 400","ER364",2692,null,null,"/","C stockage \nECS","/",3661238551220,193,1200,850,1794,"C7"]
[]
["OPTIONS BALLONS SOLAIRES OBS / OBES / OBS … N"]
[null,"POUR PREPARATEURS SOLAIRES"]
[100019427,"VASE D'EXPANSION  18 L","EG117",97,null,null,"/","/","/",3661238563025,4.22,400,285,290,"C7"]
[100019428,"VASE D'EXPANSION  25 L","EG118",112,null,null,"/","/","/",3661238563032,4.5999999999999996,435,315,315,"C7"]
[89807794,"FLUIDE CALOPORTEUR \"L\" 20L. MELANGE 40/60 ","EG101",78,null,null,"/","/","/",3661238045019,21.72,240,290,370,"C7"]
[null,"POUR PREPARATEURS SOLAIRES BASICSUN OBS … N"]
[100019163,"R. ELECTRIQUE 1,5 kW AVEC SONDE","ER392",225,null,null,"/","/","/",3661238551299,1.2,660,105,105,"C7"]
[100019165,"R. ELECTRIQUE 3 kW AVEC SONDE","ER394",225,null,null,"/","/","/",3661238551312,1.3,770,105,105,"C7"]
[100019166,"R. ELECTRIQUE 1,5 kW THERMOSTATIQUE","ER395",280,null,null,"/","/","/",3661238549319,1.3,665,150,125,"C7"]
[100019167,"R. ELECTRIQUE 2,3 kW THERMOSTATIQUE","ER396",280,null,null,"/","/","/",3661238549326,1.8,650,140,115,"C7"]
[100019168,"R. ELECTRIQUE 3 kW avec thermostat","ER397",280,null,null,"/","/","/",3661238549333,1.45,770,105,105,"C7"]
[100019322,"KIT DE RACCORDEMENT EAU FROIDE","ER404",112,null,null,"/","/","/",3661238553408,2.2999999999999998,870,260,150,"C7"]
[7630415,"STATION SOLAIRE DKSC 6-8 MSB","ER711",479,0.83,14090,"/","/","/",3661238631014,7.3,620,240,450,"C7"]
[100019423,"COLIS EQUIPEMENT SOLAIRE ER414","ER414",134,null,null,"/","/","/",3661238562912,5,470,310,290,"C7"]
[7630421,"REGULATION OETROSOL-AEL","ER708",291,0.12,95010,"/","/","/",3661238631038,0.88,290,205,92,"C7"]
[100019427,"VASE D'EXPANSION 18 L","EG117",97,null,null,"/","/","/",3661238563025,4.22,400,285,290,"C7"]
[100019425,"MITIGEUR THERMOSTATIQUE MMF1\" ","EC60",140,null,null,"/","/","/",3661238563018,0.65,125,105,90,"C7"]
[]
["OPTIONS BALLONS SOLAIRES"]
[null,"POUR PREPARATEURS SOLAIRES BASICSUN"]
[100010652,"KIT OECOPROTEC PROTECTION ACI SUR OETRONIC","EC431",123,null,null,"/","/","/",3661238364745,0.49,255,170,120,"C7"]
[100007832,"REGULATION POMPE DE CHARGE SLA 2","EC320",208,0.12,95010,"/","/","/",3661238101494,0.66,225,195,85,"C0"]
[89807767,"MITIGEUR THERMOSTATIQUE 1\"","EG78",136,null,null,"/","/","/",3661238045149,0.65,125,105,90,"C7"]
[]
[null,"POUR PREPARATEURS SOLAIRES BASICSUN OBESL 200-300"]
[89807777,"RESISTANCE ELECTRIQUE 3,0 kW MULTI STEATITE DN 82  ","EG88",252,null,null,"/","/","/",3661238045071,4,800,195,200,"C7"]
[89757753,"ANODE A COURANT IMPOSE","AJ39",391,0.02,95020,"/","/","/",3661238046832,0.4,425,100,55,"C0"]
[]
[null,"POUR PREPARATEURS SOLAIRES BASICSUN OBESL 400-500"]
[100007799,"RESISTANCE ELECTRIQUE 4,5 kW MULTI BLINDEE DN 117  ","EC413",671,null,null,"/","/","/",3661238156852,3.54,660,215,215,"C0"]
[89608920,"ANODE ACI CORREX UP BALLON > 300 LITRES","AM7",532,0.02,95020,"/","/","/",3661238047440,0.44,425,100,55,"C0"]
[]
["OPTIONS BASICSUN"]
["ACCESSOIRES HYDRAULIQUES ET REGULATIONS DES SYSTEMES SOLAIRES BASICSUN"]
[7630422,"REGULATION OETROSOL-PLUS","ER709",260,0.12,95010,"/","/","/",3661238631045,0.69,227,194,85,"C7"]
[100007832,"RÉGULATION POMPE DE CHARGE SLA 2","EC320",208,0.12,95010,"/","/","/",3661238101494,0.66,225,195,85,"C0"]
[89804803,"VANNE 3 VOIES 3/4\" POUR 2 CIRCUITS","EC164",237,null,null,"/","/","/",3661238046528,1.05,205,125,90,"C7"]
[89804816,"BOITIER PARA FOUDRE POUR SONDE PANNEAUX SOLAIRES","EC176",40,null,null,"/","/","/",3661238046450,0.11,220,165,40,"C7"]
[100003690,"SONDE A APPLIQUE PT1000","EC171",62,0.02,95020,"/","/","/",3661238005303,0.1,180,140,30,"C0"]
[100004651,"SONDE D'IMMERSION FK PT1000 2,5 m","EC173",62,0.02,95020,"/","/","/",3661238002418,0.15,220,150,25,"C0"]
[100008011,"SONDE CAPTEUR  PT1000 ","EC155",58,0.02,95020,"/","/","/",3661238101197,0.1,180,120,20,"C7"]
[100004652,"DEBIMETRE VOLUMIQUE V40 ","EC174",415,null,null,"/","/","/",3661238002401,1.5,240,160,110,"C7"]
[100014590,"RÉGULATION COMPTEUR D'ENERGIE WMZ 13530350 ","ER131",295,0.12,95010,"/","/","/",3661238376014,0.6,230,195,80,"C7"]
[]
[]
["INSTALLATIONS SOLAIRES CESI COMPLETES POWERSUN SUR TOITURE"]
[100008119,"CESI POWERSUN OERTLISOL OB3S 250-4 st SUR TOITURE ","EC566",5948,5,14070,"Système avec chaudière\n GMR 1000 Condens","A","XL",null,333,1200,1200,2250,"C7"]
[]
["INSTALLATIONS SOLAIRES CESI COMPLETES POWERSUN EN INTEGRATION DE TOITURE"]
[100008131,"CESI POWERSUN OERTLISOL OB3S 250-4 it INTEGRATION TOITURE ","EC568",6846,5,14070,"Système avec chaudière\n GMR 1000 Condens","A","XL",null,393.5,1200,1200,2250,"C7"]
[]
[]
[100019332,"CAPTEUR SOLAIRE D230","ER405",780,null,null,"/","/","/",3661238554818,43.8,2265,1230,105,"C7"]
[]
["ACCESSOIRES DE RACCORDEMENT HYDRAULIQUE"]
[100019333,"KIT RACCORDEMENT HYDRAULIQUE CHAMPS DE CAPTEURS D230","ER406",134,null,null,"/","/","/",3661238554825,0.6,300,100,40,"C7"]
[100019334,"KIT DE LIAISON HYDRAULIQUE ENTRE 2 CAPTEURS D230","ER407",40,null,null,"/","/","/",3661238554832,0.2,115,60,70,"C7"]
[]
["DISPOSITIF DE MONTAGE"]
[7503818,"KIT INTEGRATION BASE V 22°  1 CAPTEUR D 230 TUILES MECANIQUES","ER628",531,null,null,"/","/","/",3661238600270,23,150,800,2000,"C7"]
[7503820,"KIT INTEGRATION BASE V 22°  2 CAPTEURS D 230 TUILES MECANIQUES","ER629",742,null,null,"/","/","/",3661238600287,38,150,800,2000,"C7"]
[7503819,"KIT EXTENSION INTEGRATION V 22° 1 CAPTEUR D 230 TUILES MECANIQUES","ER630",319,null,null,"/","/","/",3661238600294,15,150,800,2000,"C7"]
[7212871,"KIT INTEGRATION BASE V 17°  1 CAPTEUR D 230 TUILES CANAL","ER631",689,null,null,"/","/","/",3661238600300,27,150,800,2000,"C7"]
[7212878,"KIT INTEGRATION BASE V 17°  2 CAPTEURS D 230 TUILES CANAL","ER632",1113,null,null,"/","/","/",3661238600416,44,150,800,2000,"C7"]
[7212874,"KIT EXTENSION INTEGRATION V 17°  1 CAPTEUR D 230 TUILES CANAL","ER633",425,null,null,"/","/","/",3661238600423,17,150,800,2000,"C7"]
[100016513,"KIT PROFILES A CLIPER POUR 1 C250 V","ER260",139,null,null,"/","/","/",3661238492394,4.5,1260,155,100,"C7"]
[100016514,"KIT PROFILES A CLIPER POUR 1 C250 H","ER261",173,null,null,"/","/","/",3661238492400,7,2280,155,100,"C7"]
[7217048,"KIT PROFILES 45 2,5M2 HZ ","ER662",98,null,null,"/","/","/",3661238492288,4.5,2280,155,100,"C7"]
[7217044,"KIT PROFILES 45 MTGE VT ","ER664",80,null,null,"/","/","/",3661238492295,2.5,1260,155,100,"C7"]
[]
["ACCESSOIRES DE MONTAGE POUR ARDOISES ET TUILES PLATES"]
[7503269,"KIT NOQUETS POUR TUILES PLATES ET ARDOISES","ER558",138,null,null,"/","/","/",3661238586611,7,150,200,360,"C7"]
[]
["FERRURES D'ANCRAGE POUR MONTAGE SUR TOITURE"]
[89807311,"4 CROCHETS ALU UNIVERSEL POUR TUILES MÉCANIQUES","EG311",98,null,null,"/","/","/",3661238045903,2.2999999999999998,365,120,140,"C7"]
[89807312,"6 CROCHETS ALU UNIVERSEL POUR TUILES MÉCANIQUES","EG312",141,null,null,"/","/","/",3661238045897,3.5,365,115,140,"C7"]
[89807313,"4 CROCHETS INOX SUR CHEVRON À TUILES MÉCANIQUES","EG313",98,null,null,"/","/","/",3661238045880,3.4,320,220,135,"C7"]
[89807314,"6 CROCHETS INOX SUR CHEVRON À TUILES MÉCANIQUES","EG314",141,null,null,"/","/","/",3661238045873,4.9000000000000004,325,225,135,"C7"]
[89807315,"4 CROCHETS INOX POUR TOITURE À TUILES PLATES","EG315",98,null,null,"/","/","/",3661238045866,2.4,300,135,95,"C7"]
[89807316,"6 CROCHETS INOX POUR TOITURE À TUILES PLATES","EG316",141,null,null,"/","/","/",3661238045859,3.5,310,140,95,"C7"]
[100015314,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES CANAL","ER136",97,null,null,"/","/","/",3661238415539,4,325,260,120,"C7"]
[100015315,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES CANAL","ER137",141,null,null,"/","/","/",3661238415546,6.5,410,305,115,"C7"]
[89807317,"4 CROCHETS INOX POUR TOITURE À TUILES CANALS / ÉTERNIT","EG317",98,null,null,"/","/","/",3661238045842,3.6,260,215,75,"C7"]
[89807318,"6 CROCHETS INOX POUR TOITURE À TUILES CANALS / ÉTERNIT","EG318",141,null,null,"/","/","/",3661238045835,5.3,260,220,75,"C7"]
[89807319,"4 CROCHETS INOX POUR TOITURE ARDOISES / BARDAGE","EG319",98,null,null,"/","/","/",3661238045828,2.2000000000000002,280,120,80,"C7"]
[89807320,"6 CROCHETS INOX POUR TOITURE ARDOISES / BARDAGE","EG320",141,null,null,"/","/","/",3661238045811,3.3,305,140,95,"C7"]
[89807782,"KIT TIRE-FONDS POUR MONTAGE 2 CAPTEURS/TUILES CANAL","EG94",247,null,null,"/","/","/",3661238045057,2.8,405,140,80,"C7"]
[89807783,"KIT TIRE-FONDS POUR MONTAGE 3 CAPTEURS/TUILES CANAL","EG95",310,null,null,"/","/","/",3661238045040,3.6,405,140,80,"C7"]
[100016517,"4 FERRURES D'ANCRAGE ALU  A CRANS MTGE SUR CHEVRON","ER264",131,null,null,"/","/","/",3661238492431,3,2120,110,95,"C7"]
[100016518,"2 FERRURES D'ANCRAGE ALU  A CRANS MTGE SUR CHEVRON","ER265",79,null,null,"/","/","/",3661238492448,1.6,2120,110,95,"C7"]
[]
["SUPPORTS INCLINABLES POUR MONTAGE EN TERRASSE (OU AU SOL)"]
[100016509,"2 SUPPORTS HL AVEC CROIX  MONTAGE VERTICAL 1 C250 SANS PROFILES","ER250",312,null,null,"/","/","/",3661238492356,21.5,2280,155,100,"C7"]
[100016510,"1 SUPPORT HL VERTICAL POUR EXTENSION 1 C250 ","ER251",161,null,null,"/","/","/",3661238492363,11.5,2280,155,100,"C7"]
[100016511,"2 SUPPORTS HL AVEC CROIX  MONTAGE HORIZONTAL 1 C250 SANS PROFILES","ER252",255,null,null,"/","/","/",3661238492370,13.5,2280,155,100,"C7"]
[100016512,"1 SUPPORT HL HORIZONTAL POUR EXTENSION 1 C250 ","ER253",145,null,null,"/","/","/",3661238492387,8,2280,155,100,"C7"]
[7217038,"2 SUPPORTS SL MONTAGE VERTICAL 1 CAPTEUR","ER658",196,null,null,"/","/","/",3661238630710,9.5,2267,145,80,"C7"]
[7217039,"1 SUPPORT SL MTGE VERTICAL POUR EXTENSION 1 CAPTEUR","ER659",91,null,null,"/","/","/",3661238630277,4.5,1945,110,95,"C7"]
[7217041,"2 SUPPORTS SL HL MONTAGE HORIZONTAL 1 CAPTEUR","ER656",156,null,null,"/","/","/",3661238630253,5.5,1250,145,80,"C7"]
[7217042,"1 SUPPORT SL HL HORIZONTAL POUR EXTENSION 1 CAPTEUR","ER657",79,null,null,"/","/","/",3661238630260,3,1250,145,80,"C7"]
[]
["OPTION MONTAGE INTEGRE EN TOITURE AVEC TUILES PLATES / ARDOISES"]
[100007882,"KIT NOQUETS POUR TUILES PLATES","EG425",234,null,null,"/","/","/",3661238101418,3.92,315,230,130,"C7"]
[]
[]
["PACKS TOIT"]
[100019693,"PACK TOIT 1 D230- 2m² CROCHET UNIVERSEL TUILES MECANIQUES","ER430",1197,null,null,"/","/","/",3661238568129,134,1270,770,2200,"C7"]
[100019694,"PACK TOIT 1 D230- 2m² SUR TOITURE ARDOISES","ER431",1197,null,null,"/","/","/",3661238568112,134,1270,770,2200,"C7"]
[100019695,"PACK TOIT 2 D230- 5m² CROCHET UNIVERSEL TUILES MECANIQUES","ER432",1977,null,null,"/","/","/",3661238568136,121,1270,770,2200,"C7"]
[100019696,"PACK TOIT 2 D230- 5m² SUR TOITURE ARDOISES","ER433",1977,null,null,"/","/","/",3661238568143,134,1270,770,2200,"C7"]
[100019697,"PACK TOIT 2 D230- 5m² SUR CHEVRON TUILES MECANIQUES","ER434",1977,null,null,"/","/","/",3661238568150,134,1270,770,2200,"C7"]
[100019698,"PACK TOIT 3 D230- 7m² CROCHET UNIVERSEL TUILES MECANIQUES","ER435",3101,null,null,"/","/","/",3661238568167,134,1270,770,2200,"C7"]
[100019699,"PACK TOIT 3 D230- 7m² SUR TOITURE ARDOISES","ER436",3101,null,null,"/","/","/",3661238568174,134,1270,770,2200,"C7"]
[100019700,"PACK TOIT 3 D230- 7m² SUR CHEVRON TUILES MECANIQUES","ER437",3101,null,null,"/","/","/",3661238568181,134,1270,770,2200,"C7"]
[100019701,"PACK TOIT 4 D230- 9m² CROCHET UNIVERSEL TUILES MECANIQUES","ER438",4110,null,null,"/","/","/",3661238568198,134,1270,770,2200,"C7"]
[100019702,"PACK TOIT 4 D230- 9m² SUR TOITURE ARDOISES","ER439",4110,null,null,"/","/","/",3661238568204,134,1270,770,2200,"C7"]
[100019703,"PACK TOIT 4 D230- 9m² SUR CHEVRON TUILES MECANIQUES","ER440",4110,null,null,"/","/","/",3661238568211,134,1270,770,2200,"C7"]
[]
["PACKS TOIT IT"]
[7615855,"PACK TOIT 1 D 230- 2m² INTEGRE V 22° TUILE MECANIQUE","ER620",1405,null,null,"/","/","/",3661238600317,103,1330,770,2200,"C7"]
[7615859,"PACK TOIT 2 D 230- 5m² INTEGRE V 22° TUILE MECANIQUE","ER621",2393,null,null,"/","/","/",3661238600324,162,1330,770,2200,"C7"]
[7615861,"PACK TOIT 3 D 230- 7m² INTEGRE V 22° TUILE MECANIQUE","ER622",3642,null,null,"/","/","/",3661238600331,221,1330,770,2200,"C7"]
[7615863,"PACK TOIT 4 D 230- 9m² INTEGRE V 22° TUILE MECANIQUE","ER623",4661,null,null,"/","/","/",3661238600348,305,1330,770,2200,"C7"]
[7615864,"PACK TOIT 1 D 230- 2m² INTEGRE V 17° TUILE CANAL","ER624",1488,null,null,"/","/","/",3661238600355,107,1330,770,2200,"C7"]
[7615866,"PACK TOIT 2 D 230- 5m² INTEGRE V 17° TUILE CANAL","ER625",2549,null,null,"/","/","/",3661238600362,168,1330,770,2200,"C7"]
[7615868,"PACK TOIT 3 D 230- 7m² INTEGRE V 17° TUILE CANAL","ER626",3797,null,null,"/","/","/",3661238600379,229,1330,770,2200,"C7"]
[7615869,"PACK TOIT 4 D 230- 9m² INTEGRE V 17° TUILE CANAL","ER627",4733,null,null,"/","/","/",3661238600386,315,1330,770,2200,"C7"]
[]
[]
[100008206,"PREPARATEUR SOLAIRE POWERSUN DT 350/3 350L","EC359",3385,5,14070,"/","C","XL",3661238371262,215,1075,820,2030,"C7"]
[100008208,"PREPARATEUR SOLAIRE POWERSUN DT 250/3 250L","EC360",3047,5,14070,"/","C","XL",3661238371279,180,1080,785,1830,"C7"]
[]
[]
[100008019,"PREPARATEUR ECS INSTANTANEE FWS 750","EC546",4808,null,null,"Pas concerné par l'étiquettage",null,null,3661238101111,252,1200,1200,2330,"C7"]
[100008150,"PREPARATEUR SOLAIRE OECOSUN DU 750-20 CL",null,{"$f":"SUM(D1074,D1075)","v":7539},null,null,"Pas concerné par l'étiquettage",null,null,null,null,null,null,null,"C0"]
[]
["COMPOSANTS"]
[100007994,"CUVE (55 kW) & HABILLAGE DU 750-20 CL","EC545",4159,null,null,"/","/","/",3661238101234,242,1200,1200,2250,"C7"]
[100008115,"COLIS COMPOSANTS OECOSUN DU 750-20 ","EC562",3380,null,null,"/","/","/",3661238372436,56,1200,1400,2295,"C7"]
[]
["OPTIONS POUR PREPARATEURS SOLAIRES  "]
[100007832,"REGULATION POMPE DE CHARGE SLA 2","EC320",208,0.12,95010,"/","/","/",3661238101494,0.66,225,195,85,"C0"]
[89807767,"MITIGEUR THERMOSTATIQUE 1\"","EG78",136,null,null,"/","/","/",3661238045149,0.65,125,105,90,"C7"]
[]
["POUR PREPARATEURS SOLAIRES < 400 L"]
[89757752,"ANODE ACI CORREX UP BALLON < 300 L","AJ38",306,0.02,95020,"/","/","/",3661238046849,0.35,250,95,50,"C0"]
[100007797,"RESISTANCE ELECTRIQUE 2,2 kW MULTI BLINDEE DN 82  ","EC410",483,null,null,"/","/","/",3661238116634,3.2,660,215,215,"C0"]
[100007830,"RESISTANCE ELECTRIQUE 2,4 kW MULTI STEATITE DN 82  ","EC411",344,null,null,"/","/","/",3661238116641,3.8,625,210,220,"C0"]
[89807777,"RESISTANCE ELECTRIQUE 3,0 kW MULTI STEATITE DN 82  ","EG88",252,null,null,"/","/","/",3661238045071,4,800,195,200,"C7"]
[100007798,"RESISTANCE ELECTRIQUE 3,3 kW MULTI BLNDEE DN 82  ","EC412",553,null,null,"/","/","/",3661238116658,3.5,660,215,215,"C0"]
[]
["POUR PREPARATEURS SOLAIRES > 400 L"]
[100007799,"RESISTANCE ELECTRIQUE 4,5 kW MULTI BLINDEE DN 117  ","EC413",671,null,null,"/","/","/",3661238156852,3.54,660,215,215,"C0"]
[89608920,"ANODE ACI CORREX UP BALLON > 300 LITRES","AM7",532,0.02,95020,"/","/","/",3661238047440,0.44,425,100,55,"C0"]
[]
[]
[100006534,"PREPARATEUR SOLAIRE OECOSUN DU 500-10",null,{"$f":"SUM(D1096:D1097)","v":6043},null,null,"/","D stockage \nECS",null,null,null,null,null,null,"C7"]
[]
["COMPOSANTS"]
[100005800,"CUVE DE PREPARATEUR SOLAIRE MOUSSE DU/C500","EC290",3769,null,null,"/","/","/",3661238091924,244,950,820,1970,"C7"]
[100008117,"COLIS COMPOSANTS OECOSUN DU 500 ","EC564",2274,null,null,"/","/","/",3661238372450,91,1200,1400,2295,"C7"]
[]
[]
[100006535,"OECOPAC DUP 500-10 ",null,{"$f":"SUM(D1103:D1104)","v":8433},null,null,"/","D stockage \nECS",null,null,null,null,null,null,"C7"]
[]
["COMPOSANTS"]
[100005800,"CUVE DE PREPARATEUR SOLAIRE MOUSSE DU/C500","EC290",3769,null,null,"/","/","/",3661238091924,244,950,820,1970,"C7"]
[100008118,"COLIS COMPOSANTS OECOPAC DUP 500 ","EC565",4664,null,null,"/","/","/",3661238372467,98,1200,800,2300,"C7"]
[]
[null,"OPTIONS OECOSUN/DENS 500"]
[89807212,"MODULE HYDRAULIQUE POUR 1 CIRCUIT DIRECT","EC92",454,null,null,"/","/","/",3661238046276,5.15,310,210,180,"C7"]
[89807213,"MODULE HYDRAULIQUE POUR 1 CIRCUIT DIRECT AVEC VANNE MOTORISEE","EC93",716,null,null,"/","/","/",3661238046269,6.24,310,210,180,"C7"]
[89807214,"MODULE HYDRAULIQUE POUR 1 CIRCUIT A TEMPERATURE FIXE","EC94",637,null,null,"/","/","/",3661238046252,5.93,310,210,180,"C7"]
[100013447,"MODUL.HYDRAUL.CIRCUIT DIR.CLASSE A ","ER73",634,0.83,14050,"/","/","/",3661238363908,4.25,310,210,180,"C7"]
[100013448,"MODUL.HYDRAUL.V3V CLASSE A","ER74",894,0.83,14050,"/","/","/",3661238363915,4.25,310,210,180,"C7"]
[100013449,"MODUL.HYD.V3V THERMOSTAT CLASSE A","ER75",817,0.83,14050,"/","/","/",3661238363922,4.25,310,210,180,"C7"]
[100005978,"KIT TUBES DE RACCORDEMENT SORTIES MODULES HYDRAULIQUES","EC296",223,null,null,"/","/","/",3661238091849,3,800,165,175,"C7"]
[100006500,"KIT DU APPOINT ELECTRIQUE 2,4 kW/mono ","EC310",473,null,null,"/","/","/",3661238091771,2.9,660,215,215,"C7"]
[100006501,"KIT DU APPOINT ELECTRIQUE 6 kW/Tri ","EC311",740,null,null,"/","/","/",3661238091764,3.1,660,215,215,"C7"]
[100006531,"MODULE SEPARATEUR DE CIRCUITS PAC ROE/+ < 15 kW","EC300",1104,null,null,"/","/","/",3661238161764,19.899999999999999,570,385,250,"C7"]
[]
[]
[100008112,"PREPARATEUR SOLAIRE OECOSUN DU 750-10 COMPLET ",null,{"$f":"SUM(D1122:D1123)","v":6887},null,null,"Arrêt production",null,null,null,null,null,null,null,"C7"]
[]
["COMPOSANTS"]
[100007977,"CUVE (25 kW) & HABILLAGE DE PREPARATEUR SOLAIRE DU/C 750","EC550",3833,null,null,"/","/","/",3661238101302,227,1200,1200,2250,"C7"]
[100008114,"COLIS COMPOSANTS OECOSUN DU 750-10 ","EC559",3054,null,null,"/","/","/",3661238372429,85,1200,1200,1670,"C7"]
[]
["OPTIONS POUR OECOSUN ET OECODENS"]
[89807212,"MODULE HYDRAULIQUE POUR 1 CIRCUIT DIRECT","EC92",454,null,null,"/","/","/",3661238046276,5.15,310,210,180,"C7"]
[89807213,"MODULE HYDRAULIQUE POUR 1 CIRCUIT DIRECT AVEC VANNE MOTORISEE","EC93",716,null,null,"/","/","/",3661238046269,6.24,310,210,180,"C7"]
[89807214,"MODULE HYDRAULIQUE POUR 1 CIRCUIT DIRECT AVEC VANNE THERMOSTATIQUE","EC94",637,null,null,"/","/","/",3661238046252,5.93,310,210,180,"C7"]
[100013447,"MODUL.HYDRAUL.CIRCUIT DIR.CLASSE A ","ER73",634,0.83,14050,"/","/","/",3661238363908,4.25,310,210,180,"C7"]
[100013448,"MODUL.HYDRAUL.V3V CLASSE A","ER74",894,0.83,14050,"/","/","/",3661238363915,4.25,310,210,180,"C7"]
[100013449,"MODUL.HYD.V3V THERMOSTAT CLASSE A","ER75",817,0.83,14050,"/","/","/",3661238363922,4.25,310,210,180,"C7"]
[89807767,"MITIGEUR THERMOSTATIQUE 1\"","EG78",136,null,null,"/","/","/",3661238045149,0.65,125,105,90,"C7"]
[89804901,"FAISEAU DE RACCORDEMENT OETROSOL C/OECOSUN/OECODENS","EC179",119,0.02,95020,"/","/","/",3661238046443,0.46,265,125,45,"C7"]
[]
["OPTIONS EXTENSION VOLUME TAMPON "]
[100005010,"BALLON TAMPON PSB 750","EC129",1645,null,null,"/","/","/",3661238001862,163,1200,1200,2100,"C7"]
[100004650,"REGULATION \"MCDB\" POUR CHARGE/DECHARGE BALLON ","EC162",270,0.12,95010,"/","/","/",3661238002425,0.97,230,195,85,"C0"]
[7604939,"STATION TRANSFERT DMCDB ","ER468",1037,null,null,"/","/","/",3661238583511,9.8000000000000007,625,320,205,"C7"]
[]
[]
[100005131,"BALLON SOLAIRE COMBI CHAUFFAGE + ECS DC 750-2","EC140",3225,null,null,"/","/","/",3661238091993,240,1200,1200,2150,"C7"]
[120767,"BALLON SOLAIRE COMBI CHAUFFAGE + ECS DC 1000",null,{"$f":"SUM(D1145:D1146)","v":4142},null,null,"/","/","/",null,null,null,null,null,"C7"]
[]
["COMPOSANTS"]
[89807226,"CUVE DC 1000","EC106",3137,null,null,"/","/","/",3661238046160,290,740,820,2200,"C7"]
[89807227,"HABILLAGE DC 1000","EC107",1005,null,null,"/","/","/",3661238046153,38,1385,415,2355,"C7"]
[]
["OPTIONS POUR PREPARATEURS SOLAIRES DC "]
[89757746,"THERMOMETRE","AJ32",51,null,null,"/","/","/",3661238046887,0.18,145,190,125,"C0"]
[89608920,"ANODE ACI CORREX UP BALLON > 300 LITRES","AM7",532,0.02,95020,"/","/","/",3661238047440,0.44,425,100,55,"C0"]
[89807767,"MITIGEUR THERMOSTATIQUE 1\"","EG78",136,null,null,"/","/","/",3661238045149,0.65,125,105,90,"C7"]
[]
["OPTIONS POUR PREPARATEURS SOLAIRES DC 1000"]
[89757750,"RESISTANCE BLINDEE 6 KW/400V A VISSER 1''1/2","AJ36",628,null,null,"/","/","/",3661238046863,2.4700000000000002,695,170,180,"C0"]
[]
["BALLONS TAMPONS POUR LE STOCKAGE DE L'EAU DE CHAUFFAGE ET LE SOUTIEN AU CHAUFFAGE "]
["CUVE"]
[7650461,"BALLON PS 600","AJ59",1429,null,null,null,null,null,3661238657380,146,1165,950,2033,"C7"]
[7650462,"BALLON PS 800 ","AJ60",1817,null,null,null,null,null,3661238657397,174,1250,1120,1930,"C7"]
[7650463,"BALLON PS 1000","AJ61",2042,null,null,null,null,null,3661238657403,202,1250,1120,2171,"C7"]
[7650464,"BALLON PS 1500","AJ62",2859,null,null,null,null,null,3661238657410,323,1970,1500,2037,"C7"]
[7650465,"BALLON PS 2000","AJ63",3369,null,null,null,null,null,3661238657427,407,1780,1329,2176,"C7"]
[7650466,"BALLON PS 2500","AJ64",3880,null,null,null,null,null,3661238657434,487,1590,2200,2035,"C7"]
[7650467,"BALLON PS 3000","AJ65",4288,null,null,null,null,null,3661238657618,517,1590,2200,2197,"C7"]
[]
["HABILLAGE RIGIDE"]
[7650489,"JAQUETTE RIGIDE 600 PS/PSE","AJ87",613,null,null,null,null,null,3661238657830,31,1165,950,2033,"C7"]
[7650490,"JAQUETTE RIGIDE 800 PS/PSE","AJ88",633,null,null,null,null,null,3661238657847,35,1250,1120,1930,"C7"]
[7650491,"JAQUETTE RIGIDE 1000 PS/PSE ","AJ89",715,null,null,null,null,null,3661238657854,39,1250,1120,2171,"C7"]
[7650492,"JAQUETTE RIGIDE 1500 PS/PSE ","AJ90",1123,null,null,null,null,null,3661238657861,44,1970,1500,2037,"C7"]
[7650493,"JAQUETTE RIGIDE 2000 PS/PSE ","AJ91",1327,null,null,null,null,null,3661238657878,49,1780,1329,2176,"C7"]
[7650494,"JAQUETTE RIGIDE 2500 PS/PSE ","AJ92",1532,null,null,null,null,null,3661238657885,54,1590,2200,2035,"C7"]
[7650495,"JAQUETTE RIGIDE 3000 PS/PSE ","AJ93",1736,null,null,null,null,null,3661238657892,61,1590,2200,2197,"C7"]
[]
["HABILLAGE SOUPLE"]
[7650513,"JAQUETTE SOUPLE M1 600 PS/PSE ","AJ107",306,null,null,null,null,null,3661238658233,33,1840,1260,210,"C7"]
[7650514,"JAQUETTE SOUPLE M1 800 PS/PSE ","AJ108",306,null,null,null,null,null,3661238658240,37,1750,1230,230,"C7"]
[7650526,"JAQUETTE SOUPLE M1 1000 PS/PSE ","AJ109",408,null,null,null,null,null,3661238658257,41,2090,1200,260,"C7"]
[7650527,"JAQUETTE SOUPLE M1 1500 PS/PSE ","AJ110",715,null,null,null,null,null,3661238658264,47,1900,1180,350,"C7"]
[7650528,"JAQUETTE SOUPLE M1 2000 PS/PSE ","AJ111",817,null,null,null,null,null,3661238658271,50,2110,1370,300,"C7"]
[7650529,"JAQUETTE SOUPLE M1 2500 PS/PSE ","AJ112",919,null,null,null,null,null,3661238658288,57,1900,1200,420,"C7"]
[7650532,"JAQUETTE SOUPLE M1 3000 PS/PSE ","AJ113",1021,null,null,null,null,null,3661238658295,62,2060,1270,420,"C7"]
[]
["BALLON DE STOCKAGE DE L'EAU CHAUDE SANITAIRE DE 800 L A 3000 L"]
["CUVE"]
[7650474,"BALLON RSB 800 ","AJ72",1919,null,null,null,null,null,3661238657687,201,1250,1120,2024,"C7"]
[7650469,"BALLON RSB 1000","AJ68",2348,null,null,null,null,null,3661238657632,207,1250,1120,2167,"C7"]
[7650470,"BALLON RSB 1500","AJ69",2655,null,null,null,null,null,3661238657649,318,1970,1500,2023,"C7"]
[7650471,"BALLON RSB 2000","AJ70",2961,null,null,null,null,null,3661238657656,344,1780,1329,2162,"C7"]
[7650472,"BALLON RSB 2500","AJ71",3574,null,null,null,null,null,3661238657663,453,1590,2200,2019,"C7"]
[7650473,"BALLON RSB 3000","AJ72",3676,null,null,null,null,null,3661238657670,480,1590,2200,2186,"C7"]
[]
["HABILLAGE RIGIDE "]
[7650497,"JAQUETTE RIGIDE 800 TP B/RSB","AJ95",633,null,null,null,null,null,3661238657915,36,1250,1120,2024,"C7"]
[7650499,"JAQUETTE RIGIDE 1000 TP B/RSB","AJ97",715,null,null,null,null,null,3661238657939,39,1970,1500,2023,"C7"]
[7650502,"JAQUETTE RIGIDE 1500 TP B/RSB ","AJ99",1123,null,null,null,null,null,3661238657953,44,1590,2200,2019,"C7"]
[7650506,"JAQUETTE RIGIDE 2000 TP B/RSB ","AJ101",1327,null,null,null,null,null,3661238657977,49,1250,1120,2024,"C7"]
[7650508,"JAQUETTE RIGIDE 2500 TP B/RSB ","AJ103",1532,null,null,null,null,null,3661238657991,54,1970,1500,2023,"C7"]
[7650511,"JAQUETTE RIGIDE 3000 TP B/RSB ","AJ105",1736,null,null,null,null,null,3661238658219,61,1590,2200,2019,"C7"]
[]
["HABILLAGE SOUPLE"]
[7650534,"JAQUETTE SOUPLE M1 800 TP B/RSB ","AJ115",306,null,null,null,null,null,3661238658318,38,1750,1230,230,"C7"]
[7650554,"JAQUETTE SOUPLE M1 1000 TP B/RSB ","AJ117",408,null,null,null,null,null,3661238658332,41,2090,1200,260,"C7"]
[7650558,"JAQUETTE SOUPLE M1 1500 TP B/RSB ","AJ119",715,null,null,null,null,null,3661238658356,47,1900,1180,350,"C7"]
[7650561,"JAQUETTE SOUPLE M1 2000 TP B/RSB ","AJ121",817,null,null,null,null,null,3661238658370,50,2110,1370,300,"C7"]
[7650563,"JAQUETTE SOUPLE M1 2500 TP B/RSB ","AJ123",919,null,null,null,null,null,3661238658394,57,1900,1200,420,"C7"]
[7650566,"JAQUETTE SOUPLE M1 3000 TP B/RSB ","AJ125",1021,null,null,null,null,null,3661238658417,62,2060,1270,420,"C7"]
[]
["HABILLAGE RIGIDE (CLASSEMENT AU FEU)"]
[7650583,"JAQUETTE RIGIDE M0 800 TP B/RSB","AJ141",1378,null,null,null,null,null,3661238658653,41,1860,800,550,"C7"]
[]
["OPTIONS"]
[89757750,"RESISTANCE BLINDEE 6 KW/400V A VISSER 1''1/2","AJ36",628,null,null,"/","/","/",3661238046863,2.4700000000000002,695,170,180,"C0"]
[100019313,"KIT ELECTRIQUE 9 KW/400V 1 1/2 ( POUR RSB 1000 A 3000 )","AJ47",650,null,null,"/","/","/",3661238553316,4.5,695,170,180,"C7"]
[100019314,"KIT ELECTRIQUE 12 KW/400V  1 1/2  ( POUR RSB 1500 A 3000 )","ER335",728,null,null,"/","/","/",3661238553323,2.8,1210,190,140,"C7"]
[7651086,"RESIST. BLIND. 9 KW 400V  DN110 ","AJ164",500,null,null,null,null,null,3661238659179,7.1,760,493,190,"C0"]
[7651088,"RESIST. BLIND. 9 KW 400V  DN110 ","AJ165",582,null,null,null,null,null,3661238659179,7.1,760,493,190,"C0"]
[7651116,"RESIST.B.30KW400V DN110 SUP.800L ","AJ166",664,null,null,null,null,null,3661238659193,10.1,760,493,190,"C0"]
[89608920,"ANODE ACI CORREX UP BALLON > 300 LITRES","AM7",532,0.02,95020,"/","/","/",3661238047440,0.44,425,100,55,"C0"]
[89757746,"THERMOMETRE","AJ32",51,null,null,"/","/","/",3661238046887,0.18,145,190,125,"C0"]
[7651078,"DOIGT DE GANT 350 MM 1/2 ","AJ162",36,null,null,null,null,null,3661238659155,1.1000000000000001,54,54,560,"C0"]
[7651082,"BRIDE LATERALE 110 A EMBOUT 1_1/2","AJ163",286,null,null,null,null,null,3661238659162,3.6,315,315,190,"C0"]
[]
["BALLON DE STOCKAGE D'EAU CHAUDE SANITAIRE DE 1000 L A 3000L"]
["CUVE"]
[7650475,"BALLON RSB 1000 ","AJ73",2553,null,null,null,null,null,3661238657694,218,1250,1120,2167,"C7"]
[7650476,"BALLON RSB 1500","AJ74",2859,null,null,null,null,null,3661238657700,328,1970,1500,2023,"C7"]
[7650477,"BALLON RSB 2000","AJ75",3165,null,null,null,null,null,3661238657717,355,1780,1329,2162,"C7"]
[7650478,"BALLON RSB 2500","AJ76",3676,null,null,null,null,null,3661238657724,466,1590,2200,2019,"C7"]
[7650479,"BALLON RSB 3000","AJ77",3880,null,null,null,null,null,3661238657731,494,1590,2200,2186,"C7"]
[]
["HABILLAGE RIGIDE (CLASSEMENT AU FEU)"]
[7650592,"JAQUETTE RIGIDE M0 1000 TH B/RSB","AJ148",1532,null,null,null,null,null,3661238658721,44,2080,800,550,"C7"]
[7650593,"JAQUETTE RIGIDE M0 1500 TH B/RSB","AJ149",1991,null,null,null,null,null,3661238658738,70,2030,1040,570,"C7"]
[7650594,"JAQUETTE RIGIDE M0 2000 TH B/RSB","AJ150",2144,null,null,null,null,null,3661238658745,76,2250,1040,570,"C7"]
[7650596,"JAQUETTE RIGIDE M0 2500 TH B/RSB","AJ151",2553,null,null,null,null,null,3661238658752,80,2250,1040,570,"C7"]
[7650597,"JAQUETTE RIGIDE M0 3000 TH B/RSB","AJ152",2604,null,null,null,null,null,3661238658769,86,2250,1040,570,"C7"]
[]
["HABILLAGE SOUPLE (CLASSEMENT AU FEU)"]
[7650555,"JAQUETTE SOUPLE M1 1000 TH B/RSB ","AJ118",408,null,null,null,null,null,3661238658349,41,2090,1200,260,"C7"]
[7650560,"JAQUETTE SOUPLE M1 1500 TH B/RSB ","AJ120",715,null,null,null,null,null,3661238658363,47,1900,1180,350,"C7"]
[7650562,"JAQUETTE SOUPLE M1 2000 TH B/RSB ","AJ122",817,null,null,null,null,null,3661238658387,50,2110,1370,300,"C7"]
[7650564,"JAQUETTE SOUPLE M1 2500 TH B/RSB ","AJ124",919,null,null,null,null,null,3661238658400,57,1900,1200,420,"C7"]
[7650567,"JAQUETTE SOUPLE M1 3000 TH B/RSB ","AJ126",1021,null,null,null,null,null,3661238658424,62,2060,1270,420,"C7"]
[]
["OPTIONS"]
[7651117,"RESIST. BLIND. 9 KW 400V DN400 ","AJ167",1286,null,null,null,null,null,3661238659209,38.1,760,493,190,"C0"]
[7651120,"RESIST. BLIND. 15 KW 400V DN400","AJ168",1583,null,null,null,null,null,3661238659223,38.1,200,150,190,"C0"]
[7651122,"RESIST. BLIND. 30 KW 400V DN400","AJ169",1634,null,null,null,null,null,3661238659230,38.1,760,493,190,"C0"]
[7651123,"RESIST. STEATITE 9 KW 400V DN400 ","AJ170",2042,null,null,null,null,null,3661238659254,51.8,1164,450,260,"C0"]
[7651124,"RESIST. STEATITE 15 KW 400V DN40","AJ171",2246,null,null,null,null,null,3661238659261,54.8,1164,450,260,"C0"]
[7651127,"RESIST. STEATITE 30 KW 400V DN400","AJ172",2450,null,null,null,null,null,3661238659278,59.8,1164,450,260,"C0"]
[7651078,"DOIGT DE GANT 350 MM 1/2 ","AJ162",36,null,null,null,null,null,3661238659155,1.1000000000000001,54,54,560,"C0"]
[89608920,"ANODE ACI CORREX UP BALLON > 300 LITRES","AM7",532,0.02,95020,"/","/","/",3661238047440,0.44,425,100,55,"C0"]
[89757746,"THERMOMETRE","AJ32",51,null,null,"/","/","/",3661238046887,0.18,145,190,125,"C0"]
[]
[]
[100012353,"1 CAPTEUR SOLAIRE SUN 3010","ER40",1656,null,null,"Pas concerné par l'étiquettage",null,null,null,40,1770,900,110,"C7"]
[100012354,"1 CAPTEUR SOLAIRE SUN 3015","ER41",1974,null,null,"Pas concerné par l'étiquettage",null,null,null,55,1770,1290,115,"C7"]
[]
["ACCESSOIRES DE MONTAGE SUN 3000"]
[100011397,"KIT DE RACCORDEMENT (EXTREMITE + BOUCHON)","EG394",112,null,null,"/","/","/",3661238340053,0.42,160,210,25,"C7"]
[100011396,"KIT DE LIAISON HYDRAULIQUE INTER COLLECTEUR","EG393",150,null,null,"/","/","/",3661238340046,0.66,260,220,100,"C7"]
[89807355,"KIT DE RACCORDEMENT FLEXIBLE CAPTEUR TUBULAIRE + SONDE CAPTEUR","EG355",197,null,null,"/","/","/",3661238045552,1.34,1060,165,95,"C7"]
[100011395,"KIT DE FIXATION 1 CAPTEUR","EG392",78,null,null,"/","/","/",3661238340039,0.56999999999999995,240,145,30,"C7"]
[100012019,"KIT DE MONTAGE 1 CAPTEUR SUN 3010","ER31",158,null,null,"/","/","/",3661238352179,6,1600,110,90,"C7"]
[100012020,"KIT DE MONTAGE 1 CAPTEUR SUN 3015","ER32",166,null,null,"/","/","/",3661238352162,5.5,1600,110,90,"C7"]
[]
["ELEMENTS DE MONTAGE SUPPLEMENTAIRES POUR TOUS TYPES DE PANNEAUX "]
[89807307,"KIT COUPLEURS (2 PCES) POUR PROFILES (FIXATION PROFILES JUXTAPOSÉS)","EG307",31,null,null,"/","/","/",3661238045941,0.18,195,100,20,"C7"]
[89807311,"4 FERRURES D'ANCRAGE ALU POUR MONTAGE SUR TUILES MÉCANIQUES","EG311",98,null,null,"/","/","/",3661238045903,2.34,365,120,140,"C7"]
[89807312,"6 FERRURES D'ANCRAGE ALU POUR MONTAGE SUR TUILES MÉCANIQUES","EG312",141,null,null,"/","/","/",3661238045897,3.46,365,115,140,"C7"]
[89807313,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES MÉCANIQUES","EG313",98,null,null,"/","/","/",3661238045880,3.37,320,220,135,"C7"]
[89807314,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES MÉCANIQUES","EG314",141,null,null,"/","/","/",3661238045873,4.93,325,225,135,"C7"]
[89807315,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES PLATES","EG315",98,null,null,"/","/","/",3661238045866,2.4,300,135,95,"C7"]
[89807316,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES PLATES","EG316",141,null,null,"/","/","/",3661238045859,3.5,310,140,95,"C7"]
[89807317,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT ETERNIT","EG317",98,null,null,"/","/","/",3661238045842,3.56,260,215,75,"C7"]
[89807318,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT ETERNIT","EG318",141,null,null,"/","/","/",3661238045835,5.3,260,220,75,"C7"]
[89807319,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT D'ARDOISES","EG319",98,null,null,"/","/","/",3661238045828,2.21,280,120,80,"C7"]
[89807320,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT D'ARDOISES","EG320",141,null,null,"/","/","/",3661238045811,3.3,305,140,95,"C7"]
[89807358,"3 SUPPORTS TERRASSE ET CROIX POUR 2 CAPTEUR EN VERTICAL","EG358",287,null,null,"/","/","/",3661238045521,8.4,1835,120,80,"C7"]
[89807359,"3 SUPPORTS TERRASSE POUR 2 CAPTEURS EN VERTICAL","EG359",245,null,null,"/","/","/",3661238045514,8,1825,120,80,"C7"]
[89807323,"2 SUPPORTS TERRASSE POUR 1 CAPTEUR EN VERTICAL","EG323",274,null,null,"/","/","/",3661238045781,6,1885,75,90,"C7"]
[89807324,"3 SUPPORTS TERRASSE POUR 2 CAPTEURS EN VERTICAL","EG324",373,null,null,"/","/","/",3661238045774,8,1855,145,80,"C7"]
[89807325,"2 SUPPORTS TERRASSE POUR 1 CAPTEUR EN HORIZONTAL","EG325",161,null,null,"/","/","/",3661238045767,3.7,1205,80,75,"C7"]
[89807358,"3 SUPPORTS AVEC CROIX STABILISATRICE POUR 2 CAPTEURS MONTAGE VERTICAL","EG358",287,null,null,"/","/","/",3661238045521,8.4,1835,120,80,"C7"]
[89807359,"3 SUPPORTS SANS CROIX STABILISATRICE POUR 2 CAPTEURS MONTAGE VERTICAL","EG359",245,null,null,"/","/","/",3661238045514,8,1825,120,80,"C7"]
[89807782,"KIT TIRE-FONDS POUR MONTAGE 2 CAPTEURS","EG94",247,null,null,"/","/","/",3661238045057,2.84,405,140,80,"C7"]
[89807783,"KIT TIRE-FONDS POUR MONTAGE 3 CAPTEURS","EG95",310,null,null,"/","/","/",3661238045040,3.73,405,140,80,"C7"]
[]
[]
[7604939,"STATION TRANSFERT DMCDB ","ER468",1037,null,null,"/","/","/",3661238583511,9.8000000000000007,625,320,205,"C7"]
[7624853,"STATION SOLAIRE SKP 7-8","ER655",447,0.17,14060,"/","/","/",3661238617018,6.32,480,300,200,"C7"]
[7630417,"STATION SOLAIRE DKSL 6-8 MSB ","ER710",562,0.83,14090,"/","/","/",3661238631021,7.7,925,230,435,"C7"]
[]
[]
[7630422,"REGULATION OETROSOL-PLUS","ER709",260,0.12,95010,"/","/","/",3661238631045,0.69,227,194,85,"C7"]
[7619972,"REGULATION SOL COLLECTIF SC5 ","ER672",609,0.12,95010,"/","/","/",3661238608689,2.2999999999999998,320,230,130,"C7"]
[100004618,"RÉGULATION \"DELTASOL ES\" POUR 2 CHAMPS DE CAPTEURS ","EC158",621,0.12,95010,"/","/","/",3661238002470,1.7,325,230,130,"C0"]
[100003690,"SONDE A APPLIQUE PT1000","EC171",62,0.02,95020,"/","/","/",3661238005303,0.1,180,140,30,"C0"]
[100004651,"SONDE D'IMMERSION FK Pt1000 2,5 m","EC173",62,0.02,95020,"/","/","/",3661238002418,0.15,220,150,25,"C0"]
[100008011,"SONDE CAPTEUR  PT1000 ","EC155",58,0.02,95020,"/","/","/",3661238101197,0.1,180,120,20,"C7"]
[89804803,"VANNE 3 VOIES 3/4\" POUR 2 CIRCUITS","EC164",237,null,null,"/","/","/",3661238046528,1.05,205,125,90,"C7"]
[89804816,"BOITIER PARA FOUDRE POUR SONDE PANNEAUX SOLAIRES","EC176",40,null,null,"/","/","/",3661238046450,0.11,220,165,40,"C7"]
[100004650,"REGULATION \"MCDB\" POUR CHARGE/DECHARGE BALLON ","EC162",270,0.12,95010,"/","/","/",3661238002425,0.97,230,195,85,"C0"]
[100011341,"KIT 2 VANNES/SONDE CAPT.EST-OUEST","EC432",454,null,null,"/","/","/",3661238340213,1.3,240,160,70,"C0"]
[]
["DOUBLE TUBE PREISOLE AVEC CABLE"]
[89807000,"TWIN TUBES CU DN15 10 METRES","EG106",467,null,null,"/","/","/",3661238046436,11,790,800,275,"C0"]
[89807001,"TWIN TUBES CU DN15 15 METRES","EG107",716,null,null,"/","/","/",3661238046429,16.2,800,795,275,"C0"]
[89807003,"JEU DE 4 COLLIERS DN15","EG109",22,null,null,"/","/","/",3661238046405,0.5,160,110,70,"C0"]
[89807002,"TWIN TUBES DN18 15 METRES","EG108",935,null,null,"/","/","/",3661238046412,22.41,805,805,330,"C0"]
[89807004,"COLLIER SUP. DN18 4X","EG110",27,null,null,"/","/","/",3661238046399,0.52,160,140,75,"C0"]
[100000417,"JEU DE 2 RACCORDS BÎCONE DN 15","EG374",25,null,null,"/","/","/",3661238011144,0.18,90,100,30,"C7"]
[100000418,"JEU DE 2 RACCORDS BÎCONE DN 18","EG375",25,null,null,"/","/","/",3661238011137,0.23,120,95,30,"C7"]
[100000419,"JEU DE 2 RÉDUCTIONS BÎCONE 18/15","EG376",12,null,null,"/","/","/",3661238011120,0.03,130,95,20,"C7"]
[7648217,"DUO FLEX DN16X15 M ","EG422",715,null,null,null,null,null,3661238655218,11,800,800,290,"C7"]
[7648218,"DUO FLEX DN20X15 M ","EG423",766,null,null,null,null,null,3661238655232,12.5,795,780,390,"C7"]
[7648219,"DUO FLEX DN20X20 M","EG424",970,null,null,null,null,null,3661238655249,15.5,830,830,435,"C7"]
[100008020,"DUO-FLEX DN16 X 15 METRES","EG455",1104,null,null,"/","/","/",3661238101104,10.5,790,790,320,"C7"]
[100008021,"DUO-FLEX DN20 X 15 METRES","EG456",1287,null,null,"/","/","/",3661238101098,14.5,780,795,325,"C7"]
[100008022,"JEU DE RACCORDS DUOFLEX DN16/BîCONE Ø 18","EG457",27,null,null,"/","/","/",3661238101081,0.32,90,80,60,"C7"]
[100008023,"JEU DE RACCORDS DUOFLEX DN20/BîCONE Ø 18","EG458",27,null,null,"/","/","/",3661238101074,0.51,90,80,60,"C7"]
[]
["FLUIDES CALOPORTEURS"]
[89807794,"FLUIDE CALOPORTEUR \"L\" 20L. MELANGE 40/60 ","EG101",78,null,null,"/","/","/",3661238045019,21.72,240,290,370,"C7"]
[89807792,"FLUIDE CALOPORTEUR \"LS\" 20L HAUTES PREFORMANCES","EG100",154,null,null,"/","/","/",3661238045033,21.53,340,290,370,"C7"]
[100017611,"FLUIDE CALOPORTEUR HAUTE PREFORMANCE BIO (-26°C) 20 LITRES","ER316",134,null,null,"/","/","/",3661238496606,21.53,340,290,370,"C7"]
[89807710,"ANTIGEL ''L' CONCENTRE EN BIDON DE 10 L","EG11",99,null,null,"/","/","/",3661238045316,10.95,220,190,295,"C7"]
[]
["VASES D'EXPANSION"]
[89807713,"VASE D'EXPANSION SOLAIRE 18 L","EG14",99,null,null,"/","/","/",3661238045309,4.2300000000000004,395,290,300,"C7"]
[89807771,"VASE D'EXPANSION SOLAIRE 25 L","EG82",115,null,null,"/","/","/",3661238045118,5.53,455,305,305,"C7"]
[89807772,"VASE D'EXPANSION SOLAIRE 35 L","EG83",181,null,null,"/","/","/",3661238045101,7.34,585,335,340,"C7"]
[89807773,"VASE D'EXPANSION SOLAIRE 50 L","EG84",348,null,null,"/","/","/",3661238045095,12.5,700,385,390,"C7"]
[100008733,"VASE D'EXPANSION 100 l","EG120",402,null,null,"/","/","/",3661238166424,17,800,460,470,"C7"]
[100008735,"VASE D'EXPANSION 200 l","EG122",637,null,null,"/","/","/",3661238166417,36,1020,560,570,"C7"]
[100008736,"VASE D'EXPANSION 300 l","EG123",1142,null,null,"/","/","/",3661238166400,68,1180,640,640,"C7"]
[89807238,"KIT D'ACCROCHAGE POUR VASE D'EXPANSION ","EC118",60,null,null,"/","/","/",3661238046047,1.35,480,130,150,"C0"]
[]
[]
[100016502,"CAPTEUR PLAN MONTAGE VERTICAL PRO C250 V","ER240",797,null,null,"/","/","/",3661238492318,2210,1320,115,48,"C7"]
[100016503,"CAPTEUR PLAN MONTAGE HORIZONTAL PRO C250 H","ER241",820,null,null,"/","/","/",3661238492301,2210,1320,115,48,"C7"]
[]
["ACCESSOIRES POUR RACCORDEMENTS HYDRAULIQUES DES PANNEAUX SOLAIRES SUN C 250 "]
["RACCORDEMENT DES CAPTEURS EN MONTAGE VERTICAL JUXTAPOSES OU HORIZONTAL SUPERPOSES"]
[100016506,"KIT DE RACCORDEMENT CHAMP DE CAPTEURS","ER245",120,null,null,"/","/","/",3661238492325,1045,165,90,1.5,"C7"]
[100016507,"KIT DE LIAISON HYDRAULIQUE ENTRE CAPTEURS","ER246",41,null,null,"/","/","/",3661238492332,1045,165,90,1.5,"C7"]
[100016508,"KIT 2 FLEXIBLES CIRCUIT SOLAIRE CHAMP CAPTEURS","ER247",132,null,null,"/","/","/",3661238492349,1045,165,90,1.5,"C7"]
[100019224,"INTERFACE DE COMMUNICATION DL3","ER139",728,0.12,95010,"/","/","/",3661238549548,0.68,230,195,85,"C7"]
[]
["ELEMENTS DE POSE SUR TOIT OU EN TERRASSE"]
["MONTAGE JUXTAPOSES SUPERPOSES SUR TOITURE OU SUPPORTS TERRASSE STANDARD"]
[100016513,"KIT PROFILES A CLIPER POUR 1 C250 V","ER260",139,null,null,"/","/","/",3661238492394,2120,110,95,8,"C7"]
[100016514,"KIT PROFILES A CLIPER POUR 1 C250 H","ER261",173,null,null,"/","/","/",3661238492400,2120,110,95,8,"C7"]
[7217044,"KIT PROFILES 45 MTGE VT ","ER664",80,null,null,"/","/","/",3661238492295,2.5,1260,155,100,"C7"]
[7217048,"KIT PROFILES 45 2,5M2 HZ ","ER662",98,null,null,"/","/","/",3661238492288,2210,1320,115,48,"C7"]
[100016509,"2 SUPPORTS HL AVEC CROIX  MONTAGE VERTICAL 1 C250 SANS PROFILES","ER250",312,null,null,"/","/","/",3661238492356,1875,75,90,6,"C7"]
[100016510,"1 SUPPORT HL VERTICAL POUR EXTENSION 1 C250 ","ER251",161,null,null,"/","/","/",3661238492363,1875,75,90,6,"C7"]
[100016511,"2 SUPPORTS HL AVEC CROIX  MONTAGE HORIZONTAL 1 C250 SANS PROFILES","ER252",255,null,null,"/","/","/",3661238492370,1875,75,90,6,"C7"]
[100016512,"1 SUPPORT HL HORIZONTAL POUR EXTENSION 1 C250 ","ER253",145,null,null,"/","/","/",3661238492387,1885,75,90,6,"C7"]
[7217038,"2 SUPPORTS SL MONTAGE VERTICAL 1 CAPTEUR","ER658",196,null,null,"/","/","/",3661238630710,9.5,2267,145,80,"C7"]
[7217039,"1 SUPPORT SL MTGE VERTICAL POUR EXTENSION 1 CAPTEUR","ER659",91,null,null,"/","/","/",3661238630277,4.5,1945,110,95,"C7"]
[7217041,"2 SUPPORTS SL HL MONTAGE HORIZONTAL 1 CAPTEUR","ER656",156,null,null,"/","/","/",3661238630253,5.5,1250,145,80,"C7"]
[7217042,"1 SUPPORT SL HL HORIZONTAL POUR EXTENSION 1 CAPTEUR","ER657",79,null,null,"/","/","/",3661238630260,3,1250,145,80,"C7"]
[]
["FERRURES D'ANCRAGE POUR MONTAGE SUR TOITURE"]
[89807311,"4 FERRURES D'ANCRAGE ALU POUR MONTAGE SUR TUILES MÉCANIQUES","EG311",98,null,null,"/","/","/",3661238045903,365,120,140,2.2999999999999998,"C7"]
[89807312,"6 FERRURES D'ANCRAGE ALU POUR MONTAGE SUR TUILES MÉCANIQUES","EG312",141,null,null,"/","/","/",3661238045897,3.46,365,115,140,"C7"]
[89807313,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES MÉCANIQUES","EG313",98,null,null,"/","/","/",3661238045880,3.37,320,220,135,"C7"]
[89807314,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES MÉCANIQUES","EG314",141,null,null,"/","/","/",3661238045873,4.93,325,225,135,"C7"]
[89807315,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES PLATES","EG315",98,null,null,"/","/","/",3661238045866,2.4,300,135,95,"C7"]
[89807316,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES PLATES","EG316",141,null,null,"/","/","/",3661238045859,3.5,310,140,95,"C7"]
[100015314,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES CANAL","ER136",97,null,null,"/","/","/",3661238415539,325,260,120,4,"C7"]
[100015315,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TUILES CANAL","ER137",141,null,null,"/","/","/",3661238415546,410,305,115,6.5,"C7"]
[89807317,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT ETERNIT","EG317",98,null,null,"/","/","/",3661238045842,3.56,260,215,75,"C7"]
[89807318,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT ETERNIT","EG318",141,null,null,"/","/","/",3661238045835,5.3,260,220,75,"C7"]
[89807319,"4 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT D'ARDOISES","EG319",98,null,null,"/","/","/",3661238045828,2.21,280,120,80,"C7"]
[89807320,"6 FERRURES D'ANCRAGE INOX POUR MONTAGE SUR TOIT D'ARDOISES","EG320",141,null,null,"/","/","/",3661238045811,3.3,305,140,95,"C7"]
[89807782,"KIT TIRE-FONDS POUR MONTAGE 2 CAPTEURS","EG94",247,null,null,"/","/","/",3661238045057,405,140,80,2.8,"C7"]
[89807783,"KIT TIRE-FONDS POUR MONTAGE 3 CAPTEURS","EG95",310,null,null,"/","/","/",3661238045040,3.73,405,140,80,"C7"]
[100016517,"4 FERRURES D'ANCRAGE ALU  A CRANS MTGE SUR CHEVRON","ER264",131,null,null,"/","/","/",3661238492431,2120,110,95,8,"C7"]
[100016518,"2 FERRURES D'ANCRAGE ALU  A CRANS MTGE SUR CHEVRON","ER265",79,null,null,"/","/","/",3661238492448,2120,110,95,8,"C7"]
[]
[]
[7212864,"KIT DE BASE 22° D'INTEGRATION TUILE MECANIQUE 1 C250 V","ER634",551,null,null,"/","/","/",3661238600430,21.8,150,800,2000,"C7"]
[7212869,"KIT DE BASE 22° D'INTEGRATION TUILE MECANIQUE 2 C250 V","ER635",795,null,null,"/","/","/",3661238600447,21.8,150,800,2000,"C7"]
[7212867,"KIT EXTENSION 22° INTEGRATION TUILE MECANIQUE 1 C 250 V","ER636",329,null,null,"/","/","/",3661238600454,16.2,150,800,2000,"C7"]
[7212866,"KIT DE BASE 22° D'INTEGRATION TUILE MECANIQUE 1 C250 H","ER637",583,null,null,"/","/","/",3661238600461,30.4,150,800,2000,"C7"]
[7212870,"KIT DE BASE 22° D'INTEGRATION TUILE MECANIQUE 2 C250 H","ER638",954,null,null,"/","/","/",3661238600478,33,150,800,2000,"C7"]
[7212868,"KIT EXTENSION 22° INTEGRATION TUILE MECANIQUE C 250 H","ER639",425,null,null,"/","/","/",3661238600485,23.8,150,800,2000,"C7"]
[7212872,"KIT DE BASE 17° D'INTEGRATION TUILE CANAL 1 C250 V ","ER640",721,null,null,"/","/","/",3661238600492,52,150,800,2000,"C7"]
[7503821,"KIT DE BASE 17° D'INTEGRATION TUILE CANAL 2 C250 V ","ER641",1113,null,null,"/","/","/",3661238600508,55,150,800,2000,"C7"]
[7212875,"KIT EXTENSION 17° INTEGRATION TUILE CANAL C 250 V ","ER642",425,null,null,"/","/","/",3661238600515,52,150,800,2000,"C7"]
[7212873,"KIT DE BASE 17° D'INTEGRATION TUILE CANAL 1 C250 H ","ER643",806,null,null,"/","/","/",3661238600522,52,150,800,2000,"C7"]
[7212880,"KIT DE BASE 17° D'INTEGRATION TUILE CANAL 2 C250 H ","ER644",1325,null,null,"/","/","/",3661238600539,55,150,800,2000,"C7"]
[7212877,"KIT EXTENSION 17° INTEGRATION TUILE CANAL C 250 H","ER645",478,null,null,"/","/","/",3661238600546,27.2,150,800,2000,"C7"]
[7619965,"TAMPON COMPLEMENTAIRE MODULE DB2","ER666",1166,null,null,"/","/","/",3661238608610,10,500,280,235,"C7"]
[]
["ACCESSOIRES DE MONTAGE POUR ARDOISES ET TUILES PLATES"]
[7503269,"KIT NOQUETS POUR TUILES PLATES ET ARDOISES","ER558",138,null,null,"/","/","/",3661238586611,7,150,200,360,"C7"]
[]
[]
["CUVE"]
[7650487,"BALLON B 802","AJ85",3247,null,null,null,null,null,3661238657816,249,1250,1120,2024,"C7"]
[7650488,"BALLON B1002","AJ86",3880,null,null,null,null,null,3661238657823,271,1250,1120,2167,"C7"]
["HABILLAGE "]
[7650497,"JAQUETTE RIGIDE 800 TP B/RSB","AJ95",633,null,null,null,null,null,3661238657915,36,1250,1120,2024,"C7"]
[7650499,"JAQUETTE RIGIDE 1000 TP B/RSB","AJ97",715,null,null,null,null,null,3661238657939,39,1970,1500,2023,"C7"]
[]
["OPTIONS"]
[89757750,"RESISTANCE BLINDEE 6 KW/400V A VISSER 1''1/2","AJ36",628,null,null,"/","/","/",3661238046863,2.4700000000000002,695,170,180,"C0"]
[7651082,"BRIDE LATERALE 110 A EMBOUT 1_1/2","AJ163",286,null,null,null,null,null,3661238659162,3.6,315,315,190,"C0"]
[7651078,"DOIGT DE GANT 350 MM 1/2 ","AJ162",36,null,null,null,null,null,3661238659155,1.1000000000000001,54,54,560,"C0"]
[89757746,"THERMOMETRE","AJ32",51,null,null,"/","/","/",3661238046887,0.18,145,190,125,"C0"]
[89608920,"ANODE ACI CORREX UP BALLON > 300 LITRES","AM7",532,0.02,95020,"/","/","/",3661238047440,0.44,425,100,55,"C0"]
[]
[]
[100017486,"MODULE TRANSFERT SOLAIRE DRAIN BACK DB-20","ER301",2772,0.83,14090,"/","/","/",3661238496071,10,500,280,235,"C7"]
[]
[]
[7630422,"REGULATION OETROSOL-PLUS","ER709",260,0.12,95010,"/","/","/",3661238631045,0.69,227,194,85,"C7"]
[]
[]
[100008019,"PREPARATEUR ECS INSTANTANEE FWS 750","EC546",4808,null,null,"Pas concerné par l'étiquettage",null,null,3661238101111,252,1200,1200,2330,"C7"]
[100008150,"PREPARATEUR SOLAIRE OECOSUN DU 750-20 CL",null,{"$f":"SUM(D1430,D1431)","v":7539},null,null,"Pas concerné par l'étiquettage",null,null,3661238101232,null,null,null,null,"C7"]
[100017466,"PREPARATEUR SOLAIRE FWS 1500 COMPLET",null,{"$f":"D1432+D1433","v":7103},null,null,"Pas concerné par l'étiquettage",null,null,3661238495784,292,null,null,null,"C7"]
[]
["COMPOSANTS"]
[100007994,"CUVE (55 kW) & HABILLAGE DU 750-20 CL","EC545",4159,null,null,"/","/","/",3661238101234,242,1200,1200,2250,"C7"]
[100008115,"COLIS COMPOSANTS OECOSUN DU 750-20 ","EC562",3380,null,null,"/","/","/",3661238372436,56,1200,1400,2295,"C7"]
[100017463,"CUVE PREPARATEUR ECS FWS 1500","ER181",6005,null,null,"/","/","/",3661238495760,252,1200,1200,2330,"C7"]
[100017465,"HABILLAGE PREPARATEUR FWS 1500","ER182",1098,null,null,"/","/","/",3661238495777,40,1200,350,2100,"C7"]
[]
["OPTIONS"]
[100015099,"KIT DE BOUCLAGE ECS","ER29",178,null,null,"/","/","/",3661238496194,2.4,410,300,40,"C7"]
[89757746,"THERMOMETRE","AJ32",51,null,null,"/","/","/",3661238046887,0.18,145,190,125,"C0"]
[]
["ACCESSOIRES HYDRAULIQUES"]
["STATIONS SOLAIRES"]
[7619964,"STATION SOLAIRE SKS 13-45","ER665",676,0.17,14060,"/","/","/",3661238608627,27.8,680,430,250,"C7"]
[100017486,"MODULE TRANSFERT SOLAIRE DRAIN BACK DB-20","ER301",2772,0.83,14090,"/","/","/",3661238496071,10,500,280,235,"C7"]
[7619966,"STATION SOLAIRE STS 14-30 CME","ER667",2705,0.42,"9.14","/","/","/",3661238608634,19.8,670,370,310,"C7"]
[7619967,"STATION SOLAIRE STS 14-50 CME","ER668",3121,0.42,"9.14","/","/","/",3661238608641,35,860,675,380,"C7"]
[7619968,"STATION SOLAIRE STS 14-100 CME","ER669",6242,0.42,"9.14","/","/","/",3661238608658,44,860,680,365,"C7"]
["RÉGULATIONS SOLAIRES OETROSOL/DELTASOL",null,null,null,null,null,null,null,null,null,""]
[100017500,"RÉGULATION \"DELTASOL E\" POUR STATION TRANSFERT SOLAIRE","ER315",717,0.12,95010,"/","/","/",3661238496217,230,200,90,1.3,"C7"]
[7630422,"REGULATION OETROSOL-PLUS","ER709",260,0.12,95010,"/","/","/",3661238631045,0.69,227,194,85,"C7"]
[]
["COMPTAGE D'ENERGIE"]
[100014590,"RÉGULATION COMPTEUR D'ENERGIE WMZ 13530350 ","ER131",295,0.12,95010,"/","/","/",3661238376014,0.6,230,195,80,"C7"]
[100013514,"DATALOGGER DL2 POUR GRS","ER55",460,0.12,95010,"/","/","/",3661238364394,110,90,40,0.1,"C7"]
[100017498,"CENTRALE DE MESURE D'ENERGIE CME","ER313",1675,0.12,95010,"/","/","/",3661238496194,1.18,280,210,120,"C7"]
["RÉGULATION CHARGE BALLON"]
[100004650,"REGULATION \"MCDB\" POUR CHARGE/DECHARGE BALLON ","EC162",270,0.12,95010,"/","/","/",3661238002425,0.97,230,195,85,"C0"]
[100007832,"RÉGULATION POMPE DE CHARGE SLA 2","EC320",208,0.12,95010,"/","/","/",3661238101494,225,195,85,0.7,"C0"]
[]
["OPTIONS"]
[null,"OPTIONS POUR REGULATION CIRCUIT SOLAIRE"]
[7630423,"KIT RACCORDEMENT PMW 2e POMPE SOLAIRE OETROSOL-PLUS","ER712",52,0.02,95020,"/","/","/",3661238631052,0.8,null,null,null,"C7"]
[7630424,"KIT CABLE DE LIAISON ModBUS (3m) OETROSOL-PLUS","ER713",32,0.02,95020,"/","/","/",3661238631069,0.11,null,null,null,"C7"]
[100017499,"MODULE REPORT DE PANNE OETROSOL AM1","ER314",180,0.12,95010,"/","/","/",3661238496200,0.13,170,100,30,"C7"]
[100011341,"KIT 2 VANNES/SONDE CAPT.EST-OUEST","EC432",454,null,null,"/","/","/",3661238340213,1.3,240,160,70,"C0"]
[89804803,"VANNE 3 VOIES 3/4\" POUR 2 CIRCUITS","EC164",237,null,null,"/","/","/",3661238046528,205,125,90,1.1000000000000001,"C7"]
[89804816,"BOITIER PARA FOUDRE POUR SONDE PANNEAUX SOLAIRES","EC176",40,null,null,"/","/","/",3661238046450,0.11,220,165,40,"C7"]
[89804815,"SONDE D'IRRADIATION CS10","EC175",145,null,null,"/","/","/",3661238046467,0.05,190,120,30,"C7"]
[100008011,"SONDE CAPTEUR  PT1000 ","EC155",58,0.02,95020,"/","/","/",3661238101197,0.1,180,120,20,"C7"]
[null,"OPTIONS POUR COMPTAGE D'ENERGIE "]
[100004652,"DEBIMETRE VOLUMIQUE V40-15","EC174",415,null,null,"/","/","/",3661238002401,1.5,240,160,110,"C7"]
[100017493,"COMPTEUR EAU FROIDE ACS 5m3/H","ER308",763,null,null,"/","/","/",3661238496149,10,500,280,235,"C7"]
[100017492,"COMPTEUR EAU FROIDE ACS 3,5m3/H","ER307",692,null,null,"/","/","/",3661238496132,10,500,280,235,"C7"]
[100017494,"COMPTEUR EAU FROIDE ACS 10m3/H","ER309",981,null,null,"/","/","/",3661238496156,10,500,280,235,"C7"]
[100017495,"COMPT.FLU.CHAUD US ECHO 1.5M3","ER310",439,null,null,"/","/","/",3661238496163,10,500,280,235,"C7"]
[100017496,"COMPT.FLU.CHAUD US ECHO 2.5M3","ER311",486,null,null,"/","/","/",3661238496170,10,500,280,235,"C7"]
[100017497,"COMPT.FLU.CHAUD US ECHO 3.5M3/H ","ER312",542,null,null,"/","/","/",3661238496187,10,500,280,235,"C7"]
[100017498,"CENTRALE DE MESURE D'ENERGIE CME","ER313",1675,0.12,95010,"/","/","/",3661238496194,1.18,280,210,120,"C7"]
[]
["OPTIONS POUR INSTALLATIONS SOLAIRES"]
[89807349,"POIGNETS DE TRANSPORT ET DE MANUTENTION (4 PIECES)","EG349",144,null,null,"/","/","/",3661238045606,1.22,220,220,80,"C7"]
[89807769,"POMPE A MAIN POUR AJOUT DE FLUIDE","EG80",177,null,null,"/","/","/",3661238045132,1.01,215,150,80,"C7"]
[89807797,"DENSIMETRE (ANTIGEL \"L\") A CADRAN","EG102",52,null,null,"/","/","/",3661238045002,0.14000000000000001,160,125,40,"C7"]
[89807798,"DENSIMETRE (AEROMETRE) FLUIDE \"L\"+\"LS\"","EG103",177,null,null,"/","/","/",3661238044999,0.31,230,130,60,"C7"]
[89807799,"REFRACTOMETRE POUR FLUIDE \"L\"+\"LS\"","EG104",370,null,null,"/","/","/",3661238044982,0.32,210,80,55,"C7"]
[89807770,"STATION DE REMPLISSAGE (POMPE)","EG81",1065,0.83,14050,"/","/","/",3661238045125,24.1,1020,465,495,"C7"]
[100020025,"NETTOYANT CIRCUIT SOLAIRE SOLRNET","ER318",302,null,null,null,null,null,3661238572195,22,270,240,400,"C7"]
[]
["FAMILLE:","CHAUDIERE  MURALE GAZ A CONDENSATION"]
[]
[]
[100020008,"GMX-M 2024 CONDENS HOR",null,{"$f":"D1498+D1501","v":2150},null,null,"A","A","XL",null,null,null,null,null,"C5"]
[100020009,"GMX-M 2024 CONDENS VER",null,{"$f":"D1498+D1502+D1503","v":2214},null,null,"A","A","XL",null,null,null,null,null,"C5"]
[100020011,"GMX-M 2024 COMBI CONDENS HOR",null,{"$f":"D1499+D1501","v":2331},null,null,"A","A","XL",null,null,null,null,null,"C5"]
[100020012,"GMX-M 2024 COMBI CONDENS VER",null,{"$f":"D1499+D1502+D1503","v":2395},null,null,"A","A","XL",null,null,null,null,null,"C5"]
[100020013,"GMX-M 2030 COMBI CONDENS HOR",null,{"$f":"D1500+D1501","v":2828},null,null,"A","A","XL",null,null,null,null,null,"C5"]
[100020014,"GMX-M 2030 COMBI CONDENS VER",null,{"$f":"D1500+D1502+D1503","v":2892},null,null,"A","A","XL",null,null,null,null,null,"C5"]
[]
["COMPOSANTS"]
[90864,"GMX-M 2024 CONDENS ","HR64",2034,5,14070,"A","A","XL",8713809255831,39,600,400,510,"C5"]
[90865,"GMX-M 2024 COMBI CONDENS ","HR65",2215,5,14070,"A","A","XL",8713809255848,40,600,400,510,"C5"]
[90866,"GMX-M 2030 COMBI CONDENS ","HR66",2712,5,14070,"A","A","XL",8713809255855,41.5,600,400,510,"C5"]
[100008296,"TERMINAL HORIZONTAL PPS Ø 60/100 MM LG=800 MM","DY871",116,null,null,"/","/","/",3661238168022,2.8,1200,200,200,"C0"]
["S101688","ADAPTATEUR AIR/FUMEES D80/125","HR68",25,null,null,"/","/","/",8713809243722,0.3,175,180,130,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
[]
[100020015,"GMX-M 2024 Condens HOR BM 80",null,{"$f":"D1512+D1513+D1514+D1517+D1518","v":3054},null,null,"A","A","XL",null,91.2,null,null,null,"C5"]
[100020016,"GMX-M 2024 Condens VER BM 80",null,{"$f":"D1512+D1513+D1514+D1517+D1519+D1520","v":3118},null,null,"A","A","XL",null,92.9,null,null,null,"C5"]
[100020017,"GMX-M 2024 Condens HOR OBU 130",null,{"$f":"D1512+D1515+D1516+D1517+D1518","v":3227},null,null,"A","A","XL",null,110.2,null,null,null,"C5"]
[100020018,"GMX-M 2024 Condens VER OBU 130",null,{"$f":"D1511+D1512+D1515+D1516+D1517+D1519+D1520","v":3291},null,null,"A","A","XL",null,111.9,null,null,null,"C5"]
[]
["COMPOSANTS"]
[90864,"GMX-M 2024 CONDENS ","HR64",2034,5,14070,"A","A","XL",8713809255831,39,600,390,520,"C5"]
[100005562,"BALLON JUXTAPOSABLE  BMR 80  ROND","EE53",750,null,null,"/","/","/",3661238092013,48,510,490,1040,"C0"]
[7601255,"KIT DE RACCORDEMENT POUR BMR 80","HR93",107,null,null,"/","/","/",3661238572317,1.6,405,210,110,"C5"]
[89539164,"OBU 130","EE29",958,null,null,"/","/","/",3661238047617,67.5,700,700,980,"C0"]
[7600413,"KIT DE RACCORDEMENT POUR BALLON DE 130 L","HR92",72,null,null,"/","/","/",3661238572324,0.96,400,210,110,"C5"]
[100005661,"SONDE BALLON 5M LONG NTC 12K","AD226",47,0.02,95020,"/","/","/",3661238109452,0.1,140,70,115,"C5"]
[100008296,"TERMINAL HORIZONTAL PPS Ø 60/100 MM LG=800 MM","DY871",116,null,null,"/","/","/",3661238168022,2.8,1200,200,200,"C0"]
["S101688","ADAPTATEUR AIR/FUMEES D80/125","HR68",25,null,null,"/","/","/",8713809243722,0.2,175,180,130,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
[]
[7614687,"GMR 2024 CONDENS HOR FILAIRE",null,{"$f":"D1531+D1534+D1537+D1538+D1539","v":2441},null,null,"A+ avec sonde\next. et int."," /"," /",3661238667952,null,null,null,null,"C5"]
[7614688,"GMR 2024 CONDENS VER FILAIRE",null,{"$f":"D1531+D1535+D1536+D1537+D1538+D1539","v":2505},null,null,"A+ avec sonde\next. et int."," /"," /",3661238667969,null,null,null,null,"C5"]
[7614689,"GMR 2024 COMBI CONDENS HOR FILAIRE",null,{"$f":"D1532+D1534+D1537+D1538+D1539","v":2622},null,null,"A+ avec sonde\next. et int.","A","XL",3661238667976,null,null,null,null,"C5"]
[7614690,"GMR 2024 COMBI CONDENS VER FILAIRE",null,{"$f":"D1532+D1535+D1536+D1537+D1538+D1539","v":2686},null,null,"A+ avec sonde\next. et int.","A","XL",3661238667983,null,null,null,null,"C5"]
[7614691,"GMR 2030 COMBI CONDENS HOR FILAIRE",null,{"$f":"D1533+D1534+D1537+D1538+D1539","v":3119},null,null,"A+ avec sonde\next. et int.","A","XL",3661238668003,null,null,null,null,"C5"]
[7614692,"GMR 2030 COMBI CONDENS VER FILAIRE",null,{"$f":"D1533+D1535+D1536+D1537+D1538+D1539","v":3183},null,null,"A+ avec sonde\next. et int.","A","XL",3661238668010,null,null,null,null,"C5"]
[]
["COMPOSANTS"]
[90864,"GMX-M 2024 CONDENS ","HR64",2034,5,14070,"A"," /"," /",8713809255831,39,600,400,510,"C5"]
[90865,"GMX-M 2024 COMBI CONDENS ","HR65",2215,5,14070,"A","A","XL",8713809255848,40,600,400,510,"C5"]
[90866,"GMX-M 2030 COMBI CONDENS ","HR66",2712,5,14070,"A","A","XL",8713809255855,41.5,600,400,510,"C5"]
[100008296,"TERMINAL HORIZONTAL PPS Ø 60/100 MM LG=800 MM","DY871",116,null,null,"/","/","/",3661238168022,2.8,1200,200,200,"C0"]
["S101688","ADAPTATEUR AIR/FUMEES D80/125","HR68",25,null,null,"/","/","/",8713809243722,0.3,175,180,130,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[7609765,"THERMOSTAT D'AMBIANCE MODULANT FILAIRE RS200 -3","AD306",206,0.12,95010,"/","/","/",8713809266462,0.35099999999999998,150,100,50,"C0"]
["S103361","CACHE TUYAUTERIE","HR72",44,null,null,"/","/","/",8713809260972,0.84,370,370,150,"C0"]
[85757741,"SONDE EXTERIEURE","FM46",41,0.02,95020,"/","/","/",3661238022751,0.12,200,150,40,"C0"]
[]
[]
[7614693,"GMR 2024 CONDENS HOR RADIO",null,{"$f":"D1550+D1553+D1556+D1557+D1558","v":2575},null,null,"A+ avec sonde\next. et int.","/","/",null,null,null,null,null,"C5"]
[7614694,"GMR 2024 CONDENS VER RADIO",null,{"$f":"D1550+D1554+D1555+D1556+D1557+D1558","v":2639},null,null,"A+ avec sonde\next. et int."," /"," /",null,null,null,null,null,"C5"]
[7614695,"GMR 2024 COMBI CONDENS HOR RADIO",null,{"$f":"D1551+D1553+D1556+D1557+D1558","v":2756},null,null,"A+ avec sonde\next. et int.","A","XL",null,null,null,null,null,"C5"]
[7614696,"GMR 2024 COMBI CONDENS VER RADIO",null,{"$f":"D1551+D1554+D1555+D1556+D1557+D1558","v":2820},null,null,"A+ avec sonde\next. et int.","A","XL",null,null,null,null,null,"C5"]
[7614697,"GMR 2030 COMBI CONDENS HOR RADIO",null,{"$f":"D1552+D1553+D1556+D1557+D1558","v":3253},null,null,"A+ avec sonde\next. et int.","A","XL",null,null,null,null,null,"C5"]
[7614698,"GMR 2030 COMBI CONDENS VER RADIO",null,{"$f":"D1552+D1554+D1555+D1556+D1557+D1558","v":3317},null,null,"A+ avec sonde\next. et int.","A","XL",null,null,null,null,null,"C5"]
[]
["COMPOSANTS"]
[90864,"GMX-M 2024 CONDENS ","HR64",2034,5,14070,"A","/","/",8713809255831,39,600,400,510,"C5"]
[90865,"GMX-M 2024 COMBI CONDENS ","HR65",2215,5,14070,"A","A","XL",8713809255848,40,600,400,510,"C5"]
[90866,"GMX-M 2030 COMBI CONDENS ","HR66",2712,5,14070,"A","A","XL",8713809255855,41.5,600,400,510,"C5"]
[100008296,"TERMINAL HORIZONTAL PPS Ø 60/100 MM LG=800 MM","DY871",116,null,null,"/","/","/",3661238168022,2.8,1200,200,200,"C0"]
["S101688","ADAPTATEUR AIR/FUMEES D80/125","HR68",25,null,null,"/","/","/",8713809243722,0.3,175,180,130,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[7609764,"THERMOSTAT D'AMBIANCE MODULANT RADIO RS200 -3R","AD305",340,0.12,95010,"/","/","/",8713809266455,0.76600000000000001,150,100,110,"C0"]
["S103361","CACHE TUYAUTERIE","HR72",44,null,null,"/","/","/",8713809260972,0.84,370,370,150,"C0"]
[85757741,"SONDE EXTERIEURE","FM46",41,0.02,95020,"/","/","/",3661238022751,0.12,200,150,40,"C0"]
[]
[]
[7614699,"GMR 2024 CONDENS HOR FILAIRE BM 80",null,{"$f":"D1567+D1568+D1569+D1572+D1573+D1576+D1577+D1578","v":3345},null,null,"A+ avec sonde\next. et int.","A","XL",null,91.2,null,null,null,"C5"]
[7614700,"GMR 2024 CONDENS VER FILAIRE BM 80",null,{"$f":"D1567+D1568+D1569+D1572+D1574+D1575+D1576+D1577+D1578","v":3409},null,null,"A+ avec sonde\next. et int.","A","XL",null,92.9,null,null,null,"C5"]
[7614701,"GMR 2024 CONDENS HOR FILAIRE OBU 130",null,{"$f":"D1567+D1570+D1571+D1572+D1573+D1576+D1577+D1578","v":3518},null,null,"A+ avec sonde\next. et int.","A","XL",null,110.2,null,null,null,"C5"]
[7614702,"GMR 2024 Condens VER FILAIRE OBU 130",null,{"$f":"D1566+D1567+D1570+D1571+D1572+D1574+D1575+D1576+D1577+D1578","v":3582},null,null,"A+ avec sonde\next. et int.","A","XL",null,111.9,null,null,null,"C5"]
[]
["COMPOSANTS"]
[90864,"GMX-M 2024 CONDENS ","HR64",2034,5,14070,"A","/","/",8713809255831,39,600,390,520,"C5"]
[100005562,"BALLON JUXTAPOSABLE  BMR 80  ROND","EE53",750,null,null,"/","/","/",3661238092013,48,510,490,1040,"C0"]
[7601255,"KIT DE RACCORDEMENT POUR BMR 80","HR93",107,null,null,"/","/","/",3661238572317,1.6,405,210,110,"C5"]
[89539164,"OBU 130","EE29",958,null,null,"/","/","/",3661238047617,67.5,700,700,980,"C0"]
[7600413,"KIT DE RACCORDEMENT POUR BALLON DE 130 L","HR92",72,null,null,"/","/","/",3661238572324,0.96,400,210,110,"C5"]
[100005661,"SONDE BALLON 5M LONG NTC 12K","AD226",47,0.02,95020,"/","/","/",3661238109452,0.1,140,70,115,"C5"]
[100008296,"TERMINAL HORIZONTAL PPS Ø 60/100 MM LG=800 MM","DY871",116,null,null,"/","/","/",3661238168022,2.8,1200,200,200,"C0"]
["S101688","ADAPTATEUR AIR/FUMEES D80/125","HR68",25,null,null,"/","/","/",8713809243722,0.2,175,180,130,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[7609765,"THERMOSTAT D'AMBIANCE MODULANT FILAIRE RS200 -3","AD306",206,0.12,95010,"/","/","/",8713809266462,0.35099999999999998,150,100,50,"C0"]
["S103361","CACHE TUYAUTERIE","HR72",44,null,null,"/","/","/",8713809260972,0.84,370,370,150,"C0"]
[85757741,"SONDE EXTERIEURE","FM46",41,0.02,95020,"/","/","/",3661238022751,0.12,200,150,40,"C0"]
[]
[]
[7614703,"GMR 2024 CONDENS HOR RADIO BM 80",null,{"$f":"D1587+D1588+D1589+D1592+D1593+D1596+D1597+D1598","v":3479},null,null,"A+ avec sonde\next. et int.","A","XL",null,91.2,null,null,null,"C5"]
[7614704,"GMR 2024 CONDENS VER RADIO BM 80",null,{"$f":"D1587+D1588+D1589+D1592+D1594+D1595+D1596+D1597+D1598","v":3543},null,null,"A+ avec sonde\next. et int.","A","XL",null,92.9,null,null,null,"C5"]
[7614705,"GMR 2024 CONDENS HOR RADIO OBU 130",null,{"$f":"D1587+D1590+D1591+D1592+D1593+D1596+D1597+D1598","v":3652},null,null,"A+ avec sonde\next. et int.","A","XL",null,110.2,null,null,null,"C5"]
[7614706,"GMR 2024 CONDENS VER RADIO OBU 130",null,{"$f":"D1586+D1587+D1590+D1591+D1592+D1594+D1595+D1596+D1597+D1598","v":3716},null,null,"A+ avec sonde\next. et int.","A","XL",null,111.9,null,null,null,"C5"]
[]
["COMPOSANTS"]
[90864,"GMX-M 2024 CONDENS ","HR64",2034,5,14070,"A","/","/",8713809255831,39,600,390,520,"C5"]
[100005562,"BALLON JUXTAPOSABLE  BMR 80  ROND","EE53",750,null,null,"/","/","/",3661238092013,48,510,490,1040,"C0"]
[7601255,"KIT DE RACCORDEMENT POUR BMR 80","HR93",107,null,null,"/","/","/",3661238572317,1.6,405,210,110,"C5"]
[89539164,"OBU 130","EE29",958,null,null,"/","/","/",3661238047617,67.5,700,700,980,"C0"]
[7600413,"KIT DE RACCORDEMENT POUR BALLON DE 130 L","HR92",72,null,null,"/","/","/",3661238572324,0.96,400,210,110,"C5"]
[100005661,"SONDE BALLON 5M LONG NTC 12K","AD226",47,0.02,95020,"/","/","/",3661238109452,0.1,140,70,115,"C5"]
[100008296,"TERMINAL HORIZONTAL PPS Ø 60/100 MM LG=800 MM","DY871",116,null,null,"/","/","/",3661238168022,2.8,1200,200,200,"C0"]
["S101688","ADAPTATEUR AIR/FUMEES D80/125","HR68",25,null,null,"/","/","/",8713809243722,0.2,175,180,130,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[7609764,"THERMOSTAT D'AMBIANCE MODULANT RADIO RS200 -3R","AD305",340,0.12,95010,"/","/","/",8713809266455,0.76600000000000001,150,100,110,"C0"]
["S103361","CACHE TUYAUTERIE","HR72",44,null,null,"/","/","/",8713809260972,0.84,370,370,150,"C0"]
[85757741,"SONDE EXTERIEURE","FM46",41,0.02,95020,"/","/","/",3661238022751,0.12,200,150,40,"C0"]
[]
["OPTIONS CHAUDIERES"]
["S103219","CADRE RÉHAUSSEUR ","HR79",123,null,null,"/","/","/",8713809261085,1.9,605,410,170,"C0"]
["S101703","KIT TUBULURE DE RACCORDEMENT POUR CADRE REHAUSSEUR","HR80",107,null,null,"/","/","/",8713809261092,1.2,650,200,130,"C0"]
["S103361","CACHE TUYAUTERIE","HR72",44,null,null,"/","/","/",8713809260972,0.84,370,370,150,"C0"]
["S101711","ADAPTATEUR BI-FLUX   2x80","HR70",30,null,null,"/","/","/",8713809243753,0.22,240,180,180,"C0"]
[100020019,"KIT DE RACCORDEMENT 3CEP Ø 80/125MM","DY921",146,null,null,"/","/","/",3661238571815,2.2000000000000002,650,205,200,"C0"]
[7600374,"DOSSERET DE MONTAGE CHAUFFAGE SEUL","HR75",190,null,null,"/","/","/",8713809261054,2.5499999999999998,350,260,150,"C0"]
[7600371,"DOSSERET DE MONTAGE CHAUDIÈRE MIXTE","HR74",225,null,null,"/","/","/",8713809261047,2,350,260,150,"C0"]
[7600630,"KIT TUBULURE DE RACCORDEMENT NEUF","HR77",45,null,null,"/","/","/",8713809261061,0.4,200,100,50,"C0"]
[7600394,"KIT REMPLACEMENT  A VISSER - C&M NECTRA","HR88",75,null,null,"/","/","/",8713809261108,1.7,320,240,180,"C0"]
[7600407,"KIT REMPLACEMENT  A VISSER - ELM","HR89",75,null,null,"/","/","/",8713809261115,1.5,320,240,180,"C0"]
[7600409,"KIT REMPLACEMENT  A VISSER - C&M CELTIC","HR90",75,null,null,"/","/","/",8713809261122,1.64,320,240,180,"C0"]
[7600410,"KIT REMPLACEMENT  A VISSER - SD","HR91",75,null,null,"/","/","/",8713809261139,1.62,320,240,180,"C0"]
["S101706","POMPE CLASSE A","HR78",258,null,null,"/","/","/",8713809261078,1.18,150,150,125,"C0"]
[7601016,"CACHE TUBULURE POUR KIT DE REMPLACEMENT A VISSER","HR73",67,null,null,"/","/","/",8713809260965,2,375,345,260,"C0"]
["S101690","KIT SONDE TEMPERATURE FUMEE","HR71",67,0.02,95020,"/","/","/",8713809261030,0.1,200,130,50,"C0"]
["S101707","BROSSE DE NETTOYAGE ECHANGEUR","HR81",30,null,null,"/","/","/",8713809259976,0.2,365,290,50,"C0"]
["S101708","KIT DE NETTOYAGE ECHANGEUR A PLAQUES","HR82",235,null,null,"/","/","/",8713809243746,0.9,300,155,140,"C0"]
["S101739","OUTIL DE SERVICE ","HR83",157,0.12,95010,"/","/","/",8713809259952,0.23,180,100,80,"C0"]
[100016399,"KIT DE REMPLACEMENT FLEXIBLE PRINCIPAUX CONCURENTS","HX17",79,null,null,"/","/","/",3661238491441,1.1000000000000001,520,100,55,"C0"]
[7613605,"STATION DE NEUTRALISATION DN1","SA1",344,null,null,"/","/","/",3661238592117,14.5,350,230,350,"C0"]
[7613606,"SUPPORT FIXATION MURAL","SA2",63,null,null,"/","/","/",3661238592124,2.1,300,240,160,"C0"]
[7613609,"STATION DE NEUTRALISATION DN2 ","SA3",603,null,null,"/","/","/",3661238592131,29.5,450,320,400,"C0"]
[85317025,"RECHARGE 2 KG POUR NEUTRALISATION","HC35",140,null,null,"/","/","/",3661238091610,3.7,510,315,190,"C0"]
[100019963,"VENTOUSE HORIZONTALE PPS 60/100 SANS COUDE ","DY920",77,null,null,"/","/","/",3661238571211,2.2999999999999998,1210,265,250,"C0"]
["S101712","COUDE REDUIT POUR VENTOUSE HORIZONTALE","HR67",30,null,null,"/","/","/",8713809243760,0.4,250,200,180,"C0"]
[100020045,"KIT FILTRE FERNOX TF1",null,258,null,null,null,null,null,null,null,null,null,null,"C0"]
[]
["REGULATIONS",null,null,null,null,null,null,null,null,""]
[88017904,"THERMOSTAT AMBIANCE PROGRAMMABLE","AD191",161,0.12,95010,"/","/","/",3661238102415,0.25,135,90,55,"C0"]
[88017010,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (SANS FILS)","AD192",286,0.12,95010,"/","/","/",3661238102439,0.42499999999999999,180,150,90,"C0"]
[85757741,"SONDE EXTERIEURE","FM46",41,0.02,95020,"/","/","/",3661238022751,0.1,200,150,40,"C0"]
[7609764,"THERMOSTAT D'AMBIANCE MODULANT RADIO RS200 -3R","AD305",340,0.12,95010,"/","/","/",8713809266455,0.76600000000000001,150,100,110,"C0"]
[7609765,"THERMOSTAT D'AMBIANCE MODULANT FILAIRE RS200 -3","AD306",206,0.12,95010,"/","/","/",8713809266462,0.35099999999999998,150,100,50,"C0"]
[7612346," COMMANDE A DISTANCE SIMPLIFIEE RS20-OT FILAIRE","AD302",106,0.12,95010,"/","/","/",3661238599666,0.151,109,90,48,"C0"]
[]
["FUMISTERIE"]
[null,"ALU Ø 80 MM"]
[84887600,"TUBE D'INSPECTION Ø 80 mm ","DY600",48,null,null,"/","/","/",3661238013094,0.49,300,145,150,"C0"]
[84887738,"TE DE VISITE Ø 80 mm ","DY738",71,null,null,"/","/","/",3661238011755,0.66,285,215,165,"C0"]
[84887604,"RALLONGE Ø 80 mm    L= 250 mm  (2 PIECES)","DY604",37,null,null,"/","/","/",3661238013056,0.65,255,170,175,"C0"]
[84887605,"RALLONGE Ø 80 mm    L=  500 mm  (2 PIECES)","DY605",45,null,null,"/","/","/",3661238013049,1.26,520,175,170,"C0"]
[84887606,"RALLONGE 1000 mm  (2 PIECES)","DY606",72,null,null,"/","/","/",3661238013032,2.52,1020,175,175,"C0"]
[84887607,"RALLONGE Ø 80 mm    L=  1950 mm   (2 PIECES)","DY607",120,null,null,"/","/","/",3661238013025,5,1985,170,175,"C0"]
[84887608,"COUDE A 90°","DY608",24,null,null,"/","/","/",3661238013018,0.34,155,160,160,"C0"]
[84887609,"COUDE A 45°  (2 PIECES)","DY609",40,null,null,"/","/","/",3661238013001,0.48,200,200,150,"C0"]
[null,"PPS/ALU 60/100"]
[100008296,"TERMINAL HORIZONTAL PPS  Ø 60/100 mm LG = 800 mm","DY871",116,null,null,"/","/","/",3661238168022,2.78,1200,200,200,"C0"]
[100017526,"TERMINAL REFTROFIT Ø 60/95","DY912",115,null,null,"/","/","/",3661238496323,0.9,1200,180,110,"C0"]
[84887681,"PPS-ALU RALLONGE CONCENTRIQUE  ø 60/100 mm L=  500 mm","DY681",41,null,null,"/","/","/",3661238012288,0.72,510,135,140,"C0"]
[84887682,"PPS-ALU RALLONGE CONCENTRIQUE ø 60/100 mm L=1000 mm","DY682",51,null,null,"/","/","/",3661238012271,1.38,1010,130,135,"C0"]
[84887683,"PPS-ALU RALLONGE CONCENTRIQUE ø 60/100mm L=1950mm","DY683",104,null,null,"/","/","/",3661238012264,2.81,1960,150,150,"C0"]
[84887684,"PPS-ALU COUDE CONCENTRIQUE MOULE à 87° ø 60/100 mm","DY684",43,null,null,"/","/","/",3661238012257,0.53,200,200,150,"C0"]
[84887685,"PPS-ALU COUDE CONCENTRIQUE MOULE à 45° ø 60/100 mm (2 PIECES)","DY685",80,null,null,"/","/","/",3661238012240,0.65,250,185,150,"C0"]
[84887686,"PPS-ALU COUDE CONCENTRIQUE MOULE à 30° ø 60/100 mm (2 PIECES)","DY686",159,null,null,"/","/","/",3661238012233,0.63,250,190,155,"C0"]
[84887687,"PPS-ALU COUDE CONCENTRIQUE MOULE à 15° ø 60/100 mm (2 PIECES)","DY687",159,null,null,"/","/","/",3661238012226,0.64,255,195,150,"C0"]
[84887688,"PPS-ALU MANCHON DE COMPENSATION DE 50 à 250 mm","DY688",71,null,null,"/","/","/",3661238012219,0.51,515,135,140,"C0"]
[84887689,"PPS-ALU  PIECE DE REVISIONDROITE  Ø 60/100 mm","DY689",131,null,null,"/","/","/",3661238012202,0.56999999999999995,255,185,150,"C0"]
[84887737,"PPS-ALU  Té DE REVISION  Ø 60/100 mm","DY737",131,null,null,"/","/","/",3661238011762,0.6,255,185,145,"C0"]
[84887702,"KIT DE RACCORDEMENT CHAUDIERE ALU/PPS Ø 60/100 mm","DY702",181,null,null,"/","/","/",3661238012080,1.94,500,290,260,"C0"]
[null,"FLEXIBLE PPS Ø 80"]
[84887716,"KIT N° 3 RACCORDEMENT CHAUDIERE  PPS ø 80/125 mm","DY716",144,null,null,"/","/","/",3661238011953,2.36,500,290,260,"C0"]
[100015325,"KIT N° 1 RACCORDEMENT CHEMINÉE FLEXIBLE PPS Ø 80 mm","DY895",236,null,null,"/","/","/",3661238380110,2.87,395,395,380,"C0"]
[100015327,"TUBE FLEXIBLE LG=12,5M","DY897",354,null,null,"/","/","/",3661238380134,8.6999999999999993,1200,1220,250,"C0"]
[100015326,"TUBE FLEXIBLE LG=50M","DY896",1242,null,null,"/","/","/",3661238380127,35,1600,1660,410,"C0"]
[84887618,"ETOILE DE CENTRAGE POUR FLEXIBLE Ø 80 MM (5 PIÈCES)","DY618",37,null,null,"/","/","/",3661238012912,0.2,300,300,70,"C0"]
[100015328,"PIÈCE DE COUPLAGE FLEXIBLE Ø 80 mm","DY898",71,null,null,"/","/","/",3661238380141,0.25,150,150,150,"C0"]
[100015331,"OUTIL D'AIDE À L'INSERTION Ø 80 mm","DY901",177,null,null,"/","/","/",3661238380172,1.4,300,210,185,"C0"]
[100015330,"PIÈCE D'INSPECTION POUR TUBE FLEXIBLE","DY900",127,null,null,"/","/","/",3661238380165,0.5,295,140,140,"C0"]
[100015329,"TERMINAL AVEC SOLIN FLEX. Ø 80 mm","DY899",177,null,null,"/","/","/",3661238380158,1.74,385,385,250,"C0"]
[100015880,"ADAPTATEUR PPS FLEX Ø 80 mm","DY904",42,null,null,"/","/","/",3661238417632,0.125,316,236,152,"C0"]
[100015881,"ADAPTATEUR PPS  Ø 110","DY905",50,null,null,"/","/","/",3661238417625,1.6,396,296,263,"C0"]
[84887589,"TERMINAL AVEC SOLIN PPS D100-110","DY189",230,null,null,"/","/","/",3661238013100,1.51,390,395,275,"C0"]
[300007172,"GRILLE DE PROTECTION INOX D.90MM",null,null,null,null,"/","/","/",null,null,null,null,null,"P/R"]
[300007173,"GRILLE DE PROTECTION INOX D.120MM",null,null,null,null,null,null,null,null,null,null,null,null,"P/R"]
[null,"CONDUITS 80 PPS"]
[84887701,"KIT  RACCORDEMENT CHEMINEE PPS Ø 60/80 MM ","DY701",270,null,null,"/","/","/",3661238012097,2.83,395,400,385,"C0"]
[100017527,"KIT DE BASE PPS/ALU Ø 80/125 ","DY913",166,null,null,"/","/","/",3661238496330,3.7,600,400,275,"C0"]
[84887717,"KIT N° 1 KIT DE RACCORDEMENT CHEMINEE PPS Ø 80 mm","DY717",157,null,null,"/","/","/",3661238011946,2.89,395,405,390,"C0"]
[84887546,"PIÈCE DE VISITE Ø 80 mm droite","DY146",58,null,null,"/","/","/",3661238013506,0.28999999999999998,300,145,150,"C0"]
[100008301,"COUDE DE REVISION 87° PPS Ø80mm","DY877",41,null,null,"/","/","/",3661238102026,0.24,190,195,145,"C0"]
[84887613,"RALLONGE PPS Ø 80 mm   L= 250 mm (2 PCS)","DY613",40,null,null,"/","/","/",3661238012967,0.37,250,170,175,"C0"]
[84887614,"RALLONGE PPS  Ø 80 mm   L=  500 mm (2 PCS)","DY614",38,null,null,"/","/","/",3661238012950,0.68,500,160,150,"C0"]
[84887615,"RALLONGE PPS  Ø 80 mm   L=  1000 mm (2 PCS)","DY615",51,null,null,"/","/","/",3661238012943,1.25,1000,160,145,"C0"]
[84887550,"RALLONGE PPS Ø 80 mm   L=  2000 mm  (2 PIECES)","DY150",77,null,null,"/","/","/",3661238013469,2.4900000000000002,1960,150,150,"C0"]
[84887552,"COUDE PPS à 90°","DY152",16,null,null,"/","/","/",3661238013445,0.2,255,145,150,"C0"]
[84887554,"COUDE PPS à 45°  (2 PCS)","DY154",35,null,null,"/","/","/",3661238013421,0.32,200,200,150,"C0"]
[84887563,"T PPS  AVEC COUVERCLE D'INSPECTION","DY163",58,null,null,"/","/","/",3661238013353,0.39,290,220,170,"C0"]
[84887551,"COLLIER DE CENTRAGE Ø 80 mm (2 PIECES)","DY151",14,null,null,"/","/","/",3661238013452,0.1,300,300,40,"C0"]
[null,"PPS/ALU 80/125"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 mm NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[100002733,"TERMINAL VERTICAL PPS Ø 80/125 mm ROUGE","DY844",154,null,null,"/","/","/",3661238006614,4.2,1210,265,240,"C0"]
[84887524,"PIECE D'INSPECTION DROITE ALU/PPS Ø 80/125 mm","DY124",110,null,null,"/","/","/",3661238013704,0.55000000000000004,300,145,150,"C0"]
[84887525,"T D'INSPECTION ALU/PPS Ø 80/125 mm","DY125",126,null,null,"/","/","/",3661238013698,0.82,315,235,150,"C0"]
[100008311,"COUDE DE REVISION ALU/PPS Ø 80/125 mm","DY875",115,null,null,"/","/","/",3661238101920,0.68,195,195,145,"C0"]
[84887526,"RALLONGE CONCENTRIQUE ALU/PPS  80/125 L= 250 mm","DY126",41,null,null,"/","/","/",3661238013681,0.47,255,145,150,"C0"]
[84887527,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 L= 500mm","DY127",47,null,null,"/","/","/",3661238013674,0.9,520,140,140,"C0"]
[84887528,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 L=1000 mm","DY128",69,null,null,"/","/","/",3661238013667,1.7,1010,135,140,"C0"]
[84887529,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 L=1950 mm","DY129",120,null,null,"/","/","/",3661238013650,3.5,1960,150,150,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 mm","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[84887532,"COUDE CONCENTRIQUE 45° ALU/PPS Ø 80/125 mm (2 PCES)","DY132",77,null,null,"/","/","/",3661238013629,1,315,235,150,"C0"]
[84887708,"ADAPTATEUR ALU Ø 60/100 MM SUR 80/125 MM","DY708",58,null,null,"/","/","/",3661238012028,0.33,255,145,150,"C0"]
[100011367,"KIT DE TRANSFORMATION 3CE PRESSION ","DY884",40,null,null,"/","/","/",3661238415362,0.15,180,130,15,"C0"]
[null,"Divers"]
[84887411,"SORTIE HORIZONTALE TOIT PENTE DE 30° A 45° ( uniquement pour tuiles mécaniques)","DY11",179,null,null,"/","/","/",3661238013940,3.57,1020,700,370,"C0"]
[84837729,"SORTIE DE TOIT EN PENTE DE 40° A 60° ( uniquement pour tuiles mécaniques)","CX49",178,null,null,"/","/","/",3661238014367,3.5,920,700,320,"C0"]
[84837731,"EMBASE D'ETANCHE TOIT PLAT","CX51",43,null,null,"/","/","/",3661238014343,0.5,400,400,155,"C0"]
[84837121,"TUILE A DOUILLE 5 A 25 NOIRE","CX121",112,null,null,"/","/","/",3661238014428,2.96,510,250,145,"C0"]
[84837732,"TUILE A DOUILLE 25A35' NOIRE","CX52",77,null,null,"/","/","/",3661238014336,3,520,250,145,"C0"]
[84837734,"TUILE A DOUILLE 35 A 55° NOIRE ","CX63",97,null,null,"/","/","/",3661238014312,3.17,510,265,180,"C0"]
[84837120,"TUILE A DOUILLE 5 A 25° ROUGE","CX120",112,null,null,"/","/","/",3661238014435,3.02,515,245,145,"C0"]
[84837783,"TUILE A DOUILLE 25 A 35 ROUGE","CX83",77,null,null,"/","/","/",3661238014213,3,515,250,150,"C0"]
[84837784,"TUILE A DOUILLE 25 A 55 ROUGE","CX84",97,null,null,"/","/","/",3661238014206,2.95,520,265,180,"C0"]
[84837738,"MANCHON DE COMPENS LG 300","CX67",58,null,null,"/","/","/",3661238014275,1,515,135,140,"C0"]
[84837741,"PLATINE DE FINITION INTER","CX72",16,null,null,"/","/","/",3661238014251,0.54,245,210,3,"C0"]
[84887566,"PANIER DE PROTECTION INOX","DY166",80,null,null,"/","/","/",3661238013339,1.38,220,210,200,"C0"]
[84887752,"PLAQUE DE FINITION CHEMINEE ","DY752",36,null,null,"/","/","/",3661238011649,0.2,310,230,140,"C0"]
[]
[]
[7631981,"GMR 1024 CONDENS HOR-2",null,{"$f":"D1729+D1733","v":2226},null,null,"A"," /"," /",3661238635913,null,null,null,null,"C5"]
[7631983,"GMR 1024 CONDENS VER-2",null,{"$f":"D1729+D1735+D1734","v":2320},null,null,"A"," /"," /",3661238636019,null,null,null,null,"C5"]
[7631984,"GMR 1024 COMBI CONDENS HOR-2",null,{"$f":"D1730+D1733","v":2408},null,null,"A","A","XL",3661238636026,null,null,null,null,"C5"]
[7631985,"GMR 1024 COMBI CONDENS VER-2",null,{"$f":"D1730+D1734+D1735","v":2502},null,null,"A","A","XL",3661238636033,null,null,null,null,"C5"]
[7631986,"GMR 1030 COMBI CONDENS HOR-2",null,{"$f":"D1731+D1733","v":2898},null,null,"A","A","XL",3661238636040,null,null,null,null,"C5"]
[7631987,"GMR 1030 COMBI CONDENS VER-2",null,{"$f":"D1731+D1734+D1735","v":2992},null,null,"A","A","XL",3661238636057,null,null,null,null,"C5"]
[7631988,"GMR 1034 COMBI CONDENS HOR-2",null,{"$f":"D1732+D1733","v":3050},null,null,"A","A","XL",3661238636064,null,null,null,null,"C5"]
[7631989,"GMR 1034 COMBI CONDENS VER-2",null,{"$f":"D1732+D1734+D1735","v":3144},null,null,"A","A","XL",3661238636071,null,null,null,null,"C5"]
[]
["COMPOSANTS"]
[7625487,"GMR 1024 CONDENS -2","HG132",2110,5,14070,"A"," /"," /",8713809270605,38,870,450,350,"C5"]
[7625488,"GMR 1024  COMBI CONDENS -2","HG133",2292,5,14070,"A","A","XL",8713809270612,39,870,450,350,"C5"]
[7625489,"GMR 1030 COMBI CONDENS -2","HG134",2782,5,14070,"A","A","XL",8713809270629,41,870,450,350,"C5"]
[7625490,"GMR 1034 COMBI CONDENS -2","HG135",2934,5,14070,"A","A","XL",8713809270636,42,870,450,350,"C5"]
[100008296,"TERMINAL HORIZONTAL PPS  Ø 60/100 mm LG = 800 mm","DY871",116,null,null,"/","/","/",3661238168022,2.78,1200,200,200,"C0"]
["S100465","ADAPTATEUR AIR/FUMEES Ø 80/125","HR38",55,null,null,"/","/","/",3661238369917,1,190,190,130,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 mm NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
["GMR 1000 CONDENS-2 AVEC ECS PAR BALLON SEPARE"]
[7631990,"GMR 1024 CONDENS HOR BM 80-2",null,{"$f":"D1744+D1745+D1746+D1749+D1750","v":3130},null,null,"A","A","XL",3661238636132,null,null,null,null,"C5"]
[7631991,"GMR 1024 CONDENS VER BM 80-2",null,{"$f":"D1744+D1745+D1746+D1749+D1751+D1752","v":3224},null,null,"A","A","XL",3661238636125,null,null,null,null,"C5"]
[7631992,"GMR 1024 CONDENS HOR OBU 130-2",null,{"$f":"D1744+D1747+D1748+D1749+D1750","v":3307},null,null,"A","A","XL",3661238636118,null,null,null,null,"C5"]
[7631993,"GMR 1024 CONDENS VER OBU 130-2",null,{"$f":"D1744+D1747+D1748+D1749+D1751+D1752","v":3401},null,null,"A","A","XL",3661238636101,null,null,null,null,"C5"]
[]
["COMPOSANTS"]
[7625487,"GMR 1024 CONDENS -2","HG132",2110,5,14070,"A"," /"," /",8713809270605,38,870,450,350,"C5"]
[100005562,"BALLON JUXTAPOSABLE  BMR 80  ROND","EE53",750,null,null,"/","/","/",3661238092013,48,510,490,1040,"C0"]
[100011287,"KIT DE RACCORDEMENT BMR 80","HG56",107,null,null,"/","/","/",3661238338371,1.27,400,210,110,"C5"]
[89539164,"OBU 130","EE29",958,null,null,"/","/","/",3661238092112,67.5,700,700,980,"C0"]
[100011288,"KIT DE RACCORDEMENT POUR BALLON DE 130 L","HG57",76,null,null,"/","/","/",3661238338388,0.76,400,210,110,"C5"]
[100005661,"SONDE BALLON 5M LONG NTC 12K","AD226",47,0.02,95020,"/","/","/",3661238109452,0.15,140,70,115,"C5"]
[100008296,"TERMINAL HORIZONTAL PPS  Ø 60/100 mm LG = 800 mm","DY871",116,null,null,"/","/","/",3661238168022,2.78,1200,200,200,"C0"]
["S100465","ADAPTATEUR AIR/FUMEES Ø 80/125","HR38",55,null,null,"/","/","/",3661238369917,1,190,190,130,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 mm NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
[]
[7631994,"GMR 1024 CS CONDENS HOR-2",null,{"$f":"SUM(D1760+D1759)","v":3209},null,null,"A","A","XL",3661238636095,null,null,null,null,"C5"]
[7631995,"GMR 1024 CS CONDENS VER-2",null,{"$f":"D1759+D1762+D1763","v":3303},null,null,"A","A","XL",3661238636088,null,null,null,null,"C5"]
[]
["COMPOSANTS"]
[7625453,"GMR 1024  CS CONDENS-2","HG150",3093,5,14070,"A","A","XL",3661238630932,75,680,1150,630,"C5"]
[100008296,"TERMINAL HORIZONTAL PPS Ø 60/100 mm LG=800 mm","DY871",116,null,null,"/","/","/",3661238168022,2.78,1200,200,200,"C0"]
[84887708,"ADAPTATEUR ALU Ø 60/100 MM SUR 80/125 MM","DY708",58,null,null,"/","/","/",3661238012028,0.33,255,145,150,"C0"]
["S100465","ADAPTATEUR AIR/FUMEES Ø 80/125","HR38",55,null,null,"/","/","/",3661238369917,1,190,190,130,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 mm NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
["OPTIONS"]
[100005628,"CADRE REHAUSSEUR","HG19",180,null,null,"/","/","/",3661238109513,5.0999999999999996,715,425,145,"C0"]
[100009391,"KIT  TUYAUX POUR CADRE REHAUSSEUR 16/18","HG43",95,null,null,"/","/","/",3661238338302,0.69,365,270,30,"C0"]
[100014501,"DOSSERET REHAUSSE 80MM ","HG104",158,null,null,"/","/","/",3661238378926,3.9,715,420,115,"C0"]
[100005630,"CACHE TUYAUTERIE","HG21",55,null,null,"/","/","/",3661238109490,0.77,420,230,55,"C0"]
[100005637,"KIT COLLECTEUR D'ECOULEMENT","HG28",48,null,null,"/","/","/",3661238109476,0.36,305,160,140,"C0"]
[100005825,"ADAPTATEUR BI-FLUX   2x80","DY868",64,null,null,"/","/","/",3661238162204,0.42,310,160,140,"C0"]
[100011289,"DOSSERET DE MONTAGE SEPARE AVEC DISCONECTEUR POUR CHAUFFAGE SEUL (POUR prémontage)","HG58",359,null,null,"/","/","/",3661238338319,5.5,720,430,140,"C0"]
[100011290,"DOSSERET DE MONTAGE SEPARE AVEC DISCONECTEUR POUR CHAUDIERE MIXTE (POUR PREMONTAGE)","HG59",317,null,null,"/","/","/",3661238338326,6,null,null,null,"C0"]
[100005824,"BRULEUR PROPANE POUR 34/39 kW","HG31",121,null,null,"/","/","/",3661238162211,0.52,305,160,140,"C0"]
[7613605,"STATION DE NEUTRALISATION DN1","SA1",344,null,null,"/","/","/",3661238592117,14.5,350,230,350,"C0"]
[7613606,"SUPPORT FIXATION MURAL","SA2",63,null,null,"/","/","/",3661238592124,2.1,300,240,160,"C0"]
[85317025,"RECHARGE 2 KG POUR NEUTRALISATION","HC35",140,null,null,"/","/","/",3661238091610,3.65,510,315,190,"C0"]
[100009334,"KIT DE REMPLACEMENT GMR 1000 A VISSER ELM","HG36",79,null,null,"/","/","/",3661238338333,1.35,410,210,120,"C0"]
[100009335,"KIT  REMPLAC A VISSER GMR 1000 SAUNIER DUVAL","HG37",79,null,null,"/","/","/",3661238338340,1.34,410,210,120,"C0"]
[100009336,"KIT  REMPLAC A VISSER GMR 1000 C &M Nectra","HG38",79,null,null,"/","/","/",3661238338357,1.49,410,210,120,"C0"]
[100009337,"KIT  REMPLAC A VISSER GMR 1000 C &M Celtic","HG39",79,null,null,"/","/","/",3661238338364,1.19,410,210,120,"C0"]
[100013114,"KIT  REMP. A VIS. SAUNIER DUV (avec rattrap sortie ventouse) ","HG97",79,null,null,"/","/","/",3661238363144,1.45,410,210,120,"C0"]
[100013115,"KIT  REMP. A VIS. C&M CELTIC (avec rattrap sortie ventouse) ","HG98",79,null,null,"/","/","/",3661238362246,1.41,410,210,120,"C0"]
[100014110,"KIT  REMP. A VIS. ELM GVM720  (avec rattrap sortie ventouse) ","HG99",79,null,null,"/","/","/",3661238369177,1.1299999999999999,410,210,120,"C0"]
[100012812,"CACHE TUBULURES","HG94",71,null,null,"/","/","/",3661238361416,2,420,420,200,"C0"]
[100011367,"KIT DE TRANSFORMATION 3CE PRESSION","DY884",40,null,null,"/","/","/",3661238415362,0.15,180,130,15,"C0"]
[100009893,"KIT DE CONVERSION PROPANE GMR 1000","HG44",14,null,null,"/","/","/",3661238339910,0.02,220,140,10,"C0"]
[100011888,"VENT. HORIZ. RECENTRE Ø 60/100 ","DY885",156,null,null,"/","/","/",3661238374959,2.86,1170,190,195,"C0"]
[100013303,"VENT. HORIZ. RECENTRE/REH Ø 60/100 (rehaussé)","DY886",156,null,null,"/","/","/",3661238368095,1.9,1015,190,190,"C0"]
[]
["REGULATIONS "]
[88017904,"THERMOSTAT AMBIANCE PROGRAMMABLE","AD191",161,0.12,95010,"/","/","/",3661238102415,0.25,135,90,55,"C0"]
[88017010,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (SANS FILS)","AD192",286,0.12,95010,"/","/","/",3661238102439,0.42499999999999999,180,150,90,"C0"]
[100005660,"SONDE EXTERIEURE RH","AD225",48,0.02,95020,"/","/","/",3661238109469,0.11,140,70,115,"C0"]
[7609764,"THERMOSTAT D'AMBIANCE MODULANT RADIO RS200 -3R","AD305",340,0.12,95010,"/","/","/",8713809266455,0.76600000000000001,150,100,110,"C0"]
[7609765,"THERMOSTAT D'AMBIANCE MODULANT FILAIRE RS200 -3","AD306",206,0.12,95010,"/","/","/",8713809266462,0.35099999999999998,150,100,50,"C0"]
[7612346," COMMANDE A DISTANCE SIMPLIFIEE RS20-OT FILAIRE","AD302",106,0.12,95010,"/","/","/",3661238599666,0.151,109,90,48,"C0"]
[]
["OPTIONS CHAUDIERES"]
[100009391,"KIT TUBULURE DE RACCORDEMENT POUR CADRE RÉHAUSSEUR","HG43",95,null,null,"/","/","/",3661238338302,0.69,365,270,30,"C0"]
[100005825,"ADAPTATEUR BI-FLUX   2x80","DY868",64,null,null,"/","/","/",3661238162204,0.42,310,160,140,"C0"]
[100009893,"KIT DE CONVERSION PROPANE GMR 1000","HG44",15,null,null,"/","/","/",3661238339910,0.02,220,140,10,"C0"]
[7613605,"STATION DE NEUTRALISATION DN1","SA1",344,null,null,"/","/","/",3661238592117,14.5,350,230,350,"C0"]
[7613606,"SUPPORT FIXATION MURAL","SA2",63,null,null,"/","/","/",3661238592124,2.1,300,240,160,"C0"]
[85317025,"RECHARGE 2 KG POUR NEUTRALISATION","HC35",140,null,null,"/","/","/",3661238091610,3.65,510,315,190,"C0"]
[100020045,"KIT FILTRE FERNOX TF1",null,258,null,null,"/","/","/",null,null,null,null,null,"C0"]
[]
["OPTIONS SPECIFIQUES"]
[117422,"CADRE RÉHAUSSEUR POUR MCR BIC","HG75",201,null,null,"/","/","/",3661238350960,7,1070,690,160,"C0"]
[117433,"CACHE TUYAUTERIE MCR BIC","HG76",71,null,null,"/","/","/",3661238350977,1.3,650,380,170,"C0"]
[117167,"VASE D'EXPANSION SANITAIRE","HG77",97,null,null,"/","/","/",3661238350953,1.5,310,210,130,"C0"]
[]
["FUMISTERIE"]
[null,"ALU/ALU  Ø 60/100 mm "]
[100016485,"TERMINAL HORIZONTAL D60/100 L800 ","DY908",97,null,null,null,null,null,3661238494619,3,1000,160,155,"C0"]
[84887735,"TERMINAL VERTICAL D80/125 NOIR ","DY735",167,null,null,null,null,null,3661238011786,5,1350,255,290,"C0"]
[84887736,"TERMINAL VERTICAL D80/125 ROUGE","DY736",167,null,null,null,null,null,3661238011779,5,1350,255,290,"C0"]
[84887746,"RALLONGE LG 250 mm ","DY746",36,null,null,"/","/","/",3661238011687,0.49,260,145,150,"C0"]
[84887652,"RALLONGE ALU Ø 60/100 L 500MM","DY652",43,null,null,"/","/","/",3661238012578,0.96,515,135,140,"C0"]
[84887653,"RALLONGE CONCENTRIQUE Ø 60/100 mm  L1000 mm ","DY653",58,null,null,"/","/","/",3661238012561,1.86,1020,135,140,"C0"]
[84887654,"RALLONGE CONCENTRIQUE Ø 60/100 mm  L 1950 mm ","DY654",108,null,null,"/","/","/",3661238012554,3.66,1960,150,150,"C0"]
[84887655,"COUDE ALU 87° Ø  60/100 ","DY655",44,null,null,"/","/","/",3661238012547,0.69,200,200,150,"C0"]
[84887656,"2 COUDES 45°  ALU Ø  60/100 ","DY656",83,null,null,"/","/","/",3661238012530,0.83,255,185,150,"C0"]
[84887659,"MANCHON DE COMPENSATION DE 50 A 250 mm ","DY659",62,null,null,"/","/","/",3661238012509,0.83,510,135,140,"C0"]
[84887660,"TE DE VISITE Ø 60/100 mm ","DY660",140,null,null,"/","/","/",3661238012493,0.85,500,405,160,"C0"]
[100016487,"RECUPERATEUR CONDENSATS 60/100 ","DY910",93,null,null,null,null,null,3661238494633,0.66,320,240,155,"C0"]
[100016488,"RACCORD 3CE (C42) D60/100 L250 ","DY911",100,null,null,null,null,null,3661238494640,1.67,510,160,155,"C0"]
[300007172,"GRILLE DE PROTECTION INOX D.90MM",null,"CPR",null,null,null,null,null,3661238123632,0.19,15,15,16,"P/R"]
[null,"ALU Ø 80 MM"]
[84887600,"TUBE D'INSPECTION Ø 80 mm ","DY600",48,null,null,"/","/","/",3661238013094,0.49,300,145,150,"C0"]
[84887738,"TE DE VISITE Ø 80 mm ","DY738",71,null,null,"/","/","/",3661238011755,0.66,285,215,165,"C0"]
[84887604,"RALLONGE Ø 80 mm    L= 250 mm  (2 PIECES)","DY604",37,null,null,"/","/","/",3661238013056,0.65,255,170,175,"C0"]
[84887605,"RALLONGE Ø 80 mm    L=  500 mm  (2 PIECES)","DY605",45,null,null,"/","/","/",3661238013049,1.26,520,175,170,"C0"]
[84887606,"RALLONGE 1000 mm  (2 PIECES)","DY606",72,null,null,"/","/","/",3661238013032,2.52,1020,175,175,"C0"]
[84887607,"RALLONGE Ø 80 mm    L=  1950 mm   (2 PIECES)","DY607",120,null,null,"/","/","/",3661238013025,5,1985,170,175,"C0"]
[84887608,"COUDE A 90°","DY608",24,null,null,"/","/","/",3661238013018,0.34,155,160,160,"C0"]
[84887609,"COUDE A 45°  (2 PIECES)","DY609",40,null,null,"/","/","/",3661238013001,0.48,200,200,150,"C0"]
[null,"ALU/ALU Ø 80/125 mm"]
[84837735,"RALLONGE LG 250mm ","CX64",44,null,null,"/","/","/",3661238014305,0.61,255,145,150,"C0"]
[84837736,"RALLONGE LG 500 mm ","CX65",50,null,null,"/","/","/",3661238014299,1.18,510,135,140,"C0"]
[84837737,"RALLONGE LG 1000 mm ","CX66",75,null,null,"/","/","/",3661238014282,2.2999999999999998,1020,130,140,"C0"]
[84837793,"RALLONGE CONCENTRIQUE 80/125 L=1950 mm ","CX93",144,null,null,"/","/","/",3661238014169,4.5599999999999996,1960,150,150,"C0"]
[84837738,"MANCHON DE COMPENS LG 300","CX67",58,null,null,"/","/","/",3661238014275,1,515,135,140,"C0"]
[84837743,"COUDE 87'VENT.VERT80/125mm ","CX76",74,null,null,"/","/","/",3661238014244,0.82,200,200,145,"C0"]
[84837739,"2 COUDES 45 °","CX68",113,null,null,"/","/","/",3661238014268,1.24,315,235,150,"C0"]
[100016486,"RECUPERATEUR COND 60/100 80/125 ","DY909",90,null,null,null,null,null,3661238494626,1.26,290,220,170,"C0"]
[84887460,"KIT D'INSTALLATION MONTAGE EXT.  ","DY60",376,null,null,null,null,null,3661238013810,5.16,590,400,410,"C0"]
[null,"PPS/ALU 60/100"]
[100008296,"TERMINAL HORIZONTAL PPS  Ø 60/100 mm LG = 800 mm","DY871",116,null,null,"/","/","/",3661238168022,2.78,1200,200,200,"C0"]
[100017526,"TERMINAL REFTROFIT Ø 60/95","DY912",115,null,null,"/","/","/",3661238496323,0.9,1200,180,110,"C0"]
[84887681,"PPS-ALU RALLONGE CONCENTRIQUE  ø 60/100 mm L=  500 mm","DY681",41,null,null,"/","/","/",3661238012288,0.72,510,135,140,"C0"]
[84887682,"PPS-ALU RALLONGE CONCENTRIQUE ø 60/100 mm L=1000 mm","DY682",51,null,null,"/","/","/",3661238012271,1.38,1010,130,135,"C0"]
[84887683,"PPS-ALU RALLONGE CONCENTRIQUE ø 60/100mm L=1950mm","DY683",104,null,null,"/","/","/",3661238012264,2.81,1960,150,150,"C0"]
[84887684,"PPS-ALU COUDE CONCENTRIQUE MOULE à 87° ø 60/100 mm","DY684",43,null,null,"/","/","/",3661238012257,0.53,200,200,150,"C0"]
[84887685,"PPS-ALU COUDE CONCENTRIQUE MOULE à 45° ø 60/100 mm (2 PIECES)","DY685",80,null,null,"/","/","/",3661238012240,0.65,250,185,150,"C0"]
[84887686,"PPS-ALU COUDE CONCENTRIQUE MOULE à 30° ø 60/100 mm (2 PIECES)","DY686",159,null,null,"/","/","/",3661238012233,0.63,250,190,155,"C0"]
[84887687,"PPS-ALU COUDE CONCENTRIQUE MOULE à 15° ø 60/100 mm (2 PIECES)","DY687",159,null,null,"/","/","/",3661238012226,0.64,255,195,150,"C0"]
[84887688,"PPS-ALU MANCHON DE COMPENSATION DE 50 à 250 mm","DY688",71,null,null,"/","/","/",3661238012219,0.51,515,135,140,"C0"]
[84887689,"PPS-ALU  PIECE DE REVISIONDROITE  Ø 60/100 mm","DY689",131,null,null,"/","/","/",3661238012202,0.56999999999999995,255,185,150,"C0"]
[84887737,"PPS-ALU  Té DE REVISION  Ø 60/100 mm","DY737",131,null,null,"/","/","/",3661238011762,0.6,255,185,145,"C0"]
[84887702,"KIT DE RACCORDEMENT CHAUDIERE ALU/PPS Ø 60/100 mm","DY702",181,null,null,"/","/","/",3661238012080,1.94,500,290,260,"C0"]
[null,"FLEXIBLE PPS Ø 80"]
[84887716,"KIT N° 3 RACCORDEMENT CHAUDIERE  PPS ø 80/125 mm","DY716",144,null,null,"/","/","/",3661238011953,2.36,500,290,260,"C0"]
[100015325,"KIT N° 1 RACCORDEMENT CHEMINÉE FLEXIBLE PPS Ø 80 mm","DY895",236,null,null,"/","/","/",3661238380110,2.87,395,395,380,"C0"]
[100015327,"TUBE FLEXIBLE LG=12,5M","DY897",354,null,null,"/","/","/",3661238380134,8.6999999999999993,1200,1220,250,"C0"]
[100015326,"TUBE FLEXIBLE LG=50M","DY896",1242,null,null,"/","/","/",3661238380127,35,1600,1660,410,"C0"]
[84887618,"ETOILE DE CENTRAGE POUR FLEXIBLE Ø 80 MM (5 PIÈCES)","DY618",37,null,null,"/","/","/",3661238012912,0.2,300,300,70,"C0"]
[100015328,"PIÈCE DE COUPLAGE FLEXIBLE Ø 80 mm","DY898",71,null,null,"/","/","/",3661238380141,0.25,150,150,150,"C0"]
[100015331,"OUTIL D'AIDE À L'INSERTION Ø 80 mm","DY901",177,null,null,"/","/","/",3661238380172,1.4,300,210,185,"C0"]
[100015330,"PIÈCE D'INSPECTION POUR TUBE FLEXIBLE","DY900",127,null,null,"/","/","/",3661238380165,0.5,295,140,140,"C0"]
[100015329,"TERMINAL AVEC SOLIN FLEX. Ø 80 mm","DY899",177,null,null,"/","/","/",3661238380158,1.74,385,385,250,"C0"]
[100015318,"ADAPTATEUR PPS D80M-110F","DY902",52,null,null,"/","/","/",3661238379909,0.25,150,150,150,"C0"]
[100015880,"ADAPTATEUR PPS FLEX Ø 80 mm","DY904",42,null,null,"/","/","/",3661238417632,0.125,316,236,152,"C0"]
[100015881,"ADAPTATEUR PPS  Ø 110","DY905",50,null,null,"/","/","/",3661238417625,1.6,396,296,263,"C0"]
[null,"CONDUITS 80 PPS"]
[84887701,"KIT  RACCORDEMENT CHEMINEE PPS Ø 60/80 MM ","DY701",270,null,null,"/","/","/",3661238012097,2.83,395,400,385,"C0"]
[100017527,"KIT DE BASE PPS/ALU Ø 80/125 ","DY913",166,null,null,"/","/","/",3661238496330,3.7,600,400,275,"C0"]
[84887717,"KIT N° 1 KIT DE RACCORDEMENT CHEMINEE PPS Ø 80 mm","DY717",157,null,null,"/","/","/",3661238011946,2.89,395,405,390,"C0"]
[84887546,"PIÈCE DE VISITE Ø 80 mm droite","DY146",58,null,null,"/","/","/",3661238013506,0.28999999999999998,300,145,150,"C0"]
[100008301,"COUDE DE REVISION 87° PPS Ø80mm","DY877",41,null,null,"/","/","/",3661238102026,0.24,190,195,145,"C0"]
[84887613,"RALLONGE PPS Ø 80 mm   L= 250 mm (2 PCS)","DY613",40,null,null,"/","/","/",3661238012967,0.37,250,170,175,"C0"]
[84887614,"RALLONGE PPS  Ø 80 mm   L=  500 mm (2 PCS)","DY614",38,null,null,"/","/","/",3661238012950,0.68,500,160,150,"C0"]
[84887615,"RALLONGE PPS  Ø 80 mm   L=  1000 mm (2 PCS)","DY615",51,null,null,"/","/","/",3661238012943,1.25,1000,160,145,"C0"]
[84887550,"RALLONGE PPS Ø 80 mm   L=  2000 mm  (2 PIECES)","DY150",77,null,null,"/","/","/",3661238013469,2.4900000000000002,1960,150,150,"C0"]
[84887552,"COUDE PPS à 90°","DY152",16,null,null,"/","/","/",3661238013445,0.2,255,145,150,"C0"]
[84887554,"COUDE PPS à 45°  (2 PCS)","DY154",35,null,null,"/","/","/",3661238013421,0.32,200,200,150,"C0"]
[84887563,"T PPS  AVEC COUVERCLE D'INSPECTION","DY163",58,null,null,"/","/","/",3661238013353,0.39,290,220,170,"C0"]
[84887551,"COLLIER DE CENTRAGE Ø 80 mm (2 PIECES)","DY151",14,null,null,"/","/","/",3661238013452,0.1,300,300,40,"C0"]
[null,"PPS/ALU 80/125"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 mm NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[100002733,"TERMINAL VERTICAL PPS Ø 80/125 mm ROUGE","DY844",154,null,null,"/","/","/",3661238006614,4.2,1210,265,240,"C0"]
[84887524,"PIECE D'INSPECTION DROITE ALU/PPS Ø 80/125 mm","DY124",110,null,null,"/","/","/",3661238013704,0.55000000000000004,300,145,150,"C0"]
[84887525,"T D'INSPECTION ALU/PPS Ø 80/125 mm","DY125",126,null,null,"/","/","/",3661238013698,0.82,315,235,150,"C0"]
[100008311,"COUDE DE REVISION ALU/PPS Ø 80/125 mm","DY875",115,null,null,"/","/","/",3661238101920,0.68,195,195,145,"C0"]
[84887526,"RALLONGE CONCENTRIQUE ALU/PPS  80/125 L= 250 mm","DY126",41,null,null,"/","/","/",3661238013681,0.47,255,145,150,"C0"]
[84887527,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 L= 500mm","DY127",47,null,null,"/","/","/",3661238013674,0.9,520,140,140,"C0"]
[84887528,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 L=1000 mm","DY128",69,null,null,"/","/","/",3661238013667,1.7,1010,135,140,"C0"]
[84887529,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 L=1950 mm","DY129",120,null,null,"/","/","/",3661238013650,3.5,1960,150,150,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 mm","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[84887532,"COUDE CONCENTRIQUE 45° ALU/PPS Ø 80/125 mm (2 PCES)","DY132",77,null,null,"/","/","/",3661238013629,1,315,235,150,"C0"]
[84887708,"ADAPTATEUR ALU Ø 60/100 MM SUR 80/125 MM","DY708",58,null,null,"/","/","/",3661238012028,0.33,255,145,150,"C0"]
[100011367,"KIT DE TRANSFORMATION 3CE PRESSION ","DY884",40,null,null,"/","/","/",3661238415362,0.15,180,130,15,"C0"]
[null,"Divers"]
[84887411,"SORTIE HORIZONTALE TOIT PENTE DE 30° A 45° ( uniquement pour tuiles mécaniques)","DY11",179,null,null,"/","/","/",3661238013940,3.57,1020,700,370,"C0"]
[84837729,"SORTIE DE TOIT EN PENTE DE 40° A 60° ( uniquement pour tuiles mécaniques)","CX49",178,null,null,"/","/","/",3661238014367,3.5,920,700,320,"C0"]
[84837731,"EMBASE D'ETANCHE TOIT PLAT","CX51",43,null,null,"/","/","/",3661238014343,0.5,400,400,155,"C0"]
[84837121,"TUILE A DOUILLE 5 A 25 NOIRE","CX121",112,null,null,"/","/","/",3661238014428,2.96,510,250,145,"C0"]
[84837732,"TUILE A DOUILLE 25A35' NOIRE","CX52",77,null,null,"/","/","/",3661238014336,3,520,250,145,"C0"]
[84837734,"TUILE A DOUILLE 35 A 55° NOIRE ","CX63",97,null,null,"/","/","/",3661238014312,3.17,510,265,180,"C0"]
[84837120,"TUILE A DOUILLE 5 A 25° ROUGE","CX120",112,null,null,"/","/","/",3661238014435,3.02,515,245,145,"C0"]
[84837783,"TUILE A DOUILLE 25 A 35 ROUGE","CX83",77,null,null,"/","/","/",3661238014213,3,515,250,150,"C0"]
[84837784,"TUILE A DOUILLE 25 A 55 ROUGE","CX84",97,null,null,"/","/","/",3661238014206,2.95,520,265,180,"C0"]
[84837738,"MANCHON DE COMPENS LG 300","CX67",58,null,null,"/","/","/",3661238014275,1,515,135,140,"C0"]
[84837741,"PLATINE DE FINITION INTER","CX72",16,null,null,"/","/","/",3661238014251,0.54,245,210,3,"C0"]
[84887566,"PANIER DE PROTECTION INOX","DY166",80,null,null,"/","/","/",3661238013339,1.38,220,210,200,"C0"]
[84887752,"PLAQUE DE FINITION CHEMINEE ","DY752",36,null,null,"/","/","/",3661238011649,0.2,310,230,140,"C0"]
[]
[]
[100014281,"GMR 3015 Condens HOR  ",null,{"$f":"D1944+D1953","v":3127},null,null,"A","/","/",3661238554337,null,null,null,null,"C0"]
[100014283,"GMR 3015 CondensVER ",null,{"$f":"D1944+D1954+D1955","v":3150},null,null,"A","/","/",3661238554344,null,null,null,null,"C0"]
[100014284,"GMR 3025 Condens HOR",null,{"$f":"D1945+D1953","v":3307},null,null,"A","/","/",3661238554351,null,null,null,null,"C0"]
[100014286,"GMR 3025 Condens VER",null,{"$f":"D1945+D1954+D1955","v":3330},null,null,"A","/","/",3661238554368,null,null,null,null,"C0"]
[100014287,"GMR 3025 Combi Condens HOR",null,{"$f":"+D1946+D1953","v":3384},null,null,"A","A","XL",3661238554375,null,null,null,null,"C0"]
[100014288,"GMR 3025 Combi Condens VER",null,{"$f":"D1946+D1954+D1955","v":3407},null,null,"A","A","XL",3661238554382,null,null,null,null,"C0"]
[100014289,"GMR 3025 CS Condens HOR",null,{"$f":"D1947+D1953","v":4335},null,null,"A","A","XL",3661238554399,null,null,null,null,"C0"]
[100014290,"GMR 3025 CS Condens VER",null,{"$f":"D1947+D1954+D1955","v":4358},null,null,"A","A","XL",3661238554405,null,null,null,null,"C0"]
[100014292,"GMR 3035 Condens HOR",null,{"$f":"D1948+D1953","v":3549},null,null,"A","/","/",3661238554412,null,null,null,null,"C0"]
[100014293,"GMR 3035 Condens VER",null,{"$f":"D1948+D1954+D1955","v":3572},null,null,"A","/","/",3661238554429,null,null,null,null,"C0"]
[]
[100014294,"GMR 3015 Condens HOR BS 60 ",null,{"$f":"D1944+D1949+D1950+D1953","v":4169},null,null,"A","A","XL",3661238554436,null,null,null,null,"C0"]
[100014295,"GMR 3015 Condens VER BS 60",null,{"$f":"D1944+D1949+D1950+D1954+D1955","v":4192},null,null,"A","A","XL",3661238554450,null,null,null,null,"C0"]
[100014296,"GMR 3015 Condens HOR OBU 130",null,{"$f":"D1944+D1951+D1952+D1953+D1956","v":4253},null,null,"A","A","XL",3661238554467,null,null,null,null,"C0"]
[100014297,"GMR 3015 Condens  VER OBU 130",null,{"$f":"D1944+D1951+D1952+D1954+D1955+D1956","v":4276},null,null,"A","A","XL",3661238554474,null,null,null,null,"C0"]
[100014298,"GMR 3025 Condens HOR BS 60 ",null,{"$f":"D1945+D1949+D1950+D1953","v":4349},null,null,"A","A","XL",3661238554481,null,null,null,null,"C0"]
[100014299,"GMR 3025 Condens VER BS 60",null,{"$f":"D1945+D1949+D1950+D1954+D1955","v":4372},null,null,"A","A","XL",3661238554498,null,null,null,null,"C0"]
[100014300,"GMR 3025 Condens HOR OBU 130",null,{"$f":"D1945+D1951+D1952+D1953+D1956","v":4433},null,null,"A","A","XL",3661238554504,null,null,null,null,"C0"]
[100014301,"GMR 3025 Condens  VER OBU 130",null,{"$f":"D1945+D1951+D1952+D1954+D1955+D1956","v":4456},null,null,"A","A","XL",3661238554511,null,null,null,null,"C0"]
[100014302,"GMR 3035 Condens HOR BS 60 ",null,{"$f":"D1948+D1949+D1950+D1953","v":4591},null,null,"A","A","XL",3661238554528,null,null,null,null,"C0"]
[100014303,"GMR 3035 Condens VER BS 60",null,{"$f":"D1948+D1949+D1950+D1954+D1955","v":4614},null,null,"A","A","XL",3661238554535,null,null,null,null,"C0"]
[100014304,"GMR 3035 Condens HOR OBU 130",null,{"$f":"D1948+D1951+D1952+D1953+D1956","v":4675},null,null,"A","A","XL",3661238554542,null,null,null,null,"C0"]
[100014305,"GMR 3035 Condens  VER OBU 130",null,{"$f":"D1948+D1951+D1952+D1954+D1955+D1956","v":4698},null,null,"A","A","XL",3661238554559,null,null,null,null,"C0"]
[]
["COMPOSANTS"]
[100013631,"GMR 3015 Condens","HR23",2940,5,14070,"A","/","/",3661238368958,40,930,530,470,"C0"]
[100013632,"GMR 3025 Condens","HR24",3120,5,14070,"A","/","/",3661238368972,40,930,530,470,"C0"]
[100013630,"GMR 3025 Combi Condens","HR22",3197,5,14070,"A","A","XL",3661238368965,40,930,530,470,"C0"]
[100013634,"GMR 3025 CS Condens","HR26",4148,5,14070,"A","A","XL",3661238414860,86,1120,700,550,"C0"]
[100013633,"GMR 3035 Condens","HR25",3362,5,14070,"A","/","/",3661238414853,40,930,520,460,"C0"]
[100013755,"BS 60","EE54",917,null,null,"/","/","/",3661238365889,50,515,515,905,"C0"]
[100013746,"KIT DE LIAISON BS 60","EA138",125,null,null,"/","/","/",3661238365803,0.85,700,100,160,"C0"]
[89539164,"OBU 130","EE29",958,null,null,"/","/","/",3661238092112,67.5,700,700,980,"C0"]
[100013532,"KIT DE LIAISON OBU130/GMR 3000 ","EA137",119,null,null,"/","/","/",3661238364462,0.8,700,100,160,"C0"]
[100013756,"TERMINAL HORIZONTAL PPS/GALVA Ø 60/100 mm","HR48",187,null,null,"/","/","/",3661238370883,3.37,1200,200,200,"C0"]
["S100465","ADAPTATEUR AIR/FUMEES Ø 80/125","HR38",55,null,null,"/","/","/",3661238369917,1,190,190,130,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 mm NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.16,200,150,30,"C0"]
[]
["OPTIONS CHAUDIERES"]
[100005825,"ADAPTATEUR BI-FLUX   2x80","DY868",64,null,null,"/","/","/",3661238162204,0.42,310,160,140,"C0"]
["S100465","ADAPTATEUR AIR/FUMEES Ø 80/125","HR38",55,null,null,"/","/","/",3661238369917,1,190,190,130,"C0"]
["S100675","CADRE REHAUSSEUR","HR39",206,null,null,"/","/","/",3661238368217,6,840,455,175,"C0"]
[" S101239","CADRE REHAUSSEURPOUR GMR 3025 CS CONDENS","HR50",237,null,null,"/","/","/",3661238377523,10,1100,640,180,"C0"]
["S100935","KIT TUBULURE POUR CADRE REHAUSSEUR FR","HR40",86,null,null,"/","/","/",3661238368224,1.3,400,320,90,"C0"]
["S100676","CACHE TUBULURE","HR42",55,null,null,"/","/","/",3661238369924,1.5,460,350,175,"C0"]
["S101205","CACHE TUBULURE POUR GMR 3025 CS CONDENS ","HR52",75,null,null,"/","/","/",3661238377547,1.44,610,380,175,"C0"]
["S100310","THERMOSTAT FUMEE","HR43",68,0.02,95020,"/","/","/",3661238369931,0.1,180,130,30,"C0"]
["S101232","THERMOSTAT FUMEE POUR GMR 3025 CS CONDENS","HR53",69,0.02,95020,"/","/","/",3661238377554,0.1,200,120,30,"C0"]
["S100761","OUIL DE NETTOYAGE ECHANGEUR A PLAQUES","HR44",113,null,null,"/","/","/",3661238368255,0.28000000000000003,170,170,40,"C0"]
["S100931","OUTIL DE NETTOYAGE CORPS CHAUDIERE","HR45",86,null,null,"/","/","/",3661238369948,0.73,310,320,160,"C0"]
[7613605,"STATION DE NEUTRALISATION DN1","SA1",344,null,null,"/","/","/",3661238592117,14.5,350,230,350,"C0"]
[7613606,"SUPPORT FIXATION MURAL","SA2",63,null,null,"/","/","/",3661238592124,2.1,300,240,160,"C0"]
[85317025,"RECHARGE 2 KG POUR NEUTRALISATION","HC35",140,null,null,"/","/","/",3661238091610,3.65,510,315,190,"C0"]
[100020164,"COLLECTEUR 2/3 CIRCUITS ","EA140",348,null,null,"/","/","/",3661238575011,6.6,660,180,200,"C0"]
[100020165,"CONSOLE MUR COLLECTEUR ","EA141",44,null,null,"/","/","/",3661238575028,1.2,220,125,70,"C0"]
[100020166,"CONSOLE MUR 1 MODULE ","EA142",116,null,null,"/","/","/",3661238575035,1.6,220,125,70,"C0"]
[100020167,"CIRCUIT DIRECT P.ELEC CLASSE A  ","EA143",644,0.83,14050,"/","/","/",3661238575042,5.0999999999999996,460,270,235,"C0"]
[100020168,"CIRCUIT V3V P.ELEC","EA144",916,0.83,14050,"/","/","/",3661238575059,6,460,270,235,"C0"]
[100020169,"MODULE HYDR COMPACT 2 CIRCUITS HEE","EA145",1146,0.83,14050,"/","/","/",3661238575066,9,525,415,210,"C0"]
[89557009,"KIT DE TRANSFORMATION G/R 3/4 '' ET 1 ''","BH84",32,null,null,"/","/","/",3661238047563,0.32500000000000001,200,140,45,"C0"]
[7613605,"STATION DE NEUTRALISATION DN1","SA1",344,null,null,"/","/","/",3661238592117,14.5,350,230,350,"C0"]
[7613606,"SUPPORT FIXATION MURAL","SA2",63,null,null,"/","/","/",3661238592124,2.1,300,240,160,"C0"]
[85317025,"RECHARGE 2 KG POUR NEUTRALISATION","HC35",140,null,null,"/","/","/",3661238091610,3.65,510,315,190,"C0"]
[100020045,"KIT FILTRE FERNOX TF1",null,258,null,null,"/","/","/",null,null,null,null,null,"C0"]
[]
["OPTIONS REGULATIONS"]
[100013304,"COLIS OPTION V3V OE-TRONIC 4","AD249",158,0.12,95010,"/","/","/",3661238363519,0.42,260,170,130,"C0"]
[100013305,"COLIS SONDE SYSTÈME OE-TRONIC 4","AD250",46,0.02,95020,"/","/","/",3661238363588,0.13400000000000001,150,210,25,"C0"]
[100013306,"SONDE EXTERIEURE RADIO ","AD251",77,0.12,95010,"/","/","/",3661238363595,0.15,150,210,40,"C0"]
[100013307,"MODULE CHAUDIERE RADIO (EMETTEUR)","AD252",123,0.12,95010,"/","/","/",3661238363601,0.32,260,160,130,"C0"]
[100013472,"CDE A DISTANCE RADIO RS 400R     ","AD255",238,0.12,95010,"/","/","/",3661238364233,0.253,175,122,60,"C0"]
[100013477,"CDE A DISTANCE FILAIRE RS 400   ","AD257",177,0.12,95010,"/","/","/",3661238364257,0.253,175,122,60,"C0"]
[88017851,"CABLE DE LIAISON BUS LG 12 M","AD134",110,0.02,95020,"/","/","/",3661238048850,0.37,350,260,30,"C0"]
[88017878,"MODULE DE TELESURVEILLANCE VOCAL TELCOM 2","AD152",704,0.12,95010,"/","/","/",3661238048751,1.05,210,190,105,"C0"]
[88017017,"SONDE DEPART v3v","AD199",80,0.02,95020,"/","/","/",3661238049185,0.21,150,200,40,"C0"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.16,200,150,30,"C0"]
["S103303","MODULE DE COMMANDE 2 CIRCUITS ","AD290",415,0.12,95010,"/","/","/",3661238549517,1.73,420,305,85,"C0"]
[]
["FUMISTERIE"]
[null,"ALU Ø 80 MM"]
[84887600,"TUBE D'INSPECTION Ø 80 mm ","DY600",48,null,null,"/","/","/",3661238013094,0.49,300,145,150,"C0"]
[84887738,"TE DE VISITE Ø 80 mm ","DY738",71,null,null,"/","/","/",3661238011755,0.66,285,215,165,"C0"]
[84887604,"RALLONGE Ø 80 mm    L= 250 mm  (2 PIECES)","DY604",37,null,null,"/","/","/",3661238013056,0.65,255,170,175,"C0"]
[84887605,"RALLONGE Ø 80 mm    L=  500 mm  (2 PIECES)","DY605",45,null,null,"/","/","/",3661238013049,1.26,520,175,170,"C0"]
[84887606,"RALLONGE 1000 mm  (2 PIECES)","DY606",72,null,null,"/","/","/",3661238013032,2.52,1020,175,175,"C0"]
[84887607,"RALLONGE Ø 80 mm    L=  1950 mm   (2 PIECES)","DY607",120,null,null,"/","/","/",3661238013025,5,1985,170,175,"C0"]
[84887608,"COUDE A 90°","DY608",24,null,null,"/","/","/",3661238013018,0.34,155,160,160,"C0"]
[84887609,"COUDE A 45°  (2 PIECES)","DY609",40,null,null,"/","/","/",3661238013001,0.48,200,200,150,"C0"]
[84887681,"PPS-ALU RALLONGE CONCENTRIQUE  ø 60/100 mm L=  500 mm","DY681",41,null,null,"/","/","/",3661238012288,0.72,510,135,140,"C0"]
[84887682,"PPS-ALU RALLONGE CONCENTRIQUE ø 60/100 mm L=1000 mm","DY682",51,null,null,"/","/","/",3661238012271,1.38,1010,130,135,"C0"]
[84887683,"PPS-ALU RALLONGE CONCENTRIQUE ø 60/100mm L=1950mm","DY683",104,null,null,"/","/","/",3661238012264,2.81,1960,150,150,"C0"]
[84887684,"PPS-ALU COUDE CONCENTRIQUE MOULE à 87° ø 60/100 mm","DY684",43,null,null,"/","/","/",3661238012257,0.53,200,200,150,"C0"]
[84887685,"PPS-ALU COUDE CONCENTRIQUE MOULE à 45° ø 60/100 mm (2 PIECES)","DY685",80,null,null,"/","/","/",3661238012240,0.65,250,185,150,"C0"]
[84887686,"PPS-ALU COUDE CONCENTRIQUE MOULE à 30° ø 60/100 mm (2 PIECES)","DY686",159,null,null,"/","/","/",3661238012233,0.63,250,190,155,"C0"]
[84887687,"PPS-ALU COUDE CONCENTRIQUE MOULE à 15° ø 60/100 mm (2 PIECES)","DY687",159,null,null,"/","/","/",3661238012226,0.64,255,195,150,"C0"]
[84887688,"PPS-ALU MANCHON DE COMPENSATION DE 50 à 250 mm","DY688",71,null,null,"/","/","/",3661238012219,0.51,515,135,140,"C0"]
[84887689,"PPS-ALU  PIECE DE REVISIONDROITE  Ø 60/100 mm","DY689",131,null,null,"/","/","/",3661238012202,0.56999999999999995,255,185,150,"C0"]
[84887737,"PPS-ALU  Té DE REVISION  Ø 60/100 mm","DY737",131,null,null,"/","/","/",3661238011762,0.6,255,185,145,"C0"]
[84887702,"KIT DE RACCORDEMENT CHAUDIERE ALU/PPS Ø 60/100 mm","DY702",181,null,null,"/","/","/",3661238012080,1.94,500,290,260,"C0"]
[null,"FLEXIBLE PPS Ø 80"]
[84887716,"KIT N° 3 RACCORDEMENT CHAUDIERE  PPS ø 80/125 mm","DY716",144,null,null,"/","/","/",3661238011953,2.36,500,290,260,"C0"]
[100015325,"KIT N° 1 RACCORDEMENT CHEMINÉE FLEXIBLE PPS Ø 80 mm","DY895",236,null,null,"/","/","/",3661238380110,2.87,395,395,380,"C0"]
[100015327,"TUBE FLEXIBLE LG=12,5M","DY897",354,null,null,"/","/","/",3661238380134,8.6999999999999993,1200,1220,250,"C0"]
[100015326,"TUBE FLEXIBLE LG=50M","DY896",1242,null,null,"/","/","/",3661238380127,35,1600,1660,410,"C0"]
[84887618,"ETOILE DE CENTRAGE POUR FLEXIBLE Ø 80  mm (2 PIÈCES)","DY618",37,null,null,"/","/","/",3661238012912,0.2,300,300,70,"C0"]
[100015328,"PIÈCE DE COUPLAGE FLEXIBLE Ø 80 mm","DY898",71,null,null,"/","/","/",3661238380141,0.25,150,150,150,"C0"]
[100015331,"OUTIL D'AIDE À L'INSERTION Ø 80 mm","DY901",177,null,null,"/","/","/",3661238380172,1.4,300,210,185,"C0"]
[100015330,"PIÈCE D'INSPECTION POUR TUBE FLEXIBLE","DY900",127,null,null,"/","/","/",3661238380165,0.5,295,140,140,"C0"]
[100015329,"TERMINAL AVEC SOLIN FLEX. Ø 80 mm","DY899",177,null,null,"/","/","/",3661238380158,1.74,385,385,250,"C0"]
[null,"CONDUITS 80 PPS"]
[84887701,"KIT  RACCORDEMENT CHEMINEE PPS Ø 60/80 MM ","DY701",270,null,null,"/","/","/",3661238012097,2.83,395,400,385,"C0"]
[100017527,"KIT DE BASE PPS/ALU Ø 80/125 ","DY913",166,null,null,"/","/","/",3661238496330,3.7,600,400,275,"C0"]
[84887717,"KIT N° 1 KIT DE RACCORDEMENT CHEMINEE PPS Ø 80 mm","DY717",157,null,null,"/","/","/",3661238011946,2.89,395,405,390,"C0"]
[84887546,"PIÈCE DE VISITE Ø 80 mm droite","DY146",58,null,null,"/","/","/",3661238013506,0.28999999999999998,300,145,150,"C0"]
[100008301,"COUDE DE REVISION 87° PPS Ø80mm","DY877",41,null,null,"/","/","/",3661238102026,0.24,190,195,145,"C0"]
[84887613,"RALLONGE PPS Ø 80 mm   L= 250 mm (2 PCS)","DY613",40,null,null,"/","/","/",3661238012967,0.37,250,170,175,"C0"]
[84887614,"RALLONGE PPS  Ø 80 mm   L=  500 mm (2 PCS)","DY614",38,null,null,"/","/","/",3661238012950,0.68,500,160,150,"C0"]
[84887615,"RALLONGE PPS  Ø 80 mm   L=  1000 mm (2 PCS)","DY615",51,null,null,"/","/","/",3661238012943,1.25,1000,160,145,"C0"]
[84887550,"RALLONGE PPS Ø 80 mm   L=  2000 mm  (2 PIECES)","DY150",77,null,null,"/","/","/",3661238013469,2.4900000000000002,1960,150,150,"C0"]
[84887552,"COUDE PPS à 90°","DY152",16,null,null,"/","/","/",3661238013445,0.2,255,145,150,"C0"]
[84887554,"COUDE PPS à 45°  (2 PCS)","DY154",35,null,null,"/","/","/",3661238013421,0.32,200,200,150,"C0"]
[84887563,"T PPS  AVEC COUVERCLE D'INSPECTION","DY163",58,null,null,"/","/","/",3661238013353,0.39,290,220,170,"C0"]
[84887551,"COLLIER DE CENTRAGE Ø 80 mm (2 PIECES)","DY151",14,null,null,"/","/","/",3661238013452,0.1,300,300,40,"C0"]
[null,"PPS/ALU 80/125"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 mm NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[100002733,"TERMINAL VERTICAL PPS Ø 80/125 mm ROUGE","DY844",154,null,null,"/","/","/",3661238006614,4.2,1210,265,240,"C0"]
[84887524,"PIECE D'INSPECTION DROITE ALU/PPS Ø 80/125 mm","DY124",110,null,null,"/","/","/",3661238013704,0.55000000000000004,300,145,150,"C0"]
[84887525,"T D'INSPECTION ALU/PPS Ø 80/125 mm","DY125",126,null,null,"/","/","/",3661238013698,0.82,315,235,150,"C0"]
[100008311,"COUDE DE REVISION ALU/PPS Ø 80/125 mm","DY875",115,null,null,"/","/","/",3661238101920,0.68,195,195,145,"C0"]
[84887526,"RALLONGE CONCENTRIQUE ALU/PPS  80/125 L= 250 mm","DY126",41,null,null,"/","/","/",3661238013681,0.47,255,145,150,"C0"]
[84887527,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 L= 500mm","DY127",47,null,null,"/","/","/",3661238013674,0.9,520,140,140,"C0"]
[84887528,"RALLONGECONCENTRIQUE ALU/PPS 80/125 L=1000 mm","DY128",69,null,null,"/","/","/",3661238013667,1.7,1010,135,140,"C0"]
[84887529,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 L=1950 mm","DY129",120,null,null,"/","/","/",3661238013650,3.5,1960,150,150,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 mm","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[84887532,"COUDE CONCENTRIQUE 45° ALU/PPS Ø 80/125 mm (2 PCES)","DY132",77,null,null,"/","/","/",3661238013629,1,315,235,150,"C0"]
[84887708,"ADAPTATEUR ALU Ø 60/100 MM SUR 80/125 MM","DY708",58,null,null,"/","/","/",3661238012028,0.33,255,145,150,"C0"]
[100014000,"KIT DE RACCORDEMENT 3CEP Ø 80/125mm","DY887",151,null,null,"/","/","/",3661238368989,2.0499999999999998,625,215,225,"C0"]
[null,"Divers"]
[84887411,"SORTIE HORIZONTALE TOIT PENTE DE 30° A 45° ( uniquement pour tuiles mécaniques)","DY11",179,null,null,"/","/","/",3661238013940,3.57,1020,700,370,"C0"]
[84837729,"SORTIE DE TOIT EN PENTE DE 40° A 60° ( uniquement pour tuiles mécaniques)","CX49",178,null,null,"/","/","/",3661238014367,3.5,920,700,320,"C0"]
[84837731,"EMBASE D'ETANCHE TOIT PLAT","CX51",43,null,null,"/","/","/",3661238014343,0.5,400,400,155,"C0"]
[84837121,"TUILE A DOUILLE 5 A 25 NOIRE","CX121",112,null,null,"/","/","/",3661238014428,2.96,510,250,145,"C0"]
[84837732,"TUILE A DOUILLE 25 A 35 NOIRE","CX52",77,null,null,"/","/","/",3661238014336,3,520,250,145,"C0"]
[84837734,"TUILE A DOUILLE 35 A 55° NOIRE ","CX63",97,null,null,"/","/","/",3661238014312,3.17,510,265,180,"C0"]
[84837120,"TUILE A DOUILLE 5 A 25° ROUGE","CX120",112,null,null,"/","/","/",3661238014435,3.02,515,245,145,"C0"]
[84837783,"TUILE A DOUILLE 25 A 35 ROUGE","CX83",77,null,null,"/","/","/",3661238014213,3,515,250,150,"C0"]
[84837784,"TUILE A DOUILLE 25 A 55 ROUGE","CX84",97,null,null,"/","/","/",3661238014206,2.95,520,265,180,"C0"]
[84837738,"MANCHON DE COMPENS LG 300","CX67",58,null,null,"/","/","/",3661238014275,1,515,135,140,"C0"]
[84837741,"PLATINE DE FINITION INTER","CX72",17,null,null,"/","/","/",3661238014251,0.54,245,210,3,"C0"]
[84887566,"PANIER DE PROTECTION INOX","DY166",80,null,null,"/","/","/",3661238013339,1.38,220,210,200,"C0"]
[]
[]
[100016211,"GMR 5045 CONDENS OE-CONTROL",null,{"$f":"D2082+D2086","v":3824},null,null,"A","/","/",3661238419926,null,null,null,null,"C0"]
[100016212,"GMR 5065 CONDENS OE-CONTROL",null,{"$f":"D2083+D2086","v":4439},null,null,"A","/","/",3661238419933,null,null,null,null,"C0"]
[100016213,"GMR 5090 CONDENS OE-CONTROL",null,{"$f":"D2084+D2086","v":6411},null,null,"Pas concerné par l'étiquetage",null,null,3661238419940,null,null,null,null,"C0"]
[100016214,"GMR 5115 CONDENS OE-CONTROL",null,{"$f":"D2085+D2086","v":7449},null,null,"Pas concerné par l'étiquetage",null,null,3661238419957,null,null,null,null,"C0"]
[100016215,"GMR 5045 CONDENS OE-TRONIC4",null,{"$f":"D2082+D2087","v":3988},null,null,"A","/","/",3661238419964,null,null,null,null,"C0"]
[100016216,"GMR 5065 CONDENS OE-TRONIC4",null,{"$f":"D2083+D2087","v":4603},null,null,"A","/","/",3661238419971,null,null,null,null,"C0"]
[100016217,"GMR 5090 CONDENS OE-TRONIC4",null,{"$f":"D2084+D2087","v":6575},null,null,"Pas concerné par l'étiquetage",null,null,3661238419988,null,null,null,null,"C0"]
[100016218,"GMR 5115 CONDENS OE-TRONIC4",null,{"$f":"D2085+D2087","v":7613},null,null,"Pas concerné par l'étiquetage",null,null,3661238419995,null,null,null,null,"C0"]
[]
["COMPOSANTS"]
[90547,"GMR 5045 CONDENS","HC226",3696,3.34,"11.14","A","/","/",3661238419728,61,1120,550,400,"C0"]
[90548,"GMR 5065 CONDENS","HC227",4311,3.34,"11.14","A","/","/",3661238419735,68,1120,550,400,"C0"]
[90549,"GMR 5090 CONDENS","HC228",6283,3.34,"11.14","Pas concerné par l'étiquettage",null,null,3661238419742,74,1120,550,480,"C0"]
[90550,"GMR 5115 CONDENS","HC229",7321,3.34,"11.14","Pas concerné par l'étiquettage",null,null,3661238419759,74,1120,550,480,"C0"]
[100016093,"HMI OE-CONTROL","AD271",128,null,null,"/","/","/",3661238418424,0.3,190,140,125,"C0"]
[100016095,"HMI OE-TRONIC4","AD273",292,null,null,"/","/","/",3661238418448,0.36,190,140,125,"C0"]
[]
["OPTIONS REGULATIONS"]
[null,"Œ-TRONIC 4"]
[100013304,"COLIS OPTION V3V OE-TRONIC 4","AD249",158,0.12,95010,"/","/","/",3661238363519,0.42,260,170,130,"C0"]
[100013305,"COLIS SONDE SYSTÈME OE-TRONIC 4","AD250",46,0.02,95020,"/","/","/",3661238363588,0.13400000000000001,150,210,25,"C0"]
[100013306,"SONDE EXTERIEURE RADIO ","AD251",77,0.12,95010,"/","/","/",3661238363595,0.15,150,210,40,"C0"]
[100013307,"MODULE CHAUDIERE RADIO (EMETTEUR)","AD252",123,0.12,95010,"/","/","/",3661238363601,0.32,260,160,130,"C0"]
[100013472,"CDE A DISTANCE RADIO RS 400R     ","AD255",238,0.12,95010,"/","/","/",3661238364233,0.253,175,122,60,"C0"]
[100013477,"CDE A DISTANCE FILAIRE RS 400   ","AD257",177,0.12,95010,"/","/","/",3661238364257,0.253,175,122,60,"C0"]
[88017851,"CABLE DE LIAISON BUS LG 12 M","AD134",110,0.02,95020,"/","/","/",3661238048850,0.37,350,260,30,"C0"]
[88017878,"MODULE DE TELESURVEILLANCE VOCAL TELCOM 2","AD152",704,0.12,95010,"/","/","/",3661238048751,1.05,210,190,105,"C0"]
[88017017,"SONDE DEPART v3v","AD199",80,0.02,95020,"/","/","/",3661238049185,0.21,150,200,40,"C0"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.16,200,150,30,"C0"]
[100005130,"SONDE POUR BALLON TAMPON ","AD216",95,0.02,95020,"/","/","/",3661238001855,0.26,210,170,35,"C0"]
["S101477","INTERFACE SCU-X03","HC258",124,0.12,95010,"/","/","/",3661238508415,0.55000000000000004,230,120,105,"C0"]
[null,"Œ-CONTROL"]
[88017838,"SONDE EXTERIEURE AF 40","AD122",83,0.02,95020,"/","/","/",3661238048898,0.1,200,150,50,"C0"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.16,200,150,30,"C0"]
[]
["OPTIONS ECS"]
[100007827,"KIT LIAISON CHAUDIERE / BALLON","EA121",602,null,null,"/","/","/",3661238116528,6.5,600,500,135,"C0"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.16,200,150,30,"C0"]
["OPTIONS "]
[100002310,"KIT DE RACCORDEMENT HYDRAULIQUE FRANCE GMR 5065 ET 5090 ","HC139",333,null,null,"/","/","/",3661238007604,4.0999999999999996,310,215,130,"C0"]
["S101539","CACHE TUBULURE","HC242",62,null,null,"/","/","/",3661238420090,2,510,390,260,"C0"]
[111920,"ISOLATION RACCORDEMENT CHAUDIÈRE","HC214",68,null,null,"/","/","/",3661238338838,0.41,530,470,250,"C0"]
[122441,"ISOLATION ARRIERE KIT DE RACCORDEMENT HYDRAULIQUE","HC252",68,null,null,"/","/","/",3661238509597,0.55000000000000004,530,255,470,"C0"]
[123182,"ISOLATION ARRIERE RACCORDEMENT CHAUDIÈRE","HC243",10,null,null,"/","/","/",3661238494411,0.39,940,540,8,"C0"]
["S100310","THERMOSTAT FUMEE","HR43",68,0.02,95020,"/","/","/",3661238369931,0.1,180,130,30,"C0"]
[84887768,"ADAPTATEUR  80 X 100MM ","DY768",55,null,null,"/","/","/",3661238011489,0.24,150,145,155,"C0"]
["S100762","ADAPTATEUR BIFLUX 2 X 80mm","DY906",64,null,null,"/","/","/",8713809218959,0.7,320,210,260,"C0"]
["S101626","ADAPTATEUR BIFLUX 2 X 100MM","DY907",74,null,null,"/","/","/",3661238420106,1.6,320,210,260,"C0"]
[100004641,"ROBINET GAZ 3/4\" DROIT","HC158",44,null,null,"/","/","/",3661238002432,0.82,200,150,125,"C0"]
[100002313,"POMPE GMR 5045 ELECTRONIQUE","HC142",324,null,null,"/","/","/",3661238007574,3.1,310,210,130,"C0"]
[7630016,"POMPE ERP 65-90-115 KW ","SA13",405,null,null,"/","/","/",3661238630727,3,null,null,null,"C0"]
[100002323,"POMPE PRIMAIRE POUR GMR 5045-5065-5090","HC147",354,null,null,"/","/","/",3661238007499,4.5999999999999996,310,210,130,"C0"]
[85317005,"VANNE TROIS VOIES AVEC MOTEUR 1\"","HC15",387,null,null,"/","/","/",3661238091696,2.36,265,170,120,"C0"]
[100019346,"BOUTEILLE DE DECOUPLAGE  60/60-1''  ","GV45",366,null,null,"/","/","/",3661238555013,3.83,690,375,205,"C0"]
[100019347,"BOUTEILLE DE DECOUPLAGE  80/60-1'' 1/4 ","GV46",438,null,null,"/","/","/",3661238555020,5.42,690,375,205,"C0"]
[100019348,"BOUTEILLE DE DECOUPLAGE  120/80-2''   ","GV47",589,null,null,"/","/","/",3661238555037,11.96,970,375,205,"C0"]
["S101463","RAIL DE MONTAGE CHAUDIERE GMR 5000 SUR SYSTEME CASCADE MC","HC245",49,null,null,"/","/","/",3661238420113,1.6,560,290,10,"C0"]
["S101655","FILTRE GAZ Ø 50 mm","HC255",518,null,null,"/","/","/",8713809234331,4.9000000000000004,465,280,230,"C0"]
[7613605,"STATION DE NEUTRALISATION DN1","SA1",344,null,null,"/","/","/",3661238592117,14.5,350,230,350,"C0"]
[7613606,"SUPPORT FIXATION MURAL","SA2",63,null,null,"/","/","/",3661238592124,2.1,300,240,160,"C0"]
[85317025,"RECHARGE 2 KG POUR NEUTRALISATION","HC35",140,null,null,"/","/","/",3661238091610,3.65,510,315,190,"C0"]
[83877009,"SYSTEME DE NEUTRALISATION DES CONDENSATS (avec pompe de relevage)","DU13",914,null,null,"/","/","/",3661238015081,15,350,230,360,"C0"]
[83877011,"STATION NEUTRALISATION","DU15",1354,null,null,"/","/","/",3661238015067,20,660,455,270,"C0"]
[100019369,"POMPE MOD UPM2 15-70 RES CLASSE A  J","JA44",235,null,null,"/","/","/",3661238563810,1.8,215,155,155,"C0"]
[100005002,"PANIER DE PROTECTION INOX  Ø 80/125","DY865",176,null,null,"/","/","/",3661238001886,2.59,275,270,270,"C0"]
[100005004,"PANIER DE PROTECTION INOX D100/150","DY866",179,null,null,"/","/","/",3661238001879,3.1,305,310,270,"C0"]
["S52484","OUTIL DE NETTOYAGE POUR GMR 5045 -5065 (L= 360 mm)","HC246",84,null,null,"/","/","/",3661238382466,0.17399999999999999,50,3,3,"C0"]
["S58286","OUTIL DE NETTOYAGE POUR GMR 5090 - 5115 (L=460 mm)","HC247",88,null,null,"/","/","/",8713809017453,0.18,725,35,50,"C0"]
[94225601,"RECHARGE DE GRANULATS DE NEUTRALISATION 10 KG**","CPR",null,null,null,"/","/","/",3661238075597,10,25,25,21.5,"P/R"]
[100018981,"RECUPERATEUR DE CONDENSATS  Ø 80/125 mm PPs/Alu","DY916",55,null,null,"/","/","/",3661238547711,0.86,200,200,150,"C0"]
[100018983,"RECUPERATEUR DE CONDENSATS  Ø 110 mm PPs","DY917",64,null,null,"/","/","/",3661238547728,0.31,400,400,275,"C0"]
[100018984,"RECUPERATEUR DE CONDENSATS  Ø 110/150 mm PPs/Alu","DY918",114,null,null,"/","/","/",3661238547735,0.76,260,170,180,"C0"]
[100018985,"RECUPERATEUR DE CONDENSATS  Ø 80 mm PPs","DY919",34,null,null,"/","/","/",3661238547742,0.18,260,145,150,"C0"]
["S101614","POMPE CHAUFFAGE EEI UPM2 25-70 130MM",null,303,null,null,"/","/","/",8713809243432,5,300,150,130,"C0"]
[7608398,"POMPE CHAUFFAGE UPML 25-115 130 MM",null,392,null,null,"/","/","/",8713809264796,3.4,305,155,140,"C0"]
[7606393,"VANNE GAS S GMR 5090 PROPANE",null,null,null,null,"/","/","/",null,null,null,null,null,"P/R"]
[]
["MONTAGE MURAL (LW)"]
["SYSTÈME DE CASCADE POUR 2 CHAUDIÈRES"]
[null,"LW.0080kW.2000",null,null,null,null,"Pas concerné par l'étiquettage"]
[null,"LW.0122kW.0200",null,null,null,null,"Pas concerné par l'étiquettage"]
[null,"LW.0168kW.0020",null,null,null,null,"Pas concerné par l'étiquettage"]
[null,"LW.0214kW.0002",null,null,null,null,"Pas concerné par l'étiquettage"]
["SYSTÈME DE CASCADE POUR 3 CHAUDIÈRES"]
[null,"LW.0120kW.3000",null,null,null,null,"Pas concerné par l'étiquettage"]
[null,"LW.0183kW.0300",null,null,null,null,"Pas concerné par l'étiquettage"]
[null,"LW.0252kW.0030",null,null,null,null,"Pas concerné par l'étiquettage"]
[null,"LW.0321kW.0003",null,null,null,null,"Pas concerné par l'étiquettage"]
["SYSTÈME DE CASCADE POUR 4 CHAUDIÈRES"]
[null,"LW.0160kW.4000",null,null,null,null,"Pas concerné par l'étiquettage"]
[null,"LW.0244kW.0400",null,null,null,null,"Pas concerné par l'étiquettage"]
[null,"LW.0336kW.0040",null,null,null,null,"Pas concerné par l'étiquettage"]
[null,"LW.0428kW.0004",null,null,null,null,"Pas concerné par l'étiquettage"]
["ALIGNEMENT AU SOL (LV)"]
["SYSTÈME DE CASCADE POUR 2 CHAUDIÈRES"]
[null,"LV.0080kW.2000",null,null,null,null,"Pas concerné par l'étiquettage"]
[null,"LV.0122kW.0200",null,null,null,null,"Pas concerné par l'étiquettage"]
[null,"LV.0168kW.0020",null,null,null,null,"Pas concerné par l'étiquettage"]
[null,"LV.0214kW.0002",null,null,null,null,"Pas concerné par l'étiquettage"]
["SYSTÈME DE CASCADE POUR 3 CHAUDIÈRES"]
[null,"LV.0120kW.3000",null,null,null,null,"Pas concerné par l'étiquettage"]
[null,"LV.0183kW.0300",null,null,null,null,"Pas concerné par l'étiquettage"]
[null,"LV.0252kW.0030",null,null,null,null,"Pas concerné par l'étiquettage"]
[null,"LV.0321kW.0003",null,null,null,null,"Pas concerné par l'étiquettage"]
["SYSTÈME DE CASCADE POUR 4 CHAUDIÈRES"]
[null,"LV.0160kW.4000",null,null,null,null,"Pas concerné par l'étiquettage"]
[null,"LV.0244kW.0400",null,null,null,null,"Pas concerné par l'étiquettage"]
[null,"LV.0336kW.0040",null,null,null,null,"Pas concerné par l'étiquettage"]
[null,"LV.0428kW.0004",null,null,null,null,"Pas concerné par l'étiquettage"]
[]
["COMPOSANTS DE BASE DES CASCADES"]
[120918,"CHASSIS DE MONTAGE GMR 5000","HC248",93,null,null,"/","/","/",3661238420120,5.5,500,660,65,"C0"]
[120842,"MONTANT-SUPPORT L GMR 5000","HC249",142,null,null,"/","/","/",3661238420137,6,1500,450,50,"C0"]
[120900,"MONTANT-SUPPORT I GMR 5000","HC250",89,null,null,"/","/","/",3661238420144,4.5,1500,50,50,"C0"]
[90777,"COLLECTEUR DN65 - 2 CHAUDIERES ","HC259",662,null,null,"/","/","/",3661238553019,61,1200,500,640,"C0"]
[90778,"COLLECTEUR DN65 - 3 CHAUDIERES ","HC260",896,null,null,"/","/","/",3661238553026,77,1705,500,640,"C0"]
[111688,"RAIL DE MONTAGE MURAL 2 CHAUDIÈRES ","HC192",43,null,null,"/","/","/",3661238339002,1.32,970,80,50,"C0"]
[111689,"RAIL DE MONTAGE MURAL 3 CHAUDIÈRES ","HC193",50,null,null,"/","/","/",3661238338999,2.0699999999999998,1500,80,50,"C0"]
[111690,"RAIL DE MONTAGE MURAL 4 CHAUDIÈRES ","HC194",66,null,null,"/","/","/",3661238338982,2.72,2030,800,50,"C0"]
[111708,"JEU DE BOUCHONS ","HC195",41,null,null,"/","/","/",3661238338937,0.67,200,130,30,"C0"]
[111701,"BRIDES PLEINES EAU DN65","HC198",148,null,null,"/","/","/",3661238338951,4.83,370,170,50,"C0"]
[114311,"BOUTEILLE DE DÉCOUPLAGE DN65 < 350 kW","HC222",617,null,null,"/","/","/",3661238362215,26.6,660,170,310,"C0"]
[111712,"BOUTEILLE DE DÉCOUPLAGE DN65","HC200",1024,null,null,"/","/","/",3661238338920,46.5,900,630,160,"C0"]
[111022,"KIT DE RACCORDEMENT AVANT FR + BE","HC202",605,null,null,"/","/","/",3661238339057,7.39,450,315,150,"C0"]
[100002312,"CIRCULATEUR 3 VITESSES GMR 5045","HC141",221,null,null,"/","/","/",3661238007581,3.1,310,210,130,"C0"]
[100002314,"CIRCULATEUR 3 VITESSES GMR 5065 ","HC143",251,null,null,"/","/","/",3661238007567,3.2,305,210,130,"C0"]
[100002316,"POMPE GMR 5090 3 VITESSES","HC145",388,null,null,"/","/","/",3661238007550,4.5,310,210,130,"C0"]
[100013027,"SONDE DE DÉPART + DOIGT DE GANT-BOUTEILLE < 350 kW","HC223",132,0.02,95020,"/","/","/",3661238362239,0.2,150,210,30,"C0"]
[100008701,"SONDE DE DÉPART + DOIGT DE GANT","HC206",155,0.02,95020,"/","/","/",3661238339255,0.21,210,160,25,"C0"]
[88017836,"CABLE BUS RX11  LG 1,5 M","AD124",84,0.02,95020,"/","/","/",3661238048911,0.06,210,160,5,"C0"]
["S103345","JEUX DE BRIDES À SOUDER DN50 POUR FILTRE A GAZ","HC261",84,null,null,"/","/","/",8713809280932,6.5,365,327,172,"C0"]
[]
["OPTIONS CASCADE"]
[111788,"COUDES DN65","HC209",664,null,null,"/","/","/",3661238338883,14,700,300,170,"C0"]
[111069,"ISOLATION COLLECTEUR","HC213",86,null,null,"/","/","/",3661238339026,0.66,530,480,280,"C0"]
[111920,"ISOLATION RACCORDEMENT CHAUDIÈRE","HC214",68,null,null,"/","/","/",3661238338838,0.41,530,470,250,"C0"]
[123182,"ISOLATION ARRIERE RACCORDEMENT CHAUDIÈRE","HC243",10,null,null,"/","/","/",3661238494411,0.39,940,540,8,"C0"]
[115269,"ISOLATION BOUTEILLE DE DÉCOUPLAGE < 350 kW","HC224",38,null,null,"/","/","/",3661238362222,0.6,660,280,220,"C0"]
[111067,"ISOLATION BOUTEILLE DE DÉCOUPLAGE","HC215",242,null,null,"/","/","/",3661238339033,3.2,300,620,960,"C0"]
[111167,"ISOLATION COUDES 90°C","HC216",103,null,null,"/","/","/",3661238339019,1.1100000000000001,610,300,500,"C0"]
[112632,"JEU DE CONTRE-BRIDES À SOUDER DN65","HC217",153,null,null,"/","/","/",3661238338821,6.58,160,160,120,"C0"]
[111807,"PIED REGLABLE","HC219",4,null,null,"/","/","/",3661238338845,0.09,230,115,5,"C0"]
[100003347,"COMMANDE EXTERNE ALARME VANNE","GR12",89,0.02,95020,"/","/","/",3661238005358,0.36,195,150,125,"C0"]
[84887768,"ADAPTATEUR  80 X 100MM ","DY768",55,null,null,"/","/","/",3661238011489,0.24,150,145,155,"C0"]
[]
["FUMISTERIE"]
[null,"ALU 80"]
[84887600,"TUBE D'INSPECTION Ø 80 mm ","DY600",48,null,null,"/","/","/",3661238013094,0.49,300,145,150,"C0"]
[84887738,"TE DE VISITE Ø 80 mm ","DY738",71,null,null,"/","/","/",3661238011755,0.66,285,215,165,"C0"]
[84887604,"RALLONGE Ø 80 mm    L= 250 mm  (2 PIECES)","DY604",37,null,null,"/","/","/",3661238013056,0.65,255,170,175,"C0"]
[84887605,"RALLONGE Ø 80 mm    L=  500 mm  (2 PIECES)","DY605",45,null,null,"/","/","/",3661238013049,1.26,520,175,170,"C0"]
[84887606,"RALLONGE 1000 mm  (2 PIECES)","DY606",72,null,null,"/","/","/",3661238013032,2.52,1020,175,175,"C0"]
[84887607,"RALLONGE Ø 80 mm    L=  1950 mm   (2 PIECES)","DY607",120,null,null,"/","/","/",3661238013025,5,1985,170,175,"C0"]
[84887551,"COLLIER DE CENTRAGE Ø 80mm  (2 PIECES)","DY151",14,null,null,"/","/","/",3661238013452,0.1,300,300,40,"C0"]
[84887608,"COUDE A 90°","DY608",24,null,null,"/","/","/",3661238013018,0.34,155,160,160,"C0"]
[84887609,"COUDE A 45°  (2 PIECES)","DY609",40,null,null,"/","/","/",3661238013001,0.48,200,200,150,"C0"]
[84887711,"KIT N° 1 RACCORDEMENT CHEMINEE Ø  80 ","DY711",185,null,null,"/","/","/",3661238011991,3.66,595,400,410,"C0"]
[null," PIECE  SPECIFIQUE POUR RACCORDEMENT EN  BIFLUX C53 Ø 80"]
[100002361,"PIECE D'ADAPTATION BIFLUX 2x80","DY819",44,null,null,"/","/","/",3661238007338,0.1,340,240,30,"C0"]
[84887438,"PRISE D'AIR EXTERIEURE LG=500 mm","DY38",99,null,null,"/","/","/",3661238013858,1.23,690,245,145,"C0"]
[null,"FLEXIBLE PPS Ø 80"]
[84887716,"KIT N° 3 RACCORDEMENT CHAUDIERE  PPS Ø 80/125 mm","DY716",144,null,null,"/","/","/",3661238011953,2.36,500,290,260,"C0"]
[100015325,"KIT N° 1 RACCORDEMENT CHEMINÉE FLEXIBLE PPS Ø 80 mm","DY895",236,null,null,"/","/","/",3661238380110,2.87,395,395,380,"C0"]
[100015327,"TUBE FLEXIBLE LG=12,5M","DY897",354,null,null,"/","/","/",3661238380134,8.6999999999999993,1200,1220,250,"C0"]
[100015326,"TUBE FLEXIBLE LG=50M","DY896",1242,null,null,"/","/","/",3661238380127,35,1600,1660,410,"C0"]
[84887618,"ETOILE DE CENTRAGE POUR FLEXIBLE Ø 80  mm (2 PIÈCES)","DY618",37,null,null,"/","/","/",3661238012912,0.2,300,300,70,"C0"]
[100015328,"PIÈCE DE COUPLAGE FLEXIBLE Ø 80 mm","DY898",71,null,null,"/","/","/",3661238380141,0.25,150,150,150,"C0"]
[100015331,"OUTIL D'AIDE À L'INSERTION Ø 80 mm","DY901",177,null,null,"/","/","/",3661238380172,1.4,300,210,185,"C0"]
[100015330,"PIÈCE D'INSPECTION POUR TUBE FLEXIBLE","DY900",127,null,null,"/","/","/",3661238380165,0.5,295,140,140,"C0"]
[100015329,"TERMINAL AVEC SOLIN FLEX. Ø 80 mm","DY899",177,null,null,"/","/","/",3661238380158,1.74,385,385,250,"C0"]
[null,"B23 EN DIAMETRE 80 PPS"]
[100017527,"KIT DE BASE PPS/ALU Ø 80/125 ","DY913",166,null,null,"/","/","/",3661238496330,3.7,600,400,275,"C0"]
[84887717,"KIT N° 1 KIT DE RACCORDEMENT CHEMINEE PPS Ø 80 mm","DY717",157,null,null,"/","/","/",3661238011946,2.89,395,405,390,"C0"]
[84887546,"PIÈCE DE VISITE Ø 80 mm droite","DY146",58,null,null,"/","/","/",3661238013506,0.28999999999999998,300,145,150,"C0"]
[84887613,"RALLONGE PPS Ø 80 mm   L= 250 mm (2 PCS)","DY613",40,null,null,"/","/","/",3661238012967,0.37,250,170,175,"C0"]
[84887614,"RALLONGE PPS  Ø 80 mm   L=  500 mm (2 PCS)","DY614",38,null,null,"/","/","/",3661238012950,0.68,500,160,150,"C0"]
[84887615,"RALLONGE PPS  Ø 80 mm   L=  1000 mm (2 PCS)","DY615",51,null,null,"/","/","/",3661238012943,1.25,1000,160,145,"C0"]
[84887550,"RALLONGE PPS Ø 80 mm   L=  2000 mm  (2 PIECES)","DY150",77,null,null,"/","/","/",3661238013469,2.4900000000000002,1960,150,150,"C0"]
[84887552,"COUDE PPS à 90°","DY152",16,null,null,"/","/","/",3661238013445,0.2,255,145,150,"C0"]
[84887554,"COUDE PPS a 45°  (2 PCS)","DY154",35,null,null,"/","/","/",3661238013421,0.32,200,200,150,"C0"]
[84887563,"T PPS  AVEC COUVERCLE  D'INSPECTION","DY163",58,null,null,"/","/","/",3661238013353,0.39,290,220,170,"C0"]
[84887551,"COLLIER DE CENTRAGE Ø 80mm (2 PIECES)","DY151",14,null,null,"/","/","/",3661238013452,0.1,300,300,40,"C0"]
[null,"PPS 80/125"]
[100011365,"KIT VENTOUSE HOR PPS/ALU Ø 80/125mm","DY882",208,null,null,"/","/","/",3661238374768,4.4000000000000004,1210,265,250,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 mm NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[100002733,"TERMINAL VERTICAL PPS Ø 80/125 mm ROUGE","DY844",154,null,null,"/","/","/",3661238006614,4.2,1210,265,240,"C0"]
[100008311,"COUDE DE REVISION ALU/PPS Ø 80/125 mm","DY875",115,null,null,"/","/","/",3661238101920,0.68,195,195,145,"C0"]
[100003271,"KIT DE RACCORDEMENT CHAUDIÈRE PERPENDICULAIRE","DY849",225,null,null,"/","/","/",3661238005600,3.5,595,395,410,"C0"]
[100003272,"KIT DE RACCORDEMENT CHAUDIÈRE SOUS CONDUIT","DY850",168,null,null,"/","/","/",3661238005594,1.44,500,290,260,"C0"]
[100011365,"KIT VENTOUSE HOR PPS/ALU Ø 80/125mm","DY882",208,null,null,"/","/","/",3661238374768,4.4000000000000004,1210,265,250,"C0"]
[84887524,"PIECE D'INSPECTION DROITE ALU/PPS Ø 80/125 mm","DY124",110,null,null,"/","/","/",3661238013704,0.55000000000000004,300,145,150,"C0"]
[84887525,"T D'INSPECTION ALU/PPS Ø 80/125 mm","DY125",126,null,null,"/","/","/",3661238013698,0.82,315,235,150,"C0"]
[84887526,"RALLONGE CONCENTRIQUE ALU/PPS  80/125 L= 250 mm","DY126",41,null,null,"/","/","/",3661238013681,0.47,255,145,150,"C0"]
[84887527,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 L= 500mm","DY127",47,null,null,"/","/","/",3661238013674,0.9,520,140,140,"C0"]
[84887528,"RALLONGECONCENTRIQUE ALU/PPS 80/125 L=1000 mm","DY128",69,null,null,"/","/","/",3661238013667,1.7,1010,135,140,"C0"]
[84887529,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 L=1950 mm","DY129",120,null,null,"/","/","/",3661238013650,3.5,1960,150,150,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 mm","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[84887532,"COUDE CONCENTRIQUE 45° ALU/PPS Ø 80/125 mm (2 PCES)","DY132",77,null,null,"/","/","/",3661238013629,1,315,235,150,"C0"]
[null,"Divers"]
[84837119,"TERMINAL HORIZONTAL ALU/ALU D.80/125 MM L=730 MM","CX119",100,null,null,"/","/","/",3661238014442,2.96,1025,170,170,"C0"]
[84887411,"SORTIE HORIZONTALE TOIT PENTE DE 30° A 45° ( uniquement pour tuiles mécaniques)","DY11",179,null,null,"/","/","/",3661238013940,3.57,1020,700,370,"C0"]
[84837729,"SORTIE DE TOIT EN PENTE DE 40° A 60° ( uniquement pour tuiles mécaniques)","CX49",178,null,null,"/","/","/",3661238014367,3.5,920,700,320,"C0"]
[84837731,"EMBASE D'ETANCHE TOIT PLAT","CX51",43,null,null,"/","/","/",3661238014343,0.5,400,400,155,"C0"]
[84837121,"TUILE A DOUILLE 5 A 25 NOIRE","CX121",112,null,null,"/","/","/",3661238014428,2.96,510,250,145,"C0"]
[84837732,"TUILE A DOUILLE 25 A 35' NOIRE","CX52",77,null,null,"/","/","/",3661238014336,3,520,250,145,"C0"]
[84837734,"TUILE A DOUILLE 35 A 55° NOIRE ","CX63",97,null,null,"/","/","/",3661238014312,3.17,510,265,180,"C0"]
[84837120,"TUILE A DOUILLE 5 A 25° ROUGE","CX120",112,null,null,"/","/","/",3661238014435,3.02,515,245,145,"C0"]
[84837783,"TUILE A DOUILLE 25 A 35 ROUGE","CX83",77,null,null,"/","/","/",3661238014213,3,515,250,150,"C0"]
[84837784,"TUILE A DOUILLE 25 A 55 ROUGE","CX84",97,null,null,"/","/","/",3661238014206,2.95,520,265,180,"C0"]
[84837741,"PLATINE DE FINITION INTER","CX72",17,null,null,"/","/","/",3661238014251,0.54,245,210,3,"C0"]
[84887566,"PANIER DE PROTECTION INOX","DY166",80,null,null,"/","/","/",3661238013339,1.38,220,210,200,"C0"]
[null,"ALU / ALU Ø 100/150 mm VERTICALE"]
[84827103,"EMBASE D'ETANCHEITE POUR TOIT PLAT","CX103",58,null,null,"/","/","/",3661238014589,0.49,470,470,100,"C0"]
[84827104,"TUILE A DOUILLE NOIRE AVEC ROTULE PENTE DE 25 ° A 45 °","CX104",110,null,null,"/","/","/",3661238014572,2.97,510,260,180,"C0"]
[84827106,"TUILE A DOUILLE ROUGE AVEC ROTULE PENTE DE 25 ° A 45 °","CX106",110,null,null,"/","/","/",3661238014565,2.98,510,260,180,"C0"]
[84827111,"COLLIER DIAMETRE 150 MM","CX111",12,null,null,"/","/","/",3661238014527,0.12,200,170,20,"C0"]
[84827115,"PLATINES DE FINITION ( 2 PIECES )","CX115",27,null,null,"/","/","/",3661238014480,0.52,250,210,3,"C0"]
[null,"ALU 100"]
[84887624,"TUBE D'INSPECTION L=300 mm","DY624",108,null,null,"/","/","/",3661238012851,0.56000000000000005,305,150,150,"C0"]
[84887739,"T DE VISITE ø 100 mm","DY739",93,null,null,"/","/","/",3661238011748,0.84,310,230,145,"C0"]
[84887625,"RALLONGE  ø 100 mm   L=  500 mm (2 PIECES)","DY625",77,null,null,"/","/","/",3661238012844,1.63,1010,135,140,"C0"]
[84887626,"RALLONGE  ø 100 mm   L=  1000 mm (2 PIECES)","DY626",130,null,null,"/","/","/",3661238012837,3.37,1005,290,150,"C0"]
[84887627,"RALLONGE  ø 100 mm   L=  1950 mm  (2 PIECES)","DY627",243,null,null,"/","/","/",3661238012820,7.5,1970,300,190,"C0"]
[84887628,"ETOILE DE CENTRAGE ø 100 mm (2 PIECES)","DY628",40,null,null,"/","/","/",3661238012813,0.1,300,300,35,"C0"]
[84887629,"COUDE  90°","DY629",47,null,null,"/","/","/",3661238012806,0.41,250,145,150,"C0"]
[84887630,"COUDE 45°  (2 PIECES)","DY630",93,null,null,"/","/","/",3661238012790,0.63,255,190,150,"C0"]
[84887768,"ADAPTATEUR  80 X 100MM ","DY768",55,null,null,"/","/","/",3661238011489,0.24,150,145,155,"C0"]
[84887633,"KIT N° 1  RACCORDEMENT CHEMINEE Ø  100 ","DY633",286,null,null,"/","/","/",3661238012769,3.63,590,395,410,"C0"]
[null,"RACCORDEMENT biFLUX C53 Ø 100"]
[100002362,"PIECE D'ADAPTATION BIFLUX 2x100","DY820",44,null,null,"/","/","/",3661238007321,0.09,340,240,35,"C0"]
[100002285,"PRISE D'AIR EXTERIEUR Lg 500 mm Ø 100","DY810",97,null,null,"/","/","/",3661238007659,1.4,1005,110,110,"C0"]
[84887633,"KIT N° 1 RACCORDEMENT CHEMINEE Ø  100 ","DY633",286,null,null,"/","/","/",3661238012769,3.63,590,395,410,"C0"]
[null,"FLEXIBLE PPS 110"]
[100015287,"KIT N° 1 RACCORDEMENT CHEMINÉE FLEXIBLE PPS Ø 110 mm","DY888",354,null,null,"/","/","/",3661238380035,3.4,590,390,400,"C0"]
[100015288,"FLEXIBLE PPS Ø 110 mm LG= 15 M","DY889",533,null,null,"/","/","/",3661238380042,8.6999999999999993,1320,1280,355,"C0"]
[100015289,"FLEXIBLE PPS Ø 110 mm LG= 25 M","DY890",888,null,null,"/","/","/",3661238380059,750,1610,1610,400,"C0"]
[100002280,"ETOILES DE CENTRAGE  Ø 110 mm POUR FLEXIBLE (4 PIÈCES)","DY805",42,null,null,"/","/","/",3661238007697,0.1,325,360,80,"C0"]
[100015321,"PIÈCE DE COUPLAGE FLEXIBLE Ø 110 mm","DY891",165,null,null,"/","/","/",3661238380073,0.25,195,195,140,"C0"]
[100015323,"TUBE DE VISITE Ø 110 mm POUR FLEXIBLE PPS","DY893",236,null,null,"/","/","/",3661238380097,0.5,295,140,140,"C0"]
[100015324,"OUTIL D'AIDE À L'INSERTION  Ø 110 mm","DY894",273,null,null,"/","/","/",3661238380103,1.4,190,210,165,"C0"]
[100015322,"TERMINAL AVEC SOLIN POUR FLEX Ø 110","DY892",261,null,null,"/","/","/",3661238380080,3,590,400,265,"C0"]
[null,"PPS/ALU 110/150"]
[100002734,"TERMINAL VERTICAL PPS/GALV Ø 110/150 mm NOIR","DY845",269,null,null,"/","/","/",3661238006607,6.2,1210,265,240,"C0"]
[100002360,"KIT N° 3 RACCORDEMENT CHAUDIERE  PPS ø 100/150 mm","DY818",297,null,null,"/","/","/",3661238007345,3.7,390,295,1010,"C0"]
[100002351,"RALLONGE PPS-ALU  ø 110/150 mm L=  500 mm","DY811",69,null,null,"/","/","/",3661238007437,1.5,525,195,200,"C0"]
[100002352,"RALLONGE PPS-ALU ø 110/150 mm L=1000 mm","DY812",104,null,null,"/","/","/",3661238007420,2.7,1025,195,200,"C0"]
[100002353,"COUDE PPS-ALU  87° ø 110/150 mm  ","DY813",124,null,null,"/","/","/",3661238007413,1.6,345,265,190,"C0"]
[100002354,"COUDE PPS-ALU  45° ø 110/150 mm (2 PIECES)","DY814",218,null,null,"/","/","/",3661238007406,2.25,390,290,260,"C0"]
[100002355,"PIECE DE REVISION DROITE PPS-ALU  ø 110/150 mm","DY815",132,null,null,"/","/","/",3661238007390,1.25,340,265,190,"C0"]
[84827104,"TUILE A DOUILLE NOIRE AVEC ROTULE PENTE DE 25 ° A 45 °","CX104",110,null,null,"/","/","/",3661238014572,2.97,510,260,180,"C0"]
[84827106,"TUILE A DOUILLE ROUGE AVEC ROTULE PENTE DE 25 ° A 45 °","CX106",110,null,null,"/","/","/",3661238014565,2.98,510,260,180,"C0"]
[84827111,"COLLIER DIAMETRE 150 MM","CX111",12,null,null,"/","/","/",3661238014527,0.12,200,170,20,"C0"]
[84827115,"PLATINES DE FINITION ( 2 PIECES )","CX115",27,null,null,"/","/","/",3661238014480,0.52,250,210,3,"C0"]
[84827103,"EMBASE D'ETANCHEITE POUR TOIT PLAT","CX103",58,null,null,"/","/","/",3661238014589,0.49,470,470,100,"C0"]
[100002356,"T DE REVISION PPS-ALU  ø 110/150 mm","DY816",188,null,null,"/","/","/",3661238007383,1.25,345,265,190,"C0"]
[100002357,"ADAPTATEUR PPS-ALU  100/150 - 110/150 mm","DY817",112,null,null,"/","/","/",3661238007376,0.49,255,170,180,"C0"]
[100011364,"PPs/ALU KIT VENTOUSE HORIZONTALE ø 110/150 mm","DY881",455,null,null,"/","/","/",3661238367821,6.25,1500,400,300,"C0"]
[null,"B 23 EN DIAMETRE  PPS 110"]
[100008312,"KIT DE RACCORDEMENT CHEMINEE ø 80 - 110 mm PPS","DY876",208,null,null,"/","/","/",3661238167995,2.79,600,395,410,"C0"]
[100017529,"KIT DE BASE PPS/ALU Ø 110/150","DY914",283,null,null,"/","/","/",3661238496347,4.0999999999999996,600,396,412,"C0"]
[84887577,"KIT DE RACCORDEMENT CHEMINEE PPS Ø 110 mm ","DY177",258,null,null,"/","/","/",3661238013223,2.68,395,300,510,"C0"]
[84887578,"TUYAU PPS Ø 110 mm  LG = 1950 mm  (GRIS)","DY178",72,null,null,"/","/","/",3661238013216,2.46,1960,150,150,"C0"]
[84887579,"TUYAU PPS Ø 110 mm  LG = 1000 mm  (GRIS)","DY179",41,null,null,"/","/","/",3661238013209,1.24,1015,130,140,"C0"]
[84887580,"TUYAU PPS Ø 110 mm  LG = 500 mm  (GRIS)","DY180",31,null,null,"/","/","/",3661238013193,0.62,515,135,140,"C0"]
[84887581,"COUDE PPS 87° Ø 110 mm  (GRIS)","DY181",36,null,null,"/","/","/",3661238013186,0.33,255,190,150,"C0"]
[84887582,"COUDE PPS 45° Ø 110 mm  (GRIS)","DY182",48,null,null,"/","/","/",3661238013179,0.52,295,215,165,"C0"]
[84887583,"T DE REVISIONØ 110 mm  (GRIS)","DY183",48,null,null,"/","/","/",3661238013162,0.46,300,150,150,"C0"]
[84887587,"ETOILE DE CENTRAGE PPS  Ø 110 mm  (2 PIECES)","DY187",15,null,null,"/","/","/",3661238013124,0.1,300,300,30,"C0"]
[]
["FAMILLE:","CHAUDIERE GAZ A CONDENSATION"]
[]
[]
[100018208,"GSCR 15 HOR  ",null,{"$f":"D2352+D2355","v":3428},null,null,"A","/","/",3661238513761,null,null,null,null,"C0"]
[100018209,"GSCR 15 VER ",null,{"$f":"D2352+D2357","v":3396},null,null,"A","/","/",3661238513778,null,null,null,null,"C0"]
[100018210,"GSCR 25 HOR",null,{"$f":"D2353+D2355","v":3592},null,null,"A","/","/",3661238513785,null,null,null,null,"C0"]
[100018211,"GSCR 25 VER",null,{"$f":"D2353+D2357","v":3560},null,null,"A","/","/",3661238513792,null,null,null,null,"C0"]
[100018212,"GSCR 35 HOR  ",null,{"$f":"D2354+D2356","v":3930},null,null,"A","/","/",3661238513808,null,null,null,null,"C0"]
[100018213,"GSCR 35 VER ",null,{"$f":"D2354+D2357","v":3877},null,null,"A","/","/",3661238513815,null,null,null,null,"C0"]
[]
["COMPOSANTS"]
[100017756,"GSCR 15","JA21",3241,5,14070,"A","/","/",3661238505971,68.5,780,680,1060,"C0"]
[100017757,"GSCR 25","JA22",3405,5,14070,"A","/","/",3661238505988,68.5,780,680,1060,"C0"]
[100017758,"GSCR 35","JA23",3722,5,14070,"A","/","/",3661238505995,62,780,680,1060,"C0"]
[100013756,"TERMINAL HORIZONTAL PPS/GALVA Ø 60/100 mm","HR48",187,null,null,"/","/","/",3661238370883,3.37,1200,200,200,"C0"]
[100011365,"KIT VENTOUSE HOR PPS/ALU Ø 80/125mm","DY882",208,null,null,"/","/","/",3661238374768,4.4000000000000004,1210,265,250,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 mm NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
[]
[100018214,"GVCR 15 HOR/100HL ",null,{"$f":"D2368+D2371+D2372+D2373","v":4559},null,null,"A","A","XL ",3661238513822,null,null,null,null,"C0"]
[100018215,"GVCR 15 VER/100HL ",null,{"$f":"D2368+D2371+D2372+D2375","v":4527},null,null,"A","A","XL ",3661238513839,null,null,null,null,"C0"]
[100018216,"GVCR 25 HOR/100HL ",null,{"$f":"D2369+D2371+D2372+D2373","v":4723},null,null,"A","A","XL ",3661238513846,null,null,null,null,"C0"]
[100018217,"GVCR 25 VER/100HL ",null,{"$f":"D2369+D2371+D2372+D2375","v":4691},null,null,"A","A","XL ",3661238513853,null,null,null,null,"C0"]
[100018218,"GVCR 35 HOR/100HL ",null,{"$f":"D2370+D2371+D2372+D2374","v":5061},null,null,"A","A","XL ",3661238513860,null,null,null,null,"C0"]
[100018219,"GVCR 35 VER/100HL ",null,{"$f":"D2370+D2371+D2372+D2375","v":5008},null,null,"A","A","XL ",3661238513877,null,null,null,null,"C0"]
[]
["COMPOSANTS"]
[100017756,"GSCR 15","JA21",3241,5,14070,"A","A","XL ",3661238505971,68.5,780,680,1060,"C0"]
[100017757,"GSCR 25","JA22",3405,5,14070,"A","A","XL ",3661238505988,68.5,780,680,1060,"C0"]
[100017758,"GSCR 35","JA23",3722,5,14070,"A","A","XL ",3661238505995,62,780,680,1060,"C0"]
[100016430,"BALLON 100HL ","ER225",1062,null,null,"/","/","/",3661238493469,63,790,675,800,"C0"]
[100017392,"KIT RACC. BALLONS HL-SHL","JA9",69,null,null,"/","/","/",3661238495241,2,410,290,180,"C0"]
[100013756,"TERMINAL HORIZONTAL PPS/GALVA Ø 60/100 mm","HR48",187,null,null,"/","/","/",3661238370883,3.37,1200,200,200,"C0"]
[100011365,"KIT VENTOUSE HOR PPS/ALU Ø 80/125mm","DY882",208,null,null,"/","/","/",3661238374768,4.4000000000000004,1210,265,250,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 mm NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
[]
[100018220,"GVCR 15 HOR/160SL ",null,{"$f":"D2392+D2395+D2396+D2398","v":4449},null,null,"A","A","XL ",3661238513914,null,null,null,null,"C0"]
[100018221,"GVCR 15 VER/160SL ",null,{"$f":"D2392+D2395+D2396+D2400","v":4417},null,null,"A","A","XL ",3661238513921,null,null,null,null,"C0"]
[100018222,"GCCR 15 HOR/160SL ",null,{"$f":"D2392+D2395+D2397+D2398","v":4669},null,null,"A","A","XL ",3661238513938,null,null,null,null,"C0"]
[100018223,"GCCR 15 VER/160SL ",null,{"$f":"D2392+D2395+D2397+D2400","v":4637},null,null,"A","A","XL ",3661238513945,null,null,null,null,"C0"]
[100018224,"GVCR 25 HOR/160SL ",null,{"$f":"D2393+D2395+D2396+D2398","v":4613},null,null,"A","A","XL ",3661238513952,null,null,null,null,"C0"]
[100018225,"GVCR 25 VER/160SL ",null,{"$f":"D2393+D2395+D2396+D2400","v":4581},null,null,"A","A","XL ",3661238513969,null,null,null,null,"C0"]
[100018226,"GCCR 25 HOR/160SL ",null,{"$f":"D2393+D2395+D2397+D2398","v":4833},null,null,"A","A","XL ",3661238513976,null,null,null,null,"C0"]
[100018227,"GCCR 25 VER/160SL ",null,{"$f":"D2393+D2395+D2397+D2400","v":4801},null,null,"A","A","XL ",3661238513983,null,null,null,null,"C0"]
[100018228,"GVCR 35 HOR/160SL ",null,{"$f":"D2394+D2395+D2396+D2399","v":4951},null,null,"A","A","XL ",3661238513990,null,null,null,null,"C0"]
[100018229,"GVCR 35 VER/160SL ",null,{"$f":"D2394+D2395+D2396+D2400","v":4898},null,null,"A","A","XL ",3661238514003,null,null,null,null,"C0"]
[100018230,"GCCR 35 HOR /160SL ",null,{"$f":"D2394+D2395+D2397+D2399","v":5171},null,null,"A","A","XL ",3661238514010,null,null,null,null,"C0"]
[100018231,"GCCR 35 VER/160SL ",null,{"$f":"D2394+D2395+D2397+D2400","v":5118},null,null,"A","A","XL ",3661238514027,null,null,null,null,"C0"]
[]
["COMPOSANTS"]
[100017756,"GSCR 15","JA21",3241,5,14070,"A","A","XL ",3661238505971,68.5,780,680,1060,"C0"]
[100017757,"GSCR 25","JA22",3405,5,14070,"A","A","XL ",3661238505988,68.5,780,680,1060,"C0"]
[100017758,"GSCR 35","JA23",3722,5,14070,"A","A","XL ",3661238505995,62,780,680,1060,"C0"]
[100016428," BALLON 160SL ","ER223",952,null,null,"Pas concerné par l'étiquettage",null,null,3661238493445,91,790,675,1070,"C0"]
[100017391,"KIT RACC. BALLONS SL-SSL","JA8",69,null,null,"/","/","/",3661238495234,1.4,630,210,230,"D3"]
[100016480,"KIT DE LIAISON AGC-EGC /B 160-220","ER228",289,null,null,"/","/","/",3661238493483,6,875,685,235,"C0"]
[100013756,"TERMINAL HORIZONTAL PPS/GALVA Ø 60/100 mm","HR48",187,null,null,"/","/","/",3661238370883,3.37,1200,200,200,"C0"]
[100011365,"KIT VENTOUSE HOR PPS/ALU Ø 80/125mm","DY882",208,null,null,"/","/","/",3661238374768,4.4000000000000004,1210,265,250,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 mm NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
[]
[7606048,"GVCR 15 HOR/L160SL ",null,{"$f":"D2411+D2414+D2415+D2416","v":4577},null,null,"A","A","XL ",null,null,null,null,null,"C0"]
[7606049,"GVCR 15 VER/L160SL ",null,{"$f":"D2411+D2414+D2415+D2417","v":4545},null,null,"A","A","XL ",null,null,null,null,null,"C0"]
[7606050,"GVCR 25 HOR/L160SL ",null,{"$f":"D2412+D2414+D2415+D2416","v":4741},null,null,"A","A","XL ",null,null,null,null,null,"C0"]
[7606051,"GVCR 25 VER/L160SL ",null,{"$f":"D2412+D2414+D2415+D2417","v":4709},null,null,"A","A","XL ",null,null,null,null,null,"C0"]
[7606052,"GVCR 35 HOR/L160SL ",null,{"$f":"D2413+D2414+D2415+D2418","v":5079},null,null,"A","A","XL ",null,null,null,null,null,"C0"]
[7606053,"GVCR 35 VER/L160SL ",null,{"$f":"D2413+D2414+D2415+D2417","v":5026},null,null,"A","A","XL ",null,null,null,null,null,"C0"]
[]
["COMPOSANTS"]
[100017756,"GSCR 15","JA21",3241,5,14070,"A","/","/",3661238505971,68.5,780,680,1060,"C0"]
[100017757,"GSCR 25","JA22",3405,5,14070,"A","/","/",3661238505988,68.5,780,680,1060,"C0"]
[100017758,"GSCR 35","JA23",3722,5,14070,"A","/","/",3661238505995,62,780,680,1060,"C0"]
[100020079,"BALLON L160SL ","EC600",1080,null,null,"Pas concerné par l'étiquettage",null,null,3661238584310,97.5,680,380,1111,"C0"]
[100017392,"KIT RACC. BALLONS HL-SHL","JA9",69,null,null,"/","/","/",3661238495241,2,410,290,180,"C0"]
[100013756,"TERMINAL HORIZONTAL PPS/GALVA Ø 60/100 mm","HR48",187,null,null,"/","/","/",3661238370883,3.4,1200,200,200,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[100011365,"KIT VENTOUSE HOR PPS/ALU Ø 80/125mm","DY882",208,null,null,"/","/","/",3661238374768,4.4000000000000004,1210,265,250,"C0"]
[]
[]
[100018232,"GVCR 15 HOR /220SHL ",null,{"$f":"D2435+D2438+D2439+D2441+D2442","v":6110},null,null,"A","A","XL ",3661238514034,null,null,null,null,"C0"]
[100018233,"GVCR 15 VER /220SHL ",null,{"$f":"D2435+D2438+D2439+D2441+D2444","v":6078},null,null,"A","A","XL ",3661238514041,null,null,null,null,"C0"]
[100018234,"GCCR 15 HOR /220SHL ",null,{"$f":"D2435+D2438+D2440+D2441+D2442","v":6386},null,null,"A","A","XL ",3661238514058,null,null,null,null,"C0"]
[100018235,"GCCR 15 VER /220SHL ",null,{"$f":"D2435+D2438+D2440+D2441+D2444","v":6354},null,null,"A","A","XL ",3661238514065,null,null,null,null,"C0"]
[100018236,"GVCR 25 HOR /220SHL ",null,{"$f":"D2436+D2438+D2439+D2441+D2442","v":6274},null,null,"A","A","XL ",3661238514072,null,null,null,null,"C0"]
[100018237,"GVCR 25 VER /220SHL ",null,{"$f":"D2436+D2438+D2439+D2441+D2444","v":6242},null,null,"A","A","XL ",3661238514089,null,null,null,null,"C0"]
[100018238,"GCCR 25 HOR /220SHL ",null,{"$f":"D2436+D2438+D2440+D2441+D2442","v":6550},null,null,"A","A","XL ",3661238514096,null,null,null,null,"C0"]
[100018239,"GCCR 25 VER /220SHL ",null,{"$f":"D2436+D2438+D2440+D2441+D2444","v":6518},null,null,"A","A","XL ",3661238514102,null,null,null,null,"C0"]
[100018240,"GVCR 35 HOR /220SHL ",null,{"$f":"D2437+D2438+D2439+D2441+D2443","v":6612},null,null,"A","A","XL ",3661238514119,null,null,null,null,"C0"]
[100018241,"GVCR 35 VER /220SHL ",null,{"$f":"D2437+D2438+D2439+D2441+D2444","v":6559},null,null,"A","A","XL ",3661238514126,null,null,null,null,"C0"]
[100018242,"GCCR 35 HOR /220SHL ",null,{"$f":"D2437+D2438+D2440+D2441+D2443","v":6888},null,null,"A","A","XL ",3661238514133,null,null,null,null,"C0"]
[100018243,"GCCR 35 VER /220SHL ",null,{"$f":"D2437+D2438+D2440+D2441+D2444","v":6835},null,null,"A","A","XL ",3661238514140,null,null,null,null,"C0"]
[]
["COMPOSANTS"]
[100017756,"GSCR 15","JA21",3241,5,14070,"A","/","/",3661238505971,68.5,780,680,1060,"C0"]
[100017757,"GSCR 25","JA22",3405,5,14070,"A","/","/",3661238505988,68.5,780,680,1060,"C0"]
[100017758,"GSCR 35","JA23",3722,5,14070,"A","/","/",3661238505995,62,780,680,1060,"C0"]
[100016425,"BALLON 220SHL","ER220",2439,null,null,"/","/","/",3661238493414,132,790,675,1160,"C0"]
[100017392,"KIT RACC. BALLONS HL-SHL","JA9",69,null,null,"/","/","/",3661238495241,2,410,290,180,"C0"]
[100017431,"KIT LIAISON BS220SHL/CHAUDIERE GSCR","ER216",345,null,null,"/","/","/",3661238506619,6,875,685,235,"C0"]
[100016501,"KIT VASE D'EXPANSION 12l/10 bars ","ER229",174,null,null,"/","/","/",3661238505926,5,325,320,215,"C0"]
[100013756,"TERMINAL HORIZONTAL PPS/GALVA Ø 60/100 mm","HR48",187,null,null,"/","/","/",3661238370883,3.37,1200,200,200,"C0"]
[100011365,"KIT VENTOUSE HOR PPS/ALU Ø 80/125mm","DY882",208,null,null,"/","/","/",3661238374768,4.4000000000000004,1210,265,250,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 mm NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
["OPTIONS CHAUDIERES"]
[100017394,"KIT DE RACCORDEMENT CENTRAL COLONNE ","JA11",289,null,null,"/","/","/",3661238495265,7,820,430,280,"C0"]
[100017395,"KIT DE RACCORDEMENT GAUCHE ","JA12",289,null,null,"/","/","/",3661238495272,9.3000000000000007,625,545,295,"C0"]
[100017396,"KIT DE RACCORDEMENT DROITE COLONNE","JA13",277,null,null,"/","/","/",3661238495289,9,625,545,295,"C0"]
[100017817,"KIT DE RACCORDEMENT CHAUFFAGE SEUL  ","JA34",149,null,null,"/","/","/",3661238506787,5,625,545,295,"C0"]
[100018164,"KIT DE CONVERSION GPL 15KW ","JA39",12,null,null,"/","/","/",3661238513624,0.1,220,335,20,"C0"]
[100018165,"KIT DE CONVERSION PROPANE 25kW ","JA40",12,null,null,"/","/","/",3661238513631,0.1,220,335,20,"C0"]
[100018166,"KIT DE CONVERSION PROPANE 35kW ","JA41",12,null,null,"/","/","/",3661238513648,0.1,220,335,20,"C0"]
[100017827,"KIT DE RACCORDEMENT V3V-PLATINE","JA35",115,null,null,"/","/","/",3661238506800,9,630,210,230,"C0"]
[100017390,"KIT V3V EXTERNE","JA7",91,null,null,"/","/","/",3661238495227,1.3,630,210,230,"C0"]
[7613605,"STATION DE NEUTRALISATION DN1","SA1",344,null,null,"/","/","/",3661238592117,14.5,350,230,350,"C0"]
[7613606,"SUPPORT FIXATION MURAL","SA2",63,null,null,"/","/","/",3661238592124,2.1,300,240,160,"C0"]
[85317025,"RECHARGE 2 KG POUR NEUTRALISATION","HC35",140,null,null,"/","/","/",3661238091610,3.65,510,315,190,"C0"]
[83877009,"SYSTEME DE NEUTRALISATION DES CONDENSATS (avec pompe de relevage)","DU13",914,null,null,"/","/","/",3661238015081,15,350,230,360,"C0"]
[82197762,"SYSTEME DE NEUTRALISATION DES CONDENSATS (JUSQU'À ≈ 19.200 L CONDENSATS)","BP52",571,null,null,"/","/","/",3661238020696,9.9,760,165,210,"C0"]
[94225601,"RECHARGE DE GRANULATS DE NEUTRALISATION 10 KG**",null,null,null,null,"/","/","/"]
[100005825,"ADAPTATEUR BI-FLUX   2x80","DY868",64,null,null,"/","/","/",3661238162204,0.42,310,160,140,"C0"]
["S100465","ADAPTATEUR AIR/FUMEES Ø 80/125","HR38",55,null,null,"/","/","/",3661238369917,1,190,190,130,"C0"]
[100018253,"COUDE REDUIT  60/100 PPS/ALU ","JA43",80,null,null,"/","/","/",3661238548411,0.8,290,220,170,"C0"]
["S100310","THERMOSTAT FUMEE","HR43",68,0.02,95020,"/","/","/",3661238369931,0.1,180,130,30,"C0"]
[100018163,"KIT SONDE TEMPERATURE FUMEE","JA38",69,0.02,95020,"/","/","/",3661238513617,1,185,130,105,"C0"]
["S100931","OUTIL DE NETTOYAGE CORPS CHAUDIERE","HR45",86,null,null,"/","/","/",3661238369948,0.73,310,320,160,"C0"]
[100020164,"COLLECTEUR 2/3 CIRCUITS ","EA140",348,null,null,"/","/","/",3661238575011,6.6,660,180,200,"C0"]
[100020165,"CONSOLE MUR COLLECTEUR ","EA141",44,null,null,"/","/","/",3661238575028,1.2,220,125,70,"C0"]
[100020166,"CONSOLE MUR 1 MODULE ","EA142",116,null,null,"/","/","/",3661238575035,1.6,220,125,70,"C0"]
[100020167,"CIRCUIT DIRECT P.ELEC CLASSE A  ","EA143",644,0.83,14050,"/","/","/",3661238575042,5.0999999999999996,460,270,235,"C0"]
[100020169,"MODULE HYDR COMPACT 2 CIRCUITS HEE","EA145",1146,0.83,14050,"/","/","/",3661238575059,9,525,415,210,"C0"]
[89557009,"KIT DE TRANSFORMATION G/R 3/4 '' ET 1 ''","BH84",32,null,null,"/","/","/",3661238047563,0.32500000000000001,200,140,45,"C0"]
[100018164,"KIT DE CONVERSION GPL 15KW ","JA39",12,null,null,"/","/","/",3661238513624,0.1,220,335,20,"C0"]
[100018165,"KIT DE CONVERSION PROPANE 25kW ","JA40",12,null,null,"/","/","/",3661238513631,0.1,220,335,20,"C0"]
[100018166,"KIT DE CONVERSION PROPANE 35kW ","JA41",12,null,null,"/","/","/",3661238513648,0.1,220,335,20,"C0"]
[]
["OPTIONS REGULATIONS"]
[100013304,"COLIS OPTION V3V OE-TRONIC 4","AD249",158,0.12,95010,"/","/","/",3661238363519,0.42,260,170,130,"C0"]
[100013305,"COLIS SONDE SYSTÈME OE-TRONIC 4","AD250",46,0.02,95020,"/","/","/",3661238363588,0.13400000000000001,150,210,25,"C0"]
[100013306,"SONDE EXTERIEURE RADIO ","AD251",77,0.12,95010,"/","/","/",3661238363595,0.15,150,210,40,"C0"]
[100013307,"MODULE CHAUDIERE RADIO (EMETTEUR)","AD252",123,0.12,95010,"/","/","/",3661238363601,0.32,260,160,130,"C0"]
[100013472,"CDE A DISTANCE RADIO RS 400R     ","AD255",238,0.12,95010,"/","/","/",3661238364233,0.253,175,122,60,"C0"]
[100013477,"CDE A DISTANCE FILAIRE RS 400   ","AD257",177,0.12,95010,"/","/","/",3661238364257,0.253,175,122,60,"C0"]
[88017851,"CABLE DE LIAISON BUS LG 12 M","AD134",110,0.02,95020,"/","/","/",3661238048850,0.37,350,260,30,"C0"]
[88017878,"MODULE DE TELESURVEILLANCE VOCAL TELCOM 2","AD152",704,0.12,95010,"/","/","/",3661238048751,1.05,210,190,105,"C0"]
[88017017,"SONDE DEPART v3v","AD199",80,0.02,95020,"/","/","/",3661238049185,0.21,150,200,40,"C0"]
[100002803,"COMMANDE A DISTANCE SIMPLIFIEE AD208","AD208",104,0.12,95010,"/","/","/",3661238554931,0.2,120,85,40,"C0"]
[]
["OPTIONS ECS ET  PREPARATEURS INDEPENDANTS"]
[100017432,"KIT RECIRCULATION BS100HL","ER218",22,null,null,"/","/","/",3661238506626,0.5,250,100,100,"C0"]
[100017433,"KIT RECIRCULATION BS160/220","ER219",69,null,null,"/","/","/",3661238506633,1.5,510,460,175,"C0"]
[100018204,"VASE EXPANSION SANITAIRE 8L","ER233 ",289,null,null,"/","/","/",3661238514317,5,405,405,175,"C0"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.16,200,150,30,"C0"]
[100017393,"KIT RACC. BALLONS AUTRES","JA10",58,null,null,"/","/","/",3661238495258,1.2,630,210,230,"C0"]
[100000492,"KIT ANODE MAGNESIUM","EA103",66,null,null,"/","/","/",3661238011069,0.9,560,90,85,"C0"]
[89557009,"KIT DE TRANSFORMATION G/R 3/4 '' ET 1 ''","BH84",32,null,null,"/","/","/",3661238047563,0.32500000000000001,200,140,45,"C0"]
[]
[]
["CHAUDIERES POUR RACCORDEMENT VENTOUSE"]
[100018244,"GSCX 25 HOR",null,{"$f":"D2505+D2506","v":2794},null,null,"A","/","/",3661238514157,null,null,null,null,"D3"]
[100018245,"GSCX 25 VER",null,{"$f":"D2505+D2507+D2508","v":2888},null,null,"A","/","/",3661238514164,null,null,null,null,"D3"]
[]
["COMPOSANTS"]
[100017759,"GSCX 25","JA24",2678,5,14070,"A","/","/",3661238506008,67,780,680,1060,"D3"]
[100008296,"TERMINAL HORIZONTAL PPS Ø 60/100 mm LG=800 mm","DY871",116,null,null,"/","/","/",3661238168022,2.78,1200,200,200,"C0"]
["S100465","ADAPTATEUR AIR/FUMEES Ø 80/125","HR38",55,null,null,"/","/","/",3661238369917,1,190,190,130,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 mm NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
[]
[100018246,"GVCX 25 HOR /100SL ",null,{"$f":"D2515+D2516+D2517+D2518","v":3458},null,null,"A","A","XL ",3661238514171,null,null,null,null,"D3"]
[100018247,"GVCX 25 VER/100SL ",null,{"$f":"D2515+D2516+D2517+D2519+D2520","v":3552},null,null,"A","A","XL ",3661238514188,null,null,null,null,"D3"]
[]
["COMPOSANTS"]
[100017759,"GSCX 25","JA24",2678,5,14070,"A","/","/",3661238506008,67,780,680,1060,"D3"]
[100016431,"BALLON 100SL","ER226",595,null,null,"Pas concerné par l'étiquettage",null,null,3661238493476,72,790,675,800,"D3"]
[100017391,"KIT RACC. BALLONS SL-SSL","JA8",69,null,null,"/","/","/",3661238495234,1.4,630,210,230,"D3"]
[100008296,"TERMINAL HORIZONTAL PPS Ø 60/100 mm LG=800 mm","DY871",116,null,null,"/","/","/",3661238168022,2.78,1200,200,200,"C0"]
["S100465","ADAPTATEUR AIR/FUMEES Ø 80/125","HR38",55,null,null,"/","/","/",3661238369917,1,190,190,130,"C0"]
[100002732,"ADAPTATEUR AIR/FUMEES Ø 80/125","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
[]
[7614662,"GVCX 25 HOR/200SSL ",null,{"$f":"D2529+D2530+D2531+D2533+D2534","v":5250},null,null,"A","A","XL ",3661238514195,null,null,null,null,"D3"]
[7614663,"GVCX 25 VER/200SSL ",null,{"$f":"D2529+D2530+D2531+D2533+D2535+D2536","v":5344},null,null,"A","A","XL ",3661238514201,null,null,null,null,"D3"]
[7614664,"GCCX 25 HOR/200SSL ",null,{"$f":"D2529+D2530+D2532+D2533+D2534","v":5470},null,null,"A","A","XL ",3661238514218,null,null,null,null,"D3"]
[7614665,"GCCX 25 VER/200SSL ",null,{"$f":"D2529+D2530+D2532+D2533+D2535+D2536","v":5564},null,null,"A","A","XL ",3661238514225,null,null,null,null,"D3"]
[]
["COMPOSANTS"]
[100017759,"GSCX 25","JA24",2678,5,14070,"A","/","/",3661238506008,67,780,680,1060,"D3"]
[100016426,"BALLON 200SSL","ER221",2213,null,null,"Pas concerné par l'étiquettage",null,null,3661238493421,127,790,675,1350,"D3"]
[100017391,"KIT RACC. BALLONS SL-SSL","JA8",69,null,null,"/","/","/",3661238495234,1.4,630,210,230,"D3"]
[100016480,"KIT DE LIAISON AGC-EGC /B 160-200","ER228",289,null,null,"/","/","/",3661238493483,6,875,685,235,"C0"]
[100016501,"KIT VASE D'EXPANSION  12l/10 bars ","ER229",174,null,null,"/","/","/",3661238505926,5,325,320,215,"C0"]
[100008296,"TERMINAL HORIZONTAL PPS Ø 60/100 mm LG=800 mm","DY871",116,null,null,"/","/","/",3661238168022,2.78,1200,200,200,"C0"]
["S100465","ADAPTATEUR AIR/FUMEES Ø 80/125","HR38",55,null,null,"/","/","/",3661238369917,1,190,190,130,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 mm NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
[]
[7663875,"GVCX 25 HOR/200SHL ",null,{"$f":"D2543+D2544+D2545+D2546+D2547","v":5250},null,null,"A","A","XL ",3661238670419,null,null,null,null,"D3"]
[7663878,"GVCX 25 VER/200SHL ",null,{"$f":"D2543+D2544+D2545+D2546+D2548+D2549","v":5344},null,null,"A","A","XL ",3661238670426,null,null,null,null,"D3"]
[]
["COMPOSANTS"]
[100017759,"GSCX 25","JA24",2678,5,14070,"A","/","/",3661238506008,67,780,680,1060,"D3"]
[7652032,"BALLON 200SHL","ER770",2213,null,null,"Pas concerné par l'étiquettage",null,null,3661238660021,127,790,675,1350,"D3"]
[100017392,"KIT RACC. BALLONS HL-SHL-L SL","JA9",69,null,null,"/","/","/",3661238495241,1.5,620,220,220,"D3"]
[100016501,"KIT VASE D'EXPANSION  12l/10 bars ","ER229",174,null,null,"/","/","/",3661238505926,5,325,320,215,"C0"]
[100008296,"TERMINAL HORIZONTAL PPS Ø 60/100 mm LG=800 mm","DY871",116,null,null,"/","/","/",3661238168022,2.78,1200,200,200,"C0"]
["S100465","ADAPTATEUR AIR/FUMEES Ø 80/125","HR38",55,null,null,"/","/","/",3661238369917,1,190,190,130,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 mm NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
["OPTIONS CHAUDIERES"]
[100017394,"KIT DE RACCORDEMENT CENTRAL","JA11",289,null,null,"/","/","/",3661238495265,7,820,430,280,"C0"]
[100017395,"KIT DE RACCORDEMENT GAUCHE","JA12",289,null,null,"/","/","/",3661238495272,9.3000000000000007,625,545,295,"C0"]
[100017396,"KIT DE RACCORDEMENT DROITE","JA13",277,null,null,"/","/","/",3661238495289,9,625,545,295,"C0"]
[100017817,"KIT DE RACCORDEMENT CHAUFFAGE SEUL  ","JA34",149,null,null,"/","/","/",3661238506787,5,625,545,295,"C0"]
[100005825,"ADAPTATEUR BI-FLUX   2x80","DY868",64,null,null,"/","/","/",3661238162204,0.42,310,160,140,"C0"]
["S100465","ADAPTATEUR AIR/FUMEES Ø 80/125","HR38",55,null,null,"/","/","/",3661238369917,1,190,190,130,"C0"]
[100018253,"COUDE REDUIT  60/100 PPS/ALU ","JA43",80,null,null,"/","/","/",3661238548411,0.8,290,220,170,"C0"]
[100018163,"KIT SONDE TEMPERATURE FUMEE","JA38",69,0.02,95020,"/","/","/",3661238513617,1,185,130,105,"C0"]
["S100310","THERMOSTAT FUMEE","HR43",68,0.02,95020,"/","/","/",3661238369931,0.1,180,130,30,"C0"]
[7613605,"STATION DE NEUTRALISATION DN1","SA1",344,null,null,"/","/","/",3661238592117,14.5,350,230,350,"C0"]
[7613606,"SUPPORT FIXATION MURAL","SA2",63,null,null,"/","/","/",3661238592124,2.1,300,240,160,"C0"]
[85317025,"RECHARGE 2 KG POUR NEUTRALISATION","HC35",140,null,null,"/","/","/",3661238091610,3.65,510,315,190,"C0"]
["S100931","OUTIL DE NETTOYAGE CORPS CHAUDIERE","HR45",86,null,null,"/","/","/",3661238369948,0.73,310,320,160,"C0"]
[100018165,"KIT DE CONVERSION PROPANE 25kW ","JA40",12,null,null,"/","/","/",3661238513631,0.1,220,335,20,"C0"]
[7607001,"KIT VASE D'EXPANSION","JA74",237,null,null,"/","/","/",3661238585522,8,565,370,235,"C0"]
[]
["AUTRES OPTIONS"]
[83877009,"SYSTEME DE NEUTRALISATION DES CONDENSATS (avec pompe de relevage)","DU13",914,null,null,"/","/","/",3661238015081,15,350,230,360,"C0"]
[82197762,"SYSTEME DE NEUTRALISATION DES CONDENSATS (JUSQU'À ≈ 19.200 L CONDENSATS)","BP52",571,null,null,"/","/","/",3661238020696,9.9,760,165,210,"C0"]
[94225601,"RECHARGE DE GRANULATS DE NEUTRALISATION 10 KG**",null,null,null,null,"/","/","/"]
[7603547,"KIT DE PREMONTAGE HYDRAULIQUE ","JA68",426,null,null,"/","/","/",3661238585973,8,815,415,250,"C0"]
[]
["OPTIONS ECS ET  PREPARATEURS INDEPENDANTS"]
[100018204,"VASE EXPANSION SANITAIRE 8L","ER233 ",289,null,null,"/","/","/",3661238514317,5,405,405,175,"C0"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.16,200,150,30,"C0"]
[100017393,"KIT RACC. BALLONS AUTRES","JA10",58,null,null,"/","/","/",3661238495258,1.2,630,210,230,"C0"]
[100000492,"KIT ANODE MAGNESIUM","EA103",66,null,null,"/","/","/",3661238011069,0.9,560,90,85,"C0"]
[89557009,"KIT DE TRANSFORMATION G/R 3/4 '' ET 1 ''","BH84",32,null,null,"/","/","/",3661238047563,0.32500000000000001,200,140,45,"C0"]
[]
["OPTIONS REGULATIONS"]
[88017904,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (FILAIRE)","AD191",161,0.12,95010,"/","/","/",3661238102415,0.25,135,90,55,"C0"]
[88017010,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (SANS FILS)","AD192",286,0.12,95010,"/","/","/",3661238102439,0.42499999999999999,180,150,90,"C0"]
[85757741,"SONDE EXTERIEURE","FM46",41,0.02,95020,"/","/","/",3661238022751,0.12,200,150,40,"C0"]
[7609764,"THERMOSTAT D'AMBIANCE MODULANT RADIO RS200 -3R","AD305",340,0.12,95010,"/","/","/",8713809266455,0.76600000000000001,150,100,110,"C0"]
[7609765,"THERMOSTAT D'AMBIANCE MODULANT FILAIRE RS200 -3","AD306",206,0.12,95010,"/","/","/",8713809266462,0.35099999999999998,150,100,50,"C0"]
[7612346," COMMANDE A DISTANCE SIMPLIFIEE RS20-OT FILAIRE","AD302",106,0.12,95010,"/","/","/",3661238599666,0.151,109,90,48,"C0"]
[]
["OPTIONS GSCX 25"]
[null,"FUMISTERIE"]
[null,"PPS Ø 60 MM"]
[84887585,"TERMINAL AVEC SOLIN DIAMÉTRE 80","DY185",148,null,null,"/","/","/",3661238013148,1.52,390,380,280,"C0"]
[84887690,"RALLONGE PPS D60 L500 2X ","DY690",40,null,null,"/","/","/",3661238012196,0.5,505,135,140,"C0"]
[84887691,"RALLONGE PPS D60L1000 2X ","DY691",47,null,null,"/","/","/",3661238012189,0.96,1025,135,140,"C0"]
[84887692,"RALLONGE PPS D60 L1950 2X","DY692",77,null,null,"/","/","/",3661238012172,1.9,1960,150,150,"C0"]
[84887693,"COUDE PPS D60 87°  ","DY693",25,null,null,"/","/","/",3661238012165,0.16,155,160,160,"C0"]
[84887694,"COUDE PPS Ø 60 45° (2X)","DY694",49,null,null,"/","/","/",3661238012158,0.19,155,155,160,"C0"]
[84887673,"ETOILE DE CENTRAGE PPS Ø 60 ","DY673",14,null,null,"/","/","/",3661238012363,0.1,400,400,400,"C0"]
[84887698,"PIECE DE VISITE PPS Ø 60 DROITE","DY698",64,null,null,"/","/","/",3661238012110,0.24,295,145,150,"C0"]
[84887741,"TE DE VISITE PPS Ø 60","DY741",71,null,null,"/","/","/",3661238011724,0.24,250,145,145,"C0"]
[84887700,"KIT DE RACCORDEMENT CHEMINEE PPS 60 MM","DY700",225,null,null,"/","/","/",3661238012103,2.71,395,400,385,"C0"]
[84887701,"KIT DE RACCORDEMENT CHEMINÉE PPS 60/80 MM","DY701",270,null,null,"/","/","/",3661238012097,2.83,395,400,385,"C0"]
[84887702,"KIT DE RACCORDEMENT CHAUDIERE ALU/PPS Ø 60/100 mm","DY702",181,null,null,"/","/","/",3661238012080,1.94,500,290,260,"C0"]
[null,"ALU Ø 80 MM"]
[84887585,"TERMINAL AVEC SOLIN DIAMÉTRE 80","DY185",148,null,null,"/","/","/",3661238013148,1.52,390,380,280,"C0"]
[84887600,"TUBE D'INSPECTION Ø 80 mm ","DY600",48,null,null,"/","/","/",3661238013094,0.49,300,145,150,"C0"]
[84887738,"TE DE VISITE Ø 80 mm ","DY738",71,null,null,"/","/","/",3661238011755,0.66,285,215,165,"C0"]
[84887604,"RALLONGE Ø 80 mm    L= 250 mm  (2 PIECES)","DY604",37,null,null,"/","/","/",3661238013056,0.65,255,170,175,"C0"]
[84887605,"RALLONGE Ø 80 mm    L=  500 mm  (2 PIECES)","DY605",45,null,null,"/","/","/",3661238013049,1.26,520,175,170,"C0"]
[84887606,"RALLONGE 1000 mm (2 PIECES)","DY606",72,null,null,"/","/","/",3661238013032,2.52,1020,175,175,"C0"]
[84887607,"RALLONGE Ø 80 mm    L=  1950 mm   (2 PIECES)","DY607",120,null,null,"/","/","/",3661238013025,5,1985,170,175,"C0"]
[84887551,"COLLIER DE CENTRAGE Ø 80mm (2 PIECES)","DY151",14,null,null,"/","/","/",3661238013452,0.1,300,300,40,"C0"]
[84887608,"COUDE A 90°","DY608",24,null,null,"/","/","/",3661238013018,0.34,155,160,160,"C0"]
[84887609,"COUDE A 45°  (2 PIECES)","DY609",40,null,null,"/","/","/",3661238013001,0.48,200,200,150,"C0"]
[84887711,"KIT N°1 RACCORDEMENT CHEMINEE Ø 80 mm","DY711",185,null,null,"/","/","/",3661238011991,3.66,595,400,410,"C0"]
[100002361,"PIÈCE D'ADAPTATION BIFLUX 2X80","DY819",44,null,null,"/","/","/",3661238007338,0.1,340,240,30,"C0"]
[84887438,"PRISE D'AIR EXTERIEURE LG=500 mm","DY38",99,null,null,"/","/","/",3661238013858,1.23,690,245,145,"C0"]
[84887723,"ADAPTATEUR BI-FLUX Ø60/100 SUR 2x80","DY723",83,null,null,"/","/","/",3661238011892,0.94,285,210,165,"C0"]
[]
["OPTIONS GSCX 25"]
[null,"PPS/ALU 60/100 MM"]
[100013756,"TERMINAL HORIZONTAL PPS/GALVA Ø 60/100 mm","HR48",187,null,null,"/","/","/",3661238370883,3.37,1200,200,200,"C0"]
[84887681,"PPS-ALU RALLONGE CONCENTRIQUE  ø 60/100 mm L=  500 mm","DY681",41,null,null,"/","/","/",3661238012288,0.72,510,135,140,"C0"]
[84887682,"PPS-ALU RALLONGE CONCENTRIQUE ø 60/100 mm L=1000 mm","DY682",51,null,null,"/","/","/",3661238012271,1.38,1010,130,135,"C0"]
[84887683,"PPS-ALU RALLONGE CONCENTRIQUE ø 60/100mm L=1950mm","DY683",104,null,null,"/","/","/",3661238012264,2.81,1960,150,150,"C0"]
[84887684,"PPS-ALU COUDE CONCENTRIQUE MOULE à 87° ø 60/100 mm","DY684",43,null,null,"/","/","/",3661238012257,0.53,200,200,150,"C0"]
[84887685,"PPS-ALU COUDE CONCENTRIQUE MOULE à 45° ø 60/100 mm (2 PIECES)","DY685",80,null,null,"/","/","/",3661238012240,0.65,250,185,150,"C0"]
[84887686,"PPS-ALU COUDE CONCENTRIQUE MOULE à 30° ø 60/100 mm (2 PIECES)","DY686",159,null,null,"/","/","/",3661238012233,0.63,250,190,155,"C0"]
[84887687,"PPS-ALU COUDE CONCENTRIQUE MOULE à 15° ø 60/100 mm (2 PIECES)","DY687",159,null,null,"/","/","/",3661238012226,0.64,255,195,150,"C0"]
[84887688,"PPS-ALU MANCHON DE COMPENSATION DE 50 à 250 mm","DY688",71,null,null,"/","/","/",3661238012219,0.51,515,135,140,"C0"]
[84887689,"PPS-ALU  PIECE DE REVISIONDROITE  Ø 60/100 mm","DY689",131,null,null,"/","/","/",3661238012202,0.56999999999999995,255,185,150,"C0"]
[84887737,"PPS-ALU  Té DE REVISION  Ø 60/100 mm","DY737",131,null,null,"/","/","/",3661238011762,0.6,255,185,145,"C0"]
[84887702,"KIT DE RACCORDEMENT CHAUDIERE ALU/PPS Ø 60/100 mm","DY702",181,null,null,"/","/","/",3661238012080,1.94,500,290,260,"C0"]
[100017526,"TERMINAL REFTROFIT Ø 60/95","DY912",115,null,null,"/","/","/",3661238496323,0.9,1200,180,110,"C0"]
[null,"FLEXIBLE PPS Ø 80 MM"]
[100015325,"KIT N° 1 RACCORDEMENT CHEMINÉE FLEXIBLE PPS Ø 80 mm","DY895",236,null,null,"/","/","/",3661238380110,2.87,395,395,380,"C0"]
[100015327,"TUBE FLEXIBLE LG=12,5M","DY897",354,null,null,"/","/","/",3661238380134,8.6999999999999993,1200,1220,250,"C0"]
[100015326,"TUBE FLEXIBLE LG=50M","DY896",1242,null,null,"/","/","/",3661238380127,35,1600,1660,410,"C0"]
[84887618,"ETOILE DE CENTRAGE POUR FLEXIBLE Ø 80  mm (2 PIÈCES)","DY618",37,null,null,"/","/","/",3661238012912,0.2,300,300,70,"C0"]
[100015328,"PIÈCE DE COUPLAGE FLEXIBLE Ø 80 mm","DY898",71,null,null,"/","/","/",3661238380141,0.25,150,150,150,"C0"]
[100015331,"OUTIL D'AIDE À L'INSERTION Ø 80 mm","DY901",177,null,null,"/","/","/",3661238380172,1.4,300,210,185,"C0"]
[100015330,"PIÈCE D'INSPECTION POUR TUBE FLEXIBLE","DY900",127,null,null,"/","/","/",3661238380165,0.5,295,140,140,"C0"]
[100015329,"TERMINAL AVEC SOLIN FLEX. Ø 80 mm","DY899",177,null,null,"/","/","/",3661238380158,1.74,385,385,250,"C0"]
[100015880,"ADAPTATEUR PPS FLEX Ø 80 mm","DY904",42,null,null,"/","/","/",3661238417632,0.125,316,236,152,"C0"]
[null,"PPS Ø 80 MM"]
[100015325,"KIT N° 1 RACCORDEMENT CHEMINÉE FLEXIBLE PPS Ø 80 mm","DY895",236,null,null,"/","/","/",3661238380110,2.87,395,395,380,"C0"]
[100017527,"KIT DE BASE PPS/ALU Ø 80/125 ","DY913",166,null,null,"/","/","/",3661238496330,3.7,600,400,275,"C0"]
[84887708,"ADAPTATEUR ALU Ø 60/100 MM SUR 80/125 MM","DY708",58,null,null,"/","/","/",3661238012028,0.33,255,145,150,"C0"]
[84887717,"KIT N° 1 KIT DE RACCORDEMENT CHEMINÉE PPS Ø 80 mm","DY717",157,null,null,"/","/","/",3661238011946,2.89,395,405,390,"C0"]
[84887546,"PIÈCE DE VISITE Ø 80 mm droite","DY146",58,null,null,"/","/","/",3661238013506,0.28999999999999998,300,145,150,"C0"]
[84887613,"RALLONGE PPS Ø 80 mm   L= 250 mm (2 PCS)","DY613",40,null,null,"/","/","/",3661238012967,0.37,250,170,175,"C0"]
[84887614,"RALLONGE PPS  Ø 80 mm   L=  500 mm (2 PCS)","DY614",38,null,null,"/","/","/",3661238012950,0.68,500,160,150,"C0"]
[84887615,"RALLONGE PPS  Ø 80 mm   L=  1000 mm (2 PCS)","DY615",51,null,null,"/","/","/",3661238012943,1.25,1000,160,145,"C0"]
[84887550,"RALLONGE PPS Ø 80 mm   L=  2000 mm  (2 PIECES)","DY150",77,null,null,"/","/","/",3661238013469,2.4900000000000002,1960,150,150,"C0"]
[84887552,"COUDE PPS À 90°","DY152",16,null,null,"/","/","/",3661238013445,0.2,255,145,150,"C0"]
[84887554,"COUDE PPS a 45°  (2 PCS)","DY154",35,null,null,"/","/","/",3661238013421,0.32,200,200,150,"C0"]
[84887563,"T PPS  AVEC COUVERCLE  D'INSPECTION","DY163",58,null,null,"/","/","/",3661238013353,0.39,290,220,170,"C0"]
[84887551,"COLLIER DE CENTRAGE Ø 80mm (2 PIECES)","DY151",14,null,null,"/","/","/",3661238013452,0.1,300,300,40,"C0"]
[84887585,"TERMINAL AVEC SOLIN DIAMÉTRE 80","DY185",148,null,null,"/","/","/",3661238013148,1.52,390,380,280,"C0"]
[100008301,"COUDE DE REVISION PPS 87° Ø 80 mm (GRIS)","DY877",41,null,null,"/","/","/",3661238102026,0.24,190,195,145,"C0"]
[null,"PPS 80/125 MM"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 mm NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[100002733,"TERMINAL VERTICAL PPS Ø 80/125 mm ROUGE","DY844",154,null,null,"/","/","/",3661238006614,4.2,1210,265,240,"C0"]
[84887716,"KIT N° 3 RACCORDEMENT CHAUDIÈRE  PPS Ø 80/125 mm","DY716",144,null,null,"/","/","/",3661238011953,2.36,500,290,260,"C0"]
[84887524,"PIECE D'INSPECTION DROITE ALU/PPS Ø 80/125 mm","DY124",110,null,null,"/","/","/",3661238013704,0.55000000000000004,300,145,150,"C0"]
[100008311,"COUDE DE REVISION ALU/PPS Ø 80/125 mm","DY875",115,null,null,"/","/","/",3661238101920,0.68,195,195,145,"C0"]
[100003271,"KIT DE RACCORDEMENT CHAUDIÈRE PERPENDICULAIRE","DY849",225,null,null,"/","/","/",3661238005600,3.5,595,395,410,"C0"]
[100003272,"KIT DE RACCORDEMENT CHAUDIÈRE SOUS CONDUIT","DY850",168,null,null,"/","/","/",3661238005594,1.44,500,290,260,"C0"]
[84887525,"T D'INSPECTION ALU/PPS Ø 80/125 mm","DY125",126,null,null,"/","/","/",3661238013698,0.82,315,235,150,"C0"]
[84887526,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 LG= 250 mm","DY126",41,null,null,"/","/","/",3661238013681,0.47,255,145,150,"C0"]
[84887527,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 L= 500 mm","DY127",47,null,null,"/","/","/",3661238013674,0.9,520,140,140,"C0"]
[84887528,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 L=1000 mm","DY128",69,null,null,"/","/","/",3661238013667,1.7,1010,135,140,"C0"]
[84887529,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 L=1950 mm","DY129",120,null,null,"/","/","/",3661238013650,3.5,1960,150,150,"C0"]
[84887530,"MANCHON DE COMPENS PPS D80/125 ","DY130",71,null,null,"/","/","/",3661238013643,0.6,300,140,145,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 mm","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[84887532,"COUDE CONCENTRIQUE 45° ALU/PPS Ø 80/125 MM (2 PCES)","DY132",77,null,null,"/","/","/",3661238013629,1,315,235,150,"C0"]
[null,"DIVERS FUMISTERIE"]
[84887411,"SORTIE HORIZONTALE TOIT PENTE DE 30° A 45° ( uniquement pour tuiles mécaniques)","DY11",179,null,null,"/","/","/",3661238013940,3.57,1020,700,370,"C0"]
[84837729,"SORTIE DE TOIT EN PENTE DE 40° A 60° ( uniquement pour tuiles mécaniques)","CX49",178,null,null,"/","/","/",3661238014367,3.5,920,700,320,"C0"]
[84837731,"EMBASE D'ETANCHE TOIT PLAT","CX51",43,null,null,"/","/","/",3661238014343,0.5,400,400,155,"C0"]
[84837121,"TUILE A DOUILLE 5 A 25° NOIRE","CX121",112,null,null,"/","/","/",3661238014428,2.96,510,250,145,"C0"]
[84837732,"TUILE A DOUILLE 25 A 45° NOIRE","CX52",77,null,null,"/","/","/",3661238014336,3,520,250,145,"C0"]
[84837734,"TUILE A DOUILLE 35 A 55° NOIRE","CX63",97,null,null,"/","/","/",3661238014312,3.17,510,265,180,"C0"]
[84837120,"TUILE A DOUILLE 5 A 25° ROUGE","CX120",112,null,null,"/","/","/",3661238014435,3.02,515,245,145,"C0"]
[84837783,"TUILE A DOUILLE 25 A 45° ROUGE","CX83",77,null,null,"/","/","/",3661238014213,3,515,250,150,"C0"]
[84837784,"TUILE A DOUILLE 35 A 55° ROUGE","CX84",97,null,null,"/","/","/",3661238014206,2.95,520,265,180,"C0"]
[84837741,"PLATINE DE FINITION INTER","CX72",17,null,null,"/","/","/",3661238014251,0.54,245,210,3,"C0"]
[100005002,"PANIER DE PROTECTION INOX  Ø 80/125","DY865",176,null,null,"/","/","/",3661238001886,2.59,275,270,270,"C0"]
[84887435,"GRILLE D'AERATION EXTERIEURE 250 X 300 mm","DY35",24,null,null,"/","/","/",3661238013889,0.35,300,250,30,"C0"]
[84887436,"GRILLE D'AERATION  INTERIEUR 250X300 mm","DY36",25,null,null,"/","/","/",3661238013889,0.35,300,250,30,"C0"]
[84837779,"COLLIER DE FIXATION Ø 125 mm PATTE LONGUE","CX79",15,null,null,"/","/","/",3661238014237,0.24,230,160,200,"C0"]
[84837118,"COLLIER DE FIXATION Ø 125 MM PATTE COURTE","CX118",12,null,null,"/","/","/",3661238014459,0.19,225,185,20,"C0"]
[]
[]
[100009941,"GSR 140-45 CONDENS","HF5",6218,3.34,"11.14","A","/","/",3661238169326,110,700,900,1290,"C0"]
[100009942,"GSR 140-65 CONDENS","HF6",7176,3.34,"11.14","A","/","/",3661238169333,118,700,900,1290,"C0"]
[100009943,"GSR 140-90 CONDENS","HF7",9819,3.34,"11.14","pas concerné par l'étiquettage",null,null,3661238169340,137.5,700,900,1500,"C0"]
[100009944,"GSR 140-115 CONDENS","HF8",11045,3.34,"11.14","pas concerné par l'étiquettage",null,null,3661238169357,138,700,900,1500,"C0"]
[]
["ACCESSOIRES CHAUDIERE"]
[100013072,"KIT DE TRANSFORMATION AU PROPANE","HE38",201,null,null,"/","/","/",3661238361829,1.3,210,200,85,"C0"]
[100004641,"ROBINET GAZ 3/4\" DROIT","HC158",44,null,null,"/","/","/",3661238002432,0.82,200,150,125,"C0"]
[100002312,"POMPE GMR 5045 3 VITESSES","HC141",221,null,null,"/","/","/",3661238007581,3.1,310,210,130,"C0"]
[100002313,"POMPE GMR 5045 ELECTRONIQUE","HC142",324,null,null,"/","/","/",3661238007574,3.1,310,210,130,"C0"]
[100002314,"CIRCULATEUR 3 VITESSES GMR 5065 ","HC143",251,null,null,"/","/","/",3661238007567,3.2,305,210,130,"C0"]
[100002316,"POMPE GMR 5090 3 VITESSES","HC145",388,null,null,"/","/","/",3661238007550,4.5,310,210,130,"C0"]
[100002323,"POMPE PRIMAIRE POUR GMR 5045-5065-5090","HC147",354,null,null,"/","/","/",3661238007499,4.5999999999999996,310,210,130,"C0"]
[82197762,"SYSTEME DE NEUTRALISATION DES CONDENSATS (JUSQU'À ≈ 19.200 L CONDENSATS)","BP52",571,null,null,"/","/","/",3661238020696,9.9,760,165,210,"C0"]
[83877009,"SYSTEME DE NEUTRALISATION DES CONDENSATS (avec pompe de relevage)","DU13",914,null,null,"/","/","/",3661238015081,15,350,230,360,"C0"]
[7613605,"STATION DE NEUTRALISATION DN1","SA1",344,null,null,"/","/","/",3661238592117,14.5,350,230,350,"C0"]
[83877011,"STATION NEUTRALISATION","DU15",1354,null,null,"/","/","/",3661238015067,20,660,455,270,"C0"]
[100002685,"CLAPET OBTURATEUR FUMEES  Ø 100 mm","HC154",470,null,null,"/","/","/",3661238006683,1.84,350,235,150,"C0"]
[100003347,"COMMANDE EXTERNE ALARME VANNE","GR12",89,0.02,95020,"/","/","/",3661238005358,0.36,195,150,125,"C0"]
[]
["OPTIONS REGULATION "]
[88017878,"MODULE DE TELESURVEILLANCE VOCAL TELCOM 2","AD152",704,0.12,95010,"/","/","/",3661238048751,1.1000000000000001,210,190,105,"C0"]
[161118,"COMMANDE A DISTANCE INTERACTIVE  AD194","AD194",197,0.12,95010,"/","/","/",3661238106505,0.15,0,0,0,"C0"]
[88017017,"SONDE DEPART v3v","AD199",80,0.02,95020,"/","/","/",3661238049185,0.21,150,200,40,"C0"]
[88017014," PLATINE + SONDE V3V","AD196",180,0.02,95020,"/","/","/",3661238102422,0.52,260,170,120,"C0"]
[88017851,"CABLE DE LIAISON BUS LG 12 M","AD134",110,0.02,95020,"/","/","/",3661238048850,0.37,350,260,30,"C0"]
[]
["OPTIONS MODULES HYDRAULIQUES GSR 140-35P CONDENS"]
[100009840,"KIT VANNE MELANGEUSE 3 VOIES INT","HE24",418,null,null,"/","/","/",3661238338487,5.5,410,190,195,"C0"]
[100009842,"KIT VANNE MELANGEUSE 3 VOIES EXT. ","HE 26",127,null,null,"/","/","/",3661238338494,1.4,260,165,115,"C0"]
[100020164,"COLLECTEUR 2/3 CIRCUITS","EA140",348,null,null,"/","/","/",3661238575011,6.6,660,180,200,"C0"]
[100020165,"CONSOLE MUR COLLECTEUR ","EA141",44,null,null,"/","/","/",3661238575028,1.2,220,125,70,"C0"]
[100020166,"CONSOLE MUR 1 MODULE ","EA142",116,null,null,"/","/","/",3661238575035,1.6,220,125,70,"C0"]
[100020167,"CIRCUIT DIRECT P.ELEC CLASSE A  ","EA143",644,0.83,14050,"/","/","/",3661238575042,5.0999999999999996,460,270,235,"C0"]
[100020168,"CIRCUIT V3V P.ELEC","EA144",916,0.83,14050,"/","/","/",3661238575059,6,460,270,235,"C0"]
[100020169,"MODULE HYDR COMPACT 2 CIRCUITS HEE","EA145",1146,0.83,14050,"/","/","/",3661238575059,9,525,415,210,"C0"]
[100019346,"BOUTEILLE DE DECOUPLAGE  60/60-1''  ","GV45",366,null,null,"/","/","/",3661238555013,3.83,690,375,205,"C0"]
[100019347,"BOUTEILLE DE DECOUPLAGE  80/60-1'' 1/4 ","GV46",438,null,null,"/","/","/",3661238555020,5.42,690,375,205,"C0"]
[100019348,"BOUTEILLE DE DECOUPLAGE  120/80-2''   ","GV47",589,null,null,"/","/","/",3661238555037,11.96,970,375,205,"C0"]
[]
[null,"OPTIONS ECS"]
[100009972,"BALLON OBA 150","EA84",1508,null,null,"/","/","/",3661238375239,106.5,700,900,1290,"C0"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.16,200,150,30,"C0"]
[100007827,"KIT LIAISON CHAUDIERE / BALLON","EA121",602,null,null,"/","/","/",3661238116528,6.5,600,500,135,"C0"]
[100009192,"KIT LIAISON CHAUDIERE / BALLON OBA 150","EA122",450,null,null,"/","/","/",3661238338463,5.5,575,505,150,"C0"]
[]
[]
["ACCESSOIRES CASCADES "]
[100011703,"COLLECTEUR DN65","HE35",497,null,null,"/","/","/",3661238366015,30,700,210,480,"C0"]
[100011492,"COLLECTEUR DN100","HE34",543,null,null,"/","/","/",3661238366008,35,1200,800,700,"C0"]
[100011490,"KIT DE LIAISON HYDRAULIQUE 45 ET 65 KW","HE32",592,null,null,"/","/","/",3661238365988,5,360,300,170,"C0"]
[100011491,"KIT DE LIAISON HYDRAULIQUE 90 ET 115 KW","HE33",599,null,null,"/","/","/",3661238365988,5,360,330,170,"C0"]
[114311,"BOUTEILLE DE DÉCOUPLAGE DN65 < 350 kW","HC222",617,null,null,"/","/","/",3661238362215,26.6,650,310,170,"C0"]
[111712,"BOUTEILLE DE DÉCOUPLAGE DN65 > 350 et < 460 kW","HC200",1024,null,null,"/","/","/",3661238338920,47,740,1060,370,"C0"]
[111714,"BOUTEILLE DE DÉCOUPLAGE DN100 > 460 kW","HC201",1239,null,null,"/","/","/",3661238338913,68,940,260,630,"C0"]
[111708,"JEU DE BOUCHONS","HC195",41,null,null,"/","/","/",3661238338937,0.7,200,130,30,"C0"]
[111701,"BRIDES PLEINES EAU DN65","HC198",148,null,null,"/","/","/",3661238338951,5.3,370,170,50,"C0"]
[111703,"BRIDES PLEINES EAU DN100","HC199",188,null,null,"/","/","/",3661238338944,10.3,450,230,70,"C0"]
[100002312,"POMPE CHAUFFAGE 3 VITESSES POUR MCA 45/DTG 45","HC141",221,null,null,"/","/","/",3661238007581,3.1,310,210,130,"C0"]
[100002314,"POMPE CHAUFFAGE 3 VITESSES POUR MCA 65/DTG 65","HC143",251,null,null,"/","/","/",3661238007567,3.2,310,210,130,"C0"]
[100002316,"POMPE CHAUFFAGE 3 VITESSES POUR MCA 90-115/DTG 90-115","HC145",388,null,null,"/","/","/",3661238007550,4.5,310,210,130,"C0"]
[100013027,"SONDE DE DÉPART + DOIGT DE GANT-BOUTEILLE < 350 kW","HC223",132,0.02,95020,"/","/","/",3661238362239,0.2,220,165,25,"C0"]
[100008701,"SONDE DE DÉPART + DOIGT DE GANT-BOUTEILLE > 350 kW","HC206",155,0.02,95020,"/","/","/",3661238338883,0.2,210,160,25,"C0"]
[88017836,"CABLE BUS RX11  LG 1,5 M","AD124",84,0.02,95020,"/","/","/",3661238338876,0.1,210,160,5,"C0"]
[]
["OPTIONS HYDRAULIQUES"]
[111788,"COUDES DN65","HC209",664,null,null,"/","/","/",3661238338883,13,700,300,170,"C0"]
[111790,"COUDES DN100","HC210",892,null,null,"/","/","/",3661238338876,21,440,440,420,"C0"]
[111167,"ISOLATION COUDES 90°C","HC216",103,null,null,"/","/","/",3661238339019,1,610,300,500,"C0"]
[112632,"JEU DE CONTRE-BRIDES À SOUDER DN65","HC217",153,null,null,"/","/","/",3661238338821,1.9,160,160,120,"C0"]
[112633,"JEU DE CONTRE-BRIDES À SOUDER DN100","HC218",171,null,null,"/","/","/",3661238338814,10.3,200,200,120,"C0"]
[115269,"ISOLATION BOUTEILLE DE DÉCOUPLAGE < 350 kW","HC224",38,null,null,"/","/","/",3661238362222,0.6,660,280,220,"C0"]
[111067,"ISOLATION BOUTEILLE DE DÉCOUPLAGE DN65 > 350 et < 460 kW","HC215",242,null,null,"/","/","/",3661238339033,4,300,620,960,"C0"]
[111807,"PIED RÉGLABLE","HC219",4,null,null,"/","/","/",3661238338845,0.8,230,115,5,"C0"]
[]
["AUTRES OPTIONS"]
["S101655","FILTRE GAZ DN50","HC255",518,null,null,"/","/","/",8713809234331,4.9000000000000004,465,280,230,"C0"]
["S101656","FILTRE GAZ DN65","HC256",715,null,null,"/","/","/",8713809243586,7,310,230,220,"C0"]
["S103345","JEUX DE BRIDES À SOUDER DN50 POUR FILTRE A GAZ","HC261",84,null,null,"/","/","/",null,6,31,16,15,"C0"]
[84887768,"ADAPTATEUR  80 X 100MM ","DY768",55,null,null,"/","/","/",3661238011489,0.24,150,145,155,"C0"]
[]
[]
[115768,"GSR 233 CONDENS","GW1",9405,3.33,"11.14","Pas concerné par l'étiquettage",null,null,8713809213671,170,1250,700,1470,"C3"]
[115769,"GSR 234 CONDENS","GW2",10658,3.33,"11.14","Pas concerné par l'étiquettage",null,null,8713809213688,190,1250,700,1470,"C3"]
[115770,"GSR 235 CONDENS","GW3",12301,3.33,"11.14","Pas concerné par l'étiquettage",null,null,8713809213695,210,189.5,700,1470,"C3"]
[115771,"GSR 236 CONDENS","GW4",13683,3.33,"11.14","Pas concerné par l'étiquettage",null,null,8713809213701,230,1250,700,1470,"C3"]
[]
["OPTIONS"]
[100002442,"COLIS 2 ème RETOUR C 210 Eco ","GR5",136,null,null,"/","/","/",3661238007000,1.55,650,75,75,"C0"]
[100002443,"DOIGT DE GANT POUR SONDE DEPART","GR6",48,null,null,"/","/","/",3661238006997,0.09,215,140,30,"C0"]
[100002445,"FILTRE A L'ASPIRATION D'AIR","GR8",435,null,null,"/","/","/",3661238006973,3.7,620,270,370,"C0"]
[100011030,"THERMOSTAT DE FUMEES","GV21",59,0.02,95020,"/","/","/",3661238338678,0.17,190,150,125,"C3"]
[100011031,"PRESSOSTAT MINI GAZ POUR GSR 233 & GSR 234 ","GV22(*)",64,0.02,95020,"/","/","/",3661238338685,0.5,195,140,115,"C3"]
[100011032,"KIT DE CONVERSION AU GPL POUR GSR 233 & GSR 234","GV23",513,null,null,"/","/","/",3661238338692,0.2,0,0,0,"C3"]
[100011034,"PRESSOSTAT MINI GAZ GSR 235 & GSR 236","GV25(*)",66,0.02,95020,"/","/","/",3661238338715,0.23,340,230,50,"C3"]
[100011033,"CLAPET DE FUMEE","GV24(*)",782,null,null,"/","/","/",3661238338708,2.5099999999999998,370,265,185,"C3"]
[100011035,"KIT CCE (Uniquement GSR 235 & GSR 236)","GV26(*)",60,0.02,95020,"/","/","/",3661238338722,0.23,340,230,50,"C3"]
[100011036,"KIT DE CONVERSION AU GPL POUR GSR 235 & GSR 236","GV27",40,null,null,"/","/","/",3661238338739,0.2,220,320,20,"C3"]
[100011037,"PLATINE DE RACCORDEMENT SCU-01","GW5",107,null,null,"/","/","/",3661238369283,0.2,195,140,115,"C3"]
[100011223,"REGULATEUR PRESSION 300 mbar GDJ25 RACCORDT. Ø 1''","AD245 ",184,null,null,"/","/","/",3661238338746,1.2,180,150,150,"C3"]
[88027177,"REGULATEUR DE PRESSION 300 Mbar RACORDT. Ø 2'","GDJ50",432,null,null,"/","/","/",3661238048287,3.1,255,220,205,"B2"]
[83877009,"SYSTEME DE NEUTRALISATION DES CONDENSATS (avec pompe DE relevage)","DU13",914,null,null,"/","/","/",3661238015081,15,350,230,360,"C0"]
[83877011,"STATION NEUTRALISATION","DU15",1354,null,null,"/","/","/",3661238015067,20,660,455,270,"C0"]
[7622188,"STATION DE NEUTRALISATION DN3 ","SA9",708,null,null,"/","/","/",3661238613454,6.5,660,460,270,"C3"]
[7613613,"RECHARGE GIALIT 25KG","SA7",83,null,null,"/","/","/",3661238592179,25.2,550,350,120,"C3"]
[7613610,"STATION DE NEUTRALISATION AVEC POMPE","SA4",1222,null,null,"/","/","/",3661238592148,36.5,640,420,370,"C3"]
[100013072,"KIT DE TRANSFORMATION AU PROPANE","HE38",201,null,null,"/","/","/",3661238361829,1.3,210,200,85,"C0"]
[100002685,"CLAPET OBTURATEUR FUMEES  Ø 100 mm","HC154",470,null,null,"/","/","/",3661238006683,1.84,350,235,150,"C0"]
[180566,"RECHARGE DE GRANULATS DE NEUTRALISATION 10 KG",null,null,null,null,"/","/","/",3661238075597,10,25,22,22]
[100019347,"BOUTEILLE DE DECOUPLAGE  80/60-1'' 1/4 ","GV46",438,null,null,"/","/","/",3661238555020,5.42,690,375,205,"C0"]
[100019348,"BOUTEILLE DE DECOUPLAGE  120/80-2''   ","GV47",589,null,null,"/","/","/",3661238555037,11.96,970,375,205,"C0"]
[7628752,"REGULATEUR PRESSION GDJ 15 ","SA11",144,null,null,"/","/","/",3661238624917,0.59,130,110,110,"C0"]
[7628753,"REGULATEUR PRESSION GDJ 20 ","SA12",177,null,null,"/","/","/",3661238624924,1.2,160,140,140,"C0"]
[null,"(*) Nécessite une platine SCU-01 (GW5)"]
[]
["OPTIONS POUR OETRONIC  3"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.16,200,150,30,"C0"]
[161118,"COMMANDE A DISTANCE INTERACTIVE  AD194","AD194",197,0.12,95010,"/","/","/",3661238106505,0.15,0,0,0,"C0"]
[88017017,"SONDE DEPART v3v","AD199",80,0.02,95020,"/","/","/",3661238049185,0.21,150,200,40,"C0"]
[88017014," PLATINE + SONDE V3V","AD196",180,0.02,95020,"/","/","/",3661238102422,0.52,260,170,120,"C0"]
[88017851,"CABLE DE LIAISON BUS LG 12 M","AD134",110,0.02,95020,"/","/","/",3661238048850,0.37,350,260,30,"C0"]
[]
["FUMISTERIE"]
[null,"CONFIGURATION VENTOUSE VERTICALE EN ALU Ø 150 mm"]
[100002473,"VENTOUSE VERTICALE ALU / GALVA Ø 150/220 mm","DY835",838,null,null,"/","/","/",3661238006805,16,1900,340,520,"C3"]
[100002404,"PIECE DE RACCORDEMENT AIR POUR VENTOUSE Ø 150 mm","DY830",105,null,null,"/","/","/",3661238007154,0.46,250,165,170,"C3"]
[100002470,"TÉ D'INSPECTION Ø 150 mm ALU","DY832",225,null,null,"/","/","/",3661238006836,1.4,350,285,190,"C3"]
[84887645,"RALLONGE  Ø 150 mm   LG = 500 mm","DY645",45,null,null,"/","/","/",3661238012646,1.1599999999999999,525,170,175,"C3"]
[84887646,"RALLONGE  Ø 150 mm   LG = 1000 mm ","DY646",78,null,null,"/","/","/",3661238012639,2.34,1020,170,175,"C3"]
[84887647,"RALLONGE  Ø 150 mm   LG = 1950 mm","DY647",139,null,null,"/","/","/",3661238012622,4.4800000000000004,1985,175,175,"C3"]
[84887648,"ETOILE DE CENTRAGE Ø 150 mm (2 PIECES)","DY648",51,null,null,"/","/","/",3661238012615,0.12,300,300,45,"C3"]
[84887649,"COUDE A 87° Ø 150 mm","DY649",85,null,null,"/","/","/",3661238012608,0.81,345,265,185,"C3"]
[84887650,"COUDE A 45° Ø 150 mm  (2 PIECES)","DY650",159,null,null,"/","/","/",3661238012592,1.07,340,265,185,"C3"]
[100002402,"SOLIN POUR TOIT PLAT Ø 160/220 mm","DY828",74,null,null,"/","/","/",3661238007178,0.65,490,490,150,"C3"]
[100002403,"SOLIN POUR TOIT INCLINÉ Ø 160/220 mm","DY829",159,null,null,"/","/","/",3661238007161,9.4,795,355,360,"C3"]
[100002692,"COLLIER DE FIXATION Ø 150 mm","DY841",12,null,null,"/","/","/",3661238006669,0.11,150,150,20,"C3"]
[100002700,"PLATINES DE FINITION INTERIEURES Ø 220 mm","DY840",38,null,null,"/","/","/",3661238006638,0.7,250,320,4,"C3"]
[100004243,"RALLONGE GALVA/ALU VENTOUSE HORIZONTALE F 150/220 LONG. 1M","DY864",298,null,null,"/","/","/",3661238004498,6,1205,235,235,"C3"]
[84887435,"GRILLE D'AERATION EXTERIEURE 250 X 300 mm","DY35",24,null,null,"/","/","/",3661238013889,0.35,300,250,30,"C0"]
[84887436,"GRILLE D'AERATION  INTERIEUR 250X300 mm","DY36",25,null,null,"/","/","/",3661238013889,0.35,300,250,30,"C0"]
[null,"PPS Ø 160 mm"]
[100002400,"VENTOUSE VERTICALE PPS GALVA Ø 160/220 mm","DY826",838,null,null,"/","/","/",3661238007192,15,1890,345,520,"C3"]
[100002404,"PIECE DE RACCORDEMENT AIR POUR VENTOUSE Ø 150 mm","DY830",105,null,null,"/","/","/",3661238007154,0.46,250,165,170,"C3"]
[100002399,"ADAPTATEUR PPS  Ø 150-160 mm","DY825",103,null,null,"/","/","/",3661238007208,0.5,200,210,230,"C3"]
[100002395,"RALLONGE PPS  Ø 160 mm LG = 1000 mm","DY821",120,null,null,"/","/","/",3661238007246,2.8,1155,230,230,"C3"]
[100002396,"RALLONGE PPS  Ø 160 mm LG =  500 mm","DY822",82,null,null,"/","/","/",3661238007239,1.5,650,295,190,"C3"]
[100002397,"COUDE PPS  87° Ø 160 mm","DY823",99,null,null,"/","/","/",3661238007222,0.8,265,270,265,"C3"]
[100002398,"COUDE PPS  45° Ø 160 mm","DY824",181,null,null,"/","/","/",3661238007215,1.4,390,290,255,"C3"]
[100002471,"TUBE D'INSPECTION Ø 160 mm LG  300 mm","DY833",157,null,null,"/","/","/",3661238006829,0.97,385,295,255,"C3"]
[100002472,"COUDE  DE REVISION Ø 160 mm","DY834",185,null,null,"/","/","/",3661238006812,0.9,265,265,260,"C3"]
[100002402,"SOLIN POUR TOIT PLAT Ø 160/220 mm","DY828",74,null,null,"/","/","/",3661238007178,0.65,490,490,150,"C3"]
[100002403,"SOLIN POUR TOIT INCLINÉ Ø 160/220 mm","DY829",159,null,null,"/","/","/",3661238007161,9.4,795,355,360,"C3"]
[100002693,"COLLIER DE FIXATION Ø 160 mm","DY842",13,null,null,"/","/","/",3661238006652,0.22,220,180,30,"C3"]
[100002700,"PLATINE DE FINITION INTERIEURES Ø 220 mm","DY840",38,null,null,"/","/","/",3661238006638,0.7,250,320,4,"C3"]
[100004040,"RALLONGE VENTOUSE PPS HORIZONTALE Ø160/200 L.1M ","DY857",258,null,null,"/","/","/",3661238004993,5.58,1205,235,235,"C3"]
[null,"CONFIGURATION VENTOUSE HORIZONTALE EN PPS Ø 160 mm"]
[100002401,"VENTOUSE HORIZONTALE PPS GALVA Ø 160/220 mm","DY827",690,null,null,"/","/","/",3661238007185,8.1999999999999993,390,290,1005,"C3"]
[100002404,"PIECE DE RACCORDEMENT AIR POUR VENTOUSE Ø 150 mm","DY830",105,null,null,"/","/","/",3661238007154,0.46,250,165,170,"C3"]
[100002399,"ADAPTATEUR PPS  Ø 150-160 mm","DY825",103,null,null,"/","/","/",3661238007208,0.5,200,210,230,"C3"]
[100002395,"RALLONGE PPS  Ø 160 mm LG = 1000 mm","DY821",120,null,null,"/","/","/",3661238007246,2.8,1155,230,230,"C3"]
[100002396,"RALLONGE PPS  Ø 160 mm LG = 500 mm","DY822",82,null,null,"/","/","/",3661238007239,1.5,650,295,190,"C3"]
[100002397,"COUDE PPS  87° Ø 160 mm","DY823",99,null,null,"/","/","/",3661238007222,0.8,265,270,265,"C3"]
[100002398,"COUDE PPS  45° Ø 160 mm","DY824",181,null,null,"/","/","/",3661238007215,1.4,390,290,255,"C3"]
[100002471,"TUBE D'INSPECTION Ø 160 mm LG  300 mm","DY833",157,null,null,"/","/","/",3661238006829,0.97,385,295,255,"C3"]
[100002472,"COUDE  DE REVISION Ø 160 mm","DY834",185,null,null,"/","/","/",3661238006812,0.9,265,265,260,"C3"]
[null," ALU Ø 150 mm"]
[100002469,"VENTOUSE HORIZONTALE ALU / GALVA Ø 150/220 mm","DY831",690,null,null,"/","/","/",3661238006843,8,395,295,1210,"C3"]
[100002404,"PIECE DE RACCORDEMENT AIR POUR VENTOUSE Ø 150 mm","DY830",105,null,null,"/","/","/",3661238007154,0.46,250,165,170,"C3"]
[100002470,"TÉ D'INSPECTION Ø 150 mm ALU","DY832",225,null,null,"/","/","/",3661238006836,1.4,350,285,190,"C3"]
[84887645,"RALLONGE  Ø 150 mm   LG = 500 mm ","DY645",45,null,null,"/","/","/",3661238012646,1.1599999999999999,525,170,175,"C3"]
[84887646,"RALLONGE  Ø 150 mm   LG = 1000 mm","DY646",78,null,null,"/","/","/",3661238012639,2.34,1020,170,175,"C3"]
[84887647,"RALLONGE  Ø 150 mm   LG = 1950 mm","DY647",139,null,null,"/","/","/",3661238012622,4.4800000000000004,1985,175,175,"C3"]
[84887649,"COUDE A 87° Ø 150 mm ","DY649",85,null,null,"/","/","/",3661238012608,0.81,345,265,185,"C3"]
[84887650,"COUDE A 45° Ø 150 mm  (2 PIECES)","DY650",159,null,null,"/","/","/",3661238012592,1.07,340,265,185,"C3"]
[100003968,"COUDE 87° AVEC SUPPORT Ø 150 mm","DY855",141,null,null,"/","/","/",3661238005013,1.51,650,295,190,"C3"]
[100003969,"PLAQUE DE FINITION CHEMINEE Ø 150 mm","DY856",41,null,null,"/","/","/",3661238005006,0.39,310,235,145,"C3"]
[84887780,"TERMINAL Ø 150 mm","DY780",335,null,null,"/","/","/",3661238011373,3.23,395,400,410,"C3"]
[null,"RACCORDEMENT CHEMINEE  PPS Ø 160 mm"]
[100002399,"ADAPTATEUR PPS  Ø 150-160 mm","DY825",103,null,null,"/","/","/",3661238007208,0.5,200,210,230,"C3"]
[100002395,"RALLONGE PPS  Ø 160 mm LG =1000 mm","DY821",120,null,null,"/","/","/",3661238007246,2.8,1155,230,230,"C3"]
[100002396,"RALLONGE PPS  Ø 160 mm LG =  500 mm","DY822",82,null,null,"/","/","/",3661238007239,1.5,650,295,190,"C3"]
[100002397,"COUDE PPS  87° Ø 160 mm","DY823",99,null,null,"/","/","/",3661238007222,0.8,265,270,265,"C3"]
[100002398,"COUDE PPS  45° Ø 160 mm","DY824",181,null,null,"/","/","/",3661238007215,1.4,390,290,255,"C3"]
[100002399,"ADAPTATEUR PPS 150/160 mn","DY825",103,null,null,"/","/","/",3661238007208,0.5,200,210,230,"C3"]
[100002472,"COUDE  DE REVISION Ø 160 mm","DY834",185,null,null,"/","/","/",3661238006812,0.9,265,265,260,"C3"]
[100002471,"TUBE D'INSPECTION Ø 160 mm LG  300 mm","DY833",157,null,null,"/","/","/",3661238006829,0.97,385,295,255,"C3"]
[100002474,"COUDE PPS  87° Ø 160 mm AVEC SUPPORT","DY836",179,null,null,"/","/","/",3661238006799,1.5,390,295,255,"C3"]
[100002475,"TERMINAL AVEC SOLIN  Ø 160 mm","DY837",175,null,null,"/","/","/",3661238006782,3.2,400,405,410,"C3"]
[100002476,"PLAQUE DE FINITION CHEMINEE  Ø 160 mm","DY838",40,null,null,"/","/","/",3661238006775,0.2,300,300,35,"C3"]
[84887773,"FOURREAU Ø165mm L 500mm","DY773",41,null,null,"/","/","/",3661238011441,1.23,515,165,170,"C3"]
[100002540,"ETOILE DE CENTRAGE Ø 160 mm","DY839",51,null,null,"/","/","/",3661238006768,0.11,350,300,30,"C3"]
[100002693,"COLLIER DE FIXATION Ø 160 mm","DY842",13,null,null,"/","/","/",3661238006652,0.22,220,180,30,"C3"]
[100010270,"PLAQUE DE FINITION ","DY879",44,null,null,"/","/","/",3661238338609,0.44,305,230,145,"C0"]
[100017634,"ADAPTATEUR PPS  Ø 150-110 mm","DY915",106,null,null,"/","/","/",3661238497092,0.46,260,170,180,"C0"]
[]
[]
[100019730,"GSR 330-5 Condens VG ","JB21",17832,3.33,"11.14","Pas concerné par l'étiquettage",null,null,3661238568617,424,800,1920,2160,"C3"]
[100019731,"GSR 330-5 Condens VD","JB22",17822,3.33,"11.14","Pas concerné par l'étiquettage",null,null,3661238568624,424,800,1920,2160,"C3"]
[100019732,"GSR 330-6 Condens VG","JB23",22063,3.33,"11.14","Pas concerné par l'étiquettage",null,null,3661238568631,458,800,1920,2160,"C3"]
[100019733,"GSR 330-6 Condens VD","JB24",22063,3.33,"11.14","Pas concerné par l'étiquettage",null,null,3661238568648,458,800,1920,2160,"C3"]
[100019735,"GSR 330-7 Condens VG","JB25",26303,3.33,"11.14","Pas concerné par l'étiquettage",null,null,3661238568655,493,800,1920,2160,"C3"]
[100019736,"GSR 330-7 Condens VD","JB26",26303,3.33,"11.14","Pas concerné par l'étiquettage",null,null,3661238568662,493,800,1920,2160,"C3"]
[100019737,"GSR 330-8 Condens VG","JB27",30544,3.33,"11.14","Pas concerné par l'étiquettage",null,null,3661238568679,560,800,2230,2160,"C3"]
[100019738,"GSR 330-8 Condens VD","JB28",30544,3.33,"11.14","Pas concerné par l'étiquettage",null,null,3661238568686,560,800,2230,2160,"C3"]
[100019739,"GSR 330-9 Condens VG","JB29",34784,3.33,"11.14","Pas concerné par l'étiquettage",null,null,3661238568693,596,800,2230,2160,"C3"]
[100019740,"GSR 330-9 Condens VD","JB30",34784,3.33,"11.14","Pas concerné par l'étiquettage",null,null,3661238568709,596,800,2230,2160,"C3"]
[100019741,"GSR 330-10 Condens VG","JB31",39026,3.33,"11.14","Pas concerné par l'étiquettage",null,null,3661238568716,633,800,2230,2160,"C3"]
[100019742,"GSR 330-10 Condens VD","JB32",39026,3.33,"11.14","Pas concerné par l'étiquettage",null,null,3661238568723,633,800,2230,2160,"C3"]
[]
[100019743,"GSR 330-5 DUO Condens","JB33",37214,3.33,"11.14","Pas concerné par l'étiquettage",null,null,3661238568730,827,1600,1920,2160,"C3"]
[100019744,"GSR 330-6 DUO Condens","JB34",45696,3.33,"11.14","Pas concerné par l'étiquettage",null,null,3661238568747,891,1600,1920,2160,"C3"]
[100019745,"GSR 330-7 DUO Condens","JB35",54177,3.33,"11.14","Pas concerné par l'étiquettage",null,null,3661238568754,957,1600,1920,2160,"C3"]
[100019746,"GSR 330-8 DUO Condens","JB36",62660,3.33,"11.14","Pas concerné par l'étiquettage",null,null,3661238568761,1087,1600,2230,2160,"C3"]
[100019747,"GSR 330-9 DUO Condens","JB37",71141,3.33,"11.14","Pas concerné par l'étiquettage",null,null,3661238568778,1200,1600,2230,2160,"C3"]
[100019748,"GSR 330-10 DUO Condens","JB38",79623,3.33,"11.14","Pas concerné par l'étiquettage",null,null,3661238568785,1225,1600,2230,2160,"C3"]
[]
["OPTIONS"]
["S101806","ISOLATION ECHANGEUR GSR 330 - 5 ELEMENTS (prémonté en usine sur demande)",null,443,null,null,"/","/","/",8713809259532,4.83,1065,810,65,"C3"]
["S101807","ISOLATION ECHANGEUR GSR 330 - 6 ELEMENTS (prémonté en usine sur demande)",null,443,null,null,"/","/","/",8713809259549,5.17,1065,810,65,"C3"]
["S103307","ISOLATION ECHANGEUR GSR 330 - 7 ELEMENTS (prémonté en usine sur demande)",null,443,null,null,"/","/","/",8713809259570,5.52,1065,810,65,"C3"]
["S103308","ISOLATION ECHANGEUR GSR 330 - 8 ELEMENTS (prémonté en usine sur demande)",null,443,null,null,"/","/","/",8713809259587,5.93,1065,810,65,"C3"]
["S103309","ISOLATION ECHANGEUR GSR 330 - 9 ELEMENTS (prémonté en usine sur demande)",null,443,null,null,"/","/","/",8713809259594,6.29,1065,810,65,"C3"]
["S103310","ISOLATION ECHANGEUR GSR 330 - 10 ELEMENTS (prémonté en usine sur demande)",null,443,null,null,"/","/","/",8713809259600,6.62,1065,810,65,"C3"]
["S101776","2EME RETOUR POUR GSR 330-5 CONDENS (prémonté en usine sur demande)",null,349,null,null,"/","/","/",8713809259358,11,1000,310,310,"C3"]
["S101777","2EME RETOUR POUR GSR 330-6 CONDENS (prémonté en usine sur demande)",null,349,null,null,"/","/","/",8713809259365,11.5,640,260,380,"C3"]
["S101778","2EME RETOUR POUR GSR 330-7 CONDENS (prémonté en usine sur demande)",null,349,null,null,"/","/","/",8713809259372,12,1000,310,310,"C3"]
["S101779","2EME RETOUR POUR GSR 330-8 CONDENS (prémonté en usine sur demande)",null,349,null,null,"/","/","/",8713809259389,12,1000,310,310,"C3"]
["S101780","2EME RETOUR POUR GSR 330-9 CONDENS (prémonté sur demande en usine)",null,349,null,null,"/","/","/",8713809259396,12.5,1000,310,310,"C3"]
["S101781","2EME RETOUR POUR GSR 330-10 CONDENS (prémonté sur demande en usine)",null,349,null,null,"/","/","/",8713809259402,12.5,1000,310,310,"C3"]
["S101784","PRESSOSTAT MANQUE D'EAU (prémonté sur demande en usine) ",null,222,0.02,95020,"/","/","/",8713809259419,0.188,230,160,80,"C3"]
["S103305","CONTROLE D'ETANCHEITE BLOC GAZ HONEYWELL 5 A 9 ELTS (prémonté sur demande en usine)",null,75,0.02,95020,"/","/","/",8713809259426,0.24,140,110,67,"C3"]
["S101724","CONTROLE D'ETANCHEITE BLOC GAZ DUNGS - 10 ELTS (prémonté sur demande en usine)",null,134,0.02,95020,"/","/","/",8713809259433,"0,,228",140,70,110,"C3"]
["S103306","PRESSOSTAT GAZ MINI POUR BLOC GAZ HONEYWELL 5 A 9 ELTS (prémonté sur demande en usine)  ",null,80,0.02,95020,"/","/","/",8713809259563,0.23599999999999999,140,110,67,"C3"]
["S101805","PRESSOSTAT GAZ MINI POUR BLOC GAZ DUNGS - 10 ELTS (prémonté sur demande en usine)  ",null,129,0.02,95020,"/","/","/",8713809259440,0.23599999999999999,140,75,115,"C3"]
[100002454,"FILTRE A L'ASPIRATION D'AIR","GS20",545,null,null,"/","/","/",3661238006973,3.7,620,270,370,"C3"]
[100011223,"REGULATEUR PRESSION 300 mbar GDJ25 RACCORDT. Ø 1''","AD245 ",184,null,null,"/","/","/",3661238338746,1.2,180,150,150,"C3"]
[88027177,"REGULATEUR PRESSION 300 mbar GDJ 50 RACCORDT. Ø 2''","GDJ50",432,null,null,"/","/","/",3661238048287,3.1,255,220,205,"B2"]
["S103023","SONDE/THERMOSTAT FUMEE ",null,68,0.02,95020,"/","/","/",8713809259464,0.124,220,190,30,"C3"]
["S101775","BRIDE D'ADAPTATION DE 4 A 8 TROUS POUR POMPE",null,247,null,null,"/","/","/",8713809243807,0.9,320,320,160,"C3"]
[100002455,"COUTEAU DE NETTOYAGE","GS21",21,null,null,"/","/","/",3661238006874,0.18,725,35,35,"C3"]
[7622256,"STATION DE NEUTRALISATION 0-1300 KW DN3",null,874,null,null,"/","/","/",3661238613461,null,null,null,null,"C3"]
[7606977,"CONTRE-BRIDE DEPART/RETOUR",null,103,null,null,"/","/","/",8713809264338,null,null,null,null,"C3"]
[7606978,"CONTRE-BRIDE 2EME RETOUR",null,45,null,null,"/","/","/",8713809264345,null,null,null,null,"C3"]
[35506,"GRANULATS 6 KG FIN / 1,25 KG MOYEN  (DISPO AU CPR)",null,null,null,null,"/","/","/",8713809071271,7.8,390,170,180,"P/R"]
[83877011,"STATION NEUTRALISATION (avec pompe)","DU15",1354,null,null,"/","/","/",3661238015067,20,660,455,270,"C0"]
[94225601,"RECHARGE DE GRANULATS DE NEUTRALISATION 10 KG**",null,null,null,null,"/","/","/",3661238075597,10,25,22,22]
[]
["OPTIONS POUR TABLEAU DE COMMANDE HMI STANDARD"]
[100015062,"BOITIER OETRONIC 4-DIN AVEC FAISCEAU CABLAGE ET SONDES","AD260",818,0.12,95010,"/","/","/",3661238415911,2.0499999999999998,290,220,170,"C0"]
[100018921,"PLATINE INTERFACE MODBUS/OPENTHERM POUR CASCADE","AD287",110,0.02,95020,"/","/","/",3661238544925,0.8,150,210,20,"C3"]
[85757741,"SONDE EXTERIEURE POUR TABLEAU HMI STANDARD","FM46",41,0.02,95020,"/","/","/",3661238022751,0.12,200,150,40,"C0"]
[88017904,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (FILAIRE)","AD191",161,0.12,95010,"/","/","/",3661238102415,0.25,135,90,55,"C0"]
[88017010,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (SANS FILS)","AD192",286,0.12,95010,"/","/","/",3661238102439,0.42499999999999999,180,150,90,"C0"]
[88017836,"CABLE BUS RX11  LG 1,5 M","AD124",84,0.02,95020,"/","/","/",3661238048911,0.06,210,160,5,"C0"]
[]
["OPTIONS POUR BOITIER REGULATION OETRONIC 4-DIN"]
[100013305,"SONDE BALLON TAMPON OU SONDE DEPART CASCADE","AD250",46,0.02,95020,"/","/","/",3661238363588,0.13400000000000001,150,210,25,"C0"]
[100004781,"SONDE PLONGEUR + DOIGT DE GANT","AD218",186,0.02,95020,"/","/","/",3661238002234,0.32,190,145,120,"C0"]
[100013477,"COMMANDE A DISTANCE FILAIRE RS 400","AD257",177,0.12,95010,"/","/","/",3661238364257,0.253,175,122,60,"C0"]
[100013472," CDE A DISTANCE RADIO RS 400R     ","AD255",238,0.12,95010,"/","/","/",3661238364233,0.253,175,122,60,"C0"]
[100013307,"MODULE CHAUDIERE RADIO (EMETTEUR)","AD252",123,0.12,95010,"/","/","/",3661238363601,0.32,260,160,130,"C0"]
[100013306,"SONDE EXTERIEURE RADIO ","AD251",77,0.12,95010,"/","/","/",3661238363595,0.15,150,210,40,"C0"]
[100002803,"COMMANDE A DISTANCE SIMPLIFIEE AD208","AD208",104,0.12,95010,"/","/","/",3661238554931,0.2,120,85,40,"C0"]
[88017878,"MODULE DE TELESURVEILLANCE VOCAL  \"TELCOM 2","AD152",704,0.12,95010,"/","/","/",3661238048751,1.05,210,190,105,"C0"]
[88017836,"CABLE BUS RX11  LG 1,5 M","AD124",84,0.02,95020,"/","/","/",3661238048911,0.06,210,160,5,"C0"]
[88017835,"CABLE BUS LG 10 M AVEC UN EMBOUT DENUDE","AD123",89,0.02,95020,"/","/","/",3661238048928,0.31,350,260,20,"C0"]
[88017851,"CABLE DE LIAISON BUS LG 12 M","AD134",110,0.02,95020,"/","/","/",3661238048850,0.37,350,260,30,"C0"]
[81997720,"CABLE LIAISON BUS LG 40 M ","DB119",149,0.02,95020,"/","/","/",3661238001350,1.34,310,215,130,"C0"]
[]
["REGULATION MURALE OETRONIC 4-MR"]
[100018255,"OE-TRONIC 4 MR","AD282",1053,0.12,95010,"/","/","/",3661238514454,2,360,280,140,"C0"]
[85757741,"SONDE EXTERIEURE","FM46",41,0.02,95020,"/","/","/",3661238022751,0.12,200,150,40,"C0"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.16,200,150,30,"C0"]
[88017017,"SONDE DEPART V3V","AD199",80,0.02,95020,"/","/","/",3661238049185,0.21,150,200,40,"C0"]
[100013305,"SONDE POUR BALLON TAMPON","AD250",46,0.02,95020,"/","/","/",3661238363588,0.13400000000000001,150,210,25,"C0"]
[100013477,"COMMANDE A DISTANCE FILAIRE RS 400","AD257",177,0.12,95010,"/","/","/",3661238364257,0.253,175,122,60,"C0"]
[100013472," CDE A DISTANCE RADIO RS 400R     ","AD255",238,0.12,95010,"/","/","/",3661238364233,0.253,175,122,60,"C0"]
[100013307,"MODULE CHAUDIERE RADIO (EMETTEUR)","AD252",123,0.12,95010,"/","/","/",3661238363601,0.32,260,160,130,"C0"]
[100002803,"COMMANDE A DISTANCE SIMPLIFIEE AD208","AD208",104,0.12,95010,"/","/","/",3661238554931,0.2,120,85,40,"C0"]
[100013306,"SONDE EXTERIEURE RADIO ","AD251",77,0.12,95010,"/","/","/",3661238363595,0.15,150,210,40,"C0"]
[88017836,"CABLE BUS RX11  LG 1,5 M","AD124",84,0.02,95020,"/","/","/",3661238048911,0.06,210,160,5,"C0"]
[88017851,"CABLE DE LIAISON BUS LG 12 M","AD134",110,0.02,95020,"/","/","/",3661238048850,0.37,350,260,30,"C0"]
[81997720,"CABLE LIAIS.CDI 40M ","DB119",149,0.02,95020,"/","/","/",3661238001350,1.34,310,215,130,"C0"]
[100004781,"SONDE PLONGEUR + DOIGT DE GANT","AD218",186,0.02,95020,"/","/","/",3661238002234,0.32,190,145,120,"C0"]
[]
["ACCESSOIRES MODULES HYDRAULIQUES "]
[7622302,"MODULE HYDRAULIQUE POUR GSR 330-5 DUO CONDENS ",null,9339,null,null,"/","/","/",3661238591813,376,1170,950,1600,"C3"]
[7622304,"MODULE HYDRAULIQUE POUR GSR 330-6 DUO CONDENS ",null,9594,null,null,"/","/","/",3661238591820,378,1170,950,1600,"C3"]
[7622306,"MODULE HYDRAULIQUE POUR GSR 330-7 DUO CONDENS ",null,10072,null,null,"/","/","/",3661238591837,378,1170,950,1600,"C3"]
[7622307,"MODULE HYDRAULIQUE POUR GSR 330-8 DUO CONDENS ",null,10312,null,null,"/","/","/",3661238591844,385,1170,950,1600,"C3"]
[7622308,"MODULE HYDRAULIQUE POUR GSR 330-9 ET 10 DUO CONDENS ",null,10826,null,null,"/","/","/",3661238591851,407,1170,950,1600,"C3"]
[100016229,"GROUPE DE SECURITE",null,2700,null,null,null,null,null,3661238495661,18,600,400,200,"C3"]
[7613414,"ENSEMBLE COUDES DEPART/RETOUR POUR KIT RACC DROITE OU GAUCHE",null,940,null,null,"/","/","/",3661238591868,65,500,500,300,"C3"]
[7613415,"KIT DEMAGNETISEUR DES BOUES ",null,155,null,null,"/","/","/",3661238591875,1.5,250,200,200,"C3"]
[7616233,"MODULE HYDRAULIQUE COMPACT POUR 2 CIRCUITS","MT12",1686,0.83,14050,"/","/","/",3661238600614,12.2,530,415,215,"C3"]
[100020169,"MODULE HYDR COMPACT 2 CIRCUITS CLASSE A ","EA145",1146,0.83,14050,"/","/","/",3661238575059,9,525,415,210,"C0"]
[]
["ECHANGEUR DE CHALEUR DE SEPARATION DE CIRCUITS DE 85 à 650 Kw"]
["MODELES NON ISOLES EP NT"]
[7609004,"ECH PLAQUES NT-85","EC735",2658,null,null,"/","/","/",3661238591936,88,870,270,790,"C3"]
[7609005,"ECH PLAQUES NT-100","EC736",2754,null,null,"/","/","/",3661238592186,90,870,270,790,"C3"]
[7609007,"ECH PLAQUES NT-130","EC737",2856,null,null,"/","/","/",3661238592193,94,870,270,790,"C3"]
[7609008,"ECH PLAQUES NT-180","EC738",3148,null,null,"/","/","/",3661238592209,103,870,270,790,"C3"]
[7609084,"ECH PLAQUES NT-205","EC743",3255,null,null,"/","/","/",3661238592216,268,1390,400,860,"C3"]
[7609085,"ECH PLAQUES NT-280","EC744",3640,null,null,"/","/","/",3661238592223,282,1390,400,860,"C3"]
[7609086,"ECH PLAQUES NT-350","EC745",4018,null,null,"/","/","/",3661238592230,296,1390,400,860,"C3"]
[7609087,"ECH PLAQUES NT-425","EC746",4461,null,null,"/","/","/",3661238592247,315,1390,400,1060,"C3"]
[7609088,"ECH PLAQUES NT-500","EC747",4931,null,null,"/","/","/",3661238592254,329,1390,400,1060,"C3"]
[7609089,"ECH PLAQUES NT-575","EC748",5356,null,null,"/","/","/",366123859226,342,1390,400,1060,"C3"]
[7609090,"ECH PLAQUES NT-650","EC749",5919,null,null,"/","/","/",3661238592278,359,1390,400,1060,"C3"]
[]
["MODELES ISOLES EP NT A"]
[7609010,"ECH ISOLATION NT-85A",null,{"$f":"+D3020+D3031","v":3408},null,null,"/","/","/",3661238599031,null,null,null,null,"C3"]
[7609011,"ECH ISOLATION NT-100A",null,{"$f":"D3021+D3031","v":3504},null,null,"/","/","/",3661238610408,null,null,null,null,"C3"]
[7609012,"ECH ISOLATION NT-130A",null,{"$f":"D3022+D3031","v":3606},null,null,"/","/","/",3661238610712,null,null,null,null,"C3"]
[7609013,"ECH ISOLATION NT-180A",null,{"$f":"D3023+D3031","v":3898},null,null,"/","/","/",3661238610729,null,null,null,null,"C3"]
[7609092,"ECH ISOLATION NT-205A",null,{"$f":"D3024+D3031","v":4005},null,null,"/","/","/",3661238610736,null,null,null,null,"C3"]
[7609093,"ECH ISOLATION NT-280A",null,{"$f":"D3025+D3031","v":4390},null,null,"/","/","/",3661238610743,null,null,null,null,"C3"]
[7609094,"ECH ISOLATION NT-350A",null,4799,null,null,"/","/","/",3661238610750,null,null,null,null,"C3"]
[7609096,"ECH ISOLATION NT-425A",null,{"$f":"D3027+D3032","v":5242},null,null,"/","/","/",3661238599048,null,null,null,null,"C3"]
[7609098,"ECH ISOLATION NT-500A",null,{"$f":"D3028+D3032","v":5712},null,null,"/","/","/",3661238599055,null,null,null,null,"C3"]
[7609099,"ECH ISOLATION NT-575A",null,6165,null,null,"/","/","/",3661238599062,null,null,null,null,"C3"]
[7609100,"ECH ISOLATION NT-650A",null,{"$f":"D3030+D3033","v":6728},null,null,"/","/","/",3661238599079,null,null,null,null,"C3"]
[]
["COMPOSANTS"]
[7609004,"ECH PLAQUES NT-85","EC735",2658,null,null,"/","/","/",3661238591936,88,870,270,790,"C3"]
[7609005,"ECH PLAQUES NT-100","EC736",2754,null,null,"/","/","/",3661238592186,90,870,270,790,"C3"]
[7609007,"ECH PLAQUES NT-130","EC737",2856,null,null,"/","/","/",3661238592193,94,870,270,790,"C3"]
[7609008,"ECH PLAQUES NT-180","EC738",3148,null,null,"/","/","/",3661238592209,103,870,270,790,"C3"]
[7609084,"ECH PLAQUES NT-205","EC743",3255,null,null,"/","/","/",3661238592216,268,1390,400,860,"C3"]
[7609085,"ECH PLAQUES NT-280","EC744",3640,null,null,"/","/","/",3661238592223,282,1390,400,860,"C3"]
[7609086,"ECH PLAQUES NT-350","EC745",4018,null,null,"/","/","/",3661238592230,296,1390,400,860,"C3"]
[7609087,"ECH PLAQUES NT-425","EC746",4461,null,null,"/","/","/",3661238592247,315,1390,400,1060,"C3"]
[7609088,"ECH PLAQUES NT-500","EC747",4931,null,null,"/","/","/",3661238592254,329,1390,400,1060,"C3"]
[7609089,"ECH PLAQUES NT-575","EC748",5356,null,null,"/","/","/",366123859226,342,1390,400,1060,"C3"]
[7609090,"ECH PLAQUES NT-650","EC749",5919,null,null,"/","/","/",3661238592278,359,1390,400,1060,"C3"]
[7609101,"ISOLATION ECH NT 85-280","EC757",750,null,null,null,null,null,3661238592285,10,850,280,650,"C3"]
[7609102,"ISOLATION ECH NT 350-500","EC758",781,null,null,null,null,null,3661238592292,10,850,280,650,"C3"]
[7609103,"ISOLATION ECH NT 575-650","EC759",809,null,null,null,null,null,3661238592308,10,850,280,650,"C3"]
[]
["FUMISTERIE"]
["S103179","REDUCTION Ø250 A Ø200",null,167,null,null,"/","/","/",8713809259556,0.94,265,265,160,"C3"]
["S103118","KIT DE CONNEXION FUMEE POUR 2 X GSR 330 Condens",null,2211,null,null,"/","/","/",8713809258306,39,1200,800,800,"C3"]
["S103128","COLLECTEUR ENTREE D'AIR POUR 2 X GSR 330 Condens",null,1409,null,null,"/","/","/",8713809258313,7.9,800,400,520,"C3"]
[51202,"VENTOUSE VERTICALE ALU GALVA Ø200/300 MM",null,1808,null,null,"/","/","/",8713809136246,30,2500,530,530,"C3"]
[51203,"VENTOUSE VERTICALE ALU GALVA Ø250/350 MM",null,2132,null,null,"/","/","/",8713809136253,30,2500,530,530,"C3"]
[46157,"SOLIN POUR TOIT PLAT Ø 300 MM",null,228,null,null,"/","/","/",8713809113988,3,640,640,175,"C3"]
[46158,"SOLIN POUR TOIT PLAT Ø 350 MM",null,238,null,null,"/","/","/",8713809113995,3.25,690,690,175,"C3"]
[54443,"VENTOUSE VERTICALE 2x Ø 350 MM",null,4145,null,null,"/","/","/",8713809154219,59,1200,800,1200,"C3"]
[]
["FAMILLE:","CHAUDIERE  FIOUL AU SOL MODULANTE CONDENSATION"]
[]
[]
[100017739,"OSCR 18","MV12",6201,5,14070,"A","/","/",3661238505827,122,790,675,1335,"C0"]
[100017740,"OSCR 24","MV13",6375,5,14070,"A","/","/",3661238505834,122,790,675,1335,"C0"]
[100017741,"OSCR 30","MV14",6602,5,14070,"A","/","/",3661238505841,131,790,675,1405,"C0"]
[]
[]
[7635811,"OVCR 18/100HL",null,{"$f":"D3058+D3061+D3062","v":7559},null,null,"A","B","XL",3661238636149,null,null,null,null,"C0"]
[7635812,"OVCR 24/100HL",null,{"$f":"D3059+D3061+D3062","v":7733},null,null,"A","B","XL",3661238636156,null,null,null,null,"C0"]
[7635813,"OVCR 30/100HL",null,{"$f":"D3060+D3061+D3062","v":7960},null,null,"A","B","XL",3661238636163,null,null,null,null,"C0"]
[]
["COMPOSANTS "]
[100017739,"OSCR 18","MV12",6201,5,14070,"A","/","/",3661238505827,122,790,675,1335,"C0"]
[100017740,"OSCR 24","MV13",6375,5,14070,"A","/","/",3661238505834,122,790,675,1335,"C0"]
[100017741,"OSCR 30","MV14",6602,5,14070,"A","/","/",3661238505841,131,790,675,1405,"C0"]
[100016430,"BALLON 100HL ","ER225",1062,null,null,"/","/","/",3661238493469,66,780,675,780,"C0"]
[7611211,"KIT DE LIAISON BALLON 100L HL HEE","MV34",296,null,null,"/","/","/",3661238492134,4.2,1185,195,225,"C0"]
[]
[]
[7635814,"OCCR 18/160SL",null,{"$f":"D3070+D3073+D3074","v":7651},null,null,"A","B","XL",3661238636170,null,null,null,null,"C0"]
[7635815,"OCCR 24/160SL",null,{"$f":"D3071+D3073+D3074","v":7825},null,null,"A","B","XL",3661238636187,null,null,null,null,"C0"]
[7635816,"OCCR 30/160SL",null,{"$f":"D3072+D3073+D3074","v":8052},null,null,"A","B","XL",3661238636194,null,null,null,null,"C0"]
[]
["COMPOSANTS "]
[100017739,"OSCR 18","MV12",6201,5,14070,"A","/","/",3661238505827,122,790,675,1335,"C0"]
[100017740,"OSCR 24","MV13",6375,5,14070,"A","/","/",3661238505834,122,790,675,1335,"C0"]
[100017741,"OSCR 30","MV14",6602,5,14070,"A","/","/",3661238505841,131,790,675,1405,"C0"]
[100016428," BALLON 160SL ","ER223",952,null,null,"/","/","/",3661238493445,91,790,675,1070,"C0"]
[7608113,"KIT LIAISON BALLON 160L SL HEE ","MV32",498,null,null,"/","/","/",3661238492141,11.1,875,685,235,"C0"]
[]
[]
[7635817,"OVCR 18/L160SL",null,{"$f":"D3082+D3085+D3086","v":7577},null,null,"A","B","XL",3661238636200,null,null,null,null,"C0"]
[7635818,"OVCR 24/L160SL",null,{"$f":"D3083+D3085+D3086","v":7751},null,null,"A","B","XL",3661238636217,null,null,null,null,"C0"]
[7635819,"OVCR 30/L160SL",null,{"$f":"D3084+D3085+D3086","v":7978},null,null,"A","B","XL",3661238636224,null,null,null,null,"C0"]
[]
["COMPOSANTS "]
[100017739,"OSCR 18","MV12",6201,5,14070,"A","/","/",3661238505827,122,790,675,1335,"C0"]
[100017740,"OSCR 24","MV13",6375,5,14070,"A","/","/",3661238505834,122,790,675,1335,"C0"]
[100017741,"OSCR 30","MV14",6602,5,14070,"A","/","/",3661238505841,131,790,675,1405,"C0"]
[100020079,"BALLON L160SL ","EC600",1080,null,null,"/","/","/",3661238584310,97.5,680,680,1100,"C0"]
[7611211,"KIT DE LIAISON BALLON 100L HL HEE","MV34",296,null,null,"/","/","/",3661238492134,4.2,1185,195,225,"C0"]
[]
[]
[7635820,"OCCR 18/220SHL",null,{"$f":"+D3094+D3097+D3098+D3099","v":9386},null,null,"A","B","XL",3661238636637,null,null,null,null,"C0"]
[7635821,"OCCR 24/220SHL",null,{"$f":"+D3095+D3097+D3098+D3099","v":9560},null,null,"A","B","XL",3661238636644,null,null,null,null,"C0"]
[7635823,"OCCR 30/220SHL",null,{"$f":"D3096+D3097+D3098+D3099","v":9787},null,null,"A","B","XL",3661238636651,null,null,null,null,"C0"]
[]
["COMPOSANTS "]
[100017739,"OSCR 18","MV12",6201,5,14070,"A","/","/",3661238505827,122,790,675,1335,"C0"]
[100017740,"OSCR 24","MV13",6375,5,14070,"A","/","/",3661238505834,122,790,675,1335,"C0"]
[100017741,"OSCR 30","MV14",6602,5,14070,"A","/","/",3661238505841,131,790,675,1405,"C0"]
[100016425,"220SHL","ER220",2439,null,null,"/","/","/",3661238493414,123,780,675,1350,"C0"]
[7611256,"KIT DE LIAISON BALLON 220L SHL HEE","MV35",572,null,null,"/","/","/",3661238505810,11.7,875,675,235,"C0"]
[100016501,"KIT VASE D'EXPANSION  12l/10 bars ","ER229",174,null,null,"/","/","/",3661238505926,5,325,320,215,"C0"]
[]
[]
[7614432,"OSCR 18  HOR",null,{"$f":"D3110+D3114+D3113","v":6352},null,null,"A","/","/",3661238562424,null,null,null,null,"C0"]
[7614433,"OSCR 18  VER",null,{"$f":"D3110+D3115","v":6356},null,null,"A","/","/",3661238562431,null,null,null,null,"C0"]
[7614434,"OSCR 24  HOR",null,{"$f":"D3111+D3113+D3114","v":6526},null,null,"A","/","/",3661238562448,null,null,null,null,"C0"]
[7614435,"OSCR 24  VER",null,{"$f":"D3111+D3115","v":6530},null,null,"A","/","/",3661238562455,null,null,null,null,"C0"]
[7614436,"OSCR 30  HOR",null,{"$f":"D3112+D3113+D3114","v":6753},null,null,"A","/","/",3661238562462,null,null,null,null,"C0"]
[7614437,"OSCR 30  VER",null,{"$f":"D3112+D3115","v":6757},null,null,"A","/","/",3661238562479,null,null,null,null,"C0"]
[]
["COMPOSANTS "]
[100017739,"OSCR 18","MV12",6201,5,14070,"A","/","/",3661238505827,122,790,675,1335,"C0"]
[100017740,"OSCR 24","MV13",6375,5,14070,"A","/","/",3661238505834,122,790,675,1335,"C0"]
[100017741,"OSCR 30","MV14",6602,5,14070,"A","/","/",3661238505841,131,790,675,1405,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,"/","/","/",3661238157972,2.1,1025,170,170,"D6"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
[]
[7635838,"OVCR 18 HOR /100HL",null,{"$f":"D3126+D3129+D3130+D3131+D3132","v":7710},null,null,"A","B","XL",3661238636668,null,null,null,null,"C0"]
[7635839,"OVCR 18  VER /100HL",null,{"$f":"+D3126+D3129+D3130+D3133","v":7714},null,null,"A","B","XL",3661238636675,null,null,null,null,"C0"]
[7635840,"OVCR 24  HOR /100HL",null,{"$f":"D3127+D3129+D3130+D3131+D3132","v":7884},null,null,"A","B","XL",3661238636682,null,null,null,null,"C0"]
[7635841,"OVCR 24  VER /100HL",null,{"$f":"D3127+D3129+D3130+D3133","v":7888},null,null,"A","B","XL",3661238636699,null,null,null,null,"C0"]
[7635842,"OVCR 30  HOR /100HL",null,{"$f":"D3128+D3129+D3130+D3131+D3132","v":8111},null,null,"A","B","XL",3661238636705,null,null,null,null,"C0"]
[7635843,"OVCR 30  VER /100HL",null,{"$f":"D3128+D3129+D3130+D3133","v":8115},null,null,"A","B","XL",3661238636811,null,null,null,null,"C0"]
[]
["COMPOSANTS "]
[100017739,"OSCR 18","MV12",6201,5,14070,"A","/","/",3661238505827,122,790,675,1335,"C0"]
[100017740,"OSCR 24","MV13",6375,5,14070,"A","/","/",3661238505834,122,790,675,1335,"C0"]
[100017741,"OSCR 30","MV14",6602,5,14070,"A","/","/",3661238505841,131,790,675,1405,"C0"]
[100016430,"BALLON 100HL ","ER225",1062,null,null,"/","/","/",3661238493469,66,780,675,780,"C0"]
[7611211,"KIT DE LIAISON BALLON 100L HL HEE","MV34",296,null,null,"/","/","/",3661238492134,4.2,1185,195,225,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,"/","/","/",3661238157972,2.1,1025,170,170,"D6"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
[]
[7635844,"OCCR 18  HOR /160SL",null,{"$f":"D3144+D3147+D3148+D3150+D3149","v":7802},null,null,"A","B","XL",3661238636828,null,null,null,null,"C0"]
[7635845,"OCCR 18  VER /160SL",null,{"$f":"D3144+D3147+D3148+D3151","v":7806},null,null,"A","B","XL",3661238636835,null,null,null,null,"C0"]
[7635846,"OCCR 24  HOR /160SL",null,{"$f":"D3145+D3147+D3148+D3149+D3150","v":7976},null,null,"A","B","XL",3661238636842,null,null,null,null,"C0"]
[7635847,"OCCR 24  VER /160SL",null,{"$f":"D3145+D3147+D3148+D3151","v":7980},null,null,"A","B","XL",3661238636859,null,null,null,null,"C0"]
[7635848,"OCCR 30  HOR /160SL",null,{"$f":"D3146+D3147+D3148+D3149+D3150","v":8203},null,null,"A","B","XL",3661238636866,null,null,null,null,"C0"]
[7635849,"OCCR 30  VER /160SL",null,{"$f":"D3146+D3147+D3148+D3151","v":8207},null,null,"A","B","XL",3661238637276,null,null,null,null,"C0"]
[]
["COMPOSANTS "]
[100017739,"OSCR 18","MV12",6201,5,14070,"A","/","/",3661238505827,122,790,675,1335,"C0"]
[100017740,"OSCR 24","MV13",6375,5,14070,"A","/","/",3661238505834,122,790,675,1335,"C0"]
[100017741,"OSCR 30","MV14",6602,5,14070,"A","/","/",3661238505841,131,790,675,1405,"C0"]
[100016428," BALLON 160SL ","ER223",952,null,null,"/","/","/",3661238493445,91,790,675,1070,"C0"]
[7608113,"KIT LIAISON BALLON 160L SL HEE ","MV32",498,null,null,"/","/","/",3661238492141,11.1,875,685,235,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,"/","/","/",3661238157972,2.1,1025,170,170,"D6"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
[]
[7635824,"OVCR 18 HOR /L160SL",null,{"$f":"D3162+D3165+D3166+D3167+D3168","v":7728},null,null,"A","B","XL",3661238636620,null,null,null,null,"C0"]
[7635825,"OVCR 18  VER /L160SL",null,{"$f":"D3162+D3165+D3166+D3169","v":7732},null,null,"A","B","XL",3661238636880,null,null,null,null,"C0"]
[7635826,"OVCR 24  HOR /L160SL",null,{"$f":"D3163+D3165+D3166+D3167+D3168","v":7902},null,null,"A","B","XL",3661238636897,null,null,null,null,"C0"]
[7635827,"OVCR 24  VER /L160SL",null,{"$f":"D3163+D3165+D3166+D3169","v":7906},null,null,"A","B","XL",3661238636903,null,null,null,null,"C0"]
[7635829,"OVCR 30  HOR /L160SL",null,{"$f":"D3164+D3165+D3166+D3167+D3168","v":8129},null,null,"A","B","XL",3661238636910,null,null,null,null,"C0"]
[7635830,"OVCR 30  VER /L160SL",null,{"$f":"D3164+D3165+D3166+D3169","v":8133},null,null,"A","B","XL",3661238636927,null,null,null,null,"C0"]
[]
["COMPOSANTS "]
[100017739,"OSCR 18","MV12",6201,5,14070,"A","/","/",3661238505827,122,790,675,1335,"C0"]
[100017740,"OSCR 24","MV13",6375,5,14070,"A","/","/",3661238505834,122,790,675,1335,"C0"]
[100017741,"OSCR 30","MV14",6602,5,14070,"A","/","/",3661238505841,131,790,675,1405,"C0"]
[100020079,"BALLON L160SL ","EC600",1080,null,null,"/","/","/",3661238584310,97.5,680,680,1100,"C0"]
[7611211,"KIT DE LIAISON BALLON 100L HL HEE","MV34",296,null,null,"/","/","/",3661238492134,4.2,1185,195,225,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,"/","/","/",3661238157972,2.1,1025,170,170,"D6"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
[]
[7635850,"OCCR 18  HOR /220SHL",null,{"$f":"D3180+D3183+D3184+D3185+D3186+D3187","v":9537},null,null,"A","B","XL",3661238636934,null,null,null,null,"C0"]
[7635852,"OCCR 18  VER /220SHL",null,{"$f":"D3180+D3183+D3184+D3185+D3188","v":9541},null,null,"A","B","XL",3661238636941,null,null,null,null,"C0"]
[7635853,"OCCR 24  HOR /220SHL",null,{"$f":"D3181+D3183+D3184+D3185+D3186+D3187","v":9711},null,null,"A","B","XL",3661238636958,null,null,null,null,"C0"]
[7635855,"OCCR 24  VER /220SHL",null,{"$f":"D3181+D3183+D3184+D3185+D3188","v":9715},null,null,"A","B","XL",3661238636965,null,null,null,null,"C0"]
[7635856,"OCCR 30  HOR /220SHL",null,{"$f":"D3182+D3183+D3184+D3185+D3186+D3187","v":9938},null,null,"A","B","XL",3661238636972,null,null,null,null,"C0"]
[7635858,"OCCR 30  VER /220SHL",null,{"$f":"D3182+D3183+D3184+D3185+D3188","v":9942},null,null,"A","B","XL",3661238636989,null,null,null,null,"C0"]
[]
["COMPOSANTS "]
[100017739,"OSCR 18","MV12",6201,5,14070,"A","/","/",3661238505827,122,790,675,1335,"C0"]
[100017740,"OSCR 24","MV13",6375,5,14070,"A","/","/",3661238505834,122,790,675,1335,"C0"]
[100017741,"OSCR 30","MV14",6602,5,14070,"A","/","/",3661238505841,131,790,675,1405,"C0"]
[100016425,"220SHL","ER220 ",2439,null,null,"/","/","/",3661238493414,123,780,675,1350,"C0"]
[7611256,"KIT DE LIAISON BALLON 220L SHL HEE","MV35",572,null,null,"/","/","/",3661238505810,11.7,875,675,235,"C0"]
[100016501,"KIT VASE D'EXPANSION  12l/10 bars ","ER229",174,null,null,"/","/","/",3661238505926,5,325,320,215,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,"/","/","/",3661238157972,2.1,1025,170,170,"D6"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[]
[]
["OPTIONS CHAUDIERE"]
[100016432,"VASE D'EXPANSION 18 L","MV4",84,null,null,"/","/","/",3661238491915,3.8,300,300,410,"C0"]
[100016489,"KIT VANNE 3 VOIES  ","MV5",403,null,null,"/","/","/",3661238492110,6.5,1185,195,225,"C0"]
[100016490,"KIT CIRCUIT EXTERNE ","MV6",84,null,null,"/","/","/",3661238492127,3.8,615,465,185,"C0"]
[100017720,"KIT SORTIE ARRIERE","MV9 ",111,null,null,"/","/","/",3661238498013,0.3,325,240,50,"C0"]
[100017736,"KIT LIMITEUR DE TEMPERATURE","MV10",179,null,null,"/","/","/",3661238505735,3.5,615,465,185,"C0"]
[100019734,"MANCHETTE DE MESURE 80/125 PPs/Alu ","MV25",70,null,null,"/","/","/",3661238569614,0.45,null,null,null,"C0"]
[7608024,"KIT ADAPTATION CIRCULATEUR EXTERNE","MV30",26,null,null,"/","/","/",3661238587533,0.35,125,100,90,"C0"]
[7608112,"KIT VANNE 3 VOIES HEE ","MV31",518,null,null,"/","/","/",3661238586420,6.5,1185,195,225,"C0"]
[7608114,"KIT LIAISON BALLON EXTERNE HEE","MV33",319,null,null,"/","/","/",3661238586444,4.8600000000000003,615,465,185,"C0"]
[7608113,"KIT LIAISON BALLON 160L SL HEE ","MV32",498,null,null,"/","/","/",3661238586437,11.1,875,685,235,"C0"]
[7611211,"KIT DE LIAISON BALLON 100L HL HEE","MV34",296,null,null,"/","/","/",3661238589414,4.2,1185,195,225,"C0"]
[7611256,"KIT DE LIAISON BALLON 220L SHL HEE","MV35",572,null,null,"/","/","/",3661238589421,11.7,875,685,235,"C0"]
[7602811,"KIT V3V INTERNE - HEE","JA83",625,null,null,"/","/","/",3661238587762,5.5,620,220,220,"C0"]
[100004290,"STATION DE NEUTRALISATION","FM155",259,null,null,"/","/","/",3661238004238,7.75,490,320,185,"C0"]
[100004291,"RECHARGE STATION DE NEUTRALISATION","FM156",130,null,null,"/","/","/",3661238004221,6.14,405,265,165,"C0"]
[100004292,"COLIS SUPPORT STATION DE NEUTRALISATION ","FM157",130,null,null,"/","/","/",3661238004214,2,395,330,120,"C0"]
[100004293,"POMPE DE RELEVAGE DES CONDENSATS","FM158",343,0.83,14050,"/","/","/",3661238004207,1.91,230,115,110,"C0"]
[]
["OPTIONS REGULATION "]
[100013304,"COLIS OPTION V3V OE-TRONIC 4","AD249",158,0.12,95010,"/","/","/",3661238363519,0.42,260,170,130,"C0"]
[100013305,"COLIS SONDE SYSTÈME OE-TRONIC 4","AD250",46,0.02,95020,"/","/","/",3661238363588,0.13400000000000001,150,210,25,"C0"]
[100013306,"SONDE EXTERIEURE RADIO ","AD251",77,0.12,95010,"/","/","/",3661238363595,0.15,150,210,40,"C0"]
[100013307,"MODULE CHAUDIERE RADIO (EMETTEUR)","AD252",123,0.12,95010,"/","/","/",3661238363601,0.32,260,160,130,"C0"]
[100013472,"CDE A DISTANCE RADIO RS 400R     ","AD255",238,0.12,95010,"/","/","/",3661238364233,0.253,175,122,60,"C0"]
[100013477,"CDE A DISTANCE FILAIRE RS 400   ","AD257",177,0.12,95010,"/","/","/",3661238364257,0.253,175,122,60,"C0"]
[88017851,"CABLE DE LIAISON BUS LG 12 M","AD134",110,0.02,95020,"/","/","/",3661238048850,0.37,350,260,30,"C0"]
[88017878,"MODULE DE TELESURVEILLANCE VOCAL TELCOM 2","AD152",704,0.12,95010,"/","/","/",3661238048751,1.05,210,190,105,"C0"]
[88017017,"SONDE DEPART v3v","AD199",80,0.02,95020,"/","/","/",3661238049185,0.21,150,200,40,"C0"]
[100002803,"COMMANDE A DISTANCE SIMPLIFIEE AD208","AD208",104,0.12,95010,"/","/","/",3661238554931,0.2,120,85,40,"C0"]
[]
["OPTIONS ECS"]
[100000492,"KIT ANODE MAGNESIUM","EA103",66,null,null,"/","/","/",3661238011069,0.9,560,90,85,"C0"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.16,200,150,30,"C0"]
[100017933,"KIT DE LIAISON BALLON AUTRE","MV18",225,0.83,14050,"/","/","/",3661238511118,4.9000000000000004,615,465,185,"C0"]
[null,null,null,null,null,null,"/","/","/"]
["MODULES HYDRAULIQUES"]
[100020045,"KIT FILTRE FERNOX TF1",null,258,null,null,"/","/","/",null,null,null,null,null,"C0"]
[100020164,"COLLECTEUR 2/3 CIRCUITS ","EA140",348,null,null,"/","/","/",3661238575011,6.6,660,180,200,"C0"]
[100020165,"CONSOLE MUR COLLECTEUR ","EA141",44,null,null,"/","/","/",3661238575028,1.2,220,125,70,"C0"]
[100020166,"CONSOLE MUR 1 MODULE ","EA142",116,null,null,"/","/","/",3661238575035,1.6,220,125,70,"C0"]
[100020167,"CIRCUIT DIRECT P.ELEC CLASSE A  ","EA143",644,0.83,14050,"/","/","/",3661238575042,5.0999999999999996,460,270,235,"C0"]
[100020169,"MODULE HYDR COMPACT 2 CIRCUITS HEE","EA145",1146,0.83,14050,"/","/","/",3661238575059,9,525,415,210,"C0"]
[]
["OPTIONS DE  MODULES HYDRAULIQUES CIRCUIT V3V"]
[89997044,"KIT DE TRANSFORMATION VANNE MOTORISEE EN VANNE MANUELLE","EA79",44,null,null,"/","/","/",3661238044500,0.22,155,105,100,"C0"]
[]
["FUMISTERIE"]
[null,"PPS Ø 110 mm"]
[84887577,"KIT DE RACCORDEMENT CHEMINEE PPS Ø 110 mm","DY177",258,null,null,"/","/","/",3661238013223,2.68,395,300,510,"C0"]
[84887578,"TUYAU PPS Ø 110 mm LG = 1950 mm (GRIS)","DY178",72,null,null,"/","/","/",3661238013216,2.46,1960,150,150,"C0"]
[84887579,"TUYAU PPS Ø 110 mm LG = 1000 mm (GRIS)","DY179",41,null,null,"/","/","/",3661238013209,1.24,1015,130,140,"C0"]
[84887580,"TUYAU PPS Ø 110 mm LG = 500 mm (GRIS)","DY180",31,null,null,"/","/","/",3661238013193,0.62,515,135,140,"C0"]
[84887581,"COUDE PPS 87° Ø 110 mm (GRIS)","DY181",36,null,null,"/","/","/",3661238013186,0.33,255,190,150,"C0"]
[84887582,"COUDE PPS 45° Ø 110 mm (GRIS)","DY182",48,null,null,"/","/","/",3661238013179,0.52,295,215,165,"C0"]
[84887583,"T DE REVISION Ø 110 mm (GRIS)","DY183",48,null,null,"/","/","/",3661238013162,0.46,300,150,150,"C0"]
[84887587,"ETOILE DE CENTRAGE PPS  Ø 110 mm (2 PIECES)","DY187",15,null,null,"/","/","/",3661238013124,0.1,300,300,30,"C0"]
[84887588,"COUDE DE REVISION PPS 87° Ø 110 mm (GRIS)","DY188",72,null,null,"/","/","/",3661238013117,0.52,315,235,150,"C0"]
[84887772,"PLAQUE DE FINITION","DY772",58,null,null,"/","/","/",3661238011458,0.49,310,230,145,"C0"]
[84887773,"FOURREAU Ø165mm L 500mm","DY773",41,null,null,"/","/","/",3661238011441,1.23,515,165,170,"C3"]
[84887435,"GRILLE D'AERATION EXTERIEURE 250 X 300 mm","DY35",24,null,null,"/","/","/",3661238013889,0.35,300,250,30,"C0"]
[100015325,"KIT N° 1 RACCORDEMENT CHEMINÉE FLEXIBLE PPS Ø 80 mm","DY895",236,null,null,"/","/","/",3661238380110,2.87,395,395,380,"C0"]
[100015327,"TUBE FLEXIBLE LG=12,5M","DY897",354,null,null,"/","/","/",3661238380134,8.6999999999999993,1200,1220,250,"C0"]
[100015326,"TUBE FLEXIBLE LG=50M","DY896",1242,null,null,"/","/","/",3661238380127,35,1600,1660,410,"C0"]
[84887618,"ETOILE DE CENTRAGE POUR FLEXIBLE Ø 80  mm (2 PIÈCES)","DY618",37,null,null,"/","/","/",3661238012912,0.2,300,300,70,"C0"]
[100015328,"PIÈCE DE COUPLAGE FLEXIBLE Ø 80 mm","DY898",71,null,null,"/","/","/",3661238380141,0.25,150,150,150,"C0"]
[100015331,"OUTIL D'AIDE À L'INSERTION Ø 80 mm","DY901",177,null,null,"/","/","/",3661238380172,1.4,300,210,185,"C0"]
[100015330,"PIÈCE D'INSPECTION POUR TUBE FLEXIBLE","DY900",127,null,null,"/","/","/",3661238380165,0.5,295,140,140,"C0"]
[100015329,"TERMINAL AVEC SOLIN FLEX. Ø 80 mm","DY899",177,null,null,"/","/","/",3661238380158,1.74,385,385,250,"C0"]
[null,"PPS Ø 80 mm"]
[84887717,"KIT N° 1 KIT DE RACCORDEMENT CHEMINEE PPS Ø 80 mm","DY717",157,null,null,"/","/","/",3661238011946,2.89,395,405,390,"C0"]
[84887613,"RALLONGE PPS Ø 80 mm   L= 250 mm (2 PCS)","DY613",40,null,null,"/","/","/",3661238012967,0.37,250,170,175,"C0"]
[84887614,"RALLONGE PPS  Ø 80 mm   L=  500 mm (2 PCS)","DY614",38,null,null,"/","/","/",3661238012950,0.68,500,160,150,"C0"]
[84887615,"RALLONGE PPS  Ø 80 mm   L=  1000 mm (2 PCS)","DY615",51,null,null,"/","/","/",3661238012943,1.25,1000,160,145,"C0"]
[84887550,"RALLONGE PPS Ø 80 mm   L=  2000 mm  (2 PIECES)","DY150",77,null,null,"/","/","/",3661238013469,2.4900000000000002,1960,150,150,"C0"]
[84887552,"COUDE PPS à 90°","DY152",16,null,null,"/","/","/",3661238013445,0.2,255,145,150,"C0"]
[84887554,"COUDE PPS a 45°  (2 PCS)","DY154",35,null,null,"/","/","/",3661238013421,0.32,200,200,150,"C0"]
[100008301,"COUDE DE REVISION PPS 87° Ø 80 mm (GRIS)","DY877",41,null,null,"/","/","/",3661238102026,0.24,190,195,145,"C0"]
[84887563,"T PPS AVEC COUVERCLE D'INSPECTION","DY163",58,null,null,"/","/","/",3661238013353,0.39,290,220,170,"C0"]
[84887551,"COLLIER DE CENTRAGE Ø 80mm (2 PIECES)","DY151",14,null,null,"/","/","/",3661238013452,0.1,300,300,40,"C0"]
[84887546,"PIÈCE DE VISITE Ø 80 mm droite","DY146",58,null,null,"/","/","/",3661238013506,0.28999999999999998,300,145,150,"C0"]
[84887757,"PLAQUE DE FINITION Ø80mm","DY757",41,null,null,"/","/","/",3661238011595,0.46,310,230,150,"C0"]
[84887753,"TUYAU DE PROTECTION L500mm Ø124mm","DY753",25,null,null,"/","/","/",3661238011632,0.8,505,155,150,"C0"]
[null,"PPS Ø 80/125 mm"]
[100002733,"TERMINAL VERTICAL PPS Ø 80/125 mm ROUGE","DY844",154,null,null,"/","/","/",3661238006614,4.2,1210,265,240,"C0"]
[84887758,"PLAQUE DE FINITION Ø125mm","DY758",64,null,null,"/","/","/",3661238011588,0.52,310,235,145,"C0"]
[84887763,"TUYAU DE PROTECTION L500mm Ø141mm","DY763",30,null,null,"/","/","/",3661238011533,0.98,500,155,150,"C0"]
[84887524,"PIECE D'INSPECTION DROITE ALU/PPS Ø 80/125 mm","DY124",110,null,null,"/","/","/",3661238013704,0.55000000000000004,300,145,150,"C0"]
[84887525,"T D'INSPECTION ALU/PPS Ø 80/125 mm","DY125",126,null,null,"/","/","/",3661238013698,0.82,315,235,150,"C0"]
[84887526,"RALLONGE CONCENTRIQUE ALU/PPS  80/125 L= 250 mm","DY126",41,null,null,"/","/","/",3661238013681,0.47,255,145,150,"C0"]
[84887527,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 L= 500mm","DY127",47,null,null,"/","/","/",3661238013674,0.9,520,140,140,"C0"]
[84887528,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 L=1000 mm","DY128",69,null,null,"/","/","/",3661238013667,1.7,1010,135,140,"C0"]
[84887529,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 L=1950 mm","DY129",120,null,null,"/","/","/",3661238013650,3.5,1960,150,150,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 mm","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[84887532,"COUDE CONCENTRIQUE 45° ALU/PPS Ø 80/125 mm (2 PCES)","DY132",77,null,null,"/","/","/",3661238013629,1,315,235,150,"C0"]
[100008311,"COUDE DE REVISION ALU/PPS Ø 80/125 mm","DY875",115,null,null,"/","/","/",3661238101920,0.68,195,195,145,"C0"]
[null,"FLEXIBLE PPS Ø 80 mm"]
[100015325,"KIT N° 1 RACCORDEMENT CHEMINÉE FLEXIBLE PPS Ø 80 mm","DY895",236,null,null,"/","/","/",3661238380110,2.87,395,395,380,"C0"]
[100015327,"TUBE FLEXIBLE LG=12,5M","DY897",354,null,null,"/","/","/",3661238380134,8.6999999999999993,1200,1220,250,"C0"]
[100015326,"TUBE FLEXIBLE LG=50M","DY896",1242,null,null,"/","/","/",3661238380127,35,1600,1660,410,"C0"]
[84887618,"ETOILE DE CENTRAGE POUR FLEXIBLE Ø 80  mm (2 PIÈCES)","DY618",37,null,null,"/","/","/",3661238012912,0.2,300,300,70,"C0"]
[100015328,"PIÈCE DE COUPLAGE FLEXIBLE Ø 80 mm","DY898",71,null,null,"/","/","/",3661238380141,0.25,150,150,150,"C0"]
[100015331,"OUTIL D'AIDE À L'INSERTION Ø 80 mm","DY901",177,null,null,"/","/","/",3661238380172,1.4,300,210,185,"C0"]
[100015330,"PIÈCE D'INSPECTION POUR TUBE FLEXIBLE","DY900",127,null,null,"/","/","/",3661238380165,0.5,295,140,140,"C0"]
[100015329,"TERMINAL AVEC SOLIN FLEX. Ø 80 mm","DY899",177,null,null,"/","/","/",3661238380158,1.74,385,385,250,"C0"]
[]
[null,"ACCESSOIRES"]
[100005002,"PANIER DE PROTECTION INOX  Ø 80/125","DY865",176,null,null,"/","/","/",3661238001886,2.59,275,270,270,"C0"]
[84887411,"SORTIE HORIZONTALE TOIT PENTE DE 30° A 45° ( uniquement pour tuiles mécaniques)","DY11",179,null,null,"/","/","/",3661238013940,3.57,1020,700,370,"C0"]
[84837729,"SORTIE DE TOIT EN PENTE DE 40° A 60° ( uniquement pour tuiles mécaniques)","CX49",178,null,null,"/","/","/",3661238014367,3.5,920,700,320,"C0"]
[84837731,"EMBASE D'ETANCHE TOIT PLAT","CX51",43,null,null,"/","/","/",3661238014343,0.5,400,400,155,"C0"]
[84837121,"TUILE A DOUILLE 5 A 25 NOIRE","CX121",112,null,null,"/","/","/",3661238014428,2.96,510,250,145,"C0"]
[84837732,"TUILE A DOUILLE 25 A 35' NOIRE","CX52",77,null,null,"/","/","/",3661238014336,3,520,250,145,"C0"]
[84837734,"TUILE A DOUILLE 35 A 55° NOIRE ","CX63",97,null,null,"/","/","/",3661238014312,3.17,510,265,180,"C0"]
[84837120,"TUILE A DOUILLE 5 A 25° ROUGE","CX120",112,null,null,"/","/","/",3661238014435,3.02,515,245,145,"C0"]
[84837783,"TUILE A DOUILLE 25 A 35 ROUGE","CX83",77,null,null,"/","/","/",3661238014213,3,515,250,150,"C0"]
[84837784,"TUILE A DOUILLE 35 A 55 ROUGE","CX84",97,null,null,"/","/","/",3661238014206,2.95,520,265,180,"C0"]
[84837741,"PLATINE DE FINITION INTER","CX72",17,null,null,"/","/","/",3661238014251,0.54,245,210,3,"C0"]
[84837779,"COLLIER DE FIXATION D.125 mm PATTE LONGUE","CX79",15,null,null,"/","/","/",3661238014237,0.24,230,160,200,"C0"]
[84837118,"COLLIER DE FIXATION D.125 mm PATTE COURTE","CX118",12,null,null,"/","/","/",3661238014459,0.19,225,185,20,"C0"]
[84887551,"COLLIER DE CENTRAGE Ø 80 mm (2 PIECES)","DY151",14,null,null,"/","/","/",3661238013452,0.1,300,300,40,"C0"]
[84887566,"PANIER DE PROTECTION INOX","DY166",80,null,null,"/","/","/",3661238013339,1.38,220,210,200,"C0"]
[84837118,"COLLIER DE FIXATION Ø 125 MM PATTE COURTE","CX118",12,null,null,"/","/","/",3661238014459,0.19,225,185,20,"C0"]
[84887451,"COLLIER D'ETANCHEITE POUR MONTAGE EXTERIEUR","DY51",27,null,null,"/","/","/",3661238013841,0.15,150,130,60,"C0"]
[]
["FAMILLE:","CHAUDIERE AU  SOL  FIOUL CONDENSATION "]
[]
[]
[7660556,"FSCX-2 24",null,{"$f":"D3325+D3327","v":4386},null,null,"A système\n avec sonde extérieure","/","/",3661238668416,null,null,null,null,"D6"]
[7660566,"FSCX-2 32",null,{"$f":"D3326+D3327","v":4925},null,null,"A système\n avec sonde extérieure","/","/",3661238668423,null,null,null,null,"D6"]
[7660576,"FSCR-2 24",null,{"$f":"D3325+D3328","v":4688},null,null,"A système\n avec sonde extérieure","/","/",3661238668430,null,null,null,null,"D6"]
[7660577,"FSCR-2 32",null,{"$f":"D3326+D3328","v":5227},null,null,"A système\n avec sonde extérieure","/","/",3661238668447,null,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7657859,"FSC.-2 24","MY195",4234,5,14070,"/","/","/",3661238666436,203,1220,750,750,"D6"]
[7658099,"FSC.-2 32","MY197",4773,5,14070,"/","/","/",3661238666443,205,1220,750,1060,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[]
[]
[7660579,"FVCX-2 24/EL110SL",null,{"$f":"D3335+D3336+D3337+D3338","v":5447},null,null,"A système\n avec sonde extérieure","B","XL",3661238668454,null,null,null,null,"D6"]
[7660580,"FVCR-2 24/EL110SL",null,{"$f":"D3335+D3336+D3337+D3339","v":5749},null,null,"A système\n avec sonde extérieure","B","XL",3661238668461,null,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7657859,"FSC.-2 24","MY195",4234,5,14070,"/","/","/",3661238666436,203,1220,750,750,"D6"]
[7609915,"BALLON EL110SL","ER590",758,null,null,"/","/","/",3661238608726,83,700,680,940,"D6"]
[7613103,"KIT DE LIAISON BALLON EL110SL","ER595",303,null,null,"/","/","/",3661238608115,5,860,250,135,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[null,null,null,null,null,null,null,null,null,""]
[]
[7660581,"FVCX-2 24/EL160SL",null,{"$f":"D3348+D3350+D3351+D3352","v":5778},null,null,"A système\n avec sonde extérieure","B","XL",3661238668478,null,null,null,null,"D6"]
[7660582,"FVCX-2 32/EL160SL",null,{"$f":"D3349+D3350+D3351+D3352","v":6317},null,null,"A système\n avec sonde extérieure","B","XL",3661238668485,null,null,null,null,"D6"]
[7660583,"FVCR-2 24/EL160SL",null,{"$f":"D3348+D3350+D3351+D3353","v":6080},null,null,"A système\n avec sonde extérieure","B","XL",3661238668492,null,null,null,null,"D6"]
[7660584,"FVCR-2 32/EL160SL",null,{"$f":"D3349+D3350+D3351+D3353","v":6619},null,null,"A système\n avec sonde extérieure","B","XL",3661238668508,null,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7657859,"FSC.-2 24","MY195",4234,5,14070,"/","/","/",3661238666436,203,1220,750,750,"D6"]
[7658099,"FSC.-2 32","MY197",4773,5,14070,"/","/","/",3661238666443,205,1220,750,1060,"D6"]
[7616405,"BALLON EL160SL","ER592",989,null,null,"/","/","/",3661238608696,98,700,680,1200,"D6"]
[7613082,"KIT DE LIAISON BALLON EL160SL","ER597",403,null,null,"/","/","/",3661238608139,5,860,250,135,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[]
[]
[7660585,"FSCX-2 24 P",null,{"$f":"D3362+D3364+D3365","v":4866},null,null,"A système\n avec sonde extérieure","/","/",3661238668515,null,null,null,null,"D6"]
[7660586,"FSCX-2 32 P",null,{"$f":"D3363+D3364+D3365","v":5405},null,null,"A système\n avec sonde extérieure","/","/",3661238668522,null,null,null,null,"D6"]
[7660587,"FSCR-2 24 P",null,{"$f":"D3362+D3364+D3366","v":5168},null,null,"A système\n avec sonde extérieure","/","/",3661238668539,null,null,null,null,"D6"]
[7660588,"FSCR-2 32 P",null,{"$f":"D3363+D3364+D3366","v":5707},null,null,"A système\n avec sonde extérieure","/","/",3661238668546,null,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7657859,"FSC.-2 24","MY195",4234,5,14070,"/","/","/",3661238666436,203,1220,750,750,"D6"]
[7658099,"FSC.-2 32","MY197",4773,5,14070,"/","/","/",3661238666443,205,1220,750,1060,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,15,675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[]
[]
[7660589,"FVCX-2 24 P/EL110SL",null,{"$f":"D3373+D3374+D3375+D3376+D3377","v":5846},null,null,"A système\n avec sonde extérieure","B","XL",3661238668560,null,null,null,null,"D6"]
[7660590,"FVCR-2 24 P/EL110SL",null,{"$f":"D3373+D3374+D3375+D3376+D3378","v":6148},null,null,"A système\n avec sonde extérieure","B","XL",3661238668577,null,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7657859,"FSC.-2 24","MY195",4234,5,14070,"/","/","/",3661238666436,203,1220,750,750,"D6"]
[7609915,"BALLON EL110SL","ER590",758,null,null,"/","/","/",3661238608726,83,700,680,940,"D6"]
[7614745,"KIT DE LIAISON BALLON EL110SL EQUIPEE","ER594",222,null,null,"/","/","/",3661238608122,3.9,870,260,160,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,15,675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[null,null,null,null,null,null,null,null,null,""]
[]
[7660591,"FVCX-2 24 P/EL160SL",null,{"$f":"D3387+D3389+D3390+D3391+D3392","v":6118},null,null,"A","B","XL",3661238668584,null,null,null,null,"D6"]
[7660592,"FVCX-2 32 P/EL160SL",null,{"$f":"D3388+D3389+D3390+D3391+D3392","v":6657},null,null,"A","B","XL",3661238668591,null,null,null,null,"D6"]
[7660593,"FVCR-2 24 P/EL160SL",null,{"$f":"D3387+D3389+D3390+D3391+D3393","v":6420},null,null,"A","B","XL",3661238668607,null,null,null,null,"D6"]
[7660594,"FVCR-2 32 P/EL160SL",null,{"$f":"D3388+D3389+D3390+D3391+D3393","v":6959},null,null,"A","B","XL",3661238668614,null,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7657859,"FSC.-2 24","MY195",4234,5,14070,"/","/","/",3661238666436,203,1220,750,750,"D6"]
[7658099,"FSC.-2 32","MY197",4773,5,14070,"/","/","/",3661238666443,205,1220,750,1060,"D6"]
[7616405,"BALLON EL160SL","ER592",989,null,null,"/","/","/",3661238608696,98,700,680,1200,"D6"]
[7614827,"KIT DE LIAISON BALLON EL160SL EQUIPEE","ER596",263,null,null,"/","/","/",3661238608146,5,860,250,135,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,15,675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[]
[]
[7660595,"FSCX-2 24 F HOR",null,{"$f":"D3406+D3408+D3410+D3411","v":4587},null,null,"A système\n avec sonde extérieure","/","/",3661238668621,null,null,null,null,"D6"]
[7660596,"FSCX-2 24 F VER",null,{"$f":"D3406+D3408+D3410+D3412+D3413","v":4693},null,null,"A système\n avec sonde extérieure","/","/",3661238668638,null,null,null,null,"D6"]
[7660605,"FSCX-2 32 F HOR",null,{"$f":"D3407+D3408+D3410+D3411","v":5126},null,null,"A système\n avec sonde extérieure","/","/",3661238668645,null,null,null,null,"D6"]
[7660606,"FSCX-2 32 F VER",null,{"$f":"D3407+D3408+D3410+D3412+D3413","v":5232},null,null,"A système\n avec sonde extérieure","/","/",3661238668652,null,null,null,null,"D6"]
[7660608,"FSCR-2 24 F HOR",null,{"$f":"D3406+D3409+D3410+D3411","v":4889},null,null,"A système\n avec sonde extérieure","/","/",3661238668669,null,null,null,null,"D6"]
[7660609,"FSCR-2 24 F VER",null,{"$f":"D3406+D3409+D3410+D3412+D3413","v":4995},null,null,"A système\n avec sonde extérieure","/","/",3661238668676,null,null,null,null,"D6"]
[7660610,"FSCR-2 32 F HOR",null,{"$f":"D3407+D3409+D3410+D3411","v":5428},null,null,"A système\n avec sonde extérieure","/","/",3661238668683,null,null,null,null,"D6"]
[7660611,"FSCR-2 32 F VER",null,{"$f":"D3407+D3409+D3410+D3412+D3413","v":5534},null,null,"A système\n avec sonde extérieure","/","/",3661238668690,null,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7657859,"FSC.-2 24","MY195",4234,5,14070,"/","/","/",3661238666436,203,1220,750,750,"D6"]
[7658099,"FSC.-2 32","MY197",4773,5,14070,"/","/","/",3661238666443,205,1220,750,1060,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[7605520,"KIT FLUX FORCE FSC.","MY405",101,null,null,"/","/","/",3661238604179,1.9,510,460,175,"D6"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,"/","/","/",3661238157972,2.1,1025,170,170,"D6"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[]
[]
[7660612,"FVCX-2 24 F HOR/EL110SL",null,{"$f":"D3422+D3423+D3424+D3425+D3427+D3428","v":5648},null,null,"A système\n avec sonde extérieure","B","XL",3661238668706,null,null,null,null,"D6"]
[7660613,"FVCX-2 24 F VER/EL110SL",null,{"$f":"D3422+D3423+D3424+D3425+D3427+D3429+D3430","v":5754},null,null,"A système\n avec sonde extérieure","B","XL",3661238668713,null,null,null,null,"D6"]
[7660614,"FVCR-2 24 F HOR/EL110SL",null,{"$f":"D3422+D3423+D3424+D3426+D3427+D3428","v":5950},null,null,"A système\n avec sonde extérieure","B","XL",3661238668720,null,null,null,null,"D6"]
[7660615,"FVCR-2 24 F VER/EL110SL",null,{"$f":"D3422+D3423+D3424+D3426+D3427+D3429+D3430","v":6056},null,null,"A système\n avec sonde extérieure","B","XL",3661238668737,null,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7657859,"FSC.-2 24","MY195",4234,5,14070,"/","/","/",3661238666436,203,1220,750,750,"D6"]
[7609915,"BALLON EL110SL","ER590",758,null,null,"/","/","/",3661238608726,83,700,680,940,"D6"]
[7613103,"KIT DE LIAISON BALLON EL110SL","ER595",303,null,null,"/","/","/",3661238608115,5,860,250,135,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[7605520,"KIT FLUX FORCE FSC.","MY405",101,null,null,"/","/","/",3661238604179,1.9,510,460,175,"D6"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,"/","/","/",3661238157972,2.1,1025,170,170,"D6"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[null,null,null,null,null,null,null,null,null,""]
[]
[7660616,"FVCX-2 24 F HOR/EL160SL",null,{"$f":"D3443+D3445+D3446+D3447+D3449+D3450","v":5979},null,null,"A système\n avec sonde extérieure","B","XL",3661238668744,null,null,null,null,"D6"]
[7660618,"FVCX-2 24 F VER/EL160SL",null,{"$f":"D3443+D3445+D3446+D3447+D3449+D3451+D3452","v":6085},null,null,"A système\n avec sonde extérieure","B","XL",3661238668782,null,null,null,null,"D6"]
[7660619,"FVCX-2 32 F HOR/EL160SL",null,{"$f":"D3444+D3445+D3446+D3447+D3449+D3450","v":6518},null,null,"A système\n avec sonde extérieure","B","XL",3661238668812,null,null,null,null,"D6"]
[7660620,"FVCX-2 32 F VER/EL160SL",null,{"$f":"D3444+D3445+D3446+D3447+D3449+D3451+D3452","v":6624},null,null,"A système\n avec sonde extérieure","B","XL",3661238668799,null,null,null,null,"D6"]
[7660621,"FVCR-2 24 F HOR/EL160SL",null,{"$f":"D3443+D3445+D3446+D3448+D3449+D3450","v":6281},null,null,"A système\n avec sonde extérieure","B","XL",3661238668805,null,null,null,null,"D6"]
[7660622,"FVCR-2 24 F VER/EL160SL",null,{"$f":"D3443+D3445+D3446+D3448+D3449+D3451+D3452","v":6387},null,null,"A système\n avec sonde extérieure","B","XL",3661238668829,null,null,null,null,"D6"]
[7660623,"FVCR-2 32 F HOR/EL160SL",null,{"$f":"D3444+D3445+D3446+D3448+D3449+D3450","v":6820},null,null,"A système\n avec sonde extérieure","B","XL",3661238668836,null,null,null,null,"D6"]
[7660624,"FVCR-2 32 F VER/EL160SL",null,{"$f":"D3444+D3445+D3446+D3448+D3449+D3451+D3452","v":6926},null,null,"A système\n avec sonde extérieure","B","XL",3661238668843,null,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7657859,"FSC.-2 24","MY195",4234,5,14070,"/","/","/",3661238666436,203,1220,750,750,"D6"]
[7658099,"FSC.-2 32","MY197",4773,5,14070,"/","/","/",3661238666443,205,1220,750,1060,"D6"]
[7616405,"BALLON EL160SL","ER592",989,null,null,"/","/","/",3661238608696,98,700,680,1200,"D6"]
[7613082,"KIT DE LIAISON BALLON EL160SL","ER597",403,null,null,"/","/","/",3661238608139,5,860,250,135,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[7605520,"KIT FLUX FORCE FSC.","MY405",101,null,null,"/","/","/",3661238604179,1.9,510,460,175,"D6"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,"/","/","/",3661238157972,2.1,1025,170,170,"D6"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[]
[]
[7660625,"FSCX-2 24 PF HOR",null,{"$f":"D3465+D3467+D3468+D3470+D3471","v":5067},null,null,"A système\n avec sonde extérieure","/","/",3661238668850,null,null,null,null,"D6"]
[7660627,"FSCX-2 24 PF VER",null,{"$f":"D3465+D3467+D3468+D3470+D3472+D3473","v":5173},null,null,"A système\n avec sonde extérieure","/","/",3661238668867,null,null,null,null,"D6"]
[7660628,"FSCX-2 32 PF HOR",null,{"$f":"D3466+D3467+D3468+D3470+D3471","v":5606},null,null,"A système\n avec sonde extérieure","/","/",3661238668881,null,null,null,null,"D6"]
[7660629,"FSCX-2 32 PF VER",null,{"$f":"D3466+D3467+D3468+D3470+D3472+D3473","v":5712},null,null,"A système\n avec sonde extérieure","/","/",3661238668898,null,null,null,null,"D6"]
[7660630,"FSCR-2 24 PF HOR",null,{"$f":"D3465+D3467+D3469+D3470+D3471","v":5369},null,null,"A système\n avec sonde extérieure","/","/",3661238668904,null,null,null,null,"D6"]
[7660631,"FSCR-2 24 PF VER",null,{"$f":"D3465+D3467+D3469+D3470+D3472+D3473","v":5475},null,null,"A système\n avec sonde extérieure","/","/",3661238669017,null,null,null,null,"D6"]
[7660632,"FSCR-2 32 PF HOR",null,{"$f":"D3466+D3467+D3469+D3470+D3471","v":5908},null,null,"A système\n avec sonde extérieure","/","/",3661238669024,null,null,null,null,"D6"]
[7660633,"FSCR-2 32 PF VER",null,{"$f":"D3466+D3467+D3469+D3470+D3472+D3473","v":6014},null,null,"A système\n avec sonde extérieure","/","/",3661238669031,null,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7657859,"FSC.-2 24","MY195",4234,5,14070,"/","/","/",3661238666436,203,1220,750,750,"D6"]
[7658099,"FSC.-2 32","MY197",4773,5,14070,"/","/","/",3661238666443,205,1220,750,1060,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,15,675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[7605520,"KIT FLUX FORCE FSC.","MY405",101,null,null,"/","/","/",3661238604179,1.9,510,460,175,"D6"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,"/","/","/",3661238157972,2.1,1025,170,170,"D6"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[]
[]
[7660635,"FVCX-2 24 PF HOR/EL110SL",null,{"$f":"D3482+D3483+D3484+D3485+D3486+D3488+D3489","v":6047},null,null,"A système\n avec sonde extérieure","B","XL",3661238669048,null,null,null,null,"D6"]
[7660636,"FVCX-2 24 PF VER/EL110SL",null,{"$f":"D3482+D3483+D3484+D3485+D3486+D3488+D3490+D3491","v":6153},null,null,"A système\n avec sonde extérieure","B","XL",3661238669055,null,null,null,null,"D6"]
[7660637,"FVCR-2 24 PF HOR/EL110SL",null,{"$f":"D3482+D3483+D3484+D3485+D3487+D3488+D3489","v":6349},null,null,"A système\n avec sonde extérieure","B","XL",3661238669062,null,null,null,null,"D6"]
[7660638,"FVCR-2 24 PF VER/EL110SL",null,{"$f":"D3482+D3483+D3484+D3485+D3487+D3488+D3490+D3491","v":6455},null,null,"A système\n avec sonde extérieure","B","XL",3661238669086,null,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7657859,"FSC.-2 24","MY195",4234,5,14070,"/","/","/",3661238666436,203,1220,750,750,"D6"]
[7609915,"BALLON EL110SL","ER590",758,null,null,"/","/","/",3661238608726,83,700,680,940,"D6"]
[7614745,"KIT DE LIAISON BALLON EL110SL EQUIPEE","ER594",222,null,null,"/","/","/",3661238608122,3.9,870,260,160,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,15,675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[7605520,"KIT FLUX FORCE FSC.","MY405",101,null,null,"/","/","/",3661238604179,1.9,510,460,175,"D6"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,"/","/","/",3661238157972,2.1,1025,170,170,"D6"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[null,null,null,null,null,null,null,null,null,""]
[]
[7660639,"FVCX-2 24 PF HOR/EL160SL",null,{"$f":"D3504+D3506+D3507+D3508+D3509+D3511+D3512","v":6319},null,null,"A système\n avec sonde extérieure","B","XL",3661238669093,null,null,null,null,"D6"]
[7660640,"FVCX-2 24 PF VER/EL160SL",null,{"$f":"D3504+D3506+D3507+D3508+D3509+D3511+D3513+D3514","v":6425},null,null,"A système\n avec sonde extérieure","B","XL",3661238669109,null,null,null,null,"D6"]
[7660641,"FVCX-2 32 PF HOR/EL160SL",null,{"$f":"D3505+D3506+D3507+D3508+D3509+D3511+D3512","v":6858},null,null,"A système\n avec sonde extérieure","B","XL",3661238669116,null,null,null,null,"D6"]
[7660642,"FVCX-2 32 PF VER/EL160SL",null,{"$f":"D3505+D3506+D3507+D3508+D3509+D3511+D3513+D3514","v":6964},null,null,"A système\n avec sonde extérieure","B","XL",3661238669123,null,null,null,null,"D6"]
[7660643,"FVCR-2 24 PF HOR/EL160SL",null,{"$f":"D3504+D3506+D3507+D3508+D3510+D3511+D3512","v":6621},null,null,"A système\n avec sonde extérieure","B","XL",3661238669130,null,null,null,null,"D6"]
[7660644,"FVCR-2 24 PF VER/EL160SL",null,{"$f":"D3504+D3506+D3507+D3508+D3510+D3511+D3513+D3514","v":6727},null,null,"A système\n avec sonde extérieure","B","XL",3661238669147,null,null,null,null,"D6"]
[7660645,"FVCR-2 32 PF HOR/EL160SL",null,{"$f":"D3505+D3506+D3507+D3508+D3510+D3511+D3512","v":7160},null,null,"A système\n avec sonde extérieure","B","XL",3661238669154,null,null,null,null,"D6"]
[7660646,"FVCR-2 32 PF VER/EL160SL",null,{"$f":"D3505+D3506+D3507+D3508+D3510+D3511+D3513+D3514","v":7266},null,null,"A système\n avec sonde extérieure","B","XL",3661238669161,null,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7657859,"FSC.-2 24","MY195",4234,5,14070,"/","/","/",3661238666436,203,1220,750,750,"D6"]
[7658099,"FSC.-2 32","MY197",4773,5,14070,"/","/","/",3661238666443,205,1220,750,1060,"D6"]
[7616405,"BALLON EL160SL","ER592",989,null,null,"/","/","/",3661238608696,98,700,680,1200,"D6"]
[7614827,"KIT DE LIAISON BALLON EL160SL EQUIPEE","ER596",263,null,null,"/","/","/",3661238608146,5,860,250,135,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,15,675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[7605520,"KIT FLUX FORCE FSC.","MY405",101,null,null,"/","/","/",3661238604179,1.9,510,460,175,"D6"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,"/","/","/",3661238157972,2.1,1025,170,170,"D6"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[]
[]
[7633655,"FSCX 19",null,{"$f":"D3526+D3529","v":4038},null,null,"A système\n avec sonde extérieure","/","/",3661238637016,209.9,null,null,null,"D6"]
[7633656,"FSCX 24",null,{"$f":"D3527+D3529","v":4240},null,null,"A système\n avec sonde extérieure","/","/",3661238637023,237.9,null,null,null,"D6"]
[7633657,"FSCX 32",null,{"$f":"D3528+D3529","v":4592},null,null,"A système\n avec sonde extérieure","/","/",3661238637030,265.89999999999998,null,null,null,"D6"]
[]
[7633660,"FSCR 19",null,{"$f":"D3526+D3530","v":4340},null,null,"A système\n avec sonde extérieure","/","/",3661238637047,209.9,null,null,null,"D6"]
[7633661,"FSCR 24",null,{"$f":"D3527+D3530","v":4542},null,null,"A système\n avec sonde extérieure","/","/",3661238637054,237.9,null,null,null,"D6"]
[7633662,"FSCR 32",null,{"$f":"D3528+D3530","v":4894},null,null,"A système\n avec sonde extérieure","/","/",3661238637061,265.89999999999998,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7624096,"FSC. 19","MY103",3886,5,14070,"/","/","/",3661238617315,209,1220,750,1050,"D6"]
[7624118,"FSC. 24","MY108",4088,5,14070,"/","/","/",3661238617322,237,1220,750,1050,"D6"]
[7624125,"FSC. 32","MY113",4440,5,14070,"/","/","/",3661238617339,265,1220,750,1050,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[]
[]
[7633665,"FVCX 19/EL110SL",null,{"$f":"D3539+D3541+D3542+D3543","v":5099},null,null,"A système\n avec sonde extérieure","B","XL",3661238637078,297.89999999999998,null,null,null,"D6"]
[7633666,"FVCX 24/EL110SL",null,{"$f":"D3540+D3541+D3542+D3543","v":5301},null,null,"A système\n avec sonde extérieure","B","XL",3661238637085,325.89999999999998,null,null,null,"D6"]
[7633667,"FVCR 19/EL110SL",null,{"$f":"D3539+D3541+D3542+D3544","v":5401},null,null,"A système\n avec sonde extérieure","B","XL",3661238637092,297.89999999999998,null,null,null,"D6"]
[7633668,"FVCR 24/EL110SL",null,{"$f":"D3540+D3541+D3542+D3544","v":5603},null,null,"A système\n avec sonde extérieure","B","XL",3661238637108,325.89999999999998,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7624096,"FSC. 19","MY103",3886,5,14070,"/","/","/",3661238617315,209,1220,750,1050,"D6"]
[7624118,"FSC. 24","MY108",4088,5,14070,"/","/","/",3661238617322,237,1220,750,1050,"D6"]
[7609915,"BALLON EL110SL","ER590",758,null,null,"/","/","/",3661238608726,83,700,680,940,"D6"]
[7613103,"KIT DE LIAISON BALLON EL110SL","ER595",303,null,null,"/","/","/",3661238608115,5,860,250,135,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[null,null,null,null,null,null,null,null,null,""]
[]
[7633669,"FVCX 19/EL160SL",null,{"$f":"D3555+D3558+D3559+D3560","v":5430},null,null,"A système\n avec sonde extérieure","B","XL",3661238637115,312.89999999999998,null,null,null,"D6"]
[7633670,"FVCX 24/EL160SL",null,{"$f":"D3556+D3558+D3559+D3560","v":5632},null,null,"A système\n avec sonde extérieure","B","XL",3661238637122,340.9,null,null,null,"D6"]
[7633671,"FVCX 32/EL160SL",null,{"$f":"D3557+D3558+D3559+D3560","v":5984},null,null,"A système\n avec sonde extérieure","B","XL",3661238637139,368.9,null,null,null,"D6"]
[7633672,"FVCR 19/EL160SL",null,{"$f":"D3555+D3558+D3559+D3561","v":5732},null,null,"A système\n avec sonde extérieure","B","XL",3661238637146,312.89999999999998,null,null,null,"D6"]
[7633673,"FVCR 24/EL160SL",null,{"$f":"D3556+D3558+D3559+D3561","v":5934},null,null,"A système\n avec sonde extérieure","B","XL",3661238637153,340.9,null,null,null,"D6"]
[7633674,"FVCR 32/EL160SL",null,{"$f":"D3557+D3558+D3559+D3561","v":6286},null,null,"A système\n avec sonde extérieure","B","XL",3661238637160,368.9,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7624096,"FSC. 19","MY103",3886,5,14070,"/","/","/",3661238617315,209,1220,750,1050,"D6"]
[7624118,"FSC. 24","MY108",4088,5,14070,"/","/","/",3661238617322,237,1220,750,1050,"D6"]
[7624125,"FSC. 32","MY113",4440,5,14070,"/","/","/",3661238617339,265,1220,750,1050,"D6"]
[7616405,"BALLON EL160SL","ER592",989,null,null,"/","/","/",3661238608696,98,700,680,1200,"D6"]
[7613082,"KIT DE LIAISON BALLON EL160SL","ER597",403,null,null,"/","/","/",3661238608139,5,860,250,135,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[]
[]
[7633675,"FSCX 19 P",null,{"$f":"D3572+D3575+D3576","v":4518},null,null,"A système\n avec sonde extérieure","/","/",3661238637177,224.9,null,null,null,"D6"]
[7633676,"FSCX 24 P",null,{"$f":"D3573+D3575+D3576","v":4720},null,null,"A système\n avec sonde extérieure","/","/",3661238637177,252.9,null,null,null,"D6"]
[7633677,"FSCX 32 P",null,{"$f":"D3574+D3575+D3576","v":5072},null,null,"A système\n avec sonde extérieure","/","/",3661238637191,280.89999999999998,null,null,null,"D6"]
[7633678,"FSCR 19 P",null,{"$f":"D3572+D3575+D3577","v":4820},null,null,"A système\n avec sonde extérieure","/","/",3661238637207,224.9,null,null,null,"D6"]
[7633679,"FSCR 24 P",null,{"$f":"D3573+D3575+D3577","v":5022},null,null,"A système\n avec sonde extérieure","/","/",3661238637214,252.9,null,null,null,"D6"]
[7633680,"FSCR 32 P",null,{"$f":"D3574+D3575+D3577","v":5374},null,null,"A système\n avec sonde extérieure","/","/",3661238637221,280.89999999999998,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7624096,"FSC. 19","MY103",3886,5,14070,"/","/","/",3661238617315,209,1220,750,1050,"D6"]
[7624118,"FSC. 24","MY108",4088,5,14070,"/","/","/",3661238617322,237,1220,750,1050,"D6"]
[7624125,"FSC. 32","MY113",4440,5,14070,"/","/","/",3661238617339,265,1220,750,1050,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,15,675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[]
[]
[7633681,"FVCX 19 P/EL110SL",null,{"$f":"D3586+D3588+D3589+D3590+D3591","v":5498},null,null,"A système\n avec sonde extérieure","B","XL",3661238637238,312.89999999999998,null,null,null,"D6"]
[7633682,"FVCX 24 P/EL110SL",null,{"$f":"D3587+D3588+D3589+D3590+D3591","v":5700},null,null,"A système\n avec sonde extérieure","B","XL",3661238637245,340.9,null,null,null,"D6"]
[7633683,"FVCR 19 P/EL110SL",null,{"$f":"D3586+D3588+D3589+D3590+D3592","v":5800},null,null,"A système\n avec sonde extérieure","B","XL",3661238637252,312.89999999999998,null,null,null,"D6"]
[7633684,"FVCR 24 P/EL110SL",null,{"$f":"D3587+D3588+D3589+D3590+D3592","v":6002},null,null,"A système\n avec sonde extérieure","B","XL",3661238637269,340.9,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7624096,"FSC. 19","MY103",3886,5,14070,"/","/","/",3661238617315,209,1220,750,1050,"D6"]
[7624118,"FSC. 24","MY108",4088,5,14070,"/","/","/",3661238617322,237,1220,750,1050,"D6"]
[7609915,"BALLON EL110SL","ER590",758,null,null,"/","/","/",3661238608726,83,700,680,940,"D6"]
[7614745,"KIT DE LIAISON BALLON EL110SL EQUIPEE","ER594",222,null,null,"/","/","/",3661238608122,3.9,870,260,160,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,15,675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,"A","B","XL"]
[7633685,"FVCX 19 P/EL160SL",null,{"$f":"D3603+D3606+D3607+D3608+D3609","v":5770},null,null,"A","B","XL",3661238637283,327.9,null,null,null,"D6"]
[7633686,"FVCX 24 P/EL160SL",null,{"$f":"D3604+D3606+D3607+D3608+D3609","v":5972},null,null,"A","B","XL",3661238637290,355.9,null,null,null,"D6"]
[7633687,"FVCX 32 P/EL160SL",null,{"$f":"D3605+D3606+D3607+D3608+D3609","v":6324},null,null,"A","B","XL",3661238637306,383.9,null,null,null,"D6"]
[7633688,"FVCR 19 P/EL160SL",null,{"$f":"D3603+D3606+D3607+D3608+D3610","v":6072},null,null,"A","B","XL",3661238637313,327.9,null,null,null,"D6"]
[7633689,"FVCR 24 P/EL160SL",null,{"$f":"D3604+D3606+D3607+D3608+D3610","v":6274},null,null,"A","B","XL",3661238637320,355.9,null,null,null,"D6"]
[7633690,"FVCR 32 P/EL160SL",null,{"$f":"D3605+D3606+D3607+D3608+D3610","v":6626},null,null,"A","B","XL",3661238637337,383.9,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7624096,"FSC. 19","MY103",3886,5,14070,"/","/","/",3661238617315,209,1220,750,1050,"D6"]
[7624118,"FSC. 24","MY108",4088,5,14070,"/","/","/",3661238617322,237,1220,750,1050,"D6"]
[7624125,"FSC. 32","MY113",4440,5,14070,"/","/","/",3661238617339,265,1220,750,1050,"D6"]
[7616405,"BALLON EL160SL","ER592",989,null,null,"/","/","/",3661238608696,98,700,680,1200,"D6"]
[7614827,"KIT DE LIAISON BALLON EL160SL EQUIPEE","ER596",263,null,null,"/","/","/",3661238608146,5,860,250,135,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,15,675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[]
[]
[7633691,"FSCX 19 F HOR",null,{"$f":"D3627+D3630+D3632+D3633","v":4239},null,null,"A système\n avec sonde extérieure","/","/",3661238637344,213.9,null,null,null,"D6"]
[7633692,"FSCX 19 F VER",null,{"$f":"D3627+D3630+D3632+D3634+D3635","v":4345},null,null,"A système\n avec sonde extérieure","/","/",3661238637351,216.7,null,null,null,"D6"]
[7633693,"FSCX 24 F HOR",null,{"$f":"D3628+D3630+D3632+D3633","v":4441},null,null,"A système\n avec sonde extérieure","/","/",3661238637368,241.9,null,null,null,"D6"]
[7633694,"FSCX 24 F VER",null,{"$f":"D3628+D3630+D3632+D3634+D3635","v":4547},null,null,"A système\n avec sonde extérieure","/","/",3661238637375,244.7,null,null,null,"D6"]
[7633695,"FSCX 32 F HOR",null,{"$f":"D3629+D3630+D3632+D3633","v":4793},null,null,"A système\n avec sonde extérieure","/","/",3661238637382,269.89999999999998,null,null,null,"D6"]
[7633696,"FSCX 32 F VER",null,{"$f":"D3629+D3630+D3632+D3634+D3635","v":4899},null,null,"A système\n avec sonde extérieure","/","/",3661238637399,272.69999999999993,null,null,null,"D6"]
[7633697,"FSCR 19 F HOR",null,{"$f":"D3627+D3631+D3632+D3633","v":4541},null,null,"A système\n avec sonde extérieure","/","/",3661238637405,213.9,null,null,null,"D6"]
[7633698,"FSCR 19 F VER",null,{"$f":"D3627+D3631+D3632+D3634+D3635","v":4647},null,null,"A système\n avec sonde extérieure","/","/",3661238637412,216.7,null,null,null,"D6"]
[7633699,"FSCR 24 F HOR",null,{"$f":"D3628+D3631+D3632+D3633","v":4743},null,null,"A système\n avec sonde extérieure","/","/",3661238637429,241.9,null,null,null,"D6"]
[7633700,"FSCR 24 F VER",null,{"$f":"D3628+D3631+D3632+D3634+D3635","v":4849},null,null,"A système\n avec sonde extérieure","/","/",3661238637436,244.7,null,null,null,"D6"]
[7633701,"FSCR 32 F HOR",null,{"$f":"D3629+D3631+D3632+D3633","v":5095},null,null,"A système\n avec sonde extérieure","/","/",3661238637443,269.89999999999998,null,null,null,"D6"]
[7633702,"FSCR 32 F VER",null,{"$f":"D3629+D3631+D3632+D3634+D3635","v":5201},null,null,"A système\n avec sonde extérieure","/","/",3661238637450,272.69999999999993,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7624096,"FSC. 19","MY103",3886,5,14070,"/","/","/",3661238617315,209,1220,750,1050,"D6"]
[7624118,"FSC. 24","MY108",4088,5,14070,"/","/","/",3661238617322,237,1220,750,1050,"D6"]
[7624125,"FSC. 32","MY113",4440,5,14070,"/","/","/",3661238617339,265,1220,750,1050,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[7605520,"KIT FLUX FORCE FSC.","MY405",101,null,null,"/","/","/",3661238604179,1.9,510,460,175,"D6"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,"/","/","/",3661238157972,2.1,1025,170,170,"D6"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[]
[]
[7633703,"FVCX 19 F HOR/EL110SL",null,{"$f":"D3648+D3650+D3651+D3652+D3654+D3655","v":5300},null,null,"A système\n avec sonde extérieure","B","XL",3661238637467,301.89999999999998,null,null,null,"D6"]
[7633704,"FVCX 19 F VER/EL110SL",null,{"$f":"D3648+D3650+D3651+D3652+D3654+D3656+D3657","v":5406},null,null,"A système\n avec sonde extérieure","B","XL",3661238637474,304.69999999999993,null,null,null,"D6"]
[7633705,"FVCX 24 F HOR/EL110SL",null,{"$f":"D3649+D3650+D3651+D3652+D3654+D3655","v":5502},null,null,"A système\n avec sonde extérieure","B","XL",3661238637481,329.9,null,null,null,"D6"]
[7633706,"FVCX 24 F VER/EL110SL",null,{"$f":"D3649+D3650+D3651+D3652+D3654+D3656+D3657","v":5608},null,null,"A système\n avec sonde extérieure","B","XL",3661238637498,332.69999999999993,null,null,null,"D6"]
[7633707,"FVCR 19 F HOR/EL110SL",null,{"$f":"D3648+D3650+D3651+D3653+D3654+D3655","v":5602},null,null,"A système\n avec sonde extérieure","B","XL",3661238637504,301.89999999999998,null,null,null,"D6"]
[7633708,"FVCR 19 F VER/EL110SL",null,{"$f":"D3648+D3650+D3651+D3653+D3654+D3656+D3657","v":5708},null,null,"A système\n avec sonde extérieure","B","XL",3661238637511,304.69999999999993,null,null,null,"D6"]
[7633709,"FVCR 24 F HOR/EL110SL",null,{"$f":"D3649+D3650+D3651+D3653+D3654+D3655","v":5804},null,null,"A système\n avec sonde extérieure","B","XL",3661238637528,329.9,null,null,null,"D6"]
[7633710,"FVCR 24 F VER/EL110SL",null,{"$f":"D3649+D3650+D3651+D3653+D3654+D3656+D3657","v":5910},null,null,"A système\n avec sonde extérieure","B","XL",3661238637535,332.69999999999993,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7624096,"FSC. 19","MY103",3886,5,14070,"/","/","/",3661238617315,209,1220,750,1050,"D6"]
[7624118,"FSC. 24","MY108",4088,5,14070,"/","/","/",3661238617322,237,1220,750,1050,"D6"]
[7609915,"BALLON EL110SL","ER590",758,null,null,"/","/","/",3661238608726,83,700,680,940,"D6"]
[7613103,"KIT DE LIAISON BALLON EL110SL","ER595",303,null,null,"/","/","/",3661238608115,5,860,250,135,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[7605520,"KIT FLUX FORCE FSC.","MY405",101,null,null,"/","/","/",3661238604179,1.9,510,460,175,"D6"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,"/","/","/",3661238157972,2.1,1025,170,170,"D6"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[null,null,null,null,null,null,null,null,null,""]
[]
[7633712,"FVCX 19 F HOR/EL160SL",null,{"$f":"D3674+D3677+D3678+D3679+D3681+D3682","v":5631},null,null,"A système\n avec sonde extérieure","B","XL",3661238637542,316.89999999999998,null,null,null,"D6"]
[7633713,"FVCX 19 F VER/EL160SL",null,{"$f":"D3674+D3677+D3678+D3679+D3681+D3683+D3684","v":5737},null,null,"A système\n avec sonde extérieure","B","XL",3661238637559,319.69999999999993,null,null,null,"D6"]
[7633714,"FVCX 24 F HOR/EL160SL",null,{"$f":"D3675+D3677+D3678+D3679+D3681+D3682","v":5833},null,null,"A système\n avec sonde extérieure","B","XL",3661238637566,344.9,null,null,null,"D6"]
[7633715,"FVCX 24 F VER/EL160SL",null,{"$f":"D3675+D3677+D3678+D3679+D3681+D3683+D3684","v":5939},null,null,"A système\n avec sonde extérieure","B","XL",3661238637573,347.69999999999993,null,null,null,"D6"]
[7633716,"FVCX 32 F HOR/EL160SL",null,{"$f":"D3676+D3677+D3678+D3679+D3681+D3682","v":6185},null,null,"A système\n avec sonde extérieure","B","XL",3661238637580,372.9,null,null,null,"D6"]
[7633717,"FVCX 32 F VER/EL160SL",null,{"$f":"D3676+D3677+D3678+D3679+D3681+D3683+D3684","v":6291},null,null,"A système\n avec sonde extérieure","B","XL",3661238637597,375.69999999999993,null,null,null,"D6"]
[7633718,"FVCR 19 F HOR/EL160SL",null,{"$f":"D3674+D3677+D3678+D3680+D3681+D3682","v":5933},null,null,"A système\n avec sonde extérieure","B","XL",3661238637603,316.89999999999998,null,null,null,"D6"]
[7633719,"FVCR 19 F VER/EL160SL",null,{"$f":"D3674+D3677+D3678+D3680+D3681+D3683+D3684","v":6039},null,null,"A système\n avec sonde extérieure","B","XL",3661238637610,319.69999999999993,null,null,null,"D6"]
[7633721,"FVCR 24 F HOR/EL160SL",null,{"$f":"D3675+D3677+D3678+D3680+D3681+D3682","v":6135},null,null,"A système\n avec sonde extérieure","B","XL",3661238637627,344.9,null,null,null,"D6"]
[7633722,"FVCR 24 F VER/EL160SL",null,{"$f":"D3675+D3677+D3678+D3680+D3681+D3683+D3684","v":6241},null,null,"A système\n avec sonde extérieure","B","XL",3661238637634,347.69999999999993,null,null,null,"D6"]
[7633723,"FVCR 32 F HOR/EL160SL",null,{"$f":"D3676+D3677+D3678+D3680+D3681+D3682","v":6487},null,null,"A système\n avec sonde extérieure","B","XL",3661238637641,372.9,null,null,null,"D6"]
[7633725,"FVCR 32 F VER/EL160SL",null,{"$f":"D3676+D3677+D3678+D3680+D3681+D3683+D3684","v":6593},null,null,"A système\n avec sonde extérieure","B","XL",3661238637658,375.69999999999993,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7624096,"FSC. 19","MY103",3886,5,14070,"/","/","/",3661238617315,209,1220,750,1050,"D6"]
[7624118,"FSC. 24","MY108",4088,5,14070,"/","/","/",3661238617322,237,1220,750,1050,"D6"]
[7624125,"FSC. 32","MY113",4440,5,14070,"/","/","/",3661238617339,265,1220,750,1050,"D6"]
[7616405,"BALLON EL160SL","ER592",989,null,null,"/","/","/",3661238608696,98,700,680,1200,"D6"]
[7613082,"KIT DE LIAISON BALLON EL160SL","ER597",403,null,null,"/","/","/",3661238608139,5,860,250,135,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[7605520,"KIT FLUX FORCE FSC.","MY405",101,null,null,"/","/","/",3661238604179,1.9,510,460,175,"D6"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,"/","/","/",3661238157972,2.1,1025,170,170,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[]
[]
[7633728,"FSCX 19 PF HOR",null,{"$f":"D3701+D3704+D3705+D3707+D3708","v":4719},null,null,"A système\n avec sonde extérieure","/","/",3661238637665,228.9,null,null,null,"D6"]
[7633729,"FSCX 19 PF VER",null,{"$f":"D3701+D3704+D3705+D3707+D3709+D3710","v":4825},null,null,"A système\n avec sonde extérieure","/","/",3661238637672,231.7,null,null,null,"D6"]
[7633730,"FSCX 24 PF HOR",null,{"$f":"D3702+D3704+D3705+D3707+D3708","v":4921},null,null,"A système\n avec sonde extérieure","/","/",3661238637689,256.90000000000003,null,null,null,"D6"]
[7633731,"FSCX 24 PF VER",null,{"$f":"D3702+D3704+D3705+D3707+D3709+D3710","v":5027},null,null,"A système\n avec sonde extérieure","/","/",3661238637696,259.7,null,null,null,"D6"]
[7633732,"FSCX 32 PF HOR",null,{"$f":"D3703+D3704+D3705+D3707+D3708","v":5273},null,null,"A système\n avec sonde extérieure","/","/",3661238637702,284.89999999999998,null,null,null,"D6"]
[7633733,"FSCX 32 PF VER",null,{"$f":"D3703+D3704+D3705+D3707+D3709+D3710","v":5379},null,null,"A système\n avec sonde extérieure","/","/",3661238637719,287.69999999999993,null,null,null,"D6"]
[7633734,"FSCR 19 PF HOR",null,{"$f":"D3701+D3704+D3706+D3707+D3708","v":5021},null,null,"A système\n avec sonde extérieure","/","/",3661238637726,228.9,null,null,null,"D6"]
[7633735,"FSCR 19 PF VER",null,{"$f":"D3701+D3704+D3706+D3707+D3709+D3710","v":5127},null,null,"A système\n avec sonde extérieure","/","/",3661238637733,231.7,null,null,null,"D6"]
[7633736,"FSCR 24 PF HOR",null,{"$f":"D3702+D3704+D3706+D3707+D3708","v":5223},null,null,"A système\n avec sonde extérieure","/","/",3661238637740,256.90000000000003,null,null,null,"D6"]
[7633737,"FSCR 24 PF VER",null,{"$f":"D3702+D3704+D3706+D3707+D3709+D3710","v":5329},null,null,"A système\n avec sonde extérieure","/","/",3661238637757,259.7,null,null,null,"D6"]
[7633738,"FSCR 32 PF HOR",null,{"$f":"D3703+D3704+D3706+D3707+D3708","v":5575},null,null,"A système\n avec sonde extérieure","/","/",3661238637764,284.89999999999998,null,null,null,"D6"]
[7633739,"FSCR 32 PF VER",null,{"$f":"D3703+D3704+D3706+D3707+D3709+D3710","v":5681},null,null,"A système\n avec sonde extérieure","/","/",3661238637771,287.69999999999993,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7624096,"FSC. 19","MY103",3886,5,14070,"/","/","/",3661238617315,209,1220,750,1050,"D6"]
[7624118,"FSC. 24","MY108",4088,5,14070,"/","/","/",3661238617322,237,1220,750,1050,"D6"]
[7624125,"FSC. 32","MY113",4440,5,14070,"/","/","/",3661238617339,265,1220,750,1050,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,15,675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[7605520,"KIT FLUX FORCE FSC.","MY405",101,null,null,"/","/","/",3661238604179,1.9,510,460,175,"D6"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,"/","/","/",3661238157972,2.1,1025,170,170,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[]
[]
[7633740,"FVCX 19 PF HOR/EL110SL",null,{"$f":"D3723+D3725+D3726+D3727+D3728+D3730+D3731","v":5699},null,null,"A système\n avec sonde extérieure","B","XL",3661238637788,316.89999999999998,null,null,null,"D6"]
[7633741,"FVCX 19 PF VER/EL110SL",null,{"$f":"D3723+D3725+D3726+D3727+D3728+D3730+D3732+D3733","v":5805},null,null,"A système\n avec sonde extérieure","B","XL",3661238637795,319.69999999999993,null,null,null,"D6"]
[7633742,"FVCX 24 PF HOR/EL110SL",null,{"$f":"D3724+D3725+D3726+D3727+D3728+D3730+D3731","v":5901},null,null,"A système\n avec sonde extérieure","B","XL",3661238637801,344.9,null,null,null,"D6"]
[7633743,"FVCX 24 PF VER/EL110SL",null,{"$f":"D3724+D3725+D3726+D3727+D3728+D3730+D3732+D3733","v":6007},null,null,"A système\n avec sonde extérieure","B","XL",3661238637818,347.69999999999993,null,null,null,"D6"]
[7633744,"FVCR 19 PF HOR/EL110SL",null,{"$f":"D3723+D3725+D3726+D3727+D3729+D3730+D3731","v":6001},null,null,"A système\n avec sonde extérieure","B","XL",3661238637825,316.89999999999998,null,null,null,"D6"]
[7633745,"FVCR 19 PF VER/EL110SL",null,{"$f":"D3723+D3725+D3726+D3727+D3729+D3730+D3732+D3733","v":6107},null,null,"A système\n avec sonde extérieure","B","XL",3661238637832,319.69999999999993,null,null,null,"D6"]
[7633746,"FVCR 24 PF HOR/EL110SL",null,{"$f":"D3724+D3725+D3726+D3727+D3729+D3730+D3731","v":6203},null,null,"A système\n avec sonde extérieure","B","XL",3661238637849,344.9,null,null,null,"D6"]
[7633747,"FVCR 24 PF VER/EL110SL",null,{"$f":"D3724+D3725+D3726+D3727+D3729+D3730+D3732+D3733","v":6309},null,null,"A système\n avec sonde extérieure","B","XL",3661238637856,347.69999999999993,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7624096,"FSC. 19","MY103",3886,5,14070,"/","/","/",3661238617315,209,1220,750,1050,"D6"]
[7624118,"FSC. 24","MY108",4088,5,14070,"/","/","/",3661238617322,237,1220,750,1050,"D6"]
[7609915,"BALLON EL110SL","ER590",758,null,null,"/","/","/",3661238608726,83,700,680,940,"D6"]
[7614745,"KIT DE LIAISON BALLON EL110SL EQUIPEE","ER594",222,null,null,"/","/","/",3661238608122,3.9,870,260,160,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,15,675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[7605520,"KIT FLUX FORCE FSC.","MY405",101,null,null,"/","/","/",3661238604179,1.9,510,460,175,"D6"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,"/","/","/",3661238157972,2.1,1025,170,170,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[null,null,null,null,null,null,null,null,null,""]
[]
[7633748,"FVCX 19 PF HOR/EL160SL",null,{"$f":"D3750+D3753+D3754+D3755+D3756+D3758+D3759","v":5971},null,null,"A système\n avec sonde extérieure","B","XL",3661238637863,331.9,null,null,null,"D6"]
[7633749,"FVCX 19 PF VER/EL160SL",null,{"$f":"D3750+D3753+D3754+D3755+D3756+D3758+D3760+D3761","v":6077},null,null,"A système\n avec sonde extérieure","B","XL",3661238637870,334.69999999999993,null,null,null,"D6"]
[7633750,"FVCX 24 PF HOR/EL160SL",null,{"$f":"D3751+D3753+D3754+D3755+D3756+D3758+D3759","v":6173},null,null,"A système\n avec sonde extérieure","B","XL",3661238637887,359.9,null,null,null,"D6"]
[7633751,"FVCX 24 PF VER/EL160SL",null,{"$f":"D3751+D3753+D3754+D3755+D3756+D3758+D3760+D3761","v":6279},null,null,"A système\n avec sonde extérieure","B","XL",3661238637894,362.69999999999993,null,null,null,"D6"]
[7633752,"FVCX 32 PF HOR/EL160SL",null,{"$f":"D3752+D3753+D3754+D3755+D3756+D3758+D3759","v":6525},null,null,"A système\n avec sonde extérieure","B","XL",3661238637900,387.9,null,null,null,"D6"]
[7633753,"FVCX 32 PF VER/EL160SL",null,{"$f":"D3752+D3753+D3754+D3755+D3756+D3758+D3760+D3761","v":6631},null,null,"A système\n avec sonde extérieure","B","XL",3661238637917,390.69999999999993,null,null,null,"D6"]
[7633754,"FVCR 19 PF HOR/EL160SL",null,{"$f":"D3750+D3753+D3754+D3755+D3757+D3758+D3759","v":6273},null,null,"A système\n avec sonde extérieure","B","XL",3661238637924,331.9,null,null,null,"D6"]
[7633755,"FVCR 19 PF VER/EL160SL",null,{"$f":"D3750+D3753+D3754+D3755+D3757+D3758+D3760+D3761","v":6379},null,null,"A système\n avec sonde extérieure","B","XL",3661238637924,334.69999999999993,null,null,null,"D6"]
[7633756,"FVCR 24 PF HOR/EL160SL",null,{"$f":"D3751+D3753+D3754+D3755+D3757+D3758+D3759","v":6475},null,null,"A système\n avec sonde extérieure","B","XL",3661238637948,359.9,null,null,null,"D6"]
[7633757,"FVCR 24 PF VER/EL160SL",null,{"$f":"D3751+D3753+D3754+D3755+D3757+D3758+D3760+D3761","v":6581},null,null,"A système\n avec sonde extérieure","B","XL",3661238637955,362.69999999999993,null,null,null,"D6"]
[7633758,"FVCR 32 PF HOR/EL160SL",null,{"$f":"D3752+D3753+D3754+D3755+D3757+D3758+D3759","v":6827},null,null,"A système\n avec sonde extérieure","B","XL",3661238637962,387.9,null,null,null,"D6"]
[7633759,"FVCR 32 PF VER/EL160SL",null,{"$f":"D3752+D3753+D3754+D3755+D3757+D3758+D3760+D3761","v":6933},null,null,"A système\n avec sonde extérieure","B","XL",3661238637979,390.69999999999993,null,null,null,"D6"]
[]
["COMPOSANTS "]
[7624096,"FSC. 19","MY103",3886,5,14070,"/","/","/",3661238617315,209,1220,750,1050,"D6"]
[7624118,"FSC. 24","MY108",4088,5,14070,"/","/","/",3661238617322,237,1220,750,1050,"D6"]
[7624125,"FSC. 32","MY113",4440,5,14070,"/","/","/",3661238617339,265,1220,750,1050,"D6"]
[7616405,"BALLON EL160SL","ER592",989,null,null,"/","/","/",3661238608696,98,700,680,1200,"D6"]
[7614827,"KIT DE LIAISON BALLON EL160SL EQUIPEE","ER596",263,null,null,"/","/","/",3661238608146,5,860,250,135,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,15,675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[7605520,"KIT FLUX FORCE FSC.","MY405",101,null,null,"/","/","/",3661238604179,1.9,510,460,175,"D6"]
[100007638,"TERMINAL HORIZONTAL  Ø 80/125","FM183",100,null,null,"/","/","/",3661238157972,2.1,1025,170,170,"C0"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[null,null,null,null,null,null,null,null,null,""]
[]
["OPTIONS CHAUDIERE"]
[100004290,"STATION DE NEUTRALISATION","FM155",259,null,null,"/","/","/",3661238004238,7.8,490,320,185,"C0"]
[100004291,"RECHARGE STATION DE NEUTRALISATION","FM156",130,null,null,"/","/","/",3661238004221,6.1,405,265,165,"C0"]
[100004292,"SUPPORT STATION DE NEUTRALISATION","FM157",130,null,null,"/","/","/",3661238004214,2,395,330,120,"C0"]
[100004293,"POMPE DE RELEVAGE DES CONDENSATS","FM158",343,0.83,14050,"/","/","/",3661238004207,1.9,230,115,110,"C0"]
[100012500,"FILTRE DEGAZEUR TIGERLOOP COMBI",null,135,null,null,"/","/","/",null,null,null,null,null,"C0"]
[100020045,"KIT FILTRE FERNOX TF1",null,258,null,null,"/","/","/",null,null,null,null,null,"C0"]
[]
["OPTIONS POUR TABLEAU X OETROCOM 1 "]
[88017904,"THERMOSTAT AMBIANCE PROGRAMMABLE","AD191",161,0.12,95010,"/","/","/",3661238102415,0.2,130,90,55,"C0"]
[88017010,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (SANS FILS)","AD192",286,0.12,95010,"/","/","/",3661238102439,0.4,175,150,90,"C0"]
[7609765,"THERMOSTAT D'AMBIANCE MODULANT FILAIRE RS200 -3","AD306",206,0.12,95010,"/","/","/",8713809266462,0.4,148,100,52,"C0"]
[7609764,"THERMOSTAT D'AMBIANCE MODULANT RADIO RS200 -3R","AD305",340,0.12,95010,"/","/","/",8713809266455,0.8,150,110,110,"C0"]
[]
["OPTIONS POUR TABLEAU R OETROCOM 2"]
[7616602,"PLATINE + SONDE POUR 1 CIRCUIT AVEC VANNE MELANGEUSE","MY420",260,0.12,95010,"/","/","/",3661238625747,0.5,305,215,100,"D6"]
[88017904,"THERMOSTAT AMBIANCE PROGRAMMABLE","AD191",161,0.12,95010,"/","/","/",3661238102415,0.2,130,90,55,"C0"]
[88017010,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (SANS FILS)","AD192",286,0.12,95010,"/","/","/",3661238102439,0.4,175,150,90,"C0"]
[7609765,"THERMOSTAT D'AMBIANCE MODULANT FILAIRE RS200 -3","AD306",206,0.12,95010,"/","/","/",8713809266462,0.4,148,100,52,"C0"]
[7609764,"THERMOSTAT D'AMBIANCE MODULANT RADIO RS200 -3R","AD305",340,0.12,95010,"/","/","/",8713809266455,0.8,150,110,110,"C0"]
[]
["OPTIONS ECS"]
[100000030,"COLIS OPTION SONDE ECS","AD212",51,0.02,95020,"/","/","/",3661238011168,0.2,200,150,30,"C0"]
[7622082,"KIT ACI","MY417",124,null,null,"/","/","/",3661238614031,0.5,250,150,100,"C6"]
[7619012,"TESTEUR D'ANODE MAGNESIUM","MY408",62,null,null,"/","/","/",3661238608818,0.5,185,130,105,"D6"]
[null,null,null,null,null,null,null,null,null,""]
["MODULES HYDRAULIQUES",null,null,null,null,null,null,null,null,""]
[7627199,"OPTION 2 FLEXIBLES MONTAGE MURAL ","MY425",166,null,null,"/","/","/",3661238625723,6,860,250,135,"D6"]
[7627079,"KIT DE SECURITE POUR  FS./FSB./FSC.","MY427",129,null,null,"/","/","/",3661238627079,1.6,400,200,100,"D6"]
[89997001,"COL CROIX RAC 1''1/4 ","EA46",56,null,null,null,null,null,3661238044746,1.3,175,140,90,"C0"]
[100020164,"COLLECTEUR 2/3 CIRCUITS","EA140",348,null,null,"/","/","/",3661238575011,6.6,660,180,200,"C0"]
[100020167,"CIRCUIT DIRECT P.ELEC HEE","EA143",644,0.83,14050,"/","/","/",3661238575042,5.0999999999999996,460,270,235,"C0"]
[100020168,"CIRCUIT V3V P.ELEC HEE","EA144",916,0.83,14050,"/","/","/",3661238575059,6,460,270,235,"C0"]
[100020165,"CONSOLE MUR COLLECTEUR","EA141",44,null,null,"/","/","/",3661238575028,1.2,220,125,70,"C0"]
[100020166,"CONSOLE MUR 1 MODULE","EA142",116,null,null,"/","/","/",3661238575035,1.6,220,125,70,"C0"]
[]
[null,"PPS Ø 80 MM"]
[100015325,"KIT N° 1 RACCORDEMENT CHEMINÉE FLEXIBLE PPS Ø 80 MM","DY895",236,null,null,"/","/","/",3661238380110,3.4,395,400,390,"C0"]
[100017527,"KIT DE BASE PPS/ALU D80/125","DY913",166,null,null,"/","/","/",3661238496330,3.7,600,400,275,"C0"]
[84887708,"ADAPTATEUR PPS Ø 60/100 SUR 80/125 MM","DY708",58,null,null,"/","/","/",3661238012028,0.3,255,145,150,"C0"]
[84887701,"KIT DE RACCORDEMENT CHEMINÉE PPS 60/80 MM","DY701",270,null,null,"/","/","/",3661238012097,2.8,395,400,385,"C0"]
[84887717,"KIT N° 1 KIT DE RACCORDEMENT CHEMINÉE PPS Ø 80 MM","DY717",157,null,null,"/","/","/",3661238011946,2.9,395,405,390,"C0"]
[84887546,"PIÈCE DE VISITE Ø 80 MM DROITE","DY146",58,null,null,"/","/","/",3661238013506,0.3,300,145,150,"C0"]
[84887757,"PLAQUE DE FINITION Ø80MM","DY757",41,null,null,"/","/","/",3661238011595,0.3,310,230,140,"C0"]
[84887613,"RALLONGE PPS Ø 80 MM   LG= 250 MM (2 PIÈCES)","DY613",40,null,null,"/","/","/",3661238012967,0.4,250,170,175,"C0"]
[84887614,"RALLONGE PPS Ø 80 MM   LG= 500 MM (2 PIÈCES)","DY614",38,null,null,"/","/","/",3661238012950,0.7,500,160,150,"C0"]
[84887615,"RALLONGE PPS Ø 80 MM   LG= 1000 MM (2 PIÈCES)","DY615",51,null,null,"/","/","/",3661238012943,1.3,1000,160,145,"C0"]
[84887550,"RALLONGE PPS Ø 80 MM   LG= 2000 MM  (2 PIÈCES)","DY150",77,null,null,"/","/","/",3661238013469,2.5,1960,150,150,"C0"]
[84887552,"COUDE PPS À 90°","DY152",16,null,null,"/","/","/",3661238013445,0.2,255,145,150,"C0"]
[84887554,"COUDE PPS À 45° (2 PIECES)","DY154",35,null,null,"/","/","/",3661238013421,0.3,200,200,150,"C0"]
[84887563,"TÉ PPS  AVEC COUVERCLE D'INSPECTION","DY163",58,null,null,"/","/","/",3661238013353,0.4,290,220,170,"C0"]
[84887551,"COLLIER DE CENTRAGE Ø 80 mm (2 PIECES)","DY151",14,null,null,"/","/","/",3661238013452,0.1,300,300,40,"C0"]
[84887585,"TERMINAL AVEC SOLIN DIAMÉTRE 80","DY185",148,null,null,"/","/","/",3661238013148,1.5,390,380,280,"C0"]
[100008301,"COUDE DE REVISION PPS 87° Ø 80 MM (GRIS)","DY877",41,null,null,"/","/","/",3661238102026,0.2,190,195,145,"C0"]
[84887753,"TUYAU DE PROTECTION L500MM Ø 124MM","DY753",25,null,null,"/","/","/",3661238011632,0.4,500,155,140,"C0"]
[100015318,"ADAPTATEUR PPS Ø 80M-110F","DY902",52,null,null,"/","/","/",3661238379909,0.3,195,195,145,"C0"]
[100015319,"MANCHON PPS 80M-80F AVEC PRISE DE MESURE","DY903",47,null,null,"/","/","/",3661238380219,0.2,195,195,145,"C0"]
[7650954,"KIT CHEMINEE B23 FLEX PPS D80","DY923",300,null,null,"/","/","/",3661238659421,5.0999999999999996,706,706,347,"C0"]
[7650958,"KIT CHEMINEE C93 FLEX PPS D80 ","DY925",461,null,null,"/","/","/",3661238659445,5.2,706,706,347,"C0"]
[7650964,"KIT TELESCO. PLAFOND C93 FLEX D80 ","DY927",210,null,null,"/","/","/",3661238659469,2.5,600,396,412,"C0"]
[7650968,"TERMINAL VERTICAL PPS D60/100 NOIR","DY928",148,null,null,"/","/","/",3661238659476,2.6,1200,200,200,"C0"]
[]
[null,"PPS 80/125 MM"]
[100002732,"TERMINAL VERTICAL PPS Ø 80/125 MM NOIR","DY843",155,null,null,"/","/","/",3661238006621,4.2,1210,270,240,"C0"]
[100002733,"TERMINAL VERTICAL PPS Ø 80/125 MM ROUGE","DY844",154,null,null,"/","/","/",3661238006614,4.2,1210,265,240,"C0"]
[84887716,"KIT N° 3 RACCORDEMENT CHAUDIÈRE  PPS Ø 80/125 MM","DY716",144,null,null,"/","/","/",3661238011953,2.4,500,290,260,"C0"]
[84887524,"PIÈCE D'INSPECTION DROITE ALU/PPS Ø 80/125 MM","DY124",110,null,null,"/","/","/",3661238013704,0.6,300,145,150,"C0"]
[100008311,"COUDE DE REVISION ALU/PPS Ø 80/125 MM","DY875",115,null,null,"/","/","/",3661238101920,0.7,195,195,145,"C0"]
[100003271,"KIT DE RACCORDEMENT CHAUDIÈRE PERPENDICULAIRE","DY849",225,null,null,"/","/","/",3661238005600,3.5,595,395,410,"C0"]
[100003272,"KIT DE RACCORDEMENT CHAUDIÈRE SOUS CONDUIT","DY850",168,null,null,"/","/","/",3661238005594,1.4,500,290,260,"C0"]
[84887525,"TÉ D'INSPECTION ALU/PPS Ø 80/125 MM","DY125",126,null,null,"/","/","/",3661238013698,0.8,315,235,150,"C0"]
[84887526,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 LG= 250 MM","DY126",41,null,null,"/","/","/",3661238013681,0.5,255,145,150,"C0"]
[84887527,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 LG= 500 MM","DY127",47,null,null,"/","/","/",3661238013674,0.9,520,140,140,"C0"]
[84887528,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 LG=1000 MM","DY128",69,null,null,"/","/","/",3661238013667,1.7,1010,135,140,"C0"]
[84887529,"RALLONGE CONCENTRIQUE ALU/PPS 80/125 LG=1950 MM","DY129",120,null,null,"/","/","/",3661238013650,3.5,1960,150,150,"C0"]
[84887758,"PLAQUE DE FINITION Ø125MM","DY758",64,null,null,"/","/","/",3661238011588,0.5,310,235,145,"C0"]
[84887763,"TUYAU DE PROTECTION L500MM Ø141MM","DY763",30,null,null,"/","/","/",3661238011533,1.1000000000000001,500,160,150,"C0"]
[84887530,"MANC. COMP. D80/125","DY130",71,null,null,"/","/","/",3661238013643,0.6,300,140,145,"C0"]
[84887531,"COUDE A 87° ALU/PPS  Ø 80/125 MM","DY131",51,null,null,"/","/","/",3661238013636,0.7,200,200,150,"C0"]
[84887532,"COUDE CONCENTRIQUE 45° ALU/PPS Ø 80/125 MM (2 PIÈCES)","DY132",77,null,null,"/","/","/",3661238013629,1,315,235,150,"C0"]
[null,"FLEXIBLE PPS Ø 80 MM"]
[100015325,"KIT N° 1 RACCORDEMENT CHEMINÉE FLEXIBLE PPS Ø 80 MM","DY895",236,null,null,"/","/","/",3661238380110,3.4,395,400,390,"C0"]
[100015327,"TUBE FLEXIBLE LG=12,5M","DY897",354,null,null,"/","/","/",3661238380134,8,1200,780,370,"C0"]
[100015326,"TUBE FLEXIBLE LG=50M","DY896",1242,null,null,"/","/","/",3661238380127,26,1200,800,1170,"C0"]
[84887618,"ETOILE DE CENTRAGE POUR FLEXIBLE Ø 80 MM (2 PIÈCES)","DY618",37,null,null,"/","/","/",3661238012912,0.2,300,300,70,"C0"]
[100015328,"PIÈCE DE COUPLAGE FLEXIBLE Ø 80 MM","DY898",71,null,null,"/","/","/",3661238380141,0.3,155,155,160,"C0"]
[100015331,"OUTIL D'AIDE À L'INSERTION Ø 80 MM","DY901",177,null,null,"/","/","/",3661238380172,1.4,300,210,185,"C0"]
[100015330,"PIÈCE D'INSPECTION POUR TUBE FLEXIBLE","DY900",127,null,null,"/","/","/",3661238380165,0.5,295,145,150,"C0"]
[100015329,"TERMINAL AVEC SOLIN FLEX. Ø 80 MM","DY899",177,null,null,"/","/","/",3661238380158,1.7,395,400,265,"C0"]
[100015880,"ADAPTATEUR PPS FLEX Ø 80 MM","DY904",42,null,null,"/","/","/",3661238417632,0.1,195,195,145,"C0"]
[null,"DIVERS FUMISTERIE"]
[84887411,"SORTIE HORIZONTALE TOIT PENTE DE 30° A 45° ( uniquement pour tuiles mécaniques)","DY11",179,null,null,"/","/","/",3661238013940,3.6,1020,700,370,"C0"]
[84837729,"SORTIE DE TOIT EN PENTE DE 40° A 60° ( uniquement pour tuiles mécaniques)","CX49",178,null,null,"/","/","/",3661238014367,3.5,920,700,320,"C0"]
[84837731,"EMBASE D'ETANCHEITE POUR TOIT PLAT","CX51",43,null,null,"/","/","/",3661238014343,0.6,400,400,155,"C0"]
[84837121,"TUILE A DOUILLE 5 A 25° NOIRE","CX121",112,null,null,"/","/","/",3661238014428,3,510,250,145,"C0"]
[84837732,"TUILE A DOUILLE 25 A 45° NOIRE","CX52",77,null,null,"/","/","/",3661238014336,3,520,250,145,"C0"]
[84837734,"TUILE A DOUILLE 35 A 55° NOIRE","CX63",97,null,null,"/","/","/",3661238014312,3.2,510,265,180,"C0"]
[84837120,"TUILE A DOUILLE 5 A 25° ROUGE","CX120",112,null,null,"/","/","/",3661238014435,3,515,245,145,"C0"]
[84837783,"TUILE A DOUILLE 25 A 45° ROUGE","CX83",77,null,null,"/","/","/",3661238014213,3,515,250,150,"C0"]
[84837784,"TUILE A DOUILLE 35 A 55° ROUGE","CX84",97,null,null,"/","/","/",3661238014206,3,520,265,180,"C0"]
[84837741,"PLATINE DE FINITION INTERIEURE","CX72",17,null,null,"/","/","/",3661238014251,0.7,245,210,3,"C0"]
[100005002,"GRILLE DE PROTECTION INOX Ø 80/125 MM","DY865",176,null,null,"/","/","/",3661238001886,2.6,275,270,270,"C0"]
[84887435,"GRILLE D'AERATION EXTERIEURE 250 X 300 mm","DY35",24,null,null,"/","/","/",3661238013889,0.3,300,250,30,"C0"]
[84887436,"GRILLE D'AERATION INTERIEURE 175 CM²","DY36",25,null,null,"/","/","/",3661238013872,0.3,250,295,2,"C0"]
[84837779,"COLLIER DE FIXATION Ø 125 MM PATTE LONGUE","CX79",15,null,null,"/","/","/",3661238014237,0.4,230,160,200,"C0"]
[84837118,"COLLIER DE FIXATION Ø 125 MM PATTE COURTE","CX118",12,null,null,"/","/","/",3661238014459,0.2,225,185,20,"C0"]
[84887451,"COLLIER D'ETANCHEITE POUR MONTAGE EXTERIEUR","DY51",27,null,null,"/","/","/",3661238013841,0.2,150,130,60,"C0"]
[]
[]
[7633658,"FSCX 40",null,{"$f":"D3879+D3882","v":5602},null,null,"A système\n avec sonde extérieure","/","/",3661238667914,{"$f":"K3879+K3882","v":293.89999999999998},null,null,null,"D6"]
[7633659,"FSCX 50",null,{"$f":"D3880+D3882","v":6208},null,null,"A système\n avec sonde extérieure","/","/",3661238667921,{"$f":"K3880+K3882","v":331.9},null,null,null,"D6"]
[7633663,"FSCR 40",null,{"$f":"D3879+D3883","v":5904},null,null,"A système\n avec sonde extérieure","/","/",3661238667938,{"$f":"K3879+K3883","v":293.89999999999998},null,null,null,"D6"]
[7633664,"FSCR 50",null,{"$f":"D3880+D3883","v":6510},null,null,"A système\n avec sonde extérieure","/","/",3661238667945,{"$f":"K3880+K3883","v":331.9},null,null,null,"D6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D6"]
["COMPOSANTS"]
[7624133,"FSC. 40","MY117",5450,5,14070,"/","/","/",3661238617346,293,1425,750,1060,"D6"]
[7624884,"FSC. 50*","MY121",6056,5,14070,"/","/","/",3661238643314,331,1200,1200,1315,"D6"]
[null,"* JAQUETTE, CONDENSEUR ET BRULEUR A MONTER",null,null,null,null,"/","/","/",null,null,null,null,null,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[]
["OPTIONS ECS"]
[7639559,"KIT DE LIAISON FS/FSB/FSC - BALLON INDEPENDANT OBLC/OBPB ","ER598",489,null,null,"/","/","/",3661238641679,7,600,500,135,"D6"]
[]
["FUMISTERIE"]
[null,"PPS Ø 110 mm"]
[84887577,"KIT DE RACCORDEMENT CHEMINEE PPS Ø 110 mm","DY177",258,null,null,"/","/","/",3661238013223,2.68,395,300,510,"C0"]
[84887578,"TUYAU PPS Ø 110 mm LG = 1950 mm (GRIS)","DY178",72,null,null,"/","/","/",3661238013216,2.46,1960,150,150,"C0"]
[84887579,"TUYAU PPS Ø 110 mm LG = 1000 mm (GRIS)","DY179",41,null,null,"/","/","/",3661238013209,1.24,1015,130,140,"C0"]
[84887580,"TUYAU PPS Ø 110 mm LG = 500 mm (GRIS)","DY180",31,null,null,"/","/","/",3661238013193,0.62,515,135,140,"C0"]
[84887581,"COUDE PPS 87° Ø 110 mm (GRIS)","DY181",36,null,null,"/","/","/",3661238013186,0.33,255,190,150,"C0"]
[84887582,"COUDE PPS 45° Ø 110 mm (GRIS)","DY182",48,null,null,"/","/","/",3661238013179,0.52,295,215,165,"C0"]
[84887583,"T DE REVISION Ø 110 mm (GRIS)","DY183",48,null,null,"/","/","/",3661238013162,0.46,300,150,150,"C0"]
[84887587,"ETOILE DE CENTRAGE PPS  Ø 110 mm (2 PIECES)","DY187",15,null,null,"/","/","/",3661238013124,0.1,300,300,30,"C0"]
[84887588,"COUDE DE REVISION PPS 87° Ø 110 mm (GRIS)","DY188",72,null,null,"/","/","/",3661238013117,0.52,315,235,150,"C0"]
[84887772,"PLAQUE DE FINITION","DY772",58,null,null,"/","/","/",3661238011458,0.49,310,230,145,"C0"]
[84887773,"FOURREAU Ø165mm L 500mm","DY773",41,null,null,"/","/","/",3661238011441,1.23,515,165,170,"C3"]
[84887435,"GRILLE D'AERATION EXTERIEURE 250 X 300 mm","DY35",24,null,null,"/","/","/",3661238013889,0.35,300,250,30,"C0"]
[100015325,"KIT N° 1 RACCORDEMENT CHEMINÉE FLEXIBLE PPS Ø 80 mm","DY895",236,null,null,"/","/","/",3661238380110,2.87,395,395,380,"C0"]
[100015327,"TUBE FLEXIBLE LG=12,5M","DY897",354,null,null,"/","/","/",3661238380134,8.6999999999999993,1200,1220,250,"C0"]
[100015326,"TUBE FLEXIBLE LG=50M","DY896",1242,null,null,"/","/","/",3661238380127,35,1600,1660,410,"C0"]
[84887618,"ETOILE DE CENTRAGE POUR FLEXIBLE Ø 80  mm (2 PIÈCES)","DY618",37,null,null,"/","/","/",3661238012912,0.2,300,300,70,"C0"]
[100015328,"PIÈCE DE COUPLAGE FLEXIBLE Ø 80 mm","DY898",71,null,null,"/","/","/",3661238380141,0.25,150,150,150,"C0"]
[100015331,"OUTIL D'AIDE À L'INSERTION Ø 80 mm","DY901",177,null,null,"/","/","/",3661238380172,1.4,300,210,185,"C0"]
[100015330,"PIÈCE D'INSPECTION POUR TUBE FLEXIBLE","DY900",127,null,null,"/","/","/",3661238380165,0.5,295,140,140,"C0"]
[100015329,"TERMINAL AVEC SOLIN FLEX. Ø 80 mm","DY899",177,null,null,"/","/","/",3661238380158,1.74,385,385,250,"C0"]
[]
[]
[100019185,"PUX2 265 CONDENS CORPS MONTE",null,9136,null,null,"A","/","/",3661238549869,null,null,null,null,"C0"]
[100019186,"PUX2 266 CONDENS CORPS MONTE",null,10372,null,null,"A","/","/",3661238549876,null,null,null,null,"C0"]
[100019187,"PUX2 267 CONDENS CORPS MONTE",null,11018,null,null,"A","/","/",3661238549883,null,null,null,null,"C0"]
[100019188,"PUR 265 CONDENS + AD217  CORPS MONTE",null,9998,null,null,"A","/","/",3661238549890,null,null,null,null,"C0"]
[100019189,"PUR 266 CONDENS + AD217  CORPS MONTE",null,11234,null,null,"A","/","/",3661238549906,null,null,null,null,"C0"]
[100019190,"PUR 267 CONDENS + AD217  CORPS MONTE",null,11880,null,null,"A","/","/",3661238549913,null,null,null,null,"C0"]
[100019358,"PUX2 265 CONDENS CORPS NON MONTE",null,9140,null,null,"A","/","/",3661238562219,null,null,null,null,"C0"]
[100019359,"PUX2 266 CONDENS CORPS NON MONTE",null,10378,null,null,"A","/","/",3661238562226,null,null,null,null,"C0"]
[100019360,"PUX2 267 CONDENS CORPS NON MONTE",null,11025,null,null,"A","/","/",3661238562233,null,null,null,null,"C0"]
[100019361,"PUR 265 CONDENS + AD217  CORPS NON MONTE",null,10002,null,null,"A","/","/",3661238562240,null,null,null,null,"C0"]
[100019362,"PUR 266 CONDENS + AD217  CORPS NON MONTE",null,11240,null,null,"A","/","/",3661238562257,null,null,null,null,"C0"]
[100019363,"PUR 267 CONDENS + AD217  CORPS NON MONTE",null,11887,null,null,"A","/","/",3661238562264,null,null,null,null,"C0"]
[]
["COMPOSANTS"]
[200004483,"ELEMENT INTERMEDIAIRE PK 260",null,268,null,null,"/","/","/",3661238001787,35.83,650,410,125,"C0"]
[82270002,"ELEMENT AVANT PKR-250",null,273,null,null,"/","/","/",3661238020580,35.25,660,480,130,"C0"]
[82270003,"ELEMENT ARRIERE PKR-250",null,359,null,null,"/","/","/",3661238020573,42.5,690,410,130,"C0"]
[100004367,"CAISSE ACCESSOIRES 5 ELEMENTS","ME7",1011,null,null,"/","/","/",3661238003613,45.5,645,610,390,"C0"]
[100004368,"CAISSE ACCESSOIRES 6 ELEMENTS","ME8",1076,null,null,"/","/","/",3661238003606,49,645,610,390,"C0"]
[100004369,"CAISSE ACCESSOIRES 7 ELEMENTS","ME9",1106,null,null,"/","/","/",3661238003590,49.5,645,610,390,"C0"]
[100019219,"COLIS JAQUETTE PK265/PU265  ","MF6",1137,null,null,"/","/","/",3661238549449,37,1090,750,425,"C0"]
[100019220,"COLIS JAQUETTE PK266/PU266","MF7",1152,null,null,"/","/","/",3661238549456,34.5,1100,870,440,"C0"]
[100019221,"COLIS JAQUETTE PK267/PU267","MF8",1158,null,null,"/","/","/",3661238549470,44,1095,1045,440,"C0"]
[100004362,"CORPS ASSEMBLE 5 ELEMENTS","ME2",2443,null,null,"/","/","/",3661238003668,248,975,815,630,"C0"]
[100004363,"CORPS ASSEMBLE 6 ELEMENTS   ","ME3",2784,null,null,"/","/","/",3661238003651,294,1105,815,630,"C0"]
[100004364,"CORPS ASSEMBLE 7 ELEMENTS","ME4",3081,null,null,"/","/","/",3661238003644,332,1230,815,630,"C0"]
[82277010,"LIASSE TIGE ASSEMB. 6 EL ",null,10,null,null,"/","/","/",3661238020511,0.43,700,15,10,"C0"]
[82277011,"LIASSE TIGE ASSEMB. 7 EL  ",null,10,null,null,"/","/","/",3661238020504,0.51,825,15,7,"C0"]
[100018925,"COLIS CONDENSEUR + SIPHON  AWR430","ME74",2645,null,null,"/","/","/",3661238548312,35,570,742,731,"C0"]
[100018926,"COLIS CONDENSEUR + SIPHON  AWR440","ME75",3252,null,null,"/","/","/",3661238548329,44,570,742,891,"C0"]
[100018995,"COLIS ACCES GTUC225/PU265COND","ME71",235,null,null,"/","/","/",3661238548282,6,480,305,280,"C0"]
[100018997,"COLIS ACCES GTUC226-227/PU266-267","ME72",263,null,null,"/","/","/",3661238548299,11,480,305,280,"C0"]
[100018994,"HABILLAGE GTUC 220/PU260COND","ME70",242,null,null,"/","/","/",3661238548275,16,1150,550,135,"C0"]
[100019091,"BRULEUR  OEN 265 LZV-P ","ME85",1661,null,null,"/","/","/",3661238550018,17,800,300,400,"C0"]
[100019092,"BRULEUR  OEN 266 LZV-P","ME86",1906,null,null,"/","/","/",3661238550025,18,800,300,400,"C0"]
[100019093,"BRULEUR  OEN 267 LZV-P","ME87",2249,null,null,"/","/","/",3661238550032,23,780,370,420,"C0"]
[100019081,"COLIS DOC PU265 CONDENS","ME79",27,null,null,"/","/","/",3661238548756,1,325,240,50,"C0"]
[100019082,"COLIS DOC PU266 CONDENS","ME80",27,null,null,"/","/","/",3661238548763,1,325,240,50,"C0"]
[100019083,"COLIS DOC PU267 CONDENS","ME81",27,null,null,"/","/","/",3661238548770,1,325,240,50,"C0"]
[100004587,"TABLEAU  R/TA","FT63",1314,3.34,"11.14","/","/","/",3661238110427,5.2,415,425,195,"C0"]
[100004588,"TABLEAU CDE X2 / TA","FT64",746,3.34,"11.14","/","/","/",3661238110410,5.2,415,425,195,"C0"]
[100004294,"PLATINE 2 all./Mod./V3V","AD217",294,0.12,95010,"/","/","/",3661238004191,0.75,200,145,130,"C0"]
[]
["OPTIONS TABLEAUX"]
[88017017,"SONDE DEPART","AD199",80,0.02,95020,"/","/","/",3661238049185,0.21,150,200,40,"C0"]
[88017014,"COLIS OPTION V3V     ","AD196",180,0.02,95020,"/","/","/",3661238102422,0.52,260,170,120,"C0"]
[85757742,"SONDE FUMEES","FM47",72,0.02,95020,"/","/","/",3661238022744,0.17,210,160,40,"C0"]
[161118,"COMMANDE A DISTANCE INTERACTIVE AD194","AD194",197,0.12,95010,"/","/","/",3661238106505,0.15,null,null,null,"C0"]
[100002803,"COMMANDE A DISTANCE SIMPLIFIEE AD208","AD208",104,0.12,95010,"/","/","/",3661238554931,0.2,120,85,40,"C0"]
[88017887,"SONDES POUR BALLON TAMPON","AD160",97,0.02,95020,"/","/","/",3661238048720,0.21,210,170,40,"C7"]
[88017851,"CABLE DE LIAISON BUS LG 12 M","AD134",110,0.02,95020,"/","/","/",3661238048850,0.37,350,260,30,"C0"]
[88017904,"THERMOSTAT AMBIANCE PROGRAMMABLE","AD191",161,0.12,95010,"/","/","/",3661238102415,0.24,135,90,55,"C0"]
[88017010,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (SANS FILS)","AD192",286,0.12,95010,"/","/","/",3661238102439,0.42499999999999999,180,150,90,"C0"]
[]
["OPTIONS ECS"]
[89557009,"KIT DE TRANSFORMATION G/R 3/4 '' ET 1 ''","BH84",32,null,null,"/","/","/",3661238047563,0.32500000000000001,200,140,45,"C0"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.16,200,150,30,"C0"]
[100007835,"KIT LIAISON PK264-6","EA117",525,null,null,"/","/","/",3661238113312,6.5,600,500,135,"C0"]
[]
["TOUTES OPTIONS "]
[100019830,"KIT 2EME RETOUR ","ME117",728,null,null,"/","/","/",3661238570214,6.6,510,330,150,"C0"]
[100019474,"STATION DE NEUTRALISATION ","ME115",366,null,null,"/","/","/",3661238563520,12,null,null,null,"C0"]
[100019475,"GRANULAT DE NEUTRALISATION","ME116",222,null,null,"/","/","/",3661238563513,11,null,null,null,"C0"]
[]
[]
[100013095,"PUR 354 CONDENS CORPS VRAC",null,14825,null,null,"Pas concerné par l'étiquettage",null,null,3661238551756,null,null,null,null,"C3"]
[100012740,"PUR 355 CONDENS CORPS VRAC",null,15290,null,null,"Pas concerné par l'étiquettage",null,null,3661238551763,null,null,null,null,"C3"]
[100012741,"PUR 356 CONDENS CORPS VRAC",null,15853,null,null,"Pas concerné par l'étiquettage",null,null,3661238551770,null,null,null,null,"C3"]
[100012742,"PUR 357 CONDENS CORPS VRAC",null,22000,null,null,"Pas concerné par l'étiquettage",null,null,3661238551787,null,null,null,null,"C3"]
[100012743,"PUR 358 CONDENS CORPS VRAC",null,22975,null,null,"Pas concerné par l'étiquettage",null,null,3661238551794,null,null,null,null,"C3"]
[100012744,"PUR 359 CONDENS CORPS VRAC",null,24233,null,null,"Pas concerné par l'étiquettage",null,null,3661238551800,null,null,null,null,"C3"]
[100013096,"PUX 354 CONDENS CORPS VRAC",null,14649,null,null,"Pas concerné par l'étiquettage",null,null,3661238551817,null,null,null,null,"C3"]
[100012745,"PUX 355 CONDENS CORPS VRAC",null,15114,null,null,"Pas concerné par l'étiquettage",null,null,3661238551824,null,null,null,null,"C3"]
[100012746,"PUX 356 CONDENS CORPS VRAC",null,15677,null,null,"Pas concerné par l'étiquettage",null,null,3661238551831,null,null,null,null,"C3"]
[100012747,"PUX 357 CONDENS CORPS VRAC",null,21824,null,null,"Pas concerné par l'étiquettage",null,null,3661238551848,null,null,null,null,"C3"]
[100012748,"PUX 358 CONDENS CORPS VRAC",null,22799,null,null,"Pas concerné par l'étiquettage",null,null,3661238551855,null,null,null,null,"C3"]
[100012749,"PUX 359 CONDENS CORPS VRAC",null,24057,null,null,"Pas concerné par l'étiquettage",null,null,3661238551862,null,null,null,null,"C3"]
[100013097,"PUR 354 CONDENS CORPS ASSEMBLE",null,15151,null,null,"Pas concerné par l'étiquettage",null,null,3661238551879,null,null,null,null,"C3"]
[100012750,"PUR 355 CONDENS CORPS ASSEMBLE",null,15736,null,null,"Pas concerné par l'étiquettage",null,null,3661238551886,null,null,null,null,"C3"]
[100012751,"PUR 356 CONDENS CORPS ASSEMBLE",null,16420,null,null,"Pas concerné par l'étiquettage",null,null,3661238551893,null,null,null,null,"C3"]
[100012752,"PUR 357 CONDENS CORPS ASSEMBLE",null,22562,null,null,"Pas concerné par l'étiquettage",null,null,3661238551909,null,null,null,null,"C3"]
[100012753,"PUR 358 CONDENS CORPS ASSEMBLE",null,23541,null,null,"Pas concerné par l'étiquettage",null,null,3661238551916,null,null,null,null,"C3"]
[100012754,"PUR 359 CONDENS CORPS ASSEMBLE",null,24835,null,null,"Pas concerné par l'étiquettage",null,null,3661238551923,null,null,null,null,"C3"]
[100013098,"PUX 354 CONDENS CORPS ASSEMBLE",null,14975,null,null,"Pas concerné par l'étiquettage",null,null,3661238551930,null,null,null,null,"C3"]
[100012755,"PUX 355 CONDENS CORPS ASSEMBLE",null,15560,null,null,"Pas concerné par l'étiquettage",null,null,3661238551947,null,null,null,null,"C3"]
[100012756,"PUX 356 CONDENS CORPS ASSEMBLE",null,16244,null,null,"Pas concerné par l'étiquettage",null,null,3661238551954,null,null,null,null,"C3"]
[100012757,"PUX 357 CONDENS CORPS ASSEMBLE",null,22386,null,null,"Pas concerné par l'étiquettage",null,null,3661238551961,null,null,null,null,"C3"]
[100012758,"PUX 358 CONDENS CORPS ASSEMBLE",null,23365,null,null,"Pas concerné par l'étiquettage",null,null,3661238551978,null,null,null,null,"C3"]
[100012759,"PUX 359 CONDENS CORPS ASSEMBLE",null,24659,null,null,"Pas concerné par l'étiquettage",null,null,3661238551985,null,null,null,null,"C3"]
[]
["COMPOSANTS"]
[85537066,"CORPS GT 304 / II ASSEMBLE",null,2381,null,null,"/","/","/",3661238026186,488,1100,920,680,"C3"]
[85537067,"CORPS GT 305 / II ASSEMBLE",null,2868,null,null,"/","/","/",3661238026179,600,1085,1085,670,"C3"]
[85537068,"CORPS GT 306 / II ASSEMBLE",null,3283,null,null,"/","/","/",3661238026162,712.5,1250,1080,680,"C3"]
[85537069,"CORPS GT 307 / II ASSEMBLE",null,3710,null,null,"/","/","/",3661238026155,824,1410,1080,680,"C3"]
[85537070,"CORPS GT 308 / II ASSEMBLE",null,4133,null,null,"/","/","/",3661238026148,936,1550,1080,680,"C3"]
[85537071,"CORPS GT 309 / II ASSEMBLE",null,4598,null,null,"/","/","/",3661238026131,1048,1730,1080,680,"C3"]
[85537072,"EL. ARRIERE GT300/II CPL.",null,549,null,null,"/","/","/",3661238026124,130,1070,600,190,"C3"]
[82190001,"ELT GT  300 INTER",null,336,null,null,"/","/","/",3661238020832,111,990,600,165,"C3"]
[82190002,"ELT GT  300 AVANT",null,499,null,null,"/","/","/",3661238020825,104,1070,620,170,"C3"]
[82198944,"LIASSE TIGES ASS. GT304",null,8,null,null,"/","/","/",3661238020658,1.29,575,50,50,"C3"]
[82198945,"LIASSE TIGES ASS. GT305",null,9,null,null,"/","/","/",3661238020641,1.56,700,50,50,"C3"]
[82198946,"LIASSE TIGES ASS. GT306",null,10,null,null,"/","/","/",3661238020634,1.9,865,50,50,"C3"]
[82198947,"LIASSE TIGES ASS. GT307",null,12,null,null,"/","/","/",3661238020627,2.25,1025,50,50,"C3"]
[82198948,"LIASSE TIGES ASS. GT308",null,15,null,null,"/","/","/",3661238020610,2.61,1185,50,50,"C3"]
[82198949,"LIASSE TIGES ASS. GT309",null,22,null,null,"/","/","/",3661238020603,2.92,1330,50,50,"C3"]
[85537009,"ACC CORPS EN VRAC 4 EL","FD9",501,null,null,"/","/","/",3661238026537,47,660,615,370,"C3"]
[85537010,"ACC CORPS EN VRAC 5 EL","FD10",514,null,null,"/","/","/",3661238026520,48,660,615,370,"C3"]
[85537011,"ACC CORPS EN VRAC 6 EL","FD11",534,null,null,"/","/","/",3661238026513,49.5,660,615,370,"C3"]
[85537012,"ACC CORPS EN VRAC 7 EL","FD12",610,null,null,"/","/","/",3661238026506,49.5,660,615,370,"C3"]
[85537013,"ACC CORPS EN VRAC 8 EL","FD13",678,null,null,"/","/","/",3661238026490,50,660,615,370,"C3"]
[85537014,"ACC CORPS EN VRAC 9 EL","FD14",719,null,null,"/","/","/",3661238026483,51.5,660,615,370,"C3"]
[82197712,"COLIS TURBUL. GT304","BP16",194,null,null,"/","/","/",3661238020818,29,635,510,220,"C3"]
[82197713,"COLIS TURBUL. GT305/306","BP17",207,null,null,"/","/","/",3661238020801,36,635,510,220,"C3"]
[82197715,"COLIS TURBUL. GT307","BP19",213,null,null,"/","/","/",3661238020795,39,500,630,240,"C3"]
[82197716,"COLIS TURBUL. GT308","BP20",438,null,null,"/","/","/",3661238020788,55,635,510,380,"C3"]
[82197717,"COLIS TURBUL. GT309","BP21",492,null,null,"/","/","/",3661238020771,60,500,630,400,"C3"]
[82197718,"PORTE FOYERE D.135","BP13",283,null,null,"/","/","/",3661238020764,21.6,680,180,520,"C3"]
[85537015,"ACC COR.ASS.4-5 ELTS","FD15",290,null,null,"/","/","/",3661238026476,26,680,525,190,"C3"]
[85537019,"ACC COR.ASS.6-7-8 ELTS","FD19",364,null,null,"/","/","/",3661238026469,26.5,680,525,190,"C3"]
[85537020,"ACC COR.ASS.9 ELTS","FD20",376,null,null,"/","/","/",3661238026452,27,680,525,190,"C3"]
[100004865,"COLIS JAQUETTE LATERALE GT 334","MD7",520,null,null,"/","/","/",3661238002098,40.5,1180,980,330,"C3"]
[100004866,"COLIS JAQUETTE LATERALE GT 335","MD8",567,null,null,"/","/","/",3661238002081,44,1180,980,330,"C3"]
[100004867,"COLIS JAQUETTE LATERALE GT 336","MD9",626,null,null,"/","/","/",3661238002074,80.5,1230,1350,390,"C3"]
[100004868,"COLIS JAQUETTE LATERALE GT 337","MD10",684,null,null,"/","/","/",3661238002067,95.25,1230,1350,390,"C3"]
[100004869,"COLIS JAQUETTE LATERALE GT 338","MD11",938,null,null,"/","/","/",3661238002050,91.25,1230,1650,390,"C3"]
[100004880,"COLIS JAQUETTE LATERALE GT 339","MD12",1604,null,null,"/","/","/",3661238002043,112.25,1230,1650,390,"C3"]
[100004927,"HABILLAGE AVANT  PK 350","MG3",116,null,null,"/","/","/",3661238109919,9.5,1010,820,120,"C3"]
[85537060,"COLIS CHASSIS 4ELTS","FD30",116,null,null,"/","/","/",3661238026247,13.5,760,180,100,"C3"]
[85537061,"COLIS CHASSIS 5ELTS","FD31",133,null,null,"/","/","/",3661238026230,16,750,190,100,"C3"]
[85537062,"COLIS CHASSIS 6ELTS","FD32",144,null,null,"/","/","/",3661238026223,18.5,760,190,110,"C3"]
[85537063,"COLIS CHASSIS 7ELTS","FD33",162,null,null,"/","/","/",3661238026216,20.5,900,210,120,"C3"]
[85537064,"COLIS CHASSIS 8ELTS","FD34",174,null,null,"/","/","/",3661238026209,23,1060,210,130,"C3"]
[85537065,"COLIS CHASSIS 9ELTS","FD35",231,null,null,"/","/","/",3661238026193,25,1220,210,140,"C3"]
[100013110,"COLIS DOCUMENT TECHNIQUE FR PU 354 CONDENS","MG30",44,null,null,"/","/","/",3661238362130,0.5,410,210,125,"C3"]
[100012638,"COLIS DOCUMENT TECHNIQUE FR PU 355 CONDENS","MG20",44,null,null,"/","/","/",3661238358997,0.5,410,210,125,"C3"]
[100012639,"COLIS DOCUMENT TECHNIQUE FR PU 356 CONDENS","MG21",44,null,null,"/","/","/",3661238359024,0.5,410,210,125,"C3"]
[100012650,"COLIS DOCUMENT TECHNIQUE FR PU 357 CONDENS","MG22",44,null,null,"/","/","/",3661238359031,0.5,410,210,125,"C3"]
[100012651,"COLIS DOCUMENT TECHNIQUE FR PU 358 CONDENS","MG23",44,null,null,"/","/","/",3661238359055,0.5,410,210,125,"C3"]
[100012652,"COLIS DOCUMENT TECHNIQUE FR PU 359 CONDENS","MG24",44,null,null,"/","/","/",3661238359062,0.5,410,210,125,"C3"]
[100004380,"TABLEAU STANDARD OERTLI","MG1",325,3.34,"11.14","/","/","/",3661238111332,5.0599999999999996,800,200,200,"C3"]
[100004381,"TABLEAU R OERTLI","MG2",501,3.34,"11.14","/","/","/",3661238111325,10.39,830,430,270,"C3"]
[100011882,"CONDENSEUR RCF 301","MD169",7625,null,null,"/","/","/",3661238350915,92.55,1360,720,1250,"C3"]
[100011883,"CONDENSEUR RCF 302","MD170",12827,null,null,"/","/","/",3661238350922,166.55,1360,720,1250,"C3"]
[100011802,"COLIS HYDRAULIQUE RCF301","MD171",511,null,null,"/","/","/",3661238351462,14.3,610,460,190,"C3"]
[100011803,"COLIS HYDRAULIQUE RCF302","MD172",532,null,null,"/","/","/",3661238351479,16.899999999999999,610,460,190,"C3"]
[100011804,"COLIS FUMEES RCF301","MD173",844,null,null,"/","/","/",3661238351486,4.05,410,410,430,"C3"]
[100011805,"COLIS FUMEES RCF302","MD174",1272,null,null,"/","/","/",3661238351493,10.5,860,520,520,"C3"]
[100012940,"BRULEUR OES 255 LZ-P",null,1842,null,null,"/","/","/",3661238551992,20,800,300,400,"C3"]
[100012942,"BRULEUR OES 351 LZ-P",null,1880,null,null,"/","/","/",3661238552005,25,780,370,420,"C3"]
[100012943,"BRULEUR OES 352 LZ-P",null,1954,null,null,"/","/","/",3661238552012,25,780,370,420,"C3"]
[100012944,"BRULEUR OES 353 LZ-P",null,2016,null,null,"/","/","/",3661238552029,25,780,370,420,"C3"]
[100012945,"BRULEUR OES 354 LZ-P",null,2093,null,null,"/","/","/",3661238552036,25,780,370,420,"C3"]
[100012946,"BRULEUR OES 355 LZ-P",null,2190,null,null,"/","/","/",3661238552043,33,780,370,420,"C3"]
[]
["OPTIONS "]
[100004295,"COLIS TABLEAU DIEMATIC M3 ","MD1",1976,null,null,"/","/","/",3661238004184,12,830,430,270,"C3"]
[100004296,"COLIS TABLEAU K3    ","MD2",1186,null,null,"/","/","/",3661238004177,12,830,430,270,"C3"]
[100012250,"SIPHON GTU C 330","MD217",423,null,null,"/","/","/",3661238357914,4,500,500,500,"C3"]
[100012251,"KIT RECIRCULATION GTU C 330","MD218",421,null,null,"/","/","/",3661238357921,17,660,490,300,"C3"]
[85537074,"KIT VANNE DE CHASSE","FD37",280,null,null,"/","/","/",3661238026100,6.5,410,290,170,"C0"]
[85537075,"JEU DE 2 CONTRE-BRIDE A EPAULEMENT, Ø 2\"","FD38",73,null,null,"/","/","/",3661238026094,2.79,195,150,125,"C0"]
[85537076,"KIT DE SECURITE 115kW","FD39",175,null,null,"/","/","/",3661238026087,2.41,425,255,120,"C0"]
[85537079,"KIT DE SECURITE 115 à 330 kW","FD42",243,null,null,"/","/","/",3661238026056,3.14,470,255,115,"C0"]
[88017858,"PROLONGATEUR BUS","AD139",23,0.02,95020,"/","/","/",3661238048812,0.05,210,150,20,"C0"]
[100004970,"COLIS CARTE RELAIS+SONDES POUR K3 ","AD220",323,null,null,null,null,null,3661238001893,0.7,310,210,130,"C0"]
[100012385,"STATION DE NEUTRALISATION (Jusqu'à 350 kW)","MD225",524,null,null,"/","/","/",3661238357938,32.9,550,370,440,"C3"]
[100012685,"COLIS RECHARGE STATION DE NEUTRALISATION","MD226",195,null,null,"/","/","/",3661238359703,24.5,510,360,240,"C3"]
[]
[null,"FAMILLE : CHAUDIERE FIOUL AU  SOL  BASSE TEMPERATURE"]
[]
[]
[7633545,"FSBX 22",null,{"$f":"D4090+D4092","v":3381},null,null,"B","/","/",3661238637986,{"$f":"K4090+K4092","v":204.9},null,null,null,"D6"]
[7633548,"FSBX 29",null,{"$f":"D4091+D4092","v":3534},null,null,"B","/","/",3661238637993,{"$f":"K4091+K4092","v":232.9},null,null,null,"D6"]
[7633551,"FSBR 22",null,{"$f":"D4090+D4093","v":3683},null,null,"B","/","/",3661238638020,{"$f":"K4090+K4093","v":204.9},null,null,null,"D6"]
[7633552,"FSBR 29",null,{"$f":"D4091+D4093","v":3836},null,null,"B","/","/",3661238638037,{"$f":"K4091+K4093","v":232.9},null,null,null,"D6"]
[]
["COMPOSANTS"]
[7624149,"FSB. 22  ","MY125",3229,5,14070,"/","/","/",3661238617353,204,1220,750,1050,"D6"]
[7624151,"FSB. 29  ","MY135",3382,5,14070,"/","/","/",3661238617377,232,1220,750,1050,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[]
[]
[7633555,"FVBX 22/EL110SL",null,{"$f":"D4100+D4101+D4102+D4103","v":4442},null,null,"B","B","XL",3661238638068,{"$f":"K4100+K4101+K4102+K4103","v":292.89999999999998},null,null,null,"D6"]
[7633556,"FVBR 22/EL110SL",null,{"$f":"D4100+D4101+D4102+D4104","v":4744},null,null,"B","B","XL",3661238638075,{"$f":"K4100+K4101+K4102+K4104","v":292.89999999999998},null,null,null,"D6"]
[]
["COMPOSANTS"]
[7624149,"FSB. 22  ","MY125",3229,5,14070,"/","/","/",3661238617353,{"$f":"K4090","v":204},1220,750,1050,"D6"]
[7609915,"BALLON EL110SL","ER590",758,null,null,"/","/","/",3661238608726,83,700,680,940,"D6"]
[7613103,"KIT DE LIAISON BALLON EL110SL","ER595",303,null,null,"/","/","/",3661238608115,5,860,250,135,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[null,null,null,null,null,null,null,null,null,""]
[]
[7633557,"FVBX 22/EL160SL",null,{"$f":"D4113+D4115+D4116+D4117","v":4773},null,null,"B","B","XL",3661238638082,{"$f":"K4113+K4115+K4116+K4117","v":307.89999999999998},null,null,null,"D6"]
[7633561,"FVBX 29/EL160SL",null,{"$f":"D4114+D4115+D4116+D4117","v":4926},null,null,"B","B","XL",3661238638099,{"$f":"K4114+K4115+K4116+K4117","v":335.9},null,null,null,"D6"]
[7633562,"FVBR 22/EL160SL",null,{"$f":"D4113+D4115+D4116+D4118","v":5075},null,null,"B","B","XL",3661238638105,{"$f":"K4113+K4115+K4116+K4118","v":307.89999999999998},null,null,null,"D6"]
[7633563,"FVBR 29/EL160SL",null,{"$f":"D4114+D4115+D4116+D4118","v":5228},null,null,"B","B","XL",3661238638112,{"$f":"K4114+K4115+K4116+K4118","v":335.9},null,null,null,"D6"]
[]
["COMPOSANTS"]
[7624149,"FSB. 22  ","MY125",3229,5,14070,"/","/","/",3661238617353,{"$f":"K4100","v":204},1220,750,1050,"D6"]
[7624151,"FSB. 29  ","MY135",3382,5,14070,"/","/","/",3661238617377,{"$f":"K4091","v":232},1220,750,1050,"D6"]
[7616405,"BALLON EL160SL","ER592",989,null,null,"/","/","/",3661238608696,98,700,680,1200,"D6"]
[7613082,"KIT DE LIAISON BALLON EL160SL","ER597",403,null,null,"/","/","/",3661238608139,5,860,250,135,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[]
[]
[7633564,"FSBX 22 P",null,{"$f":"D4127+D4129+D4130","v":3861},null,null,"B","/","/",3661238638129,{"$f":"K4127+K4129+K4130","v":219.9},null,null,null,"D6"]
[7633565,"FSBX 29 P",null,{"$f":"D4128+D4129+D4130","v":4014},null,null,"B","/","/",3661238638136,{"$f":"K4128+K4129+K4130","v":247.9},null,null,null,"D6"]
[7633566,"FSBR 22 P",null,{"$f":"D4127+D4129+D4131","v":4163},null,null,"B","/","/",3661238638143,{"$f":"K4127+K4129+K4131","v":219.9},null,null,null,"D6"]
[7633567,"FSBR 29 P",null,{"$f":"D4128+D4129+D4131","v":4316},null,null,"B","/","/",3661238638150,{"$f":"K4128+K4129+K4131","v":247.9},null,null,null,"D6"]
[]
["COMPOSANTS"]
[7624149,"FSB. 22  ","MY125",3229,5,14070,"/","/","/",3661238617353,{"$f":"K4113","v":204},1220,750,1050,"D6"]
[7624151,"FSB. 29  ","MY135",3382,5,14070,"/","/","/",3661238617377,{"$f":"K4114","v":232},1220,750,1050,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,15,675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[]
[]
[7633568,"FVBX 22 P/EL110SL",null,{"$f":"D4138+D4139+D4140+D4141+D4142","v":4841},null,null,"B","B","XL",3661238638174,{"$f":"K4138+K4139+K4140+K4141+K4142","v":306.79999999999995},null,null,null,"D6"]
[7633569,"FVBR 22 P/EL110SL",null,{"$f":"D4138+D4139+D4140+D4141+D4143","v":5143},null,null,"B","B","XL",3661238638167,{"$f":"K4138+K4139+K4140+K4141+K4143","v":306.79999999999995},null,null,null,"D6"]
[]
["COMPOSANTS"]
[7624149,"FSB. 22  ","MY125",3229,5,14070,"/","/","/",3661238617353,{"$f":"K4127","v":204},1220,750,1050,"D6"]
[7609915,"BALLON EL110SL","ER590",758,null,null,"/","/","/",3661238608726,83,700,680,940,"D6"]
[7614745,"KIT DE LIAISON BALLON EL110SL EQUIPEE","ER594",222,null,null,"/","/","/",3661238608122,3.9,870,260,160,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,{"$f":"K4129","v":15},675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[null,null,null,null,null,null,null,null,null,""]
[]
[7633570,"FVBX 22 P/EL160SL",null,{"$f":"D4152+D4154+D4155+D4156+D4157","v":5113},null,null,"B","B","XL",3661238638181,{"$f":"K4152+K4154+K4155+K4156+K4157","v":322.89999999999998},null,null,null,"D6"]
[7633571,"FVBX 29 P/EL160SL",null,{"$f":"D4153+D4154+D4155+D4156+D4157","v":5266},null,null,"B","B","XL",3661238638198,{"$f":"K4153+K4154+K4155+K4156+K4157","v":350.9},null,null,null,"D6"]
[7633572,"FVBR 22 P/EL160SL",null,{"$f":"D4152+D4154+D4155+D4156+D4158","v":5415},null,null,"B","B","XL",3661238638204,{"$f":"K4152+K4154+K4155+K4156+K4158","v":322.89999999999998},null,null,null,"D6"]
[7633573,"FVBR 29 P/EL160SL",null,{"$f":"D4153+D4154+D4155+D4156+D4158","v":5568},null,null,"B","B","XL",3661238638211,{"$f":"K4153+K4154+K4155+K4156+K4158","v":350.9},null,null,null,"D6"]
[]
["COMPOSANTS"]
[7624149,"FSB. 22  ","MY125",3229,5,14070,"/","/","/",3661238617353,{"$f":"K4138","v":204},1220,750,1050,"D6"]
[7624151,"FSB. 29  ","MY135",3382,5,14070,"/","/","/",3661238617377,{"$f":"K4128","v":232},1220,750,1050,"D6"]
[7616405,"BALLON EL160SL","ER592",989,null,null,"/","/","/",3661238608696,98,700,680,1200,"D6"]
[7614827,"KIT DE LIAISON BALLON EL160SL EQUIPEE","ER596",263,null,null,"/","/","/",3661238608146,5,860,250,135,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,{"$f":"K4141","v":15},675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[null,null,null,null,null,null,null,null,null,""]
[]
[7633574,"FSBX 22 F HOR",null,{"$f":"D4171+D4173+D4175","v":3799},null,null,"B","/","/",3661238638228,{"$f":"K4171+K4173+K4175","v":217.8},null,null,null,"D6"]
[7633575,"FSBX 22 F VER",null,{"$f":"D4171+D4173+D4176+D4177","v":3887},null,null,"B","/","/",3661238638235,{"$f":"K4171+K4173+K4176+K4177","v":220.70000000000002},null,null,null,"D6"]
[7633576,"FSBX 29 F HOR",null,{"$f":"D4172+D4173+D4175","v":3950},null,null,"B","/","/",3661238638242,{"$f":"K4172+K4173+K4175","v":245.8},null,null,null,"D6"]
[7633577,"FSBX 29 F VER",null,{"$f":"D4172+D4173+D4176+D4177","v":4038},null,null,"B","/","/",3661238638259,{"$f":"K4172+K4173+K4176+K4177","v":248.70000000000002},null,null,null,"D6"]
[7633578,"FSBR 22 F HOR",null,{"$f":"D4171+D4174+D4175","v":4101},null,null,"B","/","/",3661238638266,{"$f":"K4171+K4174+K4175","v":217.8},null,null,null,"D6"]
[7633579,"FSBR 22 F VER",null,{"$f":"D4171+D4174+D4176+D4177","v":4189},null,null,"B","/","/",3661238638273,{"$f":"K4171+K4174+K4176+K4177","v":220.70000000000002},null,null,null,"D6"]
[7633580,"FSBR 29 F HOR",null,{"$f":"D4172+D4174+D4175","v":4252},null,null,"B","/","/",3661238638280,{"$f":"K4172+K4174+K4175","v":245.8},null,null,null,"D6"]
[7633581,"FSBR 29 F VER",null,{"$f":"D4172+D4174+D4176+D4177","v":4340},null,null,"B","/","/",3661238638297,{"$f":"K4172+K4174+K4176+K4177","v":248.70000000000002},null,null,null,"D6"]
[]
["COMPOSANTS"]
[7627332,"FSB. 22 FF","MY122",3415,5,14070,"/","/","/",3661238630222,214,1220,750,1050,"D6"]
[7627333,"FSB. 29 FF","MY132",3566,5,14070,"/","/","/",3661238630239,242,1220,750,1050,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[81998533,"TERMINAL HORIZONTAL STANDARD","DB90",232,null,null,"/","/","/",3661238001329,2.9,1015,150,145,"C0"]
[81998534,"TERMINAL VERTICAL NOIR","DB91",206,null,null,"/","/","/",3661238001312,4.9000000000000004,1150,260,270,"C0"]
[81998539,"COUDE A 90 °","DB96",114,null,null,"/","/","/",3661238001268,0.9,325,240,150,"C0"]
[]
[]
[7633583,"FVBX 22 F HOR/EL110SL",null,{"$f":"D4186+D4187+D4188+D4189+D4191","v":4860},null,null,"B","B","XL",3661238638303,{"$f":"K4186+K4187+K4188+K4189+K4191","v":305.79999999999995},null,null,null,"D6"]
[7633584,"FVBX 22 F VER/EL110SL",null,{"$f":"D4186+D4187+D4188+D4189+D4192+D4193","v":4948},null,null,"B","B","XL",3661238638310,{"$f":"K4186+K4187+K4188+K4189+K4192+K4193","v":308.69999999999993},null,null,null,"D6"]
[7633585,"FVBR 22 F HOR/EL110SL",null,{"$f":"D4186+D4187+D4188+D4190+D4191","v":5162},null,null,"B","B","XL",3661238638327,{"$f":"K4186+K4187+K4188+K4190+K4191","v":305.79999999999995},null,null,null,"D6"]
[7633586,"FVBR 22 F VER/EL110SL",null,{"$f":"D4186+D4187+D4188+D4190+D4192+D4193","v":5250},null,null,"B","B","XL",3661238638334,{"$f":"K4186+K4187+K4188+K4190+K4192+K4193","v":308.69999999999993},null,null,null,"D6"]
[]
["COMPOSANTS"]
[7627332,"FSB. 22 FF","MY122",3415,5,14070,"/","/","/",3661238630222,{"$f":"K4171","v":214},1220,750,1050,"D6"]
[7609915,"BALLON EL110SL","ER590",758,null,null,"/","/","/",3661238608726,{"$f":"K4139","v":83},700,680,940,"D6"]
[7613103,"KIT DE LIAISON BALLON EL110SL","ER595",303,null,null,"/","/","/",3661238608115,{"$f":"K4102","v":5},860,250,135,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[81998533,"TERMINAL HORIZONTAL STANDARD","DB90",232,null,null,"/","/","/",3661238001329,2.9,1015,150,145,"C0"]
[81998534,"TERMINAL VERTICAL NOIR","DB91",206,null,null,"/","/","/",3661238001312,4.9000000000000004,1150,260,270,"C0"]
[81998539,"COUDE A 90 °","DB96",114,null,null,"/","/","/",3661238001268,0.9,325,240,150,"C0"]
[null,null,null,null,null,null,null,null,null,""]
[]
[7633587,"FVBX 22 F HOR/EL160SL",null,{"$f":"D4206+D4208+D4209+D4210+D4212","v":5191},null,null,"B","B","XL",3661238638341,{"$f":"K4206+K4208+K4209+K4210+K4212","v":320.79999999999995},null,null,null,"D6"]
[7633588,"FVBX 22 F VER/EL160SL",null,{"$f":"D4206+D4208+D4209+D4210+D4213+D4214","v":5279},null,null,"B","B","XL",3661238638358,{"$f":"K4206+K4208+K4209+K4210+K4213+K4214","v":323.69999999999993},null,null,null,"D6"]
[7633589,"FVBX 29 F HOR/EL160SL",null,{"$f":"D4207+D4208+D4209+D4210+D4212","v":5342},null,null,"B","B","XL",3661238638365,{"$f":"K4207+K4208+K4209+K4210+K4212","v":348.79999999999995},null,null,null,"D6"]
[7633590,"FVBX 29 F VER/EL160SL",null,{"$f":"D4207+D4208+D4209+D4210+D4213+D4214","v":5430},null,null,"B","B","XL",3661238638372,{"$f":"K4207+K4208+K4209+K4210+K4213+K4214","v":351.69999999999993},null,null,null,"D6"]
[7633591,"FVBR 22 F HOR/EL160SL",null,{"$f":"D4206+D4208+D4209+D4211+D4212","v":5493},null,null,"B","B","XL",3661238638389,{"$f":"K4206+K4208+K4209+K4211+K4212","v":320.79999999999995},null,null,null,"D6"]
[7633592,"FVBR 22 F VER/EL160SL",null,{"$f":"D4206+D4208+D4209+D4211+D4213+D4214","v":5581},null,null,"B","B","XL",3661238638396,{"$f":"K4206+K4208+K4209+K4211+K4213+K4214","v":323.69999999999993},null,null,null,"D6"]
[7633593,"FVBR 29 F HOR/EL160SL",null,{"$f":"D4207+D4208+D4209+D4211+D4212","v":5644},null,null,"B","B","XL",3661238638402,{"$f":"K4207+K4208+K4209+K4211+K4212","v":348.79999999999995},null,null,null,"D6"]
[7633594,"FVBR 29 F VER/EL160SL",null,{"$f":"D4207+D4208+D4209+D4211+D4213+D4214","v":5732},null,null,"B","B","XL",3661238638419,{"$f":"K4207+K4208+K4209+K4211+K4213+K4214","v":351.69999999999993},null,null,null,"D6"]
[]
["COMPOSANTS"]
[7627332,"FSB. 22 FF","MY122",3415,5,14070,"/","/","/",3661238630222,{"$f":"K4186","v":214},1220,750,1050,"D6"]
[7627333,"FSB. 29 FF","MY132",3566,5,14070,"/","/","/",3661238630239,{"$f":"K4172","v":242},1220,750,1050,"D6"]
[7616405,"BALLON EL160SL","ER592",989,null,null,"/","/","/",3661238608696,{"$f":"K4154","v":98},700,680,1200,"D6"]
[7613082,"KIT DE LIAISON BALLON EL160SL","ER597",403,null,null,"/","/","/",3661238608139,{"$f":"K4116","v":5},860,250,135,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[81998533,"TERMINAL HORIZONTAL STANDARD","DB90",232,null,null,"/","/","/",3661238001329,2.9,1015,150,145,"C0"]
[81998534,"TERMINAL VERTICAL NOIR","DB91",206,null,null,"/","/","/",3661238001312,4.9000000000000004,1150,260,270,"C0"]
[81998539,"COUDE A 90 °","DB96",114,null,null,"/","/","/",3661238001268,0.9,325,240,150,"C0"]
[]
[]
[7633600,"FSBX 22 PF HOR",null,{"$f":"D4227+D4229+D4230+D4232","v":4279},null,null,"B","/","/",3661238638914,{"$f":"K4227+K4229+K4230+K4232","v":232.8},null,null,null,"D6"]
[7633602,"FSBX 22 PF VER",null,{"$f":"D4227+D4229+D4230+D4233+D4234","v":4367},null,null,"B","/","/",3661238638921,{"$f":"K4227+K4229+K4230+K4233+K4234","v":235.70000000000002},null,null,null,"D6"]
[7633604,"FSBX 29 PF HOR",null,{"$f":"D4228+D4229+D4230+D4232","v":4430},null,null,"B","/","/",3661238638938,{"$f":"K4228+K4229+K4230+K4232","v":260.79999999999995},null,null,null,"D6"]
[7633605,"FSBX 29 PF VER",null,{"$f":"D4228+D4229+D4230+D4233+D4234","v":4518},null,null,"B","/","/",3661238638945,{"$f":"K4228+K4229+K4230+K4233+K4234","v":263.69999999999993},null,null,null,"D6"]
[7633606,"FSBR 22 PF HOR",null,{"$f":"D4227+D4229+D4231+D4232","v":4581},null,null,"B","/","/",3661238638952,{"$f":"K4227+K4229+K4231+K4232","v":232.8},null,null,null,"D6"]
[7633607,"FSBR 22 PF VER",null,{"$f":"D4227+D4229+D4231+D4233+D4234","v":4669},null,null,"B","/","/",3661238638969,{"$f":"K4227+K4229+K4231+K4233+K4234","v":235.70000000000002},null,null,null,"D6"]
[7633608,"FSBR 29 PF HOR",null,{"$f":"D4228+D4229+D4231+D4232","v":4732},null,null,"B","/","/",3661238638976,{"$f":"K4228+K4229+K4231+K4232","v":260.79999999999995},null,null,null,"D6"]
[7633609,"FSBR 29 PF VER",null,{"$f":"D4228+D4229+D4231+D4233+D4234","v":4820},null,null,"B","/","/",3661238638983,{"$f":"K4228+K4229+K4231+K4233+K4234","v":263.69999999999993},null,null,null,"D6"]
[]
["COMPOSANTS"]
[7627332,"FSB. 22 FF","MY122",3415,5,14070,"/","/","/",3661238630222,{"$f":"K4206","v":214},1220,750,1050,"D6"]
[7627333,"FSB. 29 FF","MY132",3566,5,14070,"/","/","/",3661238630239,{"$f":"K4207","v":242},1220,750,1050,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,{"$f":"K4156","v":15},675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[81998533,"TERMINAL HORIZONTAL STANDARD","DB90",232,null,null,"/","/","/",3661238001329,2.9,1015,150,145,"C0"]
[81998534,"TERMINAL VERTICAL NOIR","DB91",206,null,null,"/","/","/",3661238001312,4.9000000000000004,1150,260,270,"C0"]
[81998539,"COUDE A 90 °","DB96",114,null,null,"/","/","/",3661238001268,0.9,325,240,150,"C0"]
[]
[]
[7633610,"FVBX 22 PF HOR/EL110SL",null,{"$f":"D4243+D4244+D4245+D4246+D4247+D4249","v":5259},null,null,"B","B","XL",3661238638990,{"$f":"K4243+K4244+K4245+K4246+K4247+K4249","v":319.69999999999993},null,null,null,"D6"]
[7633611,"FVBX 22 PF VER/EL110SL",null,{"$f":"D4243+D4244+D4245+D4246+D4247+D4250+D4251","v":5347},null,null,"B","B","XL",3661238639003,{"$f":"K4243+K4244+K4245+K4246+K4247+K4250+K4251","v":322.59999999999991},null,null,null,"D6"]
[7633612,"FVBR 22 PF HOR/EL110SL",null,{"$f":"D4243+D4244+D4245+D4246+D4248+D4249","v":5561},null,null,"B","B","XL",3661238639010,{"$f":"K4243+K4244+K4245+K4246+K4248+K4249","v":319.69999999999993},null,null,null,"D6"]
[7633613,"FVBR 22 PF VER/EL110SL",null,{"$f":"D4243+D4244+D4245+D4246+D4248+D4250+D4251","v":5649},null,null,"B","B","XL",3661238639027,{"$f":"K4243+K4244+K4245+K4246+K4248+K4250+K4251","v":322.59999999999991},null,null,null,"D6"]
[]
["COMPOSANTS"]
[7627332,"FSB. 22 FF","MY122",3415,5,14070,"/","/","/",3661238630222,{"$f":"K4227","v":214},1220,750,1050,"D6"]
[7609915,"BALLON EL110SL","ER590",758,null,null,"/","/","/",3661238608726,{"$f":"K4187","v":83},700,680,940,"D6"]
[7614745,"KIT DE LIAISON BALLON EL110SL EQUIPEE","ER594",222,null,null,"/","/","/",3661238608122,3.9,870,260,160,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,{"$f":"K4229","v":15},675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[81998533,"TERMINAL HORIZONTAL STANDARD","DB90",232,null,null,"/","/","/",3661238001329,2.9,1015,150,145,"C0"]
[81998534,"TERMINAL VERTICAL NOIR","DB91",206,null,null,"/","/","/",3661238001312,4.9000000000000004,1150,260,270,"C0"]
[81998539,"COUDE A 90 °","DB96",114,null,null,"/","/","/",3661238001268,0.9,325,240,150,"C0"]
[null,null,null,null,null,null,null,null,null,""]
[]
[7633614,"FVBX 22 PF HOR/EL160SL",null,{"$f":"D4264+D4266+D4267+D4268+D4269+D4271","v":5531},null,null,"B","B","XL",3661238639034,{"$f":"K4264+K4266+K4267+K4268+K4269+K4271","v":335.79999999999995},null,null,null,"D6"]
[7633615,"FVBX 22 PF VER/EL160SL",null,{"$f":"D4264+D4266+D4267+D4268+D4269+D4272+D4273","v":5619},null,null,"B","B","XL",3661238639041,{"$f":"K4264+K4266+K4267+K4268+K4269+K4272+K4273","v":338.69999999999993},null,null,null,"D6"]
[7633616,"FVBX 29 PF HOR/EL160SL",null,{"$f":"D4265+D4266+D4267+D4268+D4269+D4271","v":5682},null,null,"B","B","XL",3661238639058,{"$f":"K4265+K4266+K4267+K4268+K4269+K4271","v":363.79999999999995},null,null,null,"D6"]
[7633617,"FVBX 29 PF VER/EL160SL",null,{"$f":"D4265+D4266+D4267+D4268+D4269+D4272+D4273","v":5770},null,null,"B","B","XL",3661238639072,{"$f":"K4265+K4266+K4267+K4268+K4269+K4272+K4273","v":366.69999999999993},null,null,null,"D6"]
[7633618,"FVBR 22 PF HOR/EL160SL",null,{"$f":"D4264+D4266+D4267+D4268+D4270+D4271","v":5833},null,null,"B","B","XL",3661238639089,{"$f":"K4264+K4266+K4267+K4268+K4270+K4271","v":335.79999999999995},null,null,null,"D6"]
[7633619,"FVBR 22 PF VER/EL160SL",null,{"$f":"D4264+D4266+D4267+D4268+D4270+D4272+D4273","v":5921},null,null,"B","B","XL",3661238639096,{"$f":"K4264+K4266+K4267+K4268+K4270+K4272+K4273","v":338.69999999999993},null,null,null,"D6"]
[7633620,"FVBR 29 PF HOR/EL160SL",null,{"$f":"D4265+D4266+D4267+D4268+D4270+D4271","v":5984},null,null,"B","B","XL",3661238639102,{"$f":"K4265+K4266+K4267+K4268+K4270+K4271","v":363.79999999999995},null,null,null,"D6"]
[7633621,"FVBR 29 PF VER/EL160SL",null,{"$f":"D4265+D4266+D4267+D4268+D4270+D4272+D4273","v":6072},null,null,"B","B","XL",3661238639119,{"$f":"K4265+K4266+K4267+K4268+K4270+K4272+K4273","v":366.69999999999993},null,null,null,"D6"]
[]
["COMPOSANTS"]
[7627332,"FSB. 22 FF","MY122",3415,5,14070,"/","/","/",3661238630222,{"$f":"K4243","v":214},1220,750,1050,"D6"]
[7627333,"FSB. 29 FF","MY132",3566,5,14070,"/","/","/",3661238630239,{"$f":"K4228","v":242},1220,750,1050,"D6"]
[7616405,"BALLON EL160SL","ER592",989,null,null,"/","/","/",3661238608696,{"$f":"K4208","v":98},700,680,1200,"D6"]
[7614827,"KIT DE LIAISON BALLON EL160SL EQUIPEE","ER596",263,null,null,"/","/","/",3661238608146,{"$f":"K4155","v":5},860,250,135,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,{"$f":"K4246","v":15},675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[81998533,"TERMINAL HORIZONTAL STANDARD","DB90",232,null,null,"/","/","/",3661238001329,2.9,1015,150,145,"C0"]
[81998534,"TERMINAL VERTICAL NOIR","DB91",206,null,null,"/","/","/",3661238001312,4.9000000000000004,1150,260,270,"C0"]
[81998539,"COUDE A 90 °","DB96",114,null,null,"/","/","/",3661238001268,0.9,325,240,150,"C0"]
[null,null,null,null,null,null,null,null,null,""]
[]
[7633623,"FSX 22",null,{"$f":"D4282+D4284","v":2272},null,null,"Pas concerné par l'étiquettage",null,null,3661238639126,{"$f":"K4282+K4284","v":194.9},null,null,null,"D6"]
[7633624,"FSX 29",null,{"$f":"D4283+D4284","v":2434},null,null,"Pas concerné par l'étiquettage",null,null,3661238639133,{"$f":"K4283+K4284","v":222.9},null,null,null,"D6"]
[7633627,"FSR 22",null,{"$f":"D4282+D4285","v":2574},null,null,"Pas concerné par l'étiquettage",null,null,3661238639232,{"$f":"K4282+K4285","v":194.9},null,null,null,"D6"]
[7633628,"FSR 29",null,{"$f":"D4283+D4285","v":2736},null,null,"Pas concerné par l'étiquettage",null,null,3661238639249,{"$f":"K4283+K4285","v":222.9},null,null,null,"D6"]
[]
["COMPOSANTS"]
[7624147,"FS. 22","MY130",2120,5,14070,"/","/","/",3661238617360,194,1220,750,1050,"D6"]
[7624152,"FS. 29","MY140",2282,5,14070,"/","/","/",3661238617384,222,1220,750,1050,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[]
[]
[7633631,"FVX 22/EL110SL",null,{"$f":"D4292+D4293+D4294+D4295","v":3333},null,null,"Pas concerné par l'étiquettage",null,null,3661238639270,{"$f":"K4292+K4293+K4294+K4295","v":282.89999999999998},null,null,null,"D6"]
[7633632,"FVR 22/EL110SL",null,{"$f":"D4292+D4293+D4294+D4296","v":3635},null,null,"Pas concerné par l'étiquettage",null,null,3661238639287,{"$f":"K4292+K4293+K4294+K4296","v":282.89999999999998},null,null,null,"D6"]
[]
["COMPOSANTS"]
[7624147,"FS. 22","MY130",2120,5,14070,"/","/","/",3661238617360,{"$f":"K4282","v":194},1220,750,1050,"D6"]
[7609915,"BALLON EL110SL","ER590",758,null,null,"/","/","/",3661238608726,{"$f":"K4101","v":83},700,680,940,"D6"]
[7613103,"KIT DE LIAISON BALLON EL110SL","ER595",303,null,null,"/","/","/",3661238608115,{"$f":"K4102","v":5},860,250,135,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[null,null,null,null,null,null,null,null,null,""]
[]
[7633633,"FVX 22/EL160SL",null,{"$f":"D4305+D4307+D4308+D4309","v":3664},null,null,"Pas concerné par l'étiquettage",null,null,3661238639294,{"$f":"K4305+K4307+K4308+K4309","v":297.89999999999998},null,null,null,"D6"]
[7633634,"FVX 29/EL160SL",null,{"$f":"D4306+D4307+D4308+D4309","v":3826},null,null,"Pas concerné par l'étiquettage",null,null,3661238639300,{"$f":"K4306+K4307+K4308+K4309","v":325.89999999999998},null,null,null,"D6"]
[7633635,"FVR 22/EL160SL",null,{"$f":"D4305+D4307+D4308+D4310","v":3966},null,null,"Pas concerné par l'étiquettage",null,null,3661238639317,{"$f":"K4305+K4307+K4308+K4310","v":297.89999999999998},null,null,null,"D6"]
[7633636,"FVR 29/EL160SL",null,{"$f":"D4306+D4307+D4308+D4310","v":4128},null,null,"Pas concerné par l'étiquettage",null,null,3661238639324,{"$f":"K4306+K4307+K4308+K4310","v":325.89999999999998},null,null,null,"D6"]
[]
["COMPOSANTS"]
[7624147,"FS. 22","MY130",2120,5,14070,"/","/","/",3661238617360,{"$f":"K4292","v":194},1220,750,1050,"D6"]
[7624152,"FS. 29","MY140",2282,5,14070,"/","/","/",3661238617384,{"$f":"K4283","v":222},1220,750,1050,"D6"]
[7616405,"BALLON EL160SL","ER592",989,null,null,"/","/","/",3661238608696,{"$f":"K4115","v":98},700,680,1200,"D6"]
[7613082,"KIT DE LIAISON BALLON EL160SL","ER597",403,null,null,"/","/","/",3661238608139,{"$f":"K4116","v":5},860,250,135,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[]
[]
[7633637,"FSX 22 P",null,{"$f":"D4319+D4321+D4322","v":2752},null,null,"Pas concerné par l'étiquettage",null,null,3661238639331,{"$f":"K4319+K4321+K4322","v":209.9},null,null,null,"D6"]
[7633638,"FSX 29 P",null,{"$f":"D4320+D4321+D4322","v":2914},null,null,"Pas concerné par l'étiquettage",null,null,3661238639348,{"$f":"K4320+K4321+K4322","v":237.9},null,null,null,"D6"]
[7633639,"FSR 22 P",null,{"$f":"D4319+D4321+D4323","v":3054},null,null,"Pas concerné par l'étiquettage",null,null,3661238639355,{"$f":"K4319+K4321+K4323","v":209.9},null,null,null,"D6"]
[7633640,"FSR 29 P",null,{"$f":"D4320+D4321+D4323","v":3216},null,null,"Pas concerné par l'étiquettage",null,null,3661238639362,{"$f":"K4320+K4321+K4323","v":237.9},null,null,null,"D6"]
[]
["COMPOSANTS"]
[7624147,"FS. 22","MY130",2120,5,14070,"/","/","/",3661238617360,{"$f":"K4305","v":194},1220,750,1050,"D6"]
[7624152,"FS. 29","MY140",2282,5,14070,"/","/","/",3661238617384,{"$f":"K4306","v":222},1220,750,1050,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,{"$f":"K4268","v":15},675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[]
[]
[7633641,"FVX 22 P/EL110SL",null,{"$f":"D4330+D4331+D4332+D4333+D4334","v":3732},null,null,"Pas concerné par l'étiquettage",null,null,3661238639379,{"$f":"K4330+K4331+K4332+K4333+K4334","v":296.79999999999995},null,null,null,"D6"]
[7633642,"FVR 22 P/EL110SL",null,{"$f":"D4330+D4331+D4332+D4333+D4335","v":4034},null,null,"Pas concerné par l'étiquettage",null,null,3661238639393,{"$f":"K4330+K4331+K4332+K4333+K4335","v":296.79999999999995},null,null,null,"D6"]
[]
["COMPOSANTS"]
[7624147,"FS. 22","MY130",2120,5,14070,"/","/","/",3661238617360,{"$f":"K4319","v":194},1220,750,1050,"D6"]
[7609915,"BALLON EL110SL","ER590",758,null,null,"/","/","/",3661238608726,{"$f":"K4139","v":83},700,680,940,"D6"]
[7614745,"KIT DE LIAISON BALLON EL110SL EQUIPEE","ER594",222,null,null,"/","/","/",3661238608122,{"$f":"K4140","v":3.9},870,260,160,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,{"$f":"K4321","v":15},675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[null,null,null,null,""]
[]
[7633643,"FVX 22 P/EL160SL",null,{"$f":"D4344+D4346+D4347+D4348+D4349","v":4004},null,null,"Pas concerné par l'étiquettage",null,null,3661238639409,{"$f":"K4344+K4346+K4347+K4348+K4349","v":312.89999999999998},null,null,null,"D6"]
[7633644,"FVX 29 P/EL160SL",null,{"$f":"D4345+D4346+D4347+D4348+D4349","v":4166},null,null,"Pas concerné par l'étiquettage",null,null,3661238639416,{"$f":"K4345+K4346+K4347+K4348+K4349","v":340.9},null,null,null,"D6"]
[7633645,"FVR 22 P/EL160SL",null,{"$f":"D4344+D4346+D4347+D4348+D4350","v":4306},null,null,"Pas concerné par l'étiquettage",null,null,3661238639423,{"$f":"K4344+K4346+K4347+K4348+K4350","v":312.89999999999998},null,null,null,"D6"]
[7633646,"FVR 29 P/EL160SL",null,{"$f":"D4345+D4346+D4347+D4348+D4350","v":4468},null,null,"Pas concerné par l'étiquettage",null,null,3661238639430,{"$f":"K4345+K4346+K4347+K4348+K4350","v":340.9},null,null,null,"D6"]
[]
["COMPOSANTS"]
[7624147,"FS. 22","MY130",2120,5,14070,"/","/","/",3661238617360,{"$f":"K4330","v":194},1220,750,1050,"D6"]
[7624152,"FS. 29","MY140",2282,5,14070,"/","/","/",3661238617384,{"$f":"K4320","v":222},1220,750,1050,"D6"]
[7616405,"BALLON EL160SL","ER592",989,null,null,"/","/","/",3661238608696,{"$f":"K4266","v":98},700,680,1200,"D6"]
[7614827,"KIT DE LIAISON BALLON EL160SL EQUIPEE","ER596",263,null,null,"/","/","/",3661238608146,{"$f":"K4267","v":5},860,250,135,"D6"]
[7616272,"KIT EQUIPEMENT HYDRAULIQUE","MY404",480,0.83,14050,"/","/","/",3661238603097,{"$f":"K4333","v":15},675,485,180,"D6"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[null,null,null,null,null,null,null,null,null,""]
["OPTIONS FS./FSB."]
["OPTIONS POUR TABLEAU X OETROCOM 1 "]
[85757741,"SONDE EXTERIEURE","FM46",41,0.02,95020,"/","/","/",3661238022751,0.1,200,150,40,"C0"]
[88017904,"THERMOSTAT AMBIANCE PROGRAMMABLE","AD191",161,0.12,95010,"/","/","/",3661238102415,0.2,130,90,55,"C0"]
[88017010,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (SANS FILS)","AD192",286,0.12,95010,"/","/","/",3661238102439,0.4,175,150,90,"C0"]
[7609765,"THERMOSTAT D'AMBIANCE MODULANT FILAIRE RS200 -3","AD306",206,0.12,95010,"/","/","/",8713809266462,0.4,148,100,52,"C0"]
[7609764,"THERMOSTAT D'AMBIANCE MODULANT RADIO RS200 -3R","AD305",340,0.12,95010,"/","/","/",8713809266455,0.8,150,110,110,"C0"]
[]
["OPTIONS POUR TABLEAU R OETROCOM 2"]
[85757741,"SONDE EXTERIEURE","FM46",41,0.02,95020,"/","/","/",3661238022751,0.1,200,150,40,"C0"]
[7616602,"PLATINE + SONDE POUR 1 CIRCUIT AVEC VANNE MELANGEUSE","MY420",260,0.12,95010,"/","/","/",3661238625747,0.5,305,215,100,"D6"]
[88017904,"THERMOSTAT AMBIANCE PROGRAMMABLE","AD191",161,0.12,95010,"/","/","/",3661238102415,0.2,130,90,55,"C0"]
[88017010,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (SANS FILS)","AD192",286,0.12,95010,"/","/","/",3661238102439,0.4,175,150,90,"C0"]
[7609765,"THERMOSTAT D'AMBIANCE MODULANT FILAIRE RS200 -3","AD306",206,0.12,95010,"/","/","/",8713809266462,0.4,148,100,52,"C0"]
[7609764,"THERMOSTAT D'AMBIANCE MODULANT RADIO RS200 -3R","AD305",340,0.12,95010,"/","/","/",8713809266455,0.8,150,110,110,"C0"]
[]
["OPTIONS ECS"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.2,200,150,30,"C0"]
[7622082,"KIT ACI","MY417",124,null,null,"/","/","/",3661238614031,0.5,250,150,100,"C6"]
[7619012,"TESTEUR D'ANODE MAGNESIUM","MY408",62,null,null,"/","/","/",3661238608818,0.5,185,130,105,"D6"]
[]
["OPTIONS CHAUDIERE",null,null,null,null,null,null,null,null,""]
[100012500,"FILTRE DEGAZEUR TIGERLOOP COMBI",null,135,null,null,"/","/","/",null,null,null,null,null,"C0"]
[100020045,"KIT FILTRE FERNOX TF1",null,258,null,null,"/","/","/",null,null,null,null,null,"C0"]
[]
["MODULES HYDRAULIQUES",null,null,null,null,null,null,null,null,""]
[7627062,"TUBULURES DE LIAISON CHAUDIERE / MODULES DROITE FS./FSB.","MY423",171,null,null,"/","/","/",3661238625730,5.5,615,205,205,"D6"]
[7627192,"TUBULURES DE LIAISON CHAUDIERE / MODULES GAUCHE  FS./FSB.","MY424",171,null,null,"/","/","/",3661238625716,5.5,615,205,205,"D6"]
[7627199,"OPTION 2 FLEXIBLES MONTAGE MURAL ","MY425",166,null,null,"/","/","/",3661238625723,6,860,250,135,"D6"]
[7627079,"KIT DE SECURITE POUR  FS./FSB./FSC.","MY427",129,null,null,"/","/","/",3661238627079,1.6,400,200,100,"D6"]
[100020164,"COLLECTEUR 2/3 CIRCUITS","EA140",348,null,null,"/","/","/",3661238575011,6.6,660,180,200,"C0"]
[100020167,"CIRCUIT DIRECT P.ELEC HEE","EA143",644,0.83,14050,"/","/","/",3661238575042,5.0999999999999996,460,270,235,"C0"]
[100020168,"CIRCUIT V3V P.ELEC HEE","EA144",916,0.83,14050,"/","/","/",3661238575059,6,460,270,235,"C0"]
[100020165,"CONSOLE MUR COLLECTEUR","EA141",44,null,null,"/","/","/",3661238575028,1.2,220,125,70,"C0"]
[100020166,"CONSOLE MUR 1 MODULE","EA142",116,null,null,"/","/","/",3661238575035,1.6,220,125,70,"C0"]
[7629813,"TUB CHAUDIERE/MODULE DROITE EF/EFU ","MY460",171,null,null,"/","/","/",3661238627734,3.5,615,205,205,"D6"]
[7629826,"KIT DE SECURITE  EF/EFU/EFU C  ","MY480",129,null,null,"/","/","/",3661238627086,1,400,200,100,"D6"]
[]
["OPTIONS FSB. F"]
[81998533,"TERMINAL HORIZONTAL STANDARD","DB90",232,null,null,"/","/","/",3661238001329,2.9,1015,150,145,"C0"]
[81998544,"TERMINAL HORIZONTAL LONG","DB87",208,null,null,"/","/","/",3661238001220,3.5,1200,150,150,"C0"]
[81998545,"CARTOUCHE SILENCIEUX POUR TERMINAL HORIZONTAL","DB88",104,null,null,"/","/","/",3661238001213,0.7,325,145,145,"C0"]
[81998548,"MANCHON DE VISITE LG= 0.25 M","DB85",157,null,null,"/","/","/",3661238001206,1,320,150,145,"C0"]
[81998549,"COUDE DE VISITE 90°","DB86",227,null,null,"/","/","/",3661238001190,1,320,240,150,"C0"]
[81998534,"TERMINAL VERTICAL NOIR","DB91",206,null,null,"/","/","/",3661238001312,4.9000000000000004,1150,260,270,"C0"]
[81998543,"TERMINAL VERTICAL ROUGE","DB89",200,null,null,"/","/","/",3661238001237,4.8,1145,265,270,"C0"]
[81998535,"RALLONGE LG 1 M","DB92",114,null,null,"/","/","/",3661238001305,2.5,1025,145,145,"C0"]
[81998536,"RALLONGE LG 0.5 M","DB93",80,null,null,"/","/","/",3661238001299,1.3,525,150,150,"C0"]
[81998537,"RALLONGE LG 0.25 M","DB94",72,null,null,"/","/","/",3661238001282,0.8,325,150,150,"C0"]
[81998538,"MANCHON DE COMPENSATION DE 0.39 A 0.64 M","DB95",178,null,null,"/","/","/",3661238001275,1.8,520,145,150,"C0"]
[81998539,"COUDE A 90 °","DB96",114,null,null,"/","/","/",3661238001268,0.9,325,240,150,"C0"]
[81998540,"JEU DE 2 COUDES A 45 °","DB97",171,null,null,"/","/","/",3661238001251,1.1000000000000001,325,240,150,"C0"]
[81998542,"PANIER DE PROTECTION EN INOX","DB99",134,null,null,"/","/","/",3661238001244,1.6,335,330,390,"C0"]
[]
[84837731,"EMBASE D'ETANCHEITE POUR TOIT PLAT","CX51",43,null,null,"/","/","/",3661238014343,0.6,400,400,155,"C0"]
[84837121,"TUILE A DOUILLE 5 A 25° NOIRE","CX121",112,null,null,"/","/","/",3661238014428,3,510,250,145,"C0"]
[84837732,"TUILE A DOUILLE 25 A 45° NOIRE","CX52",77,null,null,"/","/","/",3661238014336,3,520,250,145,"C0"]
[84837734,"TUILE A DOUILLE 35 A 55° NOIRE","CX63",97,null,null,"/","/","/",3661238014312,3.2,510,265,180,"C0"]
[84837120,"TUILE A DOUILLE 5 A 25° ROUGE","CX120",112,null,null,"/","/","/",3661238014435,3,515,245,145,"C0"]
[84837783,"TUILE A DOUILLE 25 A 45° ROUGE","CX83",77,null,null,"/","/","/",3661238014213,3,515,250,150,"C0"]
[84837784,"TUILE A DOUILLE 35 A 55° ROUGE","CX84",97,null,null,"/","/","/",3661238014206,3,520,265,180,"C0"]
[84837729,"SORTIE DE TOIT EN PENTE DE 40° A 60° ( uniquement pour tuiles mécaniques)","CX49",178,null,null,"/","/","/",3661238014367,3.5,920,700,320,"C0"]
[84837779,"COLLIER DE FIXATION Ø 125 MM PATTE LONGUE","CX79",15,null,null,"/","/","/",3661238014237,0.4,230,160,200,"C0"]
[]
[]
[]
[7633549,"FSBX 36",null,{"$f":"D4424+D4427","v":3886},null,null,"B","/","/",3661238638006,241.9,null,null,null,"D6"]
[7633550,"FSBX 46",null,{"$f":"D4425+D4427","v":4390},null,null,"B","/","/",3661238638013,269.89999999999998,null,null,null,"D6"]
[7633553,"FSBR 36",null,{"$f":"D4424+D4428","v":4188},null,null,"B","/","/",3661238638044,241.9,null,null,null,"D6"]
[7633554,"FSBR 46",null,{"$f":"D4425+D4428","v":4692},null,null,"B","/","/",3661238638051,269.89999999999998,null,null,null,"D6"]
[]
["COMPOSANTS"]
[7624155,"FSB. 36   ","MY145",3734,5,14070,"/","/","/",3661238617391,241,1425,750,1060,"D6"]
[7624866,"FSB. 46 *","MY154",4238,5,14070,"/","/","/",3661238643321,269,1200,1200,1315,"D6"]
[null,"* JAQUETTE ET BRULEUR A MONTER"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[]
[]
[7633625,"FSX 36",null,{"$f":"D4437+D4440","v":2684},null,null,"/","/","/",3661238639218,null,null,null,null,"D6"]
[7633626,"FSX 46",null,{"$f":"D4438+D4440","v":3048},null,null,"/","/","/",3661238639225,null,null,null,null,"D6"]
[7633629,"FSR 36",null,{"$f":"D4437+D4441","v":2986},null,null,"/","/","/",3661238639256,null,null,null,null,"D6"]
[7633630,"FSR 46",null,{"$f":"D4438+D4441","v":3350},null,null,"/","/","/",3661238639263,null,null,null,null,"D6"]
[]
["COMPOSANTS"]
[7624159,"FS. 36","MY150",2532,5,14070,"/","/","/",3661238617407,250,1425,750,1060,"D6"]
[7624876,"FS. 46 *","MY158",2896,5,14070,"/","/","/",3661238643338,275,1200,1200,null,"D6"]
[null,"* JAQUETTE A MONTER",null,null,null,null,"/","/","/"]
[7605717,"TABLEAU X OETROCOM 1 ","MY409",152,null,null,"/","/","/",3661238616264,0.9,400,200,100,"D6"]
[7605715,"TABLEAU R OETROCOM 2","MY410",454,null,null,"/","/","/",3661238616271,0.9,400,200,100,"D6"]
[]
["OPTIONS ECS"]
[7639559,"KIT DE LIAISON FS/FSB/FSC - BALLON INDEPENDANT OBLC/OBPB","ER598",489,null,null,"/","/","/",3661238641679,7,600,500,135,"D6"]
[]
["FUMISTERIE"]
[null,"PPS Ø 110 mm"]
[84887577,"KIT DE RACCORDEMENT CHEMINEE PPS Ø 110 mm","DY177",258,null,null,"/","/","/",3661238013223,2.68,395,300,510,"C0"]
[84887578,"TUYAU PPS Ø 110 mm LG = 1950 mm (GRIS)","DY178",72,null,null,"/","/","/",3661238013216,2.46,1960,150,150,"C0"]
[84887579,"TUYAU PPS Ø 110 mm LG = 1000 mm (GRIS)","DY179",41,null,null,"/","/","/",3661238013209,1.24,1015,130,140,"C0"]
[84887580,"TUYAU PPS Ø 110 mm LG = 500 mm (GRIS)","DY180",31,null,null,"/","/","/",3661238013193,0.62,515,135,140,"C0"]
[84887581,"COUDE PPS 87° Ø 110 mm (GRIS)","DY181",36,null,null,"/","/","/",3661238013186,0.33,255,190,150,"C0"]
[84887582,"COUDE PPS 45° Ø 110 mm (GRIS)","DY182",48,null,null,"/","/","/",3661238013179,0.52,295,215,165,"C0"]
[84887583,"T DE REVISION Ø 110 mm (GRIS)","DY183",48,null,null,"/","/","/",3661238013162,0.46,300,150,150,"C0"]
[84887587,"ETOILE DE CENTRAGE PPS  Ø 110 mm (2 PIECES)","DY187",15,null,null,"/","/","/",3661238013124,0.1,300,300,30,"C0"]
[84887588,"COUDE DE REVISION PPS 87° Ø 110 mm (GRIS)","DY188",72,null,null,"/","/","/",3661238013117,0.52,315,235,150,"C0"]
[84887772,"PLAQUE DE FINITION","DY772",58,null,null,"/","/","/",3661238011458,0.49,310,230,145,"C0"]
[84887773,"FOURREAU Ø165mm L 500mm","DY773",41,null,null,"/","/","/",3661238011441,1.23,515,165,170,"C3"]
[84887435,"GRILLE D'AERATION EXTERIEURE 250 X 300 mm","DY35",24,null,null,"/","/","/",3661238013889,0.35,300,250,30,"C0"]
[100015325,"KIT N° 1 RACCORDEMENT CHEMINÉE FLEXIBLE PPS Ø 80 mm","DY895",236,null,null,"/","/","/",3661238380110,2.87,395,395,380,"C0"]
[100015327,"TUBE FLEXIBLE LG=12,5M","DY897",354,null,null,"/","/","/",3661238380134,8.6999999999999993,1200,1220,250,"C0"]
[100015326,"TUBE FLEXIBLE LG=50M","DY896",1242,null,null,"/","/","/",3661238380127,35,1600,1660,410,"C0"]
[84887618,"ETOILE DE CENTRAGE POUR FLEXIBLE Ø 80  mm (2 PIÈCES)","DY618",37,null,null,"/","/","/",3661238012912,0.2,300,300,70,"C0"]
[100015328,"PIÈCE DE COUPLAGE FLEXIBLE Ø 80 mm","DY898",71,null,null,"/","/","/",3661238380141,0.25,150,150,150,"C0"]
[100015331,"OUTIL D'AIDE À L'INSERTION Ø 80 mm","DY901",177,null,null,"/","/","/",3661238380172,1.4,300,210,185,"C0"]
[100015330,"PIÈCE D'INSPECTION POUR TUBE FLEXIBLE","DY900",127,null,null,"/","/","/",3661238380165,0.5,295,140,140,"C0"]
[100015329,"TERMINAL AVEC SOLIN FLEX. Ø 80 mm","DY899",177,null,null,"/","/","/",3661238380158,1.74,385,385,250,"C0"]
[]
[]
[100005999,"DK 28/100-2","FS3",2111,5,14070,"Pas concerné par l'étiquettage",null,null,3661238109421,180,750,670,1650,"D0"]
[100006000,"DK 35/150-2 ","FS4",2845,5,14070,"Pas concerné par l'étiquettage",null,null,3661238109414,230,850,790,1700,"D0"]
[]
["OPTIONS"]
[100005977,"KIT DE RACCORDEMENT CHAUFFAGE","FL13",496,null,null,"/","/","/",3661238109438,14,560,440,315,"D0"]
[85287002,"KIT DE RACCORDEMENT SANITAIRE","FL11",198,null,null,"/","/","/",3661238028708,1.9,310,210,130,"D0"]
[88017904,"THERMOSTAT AMBIANCE PROGRAMMABLE","AD191",161,0.12,95010,"/","/","/",3661238102415,0.25,135,90,55,"C0"]
[88017010,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (SANS FILS)","AD192",286,0.12,95010,"/","/","/",3661238102439,0.42499999999999999,180,150,90,"C0"]
[]
[]
[100004396,"PKX 264 CORPS MONTE",null,3638,null,null,"Pas concerné par l'étiquettage",null,null,3661238111318,null,null,null,null,"C0"]
[100004397,"PKX 265 CORPS MONTE",null,4216,null,null,"Pas concerné par l'étiquettage",null,null,3661238111301,null,null,null,null,"C0"]
[100004398,"PKX 266 CORPS MONTE",null,4572,null,null,"Pas concerné par l'étiquettage",null,null,3661238111295,null,null,null,null,"C0"]
[100004399,"PKX 267 CORPS MONTE",null,4875,null,null,"Pas concerné par l'étiquettage",null,null,3661238111288,null,null,null,null,"C0"]
[100004400,"PKX 268 CORPS MONTE",null,5185,null,null,"Pas concerné par l'étiquettage",null,null,3661238111271,null,null,null,null,"C0"]
[100004401,"PKX2 266 CORPS MONTE",null,4682,null,null,"Pas concerné par l'étiquettage",null,null,3661238111264,null,null,null,null,"C0"]
[100004402,"PKX2 267 CORPS MONTE",null,4985,null,null,"Pas concerné par l'étiquettage",null,null,3661238111257,null,null,null,null,"C0"]
[100004403,"PKX2 268 CORPS MONTE",null,5295,null,null,"Pas concerné par l'étiquettage",null,null,3661238111240,null,null,null,null,"C0"]
[100004404,"PKR 264 CORPS MONTE",null,4316,null,null,"Pas concerné par l'étiquettage",null,null,3661238111233,null,null,null,null,"C0"]
[100004405,"PKR 265 CORPS MONTE",null,4894,null,null,"Pas concerné par l'étiquettage",null,null,3661238111226,null,null,null,null,"C0"]
[100004406,"PKR 266 CORPS MONTE",null,5250,null,null,"Pas concerné par l'étiquettage",null,null,3661238111219,null,null,null,null,"C0"]
[100004407,"PKR 267 CORPS MONTE",null,5553,null,null,"Pas concerné par l'étiquettage",null,null,3661238111202,null,null,null,null,"C0"]
[100004408,"PKR 268 CORPS MONTE",null,5863,null,null,"Pas concerné par l'étiquettage",null,null,3661238111196,null,null,null,null,"C0"]
[100004409,"PKR 266 + AD217  CORPS MONTE",null,5544,null,null,"Pas concerné par l'étiquettage",null,null,3661238111189,null,null,null,null,"C0"]
[100004410,"PKR 267 + AD217  CORPS MONTE",null,5847,null,null,"Pas concerné par l'étiquettage",null,null,3661238111172,null,null,null,null,"C0"]
[100004411,"PKR 268 + AD217  CORPS MONTE",null,6157,null,null,"Pas concerné par l'étiquettage",null,null,3661238111165,null,null,null,null,"C0"]
[100004416,"PKX 264 CORPS MONTE + OBC 162 /TA",null,5767,null,null,"Pas concerné par l'étiquettage",null,null,3661238111158,null,null,null,null,"C0"]
[100004418,"PKX 265 CORPS MONTE + OBC 162 /TA",null,6345,null,null,"Pas concerné par l'étiquettage",null,null,3661238111141,null,null,null,null,"C0"]
[100004419,"PKX 264 CORPS MONTE + OBC 252 /TA",null,6110,null,null,"Pas concerné par l'étiquettage",null,null,3661238111134,null,null,null,null,"C0"]
[100004421,"PKX 265 CORPS MONTE + OBC 252 /TA",null,6688,null,null,"Pas concerné par l'étiquettage",null,null,3661238111127,null,null,null,null,"C0"]
[100004422,"PKR 264 CORPS MONTE + OBC 162 /TA",null,6445,null,null,"Pas concerné par l'étiquettage",null,null,3661238111110,null,null,null,null,"C0"]
[100004423,"PKR 265 CORPS MONTE + OBC 162 /TA",null,7023,null,null,"Pas concerné par l'étiquettage",null,null,3661238111103,null,null,null,null,"C0"]
[100004424,"PKR 264 CORPS MONTE + OBC 252 /TA",null,6788,null,null,"Pas concerné par l'étiquettage",null,null,3661238111097,null,null,null,null,"C0"]
[100004425,"PKR 265 CORPS MONTE + OBC 252 /TA",null,7366,null,null,"Pas concerné par l'étiquettage",null,null,3661238111080,null,null,null,null,"C0"]
[]
[100004478,"PKX 264 CORPS NON MONTE",null,3641,null,null,"Pas concerné par l'étiquettage",null,null,3661238110908,null,null,null,null,"C0"]
[100004479,"PKX 265 CORPS NON MONTE",null,4220,null,null,"Pas concerné par l'étiquettage",null,null,3661238110892,null,null,null,null,"C0"]
[100004480,"PKX 266 CORPS NON MONTE",null,4578,null,null,"Pas concerné par l'étiquettage",null,null,3661238110885,null,null,null,null,"C0"]
[100004481,"PKX 267 CORPS NON MONTE",null,4882,null,null,"Pas concerné par l'étiquettage",null,null,3661238110878,null,null,null,null,"C0"]
[100004482,"PKX 268 CORPS NON MONTE",null,5192,null,null,"Pas concerné par l'étiquettage",null,null,3661238110861,null,null,null,null,"C0"]
[100004483,"PKX2 266 CORPS NON MONTE",null,4688,null,null,"Pas concerné par l'étiquettage",null,null,3661238110854,null,null,null,null,"C0"]
[100004484,"PKX2 267 CORPS NON MONTE",null,4992,null,null,"Pas concerné par l'étiquettage",null,null,3661238110847,null,null,null,null,"C0"]
[100004485,"PKX2 268 CORPS NON MONTE",null,5302,null,null,"Pas concerné par l'étiquettage",null,null,3661238110830,null,null,null,null,"C0"]
[100004486,"PKR 264 CORPS NON MONTE",null,4319,null,null,"Pas concerné par l'étiquettage",null,null,3661238110823,null,null,null,null,"C0"]
[100004487,"PKR 265 CORPS NON MONTE",null,4898,null,null,"Pas concerné par l'étiquettage",null,null,3661238110816,null,null,null,null,"C0"]
[100004488,"PKR 266 CORPS NON MONTE",null,5256,null,null,"Pas concerné par l'étiquettage",null,null,3661238110809,null,null,null,null,"C0"]
[100004489,"PKR 267 CORPS NON MONTE",null,5560,null,null,"Pas concerné par l'étiquettage",null,null,3661238110793,null,null,null,null,"C0"]
[100004490,"PKR 268 CORPS NON MONTE",null,5870,null,null,"Pas concerné par l'étiquettage",null,null,3661238110786,null,null,null,null,"C0"]
[100004491,"PKR 266 + AD217  CORPS NON MONTE",null,5550,null,null,"Pas concerné par l'étiquettage",null,null,366123811077,null,null,null,null,"C0"]
[100004492,"PKR 267 + AD217  CORPS NON MONTE",null,5854,null,null,"Pas concerné par l'étiquettage",null,null,3661238110762,null,null,null,null,"C0"]
[100004493,"PKR 268 + AD217  CORPS NON MONTE",null,6164,null,null,"Pas concerné par l'étiquettage",null,null,3661238110755,null,null,null,null,"C0"]
[100004494,"PKX 264 CORPS NON MONTE + OBC 162 /TA",null,5770,null,null,"Pas concerné par l'étiquettage",null,null,3661238110748,null,null,null,null,"C0"]
[100004495,"PKX 265 CORPS NON MONTE + OBC 162 /TA",null,6349,null,null,"Pas concerné par l'étiquettage",null,null,3661238110731,null,null,null,null,"C0"]
[100004496,"PKX 264 CORPS NON MONTE + OBC 252 /TA",null,6113,null,null,"Pas concerné par l'étiquettage",null,null,3661238110724,null,null,null,null,"C0"]
[100004497,"PKX 265 CORPS NON MONTE + OBC 252 /TA",null,6692,null,null,"Pas concerné par l'étiquettage",null,null,3661238110717,null,null,null,null,"C0"]
[100004498,"PKR 264 CORPS NON MONTE + OBC 162 /TA",null,6448,null,null,"Pas concerné par l'étiquettage",null,null,3661238110700,null,null,null,null,"C0"]
[100004499,"PKR 265 CORPS NON MONTE + OBC 162 /TA",null,7027,null,null,"Pas concerné par l'étiquettage",null,null,3661238110694,null,null,null,null,"C0"]
[100004510,"PKR 264 CORPS NON MONTE + OBC 252 /TA",null,6791,null,null,"Pas concerné par l'étiquettage",null,null,3661238110687,null,null,null,null,"C0"]
[100004511,"PKR 265 CORPS NON MONTE + OBC 252 /TA",null,7370,null,null,"Pas concerné par l'étiquettage",null,null,3661238110670,null,null,null,null,"C0"]
[]
["COMPOSANTS"]
[200004483,"ELEMENT INTERMEDIAIRE PK 260",null,268,null,null,"/","/","/",3661238001787,35.83,650,410,125,"C0"]
[82270002,"ELEMENT AVANT PKR-250",null,273,null,null,"/","/","/",3661238020580,35.25,660,480,130,"C0"]
[82270003,"ELEMENT ARRIERE PKR-250",null,359,null,null,"/","/","/",3661238020573,42.5,690,410,130,"C0"]
[100004366,"CAISSE ACCESSOIRES 4 ELEMENTS","ME6",946,null,null,"/","/","/",3661238003620,45.5,645,610,390,"C0"]
[100004367,"CAISSE ACCESSOIRES 5 ELEMENTS","ME7",1011,null,null,"/","/","/",3661238003613,45.5,645,610,390,"C0"]
[100004368,"CAISSE ACCESSOIRES 6 ELEMENTS","ME8",1076,null,null,"/","/","/",3661238003606,49,645,610,390,"C0"]
[100004369,"CAISSE ACCESSOIRES 7 ELEMENTS","ME9",1106,null,null,"/","/","/",3661238003590,49.5,645,610,390,"C0"]
[100004370,"CAISSE ACCESSOIRES 8 ELEMENTS","ME10",1138,null,null,"/","/","/",3661238003583,46.5,645,610,390,"C0"]
[100004531,"COLIS JAQUETTE PKR264 ","MF1",891,null,null,"/","/","/",3661238110489,27,1085,620,425,"C0"]
[100019219,"COLIS JAQUETTE PK265/PU265  ","MF6",1137,null,null,"/","/","/",3661238110472,37,1090,750,425,"C0"]
[100019220,"COLIS JAQUETTE PK266/PU266","MF7",1152,null,null,"/","/","/",3661238110465,34.5,1100,870,440,"C0"]
[100019221,"COLIS JAQUETTE PK267/PU267","MF8",1158,null,null,"/","/","/",3661238110458,44,1095,1045,440,"C0"]
[100004535,"COLIS JAQUETTE PKR268  ","MF5",1168,null,null,"/","/","/",3661238110441,47,1130,1095,440,"C0"]
[100004361,"CORPS ASSEMBLE 4 ELEMENTS","ME1",2111,null,null,"/","/","/",3661238003675,212,845,815,630,"C0"]
[100004362,"CORPS ASSEMBLE 5 ELEMENTS","ME2",2443,null,null,"/","/","/",3661238003668,248,975,815,630,"C0"]
[100004363,"CORPS ASSEMBLE 6 ELEMENTS   ","ME3",2784,null,null,"/","/","/",3661238003651,294,1105,815,630,"C0"]
[100004364,"CORPS ASSEMBLE 7 ELEMENTS","ME4",3081,null,null,"/","/","/",3661238003644,332,1230,815,630,"C0"]
[100004365,"CORPS ASSEMBLE 8 ELEMENTS","ME5",3381,null,null,"/","/","/",3661238003637,368.5,1355,815,630,"C0"]
[82277010,"LIASSE TIGE ASSEMB. 6 EL ",null,10,null,null,"/","/","/",3661238020511,0.43,700,15,10,"C0"]
[82277011,"LIASSE TIGE ASSEMB. 7 EL  ",null,10,null,null,"/","/","/",3661238020504,0.51,825,15,7,"C0"]
[82277012,"LIASSE TIGE ASSEMB. 8 EL  ",null,10,null,null,"/","/","/",3661238020498,0.61,1000,15,7,"C0"]
[100002001,"TABLEAU CDE X /TA","FT41",636,3.34,"11.14","/","/","/",3661238112766,4.8,415,425,195,"C0"]
[100004587,"TABLEAU  R/TA","FT63",1314,3.34,"11.14","/","/","/",3661238110427,5.2,415,425,195,"C0"]
[100004588,"TABLEAU CDE X2 / TA","FT64",746,3.34,"11.14","/","/","/",3661238110410,5.2,415,425,195,"C0"]
[100004294,"PLATINE 2 all./Mod./V3V","AD217",294,0.12,95010,"/","/","/",3661238004191,0.75,200,145,130,"C0"]
[100001610,"OBC 162 /TA","BH105",1517,null,null,"/","/","/",3661238112780,94.5,680,680,1110,"C0"]
[100001611,"OBC 252 /TA","BH106",1860,null,null,"/","/","/",3661238112773,123,680,680,1480,"C0"]
[89557702,"PANNEAU AVANT","BH87",156,null,null,"/","/","/",3661238102361,3.85,680,640,100,"C0"]
[89997045,"TUB. LIAISON OBC/PKR 250","BH93",456,null,null,"/","/","/",3661238044494,6.5,575,505,140,"C0"]
[]
["OPTIONS TABLEAU"]
[100004294,"PLATINE 2 ALL./MOD./V3V","AD217",294,0.12,95010,"/","/","/",3661238004191,0.75,200,145,130,"C0"]
[88017017,"SONDE DEPART v3v","AD199",80,0.02,95020,"/","/","/",3661238049185,0.21,150,200,40,"C0"]
[88017014," PLATINE + SONDE V3V","AD196",180,0.02,95020,"/","/","/",3661238102422,0.52,260,170,120,"C0"]
[85757742,"SONDE FUMEES","FM47",72,0.02,95020,"/","/","/",3661238022744,0.17,210,160,40,"C0"]
[161118,"COMMANDE A DISTANCE INTERACTIVE AD194","AD194",197,0.12,95010,"/","/","/",3661238106505,0.15,null,null,null,"C0"]
[100002803,"COMMANDE A DISTANCE SIMPLIFIEE AD208","AD208",104,0.12,95010,"/","/","/",3661238554931,0.2,120,85,40,"C0"]
[88017887,"SONDES POUR BALLON TAMPON","AD160",97,0.02,95020,"/","/","/",3661238048720,0.21,210,170,40,"C7"]
[88017851,"CABLE DE LIAISON BUS LG 12 M","AD134",110,0.02,95020,"/","/","/",3661238048850,0.37,350,260,30,"C0"]
[88017904,"THERMOSTAT AMBIANCE PROGRAMMABLE","AD191",161,0.12,95010,"/","/","/",3661238102415,0.25,135,90,55,"C0"]
[88017010,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (SANS FILS)","AD192",286,0.12,95010,"/","/","/",3661238102439,0.42499999999999999,180,150,90,"C0"]
[]
["OPTIONS ECS"]
[100000492,"KIT ANODE MAGNESIUM","EA103",66,null,null,"/","/","/",3661238011069,0.9,560,90,85,"C0"]
[89557010,"KIT ENSEMBLE CHAUFFANT 2400 W ","BH88",565,null,null,"/","/","/",3661238102378,3.2,660,215,215,"C0"]
[89557009,"KIT DE TRANSFORMATION G/R 3/4 '' ET 1 ''","BH84",32,null,null,"/","/","/",3661238047563,0.32500000000000001,200,140,45,"C0"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.16,200,150,30,"C0"]
[100007835,"KIT LIAISON PK264-6","EA117",525,null,null,"/","/","/",3661238113312,6.5,600,500,135,"C0"]
[]
[]
[100004917,"PKX-355 CORPS NON MONTE",null,4250,null,null,"Pas concerné par l'étiquettage",null,null,3661238110014,null,null,null,null,"C3"]
[100004918,"PKX-356 CORPS NON MONTE",null,4677,null,null,"Pas concerné par l'étiquettage",null,null,3661238110007,null,null,null,null,"C3"]
[100004919,"PKX-357 CORPS NON MONTE",null,5173,null,null,"Pas concerné par l'étiquettage",null,null,3661238109995,null,null,null,null,"C3"]
[100004920,"PKX-358 CORPS NON MONTE",null,6071,null,null,"Pas concerné par l'étiquettage",null,null,3661238109988,null,null,null,null,"C3"]
[100004921,"PKX-359 CORPS NON MONTE",null,7232,null,null,"Pas concerné par l'étiquettage",null,null,3661238109971,null,null,null,null,"C3"]
[100004897,"PKX-355 CORPS MONTE ",null,4696,null,null,"Pas concerné par l'étiquettage",null,null,3661238110113,null,null,null,null,"C3"]
[100004898,"PKX-356 CORPS MONTE ",null,5244,null,null,"Pas concerné par l'étiquettage",null,null,3661238110106,null,null,null,null,"C3"]
[100004899,"PKX-357 CORPS MONTE ",null,5735,null,null,"Pas concerné par l'étiquettage",null,null,3661238110090,null,null,null,null,"C3"]
[100004910,"PKX-358 CORPS MONTE ",null,6637,null,null,"Pas concerné par l'étiquettage",null,null,3661238110083,null,null,null,null,"C3"]
[100004911,"PKX-359 CORPS MONTE ",null,7834,null,null,"Pas concerné par l'étiquettage",null,null,3661238110076,null,null,null,null,"C3"]
[100004922,"PKR-355 CORPS NON MONTE ",null,4426,null,null,"Pas concerné par l'étiquettage",null,null,3661238109964,null,null,null,null,"C3"]
[100004923,"PKR-356 CORPS NON MONTE ",null,4853,null,null,"Pas concerné par l'étiquettage",null,null,3661238109957,null,null,null,null,"C3"]
[100004924,"PKR-357 CORPS NON MONTE ",null,5349,null,null,"Pas concerné par l'étiquettage",null,null,3661238109940,null,null,null,null,"C3"]
[100004925,"PKR-358 CORPS NON MONTE ",null,6247,null,null,"Pas concerné par l'étiquettage",null,null,3661238109933,null,null,null,null,"C3"]
[100004926,"PKR-359 CORPS NON MONTE ",null,7408,null,null,"Pas concerné par l'étiquettage",null,null,3661238109926,null,null,null,null,"C3"]
[100004912,"PKR-355 CORPS MONTE     ",null,4872,null,null,"Pas concerné par l'étiquettage",null,null,3661238110069,null,null,null,null,"C3"]
[100004913,"PKR-356 CORPS MONTE     ",null,5420,null,null,"Pas concerné par l'étiquettage",null,null,3661238110052,null,null,null,null,"C3"]
[100004914,"PKR-357 CORPS MONTE     ",null,5911,null,null,"Pas concerné par l'étiquettage",null,null,3661238110045,null,null,null,null,"C3"]
[100004915,"PKR-358 CORPS MONTE     ",null,6813,null,null,"Pas concerné par l'étiquettage",null,null,3661238110038,null,null,null,null,"C3"]
[100004916,"PKR-359 CORPS MONTE     ",null,8010,null,null,"Pas concerné par l'étiquettage",null,null,3661238110021,null,null,null,null,"C3"]
[]
["COMPOSANTS"]
[85537067,"CORPS MONTE PKR355",null,2868,null,null,"/","/","/",3661238026179,600,1085,1085,670,"C3"]
[85537068,"CORPS MONTE PKR356",null,3283,null,null,"/","/","/",3661238026162,712.5,1250,1080,680,"C3"]
[85537069,"CORPS MONTE PKR357",null,3710,null,null,"/","/","/",3661238026155,824,1410,1080,680,"C3"]
[85537070,"CORPS MONTE PKR358",null,4133,null,null,"/","/","/",3661238026148,936,1550,1080,680,"C3"]
[85537071,"CORPS MONTE PKR359",null,4598,null,null,"/","/","/",3661238026131,1048,1730,1080,680,"C3"]
[100004866,"COLIS JAQUETTE LATERALE PK 355","MD8",567,null,null,"/","/","/",3661238002081,44,1180,980,330,"C3"]
[100004867,"COLIS JAQUETTE LATERALE PK 356","MD9",626,null,null,"/","/","/",3661238002074,80.5,1230,1350,390,"C3"]
[100004868,"COLIS JAQUETTE LATERALE PK 357","MD10",684,null,null,"/","/","/",3661238002067,95.25,1230,1350,390,"C3"]
[100004869,"COLIS JAQUETTE LATERALE PK 358","MD11",938,null,null,"/","/","/",3661238002050,91.25,1230,1650,390,"C3"]
[100004880,"COLIS JAQUETTE LATERALE PK 359","MD12",1604,null,null,"/","/","/",3661238002043,112.25,1230,1650,390,"C3"]
[100004927,"HABILLAGE AVANT  PK 350","MG3",116,null,null,"/","/","/",3661238109919,9.5,1010,820,120,"C3"]
[82190002,"ELEMENT AVANT   PKR350",null,499,null,null,"/","/","/",3661238020825,104,1070,620,170,"C3"]
[85537072,"ELEMENT ARRIERE PKR350",null,549,null,null,"/","/","/",3661238026124,130,1070,600,190,"C3"]
[82190001,"ELEMENT INTERM. PKR350",null,336,null,null,"/","/","/",3661238020832,111,990,600,165,"C3"]
[85537010,"ACCESSOIRES PKR355","FD10",514,null,null,"/","/","/",3661238026520,48,660,615,370,"C3"]
[85537011,"ACCESSOIRES PKR356","FD11",534,null,null,"/","/","/",3661238026513,49.5,660,615,370,"C3"]
[85537012,"ACCESSOIRES PKR357","FD12",610,null,null,"/","/","/",3661238026506,49.5,660,615,370,"C3"]
[85537013,"ACCESSOIRES PKR358 ","FD13",678,null,null,"/","/","/",3661238026490,50,660,615,370,"C3"]
[85537014,"ACCESSOIRES PKR359","FD14",719,null,null,"/","/","/",3661238026483,51.5,660,615,370,"C3"]
[82197713,"TURBULATEUR PKR355/356 ","BP17",207,null,null,"/","/","/",3661238020801,36,635,510,220,"C3"]
[82197715,"TURBULATEUR PKR357  ","BP19",213,null,null,"/","/","/",3661238020795,39,500,630,240,"C3"]
[82197716,"TURBULATEUR PKR358 ","BP20",438,null,null,"/","/","/",3661238020788,55,635,510,380,"C3"]
[82197717,"TURBULATEUR PKR359 ","BP21",492,null,null,"/","/","/",3661238020771,60,500,630,400,"C3"]
[85537015,"ACCESSOIRES CORPS ASS.  PKR 355-6","FD15",290,null,null,"/","/","/",3661238026476,26,680,525,190,"C3"]
[85537019,"ACCESSOIRES CORPS ASS.  PKR 356-7-8","FD19",364,null,null,"/","/","/",3661238026469,26.5,680,525,190,"C3"]
[85537020,"ACCESSOIRES CORPS ASS.  PKR 359","FD20",376,null,null,"/","/","/",3661238026452,27,680,525,190,"C3"]
[82198945,"TIGE ASSEMBL. PKR355",null,9,null,null,"/","/","/",3661238020641,1.56,700,50,50,"C3"]
[82198946,"TIGE ASSEMBL. PKR356",null,10,null,null,"/","/","/",3661238020634,1.9,865,50,50,"C3"]
[82198947,"TIGE ASSEMBL. PKR357",null,12,null,null,"/","/","/",3661238020627,2.25,1025,50,50,"C3"]
[82198948,"TIGE ASSEMBL. PKR358",null,15,null,null,"/","/","/",3661238020610,2.61,1185,50,50,"C3"]
[82198949,"TIGE ASSEMBL. PKR359",null,22,null,null,"/","/","/",3661238020603,2.92,1330,50,50,"C3"]
[85537061,"CHASSIS PKR355","FD31",133,null,null,"/","/","/",3661238026230,16,750,190,100,"C3"]
[85537062,"CHASSIS PKR356","FD32",144,null,null,"/","/","/",3661238026223,18.5,760,190,110,"C3"]
[85537063,"CHASSIS PKR357","FD33",162,null,null,"/","/","/",3661238026216,20.5,900,210,120,"C3"]
[85537064,"CHASSIS PKR358 ","FD34",174,null,null,"/","/","/",3661238026209,23,1060,210,130,"C3"]
[85537065,"CHASSIS PKR359","FD35",231,null,null,"/","/","/",3661238026193,25,1220,210,140,"C3"]
[100005564,"DOC.TECHN","MG5",40,null,null,"/","/","/",3661238109612,0.45,330,240,45,"C3"]
[100005565,"DOC. TECHN. ","MG6",40,null,null,"/","/","/",3661238109605,0.45,330,240,45,"C3"]
[100005566,"DOC. TECHN. ","MG7",40,null,null,"/","/","/",3661238109599,0.45,330,240,45,"C3"]
[100005567,"DOC. TECHN. ","MG8",40,null,null,"/","/","/",3661238109582,0.45,330,240,45,"C3"]
[100005568,"DOC. TECHN. ","MG9",40,null,null,"/","/","/",3661238109575,0.45,330,240,45,"C3"]
[82197718,"PORTE FOYERE PKR340 F135","BP13",283,null,null,"/","/","/",3661238020764,21.6,680,180,520,"C3"]
[100004380,"TABLEAU STANDARD OERTLI","MG1",325,3.34,"11.14","/","/","/",3661238111332,5.0599999999999996,800,200,200,"C3"]
[100004381,"TABLEAU R OERTLI","MG2",501,3.34,"11.14","/","/","/",3661238111325,10.39,830,430,270,"C3"]
[]
["OPTIONS"]
[100012592,"REA 060B",null,235,0.12,95010,"/","/","/",null,null,null,null,null,"C0"]
[125392,"REA-130B POUR 1 CIRCUIT",null,665,0.12,95010,"/","/","/",3661238108486,null,null,null,null,"C0"]
[125394,"REA-131B POUR 2 CIRCUITS",null,856,0.12,95010,"/","/","/",3661238108479,null,null,null,null,"C0"]
[125400,"REA  232B : POUR 2 CIRCUITS VANNE",null,1151,0.12,95010,"/","/","/",3661238108448,null,null,null,null,"C0"]
[126490,"CABLAGE POUR 2è VANNE MELANGEUSE",null,76,0.02,95020,"/","/","/",3661238107496,null,null,null,null,"C0"]
[125355,"STATION D'AMBIANCE","RES11",352,0.12,95010,"/","/","/",3661238108493,0.5,null,null,null,"C0"]
[125403,"SONDE WWF/ECS ( POUR TABLEAU AVEC REA)",null,49,0.02,95020,"/","/","/",3661238108431,null,null,null,null,"C0"]
[126589,"OUTIL DE MONTAGE JD-TE Plus",null,3202,null,null,"/","/","/",3661238107489,null,null,null,null,"prix net"]
[126624,"COMMANDE A DISTANCE ","RFF60",153,0.12,95010,"/","/","/",3661238107472,null,null,null,null,"C0"]
[82197729,"THERMOMETRE FUMEES    ","BP28",103,0.02,95020,"/","/","/",3661238020733,0.33,195,150,125,"C0"]
[85537076,"KIT DE SECURITE < 115 kW","FD39",175,null,null,"/","/","/",3661238026087,2.41,425,255,120,"C0"]
[85537079,"KIT DE SECURITE 115 à 330 kW","FD42",243,null,null,"/","/","/",3661238026056,3.14,470,255,115,"C0"]
[85537075,"CONTRE BRIDE 2\"","FD38",73,null,null,"/","/","/",3661238026094,2.79,195,150,125,"C0"]
[85537074,"KIT VANNE DE CHASSE","FD37",280,null,null,"/","/","/",3661238026100,6.5,410,290,170,"C0"]
[100012251,"KIT RECIRCULATION GTU C 330","MD218",421,null,null,"/","/","/",3661238357921,17,660,490,300,"C3"]
[]
[]
[100013271,"PKX450-08   CORPS NON MONTE",null,9706,null,null,"Pas concerné par l'étiquettage",null,null,3661238552050,null,null,null,null,"C3"]
[100013272,"PKX450-09   CORPS NON MONTE",null,10718,null,null,"Pas concerné par l'étiquettage",null,null,3661238552067,null,null,null,null,"C3"]
[100013273,"PKX450-10   CORPS NON MONTE",null,11612,null,null,"Pas concerné par l'étiquettage",null,null,3661238552074,null,null,null,null,"C3"]
[100013274,"PKX450-11   CORPS NON MONTE",null,12601,null,null,"Pas concerné par l'étiquettage",null,null,3661238552081,null,null,null,null,"C3"]
[100013275,"PKX450-12   CORPS NON MONTE",null,13500,null,null,"Pas concerné par l'étiquettage",null,null,3661238552098,null,null,null,null,"C3"]
[100013276,"PKX450-13   CORPS NON MONTE",null,14515,null,null,"Pas concerné par l'étiquettage",null,null,3661238552104,null,null,null,null,"C3"]
[100013277,"PKX450-14   CORPS NON MONTE",null,15338,null,null,"Pas concerné par l'étiquettage",null,null,3661238552111,null,null,null,null,"C3"]
[100013265,"PKX450-08   CORPS MONTE",null,10504,null,null,"Pas concerné par l'étiquettage",null,null,3661238552128,null,null,null,null,"C3"]
[100013266,"PKX450-09   CORPS MONTE",null,11584,null,null,"Pas concerné par l'étiquettage",null,null,3661238552135,null,null,null,null,"C3"]
[100013267,"PKX450-10   CORPS MONTE",null,12574,null,null,"Pas concerné par l'étiquettage",null,null,3661238552142,null,null,null,null,"C3"]
[100013268,"PKX450-11   CORPS MONTE",null,13652,null,null,"Pas concerné par l'étiquettage",null,null,3661238552159,null,null,null,null,"C3"]
[100013269,"PKX450-12   CORPS MONTE",null,14645,null,null,"Pas concerné par l'étiquettage",null,null,3661238552166,null,null,null,null,"C3"]
[100013280,"PKX450-13   CORPS MONTE",null,15802,null,null,"Pas concerné par l'étiquettage",null,null,3661238552173,null,null,null,null,"C3"]
[100013281,"PKX450-14   CORPS MONTE",null,16764,null,null,"Pas concerné par l'étiquettage",null,null,3661238552180,null,null,null,null,"C3"]
[100013282,"PKR450-08   CORPS NON MONTE",null,9882,null,null,"Pas concerné par l'étiquettage",null,null,3661238552197,null,null,null,null,"C3"]
[100013283,"PKR450-09   CORPS NON MONTE",null,10894,null,null,"Pas concerné par l'étiquettage",null,null,3661238552203,null,null,null,null,"C3"]
[100013284,"PKR450-10   CORPS NON MONTE",null,11788,null,null,"Pas concerné par l'étiquettage",null,null,3661238552210,null,null,null,null,"C3"]
[100013285,"PKR450-11   CORPS NON MONTE",null,12777,null,null,"Pas concerné par l'étiquettage",null,null,3661238552227,null,null,null,null,"C3"]
[100013286,"PKR450-12   CORPS NON MONTE",null,13676,null,null,"Pas concerné par l'étiquettage",null,null,3661238552234,null,null,null,null,"C3"]
[100013287,"PKR450-13   CORPS NON MONTE",null,14691,null,null,"Pas concerné par l'étiquettage",null,null,3661238552241,null,null,null,null,"C3"]
[100013288,"PKR450-14   CORPS NON MONTE",null,15514,null,null,"Pas concerné par l'étiquettage",null,null,3661238552258,null,null,null,null,"C3"]
[100013289,"PKR450-08   CORPS MONTE",null,10680,null,null,"Pas concerné par l'étiquettage",null,null,3661238552265,null,null,null,null,"C3"]
[100013290,"PKR450-09   CORPS MONTE",null,11760,null,null,"Pas concerné par l'étiquettage",null,null,3661238552272,null,null,null,null,"C3"]
[100013291,"PKR450-10   CORPS MONTE",null,12750,null,null,"Pas concerné par l'étiquettage",null,null,3661238552289,null,null,null,null,"C3"]
[100013292,"PKR450-11   CORPS MONTE",null,13828,null,null,"Pas concerné par l'étiquettage",null,null,3661238552296,null,null,null,null,"C3"]
[100013293,"PKR450-12   CORPS MONTE",null,14821,null,null,"Pas concerné par l'étiquettage",null,null,3661238552302,null,null,null,null,"C3"]
[100013294,"PKR450-13   CORPS MONTE",null,15978,null,null,"Pas concerné par l'étiquettage",null,null,3661238552319,null,null,null,null,"C3"]
[100013295,"PKR450-14   CORPS MONTE",null,16940,null,null,"Pas concerné par l'étiquettage",null,null,3661238552326,null,null,null,null,"C3"]
[]
["COMPOSANTS"]
[100013270,"JAQUETTE PIECES COMMUNES PK450 MH1","MH1",918,null,null,"/","/","/",3661238365513,94,1130,1540,370,"C3"]
[100007214,"JAQUETTE PCES VAR LAT AR 770 GT430 MP2","MP2",421,null,null,"/","/","/",3661238092884,36.5,1470,800,300,"C3"]
[100007215,"JAQUETTE PCES VAR LAT AR 930 GT430 MP3","MP3",550,null,null,"/","/","/",3661238092877,68,1520,1035,400,"C3"]
[100007216,"JAQUETTE PCES VAR LAT CENT 480 GT430 MP4","MP4",382,null,null,"/","/","/",366123809286,23.5,1470,530,300,"C3"]
[100007217,"JAQUETTE PCES VAR LAT AR 610 GT430 MP5","MP5",343,null,null,"/","/","/",3661238092853,29.5,1470,635,300,"C3"]
[82297741,"CHEM,CABLE GT400 8E CS41","CS41",27,null,null,"/","/","/",3661238019195,4.26,1470,155,25,"C3"]
[82297742,"CHEM.CABLE GT400 9E CS42","CS42",30,null,null,"/","/","/",3661238019188,4.78,1630,155,25,"C3"]
[82297743,"CHEM.CABLE GT400 10E CS43","CS43",44,null,null,"/","/","/",3661238019171,5.24,1790,155,25,"C3"]
[82297744,"CHEM.CABLE GT400 11E CS44","CS44",45,null,null,"/","/","/",3661238019164,5.74,1950,155,25,"C3"]
[82297745,"CHEM.CABLE GT400 12E CS45","CS45",47,null,null,"/","/","/",3661238019157,6.07,2110,155,25,"C3"]
[82297746,"CHEM.CABLE GT400 13E CS46","CS46",53,null,null,"/","/","/",3661238019140,6.52,2270,155,25,"C3"]
[82297747,"CHEM.CABLE GT400 14E CS47","CS47",53,null,null,"/","/","/",3661238019133,7,2430,155,25,"C3"]
[82297751,"COL.ISOL.GT407-408 CS51","CS51",45,null,null,"/","/","/",3661238019126,2.1,1180,630,150,"C3"]
[82297753,"COL.ISOL.GT409-410  CS53","CS53",53,null,null,"/","/","/",3661238019102,2.8,1180,780,180,"C3"]
[82297755,"COL.ISOL.GT411-412  CS55","CS55",62,null,null,"/","/","/",3661238019102,4,1150,900,150,"C3"]
[82297757,"COL.ISOL.GT413-414  CS57","CS57",69,null,null,"/","/","/",3661238019096,3.5,1200,740,180,"C3"]
[82290002,"ELEMENT AVANT     PKR440",null,724,null,null,"/","/","/",3661238019522,155.5,1345,815,170,"C3"]
[82298904,"ELEMENT ARRIERE PKR440",null,775,null,null,"/","/","/",3661238018952,224.5,1340,830,230,"C3"]
[82290001,"ELEMENT INTERM  NORMAL PKR440",null,674,null,null,"/","/","/",3661238019539,185,1335,845,160,"C3"]
[82290005,"ELEMENT INTERM  SPECIAL PKR440",null,664,null,null,"/","/","/",3661238019515,164.5,1335,850,165,"C3"]
[82298900,"CHASSIS ASS PKR440/08",null,269,null,null,"/","/","/",3661238018990,37,1290,125,150,"C3"]
[82298901,"CHASSIS ASS PKR440/09-10",null,293,null,null,"/","/","/",3661238018983,44,1610,125,150,"C3"]
[82298902,"CHASSIS ASS PKR440/11-12",null,317,null,null,"/","/","/",3661238018976,55,1930,125,150,"C3"]
[82298903,"CHASSIS ASS PKR440/13-14",null,377,null,null,"/","/","/",3661238018969,62,2250,125,150,"C3"]
[82297730,"COLIS TURBUL, 7-8 CS30","CS30",458,null,null,"/","/","/",3661238019232,72.5,610,650,390,"C3"]
[82297731,"COLIS TURBUL, 9-10 CS31","CS31",552,null,null,"/","/","/",3661238019225,97,610,650,390,"C3"]
[82297732,"COLIS TURBUL, 11-12 CS32","CS32",679,null,null,"/","/","/",3661238019218,120.5,760,710,450,"C3"]
[82297733,"COLIS TURBUL, 13-14 CS33","CS33",801,null,null,"/","/","/",3661238019201,144,700,750,460,"C3"]
[100013310,"DOCUMENTATION TEC GENE PK 450-",null,36,null,null,"/","/","/",3661238362918,0.5,325,240,50,"C3"]
[100013311,"DOCUMENTATION TEC GENE PK 450-",null,36,null,null,"/","/","/",366123836292,0.5,325,240,50,"C3"]
[100013312,"DOCUMENTATION TEC GENE PK 450-",null,36,null,null,"/","/","/",3661238362932,0.5,325,240,50,"C3"]
[100013313,"DOCUMENTATION TEC GENE PK 450-",null,36,null,null,"/","/","/",3661238362949,0.5,325,240,50,"C3"]
[100013314,"DOCUMENTATION TEC GENE PK 450-",null,36,null,null,"/","/","/",3661238362956,0.5,325,240,50,"C3"]
[100013315,"DOCUMENTATION TEC GENE PK 450-",null,36,null,null,"/","/","/",366123836296,0.5,325,240,50,"C3"]
[100013316,"DOCUMENTATION TEC GENE PK 450-",null,36,null,null,"/","/","/",3661238362970,0.5,325,240,50,"C3"]
[82297722,"CAISSE ACC, VAR, GT408",null,978,null,null,"/","/","/",3661238019300,96,760,710,470,"C3"]
[82297723,"CAISSE ACC, VAR, GT409",null,1012,null,null,"/","/","/",3661238019294,104,760,660,420,"C3"]
[82297724,"CAISSE ACC, VAR, GT410",null,1140,null,null,"/","/","/",3661238019287,111,760,710,470,"C3"]
[82297725,"CAISSE ACC, VAR, GT411",null,1165,null,null,"/","/","/",3661238019270,107,760,710,470,"C3"]
[82297726,"CAISSE ACC, VAR, GT412",null,1213,null,null,"/","/","/",3661238019263,113,760,710,470,"C3"]
[82297727,"CAISSE ACC, VAR, GT413",null,1281,null,null,"/","/","/",366123801925,118,760,660,420,"C3"]
[82297728,"CAISSE ACC, VAR, GT414",null,1301,null,null,"/","/","/",3661238019249,121,760,660,420,"C3"]
[82297720,"CAISSE ACC,COM,GT400 CS20","CS20",567,null,null,"/","/","/",3661238019317,70,760,710,430,"C3"]
[82298926,"CORPS GT408 ASSEMBLE",null,8190,null,null,"/","/","/",3661238018945,1640,1800,900,1450,"C3"]
[82298927,"CORPS GT409 ASSEMBLE",null,8998,null,null,"/","/","/",3661238018938,1860,1980,900,1450,"C3"]
[82298928,"CORPS GT410 ASSEMBLE",null,9896,null,null,"/","/","/",3661238018921,2040,2150,900,1450,"C3"]
[82298929,"CORPS GT411 ASSEMBLE",null,10717,null,null,"/","/","/",3661238018914,2220,2320,900,1450,"C3"]
[82298930,"CORPS GT412 ASSEMBLE",null,11533,null,null,"/","/","/",3661238018907,2400,2480,900,1450,"C3"]
[82298931,"CORPS GT413 ASSEMBLE",null,12484,null,null,"/","/","/",3661238018891,2610,2640,900,1450,"C3"]
[82298932,"CORPS GT414 ASSEMBLE",null,13317,null,null,"/","/","/",3661238018884,2795,2800,900,1450,"C3"]
[100004380,"TABLEAU STANDARD OERTLI","MG1",325,3.34,"11.14","/","/","/",3661238111332,5.0599999999999996,800,200,200,"C3"]
[100004381,"TABLEAU R OERTLI","MG2",501,3.34,"11.14","/","/","/",3661238111325,10.39,830,430,270,"C3"]
[]
["OPTIONS"]
[100012592,"REA 060B",null,235,0.12,95010,"/","/","/",null,null,null,null,null,"C0"]
[125400,"REA  232B : POUR 2 CIRCUITS VANNE",null,1151,0.12,95010,"/","/","/",3661238108448,null,null,null,null,"C0"]
[125355,"STATION D'AMBIANCE","RES11",352,0.12,95010,"/","/","/",3661238108493,0.5,null,null,null,"C0"]
[125403,"SONDE WWF/ECS ( POUR TABLEAU AVEC REA)",null,49,0.02,95020,"/","/","/",3661238108431,null,null,null,null,"C0"]
[126490,"CABLAGE POUR 2è VANNE MELANGEUSE",null,76,0.02,95020,"/","/","/",3661238107496,null,null,null,null,"C0"]
[126624,"COMMANDE A DISTANCE ","RFF60",153,0.12,95010,"/","/","/",3661238107472,null,null,null,null,"C0"]
[82197729,"THERMOMETRE FUMEES    ","BP28",103,0.02,95020,"/","/","/",3661238020733,0.33,195,150,125,"C0"]
[126589,"OUTIL DE MONTAGE JD-TE Plus",null,3202,null,null,"/","/","/",3661238107489]
[]
[]
[100013870,"PKX 550-09 CORPS NON MONTE",null,13269,null,null,"Pas concerné par l'étiquettage",null,null,3661238552418,null,null,null,null,"C3"]
[100013871,"PKX 550-10 CORPS NON MONTE",null,14014,null,null,"Pas concerné par l'étiquettage",null,null,3661238552425,null,null,null,null,"C3"]
[100013872,"PKX 550-11 CORPS NON MONTE",null,14733,null,null,"Pas concerné par l'étiquettage",null,null,3661238552432,null,null,null,null,"C3"]
[100013873,"PKX 550-12 CORPS NON MONTE",null,15443,null,null,"Pas concerné par l'étiquettage",null,null,3661238552449,null,null,null,null,"C3"]
[100013874,"PKX 550-13 CORPS NON MONTE",null,16161,null,null,"Pas concerné par l'étiquettage",null,null,3661238552456,null,null,null,null,"C3"]
[100013875,"PKX 550-14 CORPS NON MONTE",null,16872,null,null,"Pas concerné par l'étiquettage",null,null,3661238552463,null,null,null,null,"C3"]
[100013876,"PKX 550-15 CORPS NON MONTE",null,17626,null,null,"Pas concerné par l'étiquettage",null,null,3661238552470,null,null,null,null,"C3"]
[100013877,"PKX 550-16 CORPS NON MONTE",null,18569,null,null,"Pas concerné par l'étiquettage",null,null,3661238552487,null,null,null,null,"C3"]
[100013878,"PKX 550-17 CORPS NON MONTE",null,19910,null,null,"Pas concerné par l'étiquettage",null,null,3661238552494,null,null,null,null,"C3"]
[100013879,"PKX 550-18 CORPS NON MONTE",null,20819,null,null,"Pas concerné par l'étiquettage",null,null,3661238552500,null,null,null,null,"C3"]
[100013880,"PKX 550-19 CORPS NON MONTE",null,21757,null,null,"Pas concerné par l'étiquettage",null,null,3661238552517,null,null,null,null,"C3"]
[100013881,"PKX 550-20 CORPS NON MONTE",null,22355,null,null,"Pas concerné par l'étiquettage",null,null,3661238552524,null,null,null,null,"C3"]
[100013882,"PKX 550-21 CORPS NON MONTE",null,23642,null,null,"Pas concerné par l'étiquettage",null,null,3661238552531,null,null,null,null,"C3"]
[100013883,"PKX 550-22 CORPS NON MONTE",null,24555,null,null,"Pas concerné par l'étiquettage",null,null,3661238552548,null,null,null,null,"C3"]
[100013884,"PKX 550-23 CORPS NON MONTE",null,25498,null,null,"Pas concerné par l'étiquettage",null,null,3661238552555,null,null,null,null,"C3"]
[100013885,"PKX 550-24 CORPS NON MONTE",null,26428,null,null,"Pas concerné par l'étiquettage",null,null,3661238552562,null,null,null,null,"C3"]
[100013886,"PKX 550-25 CORPS NON MONTE",null,27347,null,null,"Pas concerné par l'étiquettage",null,null,3661238552579,null,null,null,null,"C3"]
[100013888,"PKX 550-09 CORPS MONTE",null,14352,null,null,"Pas concerné par l'étiquettage",null,null,3661238552586,null,null,null,null,"C3"]
[100013889,"PKX 550-10 CORPS MONTE",null,15211,null,null,"Pas concerné par l'étiquettage",null,null,3661238552593,null,null,null,null,"C3"]
[100013890,"PKX 550-11 CORPS MONTE",null,16032,null,null,"Pas concerné par l'étiquettage",null,null,3661238552609,null,null,null,null,"C3"]
[100013891,"PKX 550-12 CORPS MONTE",null,16832,null,null,"Pas concerné par l'étiquettage",null,null,3661238552616,null,null,null,null,"C3"]
[100013892,"PKX 550-13 CORPS MONTE",null,17663,null,null,"Pas concerné par l'étiquettage",null,null,3661238552623,null,null,null,null,"C3"]
[100013893,"PKX 550-14 CORPS MONTE",null,18463,null,null,"Pas concerné par l'étiquettage",null,null,3661238552630,null,null,null,null,"C3"]
[100013894,"PKX 550-15 CORPS MONTE",null,19323,null,null,"Pas concerné par l'étiquettage",null,null,3661238552647,null,null,null,null,"C3"]
[100013895,"PKX 550-16 CORPS MONTE",null,20372,null,null,"Pas concerné par l'étiquettage",null,null,3661238552654,null,null,null,null,"C3"]
[100013896,"PKX 550-17 CORPS MONTE",null,21805,null,null,"Pas concerné par l'étiquettage",null,null,3661238552661,null,null,null,null,"C3"]
[100013897,"PKX 550-18 CORPS MONTE",null,22828,null,null,"Pas concerné par l'étiquettage",null,null,3661238552678,null,null,null,null,"C3"]
[100013898,"PKX 550-19 CORPS MONTE",null,23868,null,null,"Pas concerné par l'étiquettage",null,null,3661238552685,null,null,null,null,"C3"]
[100013899,"PKX 550-20 CORPS MONTE",null,24522,null,null,"Pas concerné par l'étiquettage",null,null,3661238552692,null,null,null,null,"C3"]
[100013901,"PKX 550-21 CORPS MONTE",null,25986,null,null,"Pas concerné par l'étiquettage",null,null,3661238552708,null,null,null,null,"C3"]
[100013902,"PKX 550-22 CORPS MONTE",null,27006,null,null,"Pas concerné par l'étiquettage",null,null,3661238552715,null,null,null,null,"C3"]
[100013903,"PKX 550-23 CORPS MONTE",null,28022,null,null,"Pas concerné par l'étiquettage",null,null,3661238552722,null,null,null,null,"C3"]
[100013904,"PKX 550-24 CORPS MONTE",null,29083,null,null,"Pas concerné par l'étiquettage",null,null,3661238552739,null,null,null,null,"C3"]
[100013905,"PKX 550-25 CORPS MONTE",null,30094,null,null,"Pas concerné par l'étiquettage",null,null,3661238552746,null,null,null,null,"C3"]
[100013906,"PKR 550-09 CORPS NON MONTE",null,13445,null,null,"Pas concerné par l'étiquettage",null,null,3661238552753,null,null,null,null,"C3"]
[100013907,"PKR 550-10 CORPS NON MONTE",null,14190,null,null,"Pas concerné par l'étiquettage",null,null,3661238552760,null,null,null,null,"C3"]
[100013908,"PKR 550-11 CORPS NON MONTE",null,14909,null,null,"Pas concerné par l'étiquettage",null,null,3661238552777,null,null,null,null,"C3"]
[100013909,"PKR 550-12 CORPS NON MONTE",null,15619,null,null,"Pas concerné par l'étiquettage",null,null,3661238552784,null,null,null,null,"C3"]
[100013910,"PKR 550-13 CORPS NON MONTE",null,16337,null,null,"Pas concerné par l'étiquettage",null,null,3661238552791,null,null,null,null,"C3"]
[100013911,"PKR 550-14 CORPS NON MONTE",null,17048,null,null,"Pas concerné par l'étiquettage",null,null,3661238552807,null,null,null,null,"C3"]
[100013912,"PKR 550-15 CORPS NON MONTE",null,17802,null,null,"Pas concerné par l'étiquettage",null,null,3661238552814,null,null,null,null,"C3"]
[100013913,"PKR 550-16 CORPS NON MONTE",null,18745,null,null,"Pas concerné par l'étiquettage",null,null,3661238552821,null,null,null,null,"C3"]
[100013914,"PKR 550-17 CORPS NON MONTE",null,20086,null,null,"Pas concerné par l'étiquettage",null,null,3661238552838,null,null,null,null,"C3"]
[100013915,"PKR 550-18 CORPS NON MONTE",null,20995,null,null,"Pas concerné par l'étiquettage",null,null,3661238552845,null,null,null,null,"C3"]
[100013916,"PKR 550-19 CORPS NON MONTE",null,21933,null,null,"Pas concerné par l'étiquettage",null,null,3661238552852,null,null,null,null,"C3"]
[100013917,"PKR 550-20 CORPS NON MONTE",null,22531,null,null,"Pas concerné par l'étiquettage",null,null,3661238552869,null,null,null,null,"C3"]
[100013918,"PKR 550-21 CORPS NON MONTE",null,23818,null,null,"Pas concerné par l'étiquettage",null,null,3661238552876,null,null,null,null,"C3"]
[100013919,"PKR 550-22 CORPS NON MONTE",null,24731,null,null,"Pas concerné par l'étiquettage",null,null,3661238552883,null,null,null,null,"C3"]
[100013920,"PKR 550-23 CORPS NON MONTE",null,25674,null,null,"Pas concerné par l'étiquettage",null,null,3661238552890,null,null,null,null,"C3"]
[100013921,"PKR 550-24 CORPS NON MONTE",null,26604,null,null,"Pas concerné par l'étiquettage",null,null,3661238552906,null,null,null,null,"C3"]
[100013922,"PKR 550-25 CORPS NON MONTE",null,27523,null,null,"Pas concerné par l'étiquettage",null,null,3661238552333,null,null,null,null,"C3"]
[100013923,"PKR 550-09 CORPS MONTE",null,14528,null,null,"Pas concerné par l'étiquettage",null,null,3661238552340,null,null,null,null,"C3"]
[100013924,"PKR 550-10 CORPS MONTE",null,15387,null,null,"Pas concerné par l'étiquettage",null,null,3661238552357,null,null,null,null,"C3"]
[100013925,"PKR 550-11 CORPS MONTE",null,16208,null,null,"Pas concerné par l'étiquettage",null,null,3661238552364,null,null,null,null,"C3"]
[100013926,"PKR 550-12 CORPS MONTE",null,17008,null,null,"Pas concerné par l'étiquettage",null,null,3661238552371,null,null,null,null,"C3"]
[100013927,"PKR 550-13 CORPS MONTE",null,17839,null,null,"Pas concerné par l'étiquettage",null,null,3661238552388,null,null,null,null,"C3"]
[100013928,"PKR 550-14 CORPS MONTE",null,18639,null,null,"Pas concerné par l'étiquettage",null,null,3661238552395,null,null,null,null,"C3"]
[100013929,"PKR 550-15 CORPS MONTE",null,19499,null,null,"Pas concerné par l'étiquettage",null,null,3661238552401,null,null,null,null,"C3"]
[100013930,"PKR 550-16 CORPS MONTE",null,20548,null,null,"Pas concerné par l'étiquettage",null,null,3661238553118,null,null,null,null,"C3"]
[100013931,"PKR 550-17 CORPS MONTE",null,21981,null,null,"Pas concerné par l'étiquettage",null,null,3661238553125,null,null,null,null,"C3"]
[100013932,"PKR 550-18 CORPS MONTE",null,23004,null,null,"Pas concerné par l'étiquettage",null,null,3661238553132,null,null,null,null,"C3"]
[100013933,"PKR 550-19 CORPS MONTE",null,24044,null,null,"Pas concerné par l'étiquettage",null,null,3661238553149,null,null,null,null,"C3"]
[100013934,"PKR 550-20 CORPS MONTE",null,24698,null,null,"Pas concerné par l'étiquettage",null,null,3661238553156,null,null,null,null,"C3"]
[100013935,"PKR 550-21 CORPS MONTE",null,26162,null,null,"Pas concerné par l'étiquettage",null,null,3661238553163,null,null,null,null,"C3"]
[100013936,"PKR 550-22 CORPS MONTE",null,27182,null,null,"Pas concerné par l'étiquettage",null,null,3661238553170,null,null,null,null,"C3"]
[100013937,"PKR 550-23 CORPS MONTE",null,28198,null,null,"Pas concerné par l'étiquettage",null,null,3661238553187,null,null,null,null,"C3"]
[100013938,"PKR 550-24 CORPS MONTE",null,29259,null,null,"Pas concerné par l'étiquettage",null,null,3661238553194,null,null,null,null,"C3"]
[100013939,"PKR 550-25 CORPS MONTE",null,30270,null,null,"Pas concerné par l'étiquettage",null,null,3661238553200,null,null,null,null,"C3"]
[]
["COMPOSANTS"]
[82280001,"ELEMENT INT. NORMAL",null,669,null,null,"/","/","/",3661238019805,174.25,1335,1055,170,"C3"]
[82280002,"ELEMENT INT SPECIAL",null,761,null,null,"/","/","/",3661238019799,203,1305,1060,160,"C3"]
[82288901,"ELEMENT ARRIERE",null,958,null,null,"/","/","/",3661238019553,252,1300,1040,175,"C3"]
[82288902,"ELEMENT AVANT",null,982,null,null,"/","/","/",3661238019546,208,1305,1040,180,"C3"]
[82590501,"CHASSIS 8-9 ELEMENTS",null,268,null,null,"/","/","/",3661238018860,30,1080,120,110,"C3"]
[82590502,"CHASSIS 10-11 ELEMENTS",null,299,null,null,"/","/","/",3661238018853,31.5,1300,120,110,"C3"]
[82590503,"CHASSIS 12-13 ELEMENTS",null,350,null,null,"/","/","/",3661238018846,39.5,1520,120,110,"C3"]
[82590504,"CHASSIS 14-15 ELEMENTS",null,354,null,null,"/","/","/",3661238018839,44,1750,110,120,"C3"]
[82590505,"CHASSIS 16-17 ELEMENTS",null,360,null,null,"/","/","/",3661238018822,51.5,1965,120,110,"C3"]
[82590506,"CHASSIS 18-19 ELEMENTS",null,426,null,null,"/","/","/",3661238018815,56,2190,120,110,"C3"]
[82590507,"CHASSIS 20-21 ELEMENTS",null,403,null,null,"/","/","/",3661238018808,60,2450,120,110,"C3"]
[82590508,"CHASSIS 22-23 ELEMENTS",null,458,null,null,"/","/","/",3661238018792,61.5,2670,120,110,"C3"]
[82590509,"CHASSIS 24-25 ELEMENTS",null,502,null,null,"/","/","/",3661238018785,69,2900,120,110,"C3"]
[82287759,"TIGES ASS.+OUTILS DE CHAUF 09 ELTS",null,96,null,null,"/","/","/",3661238019720,9,1300,140,60,"C3"]
[82287760,"TIGES ASS.+OUTILS DE CHAUF 10 ELTS",null,100,null,null,"/","/","/",3661238019713,10,1300,140,60,"C3"]
[82287761,"TIGES ASS.+OUTILS DE CHAUF 11 ELTS",null,103,null,null,"/","/","/",3661238019706,10,1800,140,60,"C3"]
[82287762,"TIGES ASS.+OUTILS DE CHAUF 12 ELTS",null,107,null,null,"/","/","/",3661238019690,11,1800,140,60,"C3"]
[82287763,"TIGES ASS.+OUTILS DE CHAUF 13 ELTS",null,109,null,null,"/","/","/",3661238019683,11,1800,140,60,"C3"]
[82287764,"TIGES ASS.+OUTILS DE CHAUF 14 ELTS",null,115,null,null,"/","/","/",3661238019676,13,1800,140,60,"C3"]
[82287765,"TIGES ASS.+OUTILS DE CHAUF 15 ELTS",null,116,null,null,"/","/","/",3661238019669,13,1800,140,60,"C3"]
[82287766,"TIGES ASS.+OUTILS DE CHAUF 16 ELTS",null,131,null,null,"/","/","/",3661238019652,15,1908,140,60,"C3"]
[82287767,"TIGES ASS.+OUTILS DE CHAUF 17 ELTS",null,145,null,null,"/","/","/",3661238019645,16,2021,140,60,"C3"]
[82287768,"TIGES ASS.+OUTILS DE CHAUF 18 ELTS",null,148,null,null,"/","/","/",3661238019638,16,2133,140,60,"C3"]
[82287769,"TIGES ASS.+OUTILS DE CHAUF 19 ELTS",null,150,null,null,"/","/","/",3661238019621,16.5,2260,150,70,"C3"]
[82287770,"TIGES ASS.+OUTILS DE CHAUF 20 ELTS",null,152,null,null,"/","/","/",3661238019614,18,2398,140,60,"C3"]
[82287771,"TIGES ASS.+OUTILS DE CHAUF 21 ELTS",null,160,null,null,"/","/","/",3661238019607,18,2511,140,60,"C3"]
[82287772,"TIGES ASS.+OUTILS DE CHAUF 22 ELTS",null,162,null,null,"/","/","/",3661238019591,19,2623,140,60,"C3"]
[82287773,"TIGES ASS.+OUTILS DE CHAUF 23 ELTS",null,169,null,null,"/","/","/",3661238019584,20,2736,140,60,"C3"]
[82287774,"TIGES ASS.+OUTILS DE CHAUF 24 ELTS",null,173,null,null,"/","/","/",3661238019577,21,2848,140,60,"C3"]
[82287775,"TIGES ASS.+OUTILS DE CHAUF 25 ELTS",null,182,null,null,"/","/","/",3661238019560,20.5,3000,150,70,"C3"]
[85557089,"ACCESSOIRES CORPS 09 EL.",null,1541,null,null,"/","/","/",3661238024861,124,760,710,450,"C3"]
[85557090,"ACCESSOIRES CORPS 10 EL.",null,1542,null,null,"/","/","/",3661238024854,128,760,710,450,"C3"]
[85557091,"ACCESSOIRES CORPS 11 EL.",null,1550,null,null,"/","/","/",3661238024847,139,760,710,450,"C3"]
[85557092,"ACCESSOIRES CORPS 12 EL.",null,1471,null,null,"/","/","/",3661238024830,146,760,710,450,"C3"]
[85557093,"ACCESSOIRES CORPS 13 EL.",null,1491,null,null,"/","/","/",3661238024823,149,760,710,450,"C3"]
[85557094,"ACCESSOIRES CORPS 14 EL.",null,1515,null,null,"/","/","/",3661238024816,154,760,710,450,"C3"]
[85557095,"ACCESSOIRES CORPS 15 EL.",null,1506,null,null,"/","/","/",3661238024809,164,760,710,450,"C3"]
[85557096,"ACCESSOIRES CORPS 16 EL.",null,1633,null,null,"/","/","/",3661238024793,169,760,710,450,"C3"]
[85557097,"ACCESSOIRES CORPS 17 EL.",null,1957,null,null,"/","/","/",3661238024786,178,760,710,450,"C3"]
[85557098,"ACCESSOIRES CORPS 18 EL.",null,1739,null,null,"/","/","/",3661238024779,189,760,710,600,"C3"]
[85557099,"ACCESSOIRES CORPS 19 EL.",null,1884,null,null,"/","/","/",3661238024762,195,760,710,600,"C3"]
[85557100,"ACCESSOIRES CORPS 20 EL.",null,1614,null,null,"/","/","/",3661238024755,194,760,710,600,"C3"]
[85557101,"ACCESSOIRES CORPS 21 EL.",null,1959,null,null,"/","/","/",3661238024748,203,760,710,600,"C3"]
[85557102,"ACCESSOIRES CORPS 22 EL.",null,2037,null,null,"/","/","/",3661238024731,207,760,710,600,"C3"]
[85557103,"ACCESSOIRES CORPS 23 EL.",null,2136,null,null,"/","/","/",3661238024724,213,760,710,600,"C3"]
[85557104,"ACCESSOIRES CORPS 24 EL.",null,2283,null,null,"/","/","/",3661238024717,226,760,710,600,"C3"]
[85557105,"ACCESSOIRES CORPS 25 EL.",null,2402,null,null,"/","/","/",3661238024700,231,760,710,600,"C3"]
[85557109,"ACCESSOIRES COMPL. CV 09 EL.",null,761,null,null,"/","/","/",3661238024670,20,635,510,380,"C3"]
[85557110,"ACCESSOIRES COMPL. CV 10 EL.",null,719,null,null,"/","/","/",3661238024663,20,635,510,380,"C3"]
[85557111,"ACCESSOIRES COMPL. CV 11 EL.",null,715,null,null,"/","/","/",3661238024656,30,635,510,380,"C3"]
[85557112,"ACCESSOIRES COMPL. CV 12 EL.",null,681,null,null,"/","/","/",3661238024649,31,635,510,380,"C3"]
[85557113,"ACCESSOIRES COMPL. CV 13 EL.",null,684,null,null,"/","/","/",3661238024632,24,660,615,370,"C3"]
[85557114,"ACCESSOIRES COMPL. CV 14 EL.",null,711,null,null,"/","/","/",3661238024625,24,660,615,370,"C3"]
[85557115,"ACCESSOIRES COMPL. CV 15 EL.",null,603,null,null,"/","/","/",3661238024618,24,660,615,370,"C3"]
[85557116,"ACCESSOIRES COMPL. CV 16 EL.",null,672,null,null,"/","/","/",3661238024601,24,660,615,370,"C3"]
[85557117,"ACCESSOIRES COMPL. CV 17 EL.",null,907,null,null,"/","/","/",3661238024595,36.5,660,615,370,"C3"]
[85557118,"ACCESSOIRES COMPL. CV 18 EL.",null,801,null,null,"/","/","/",3661238024588,25,660,615,370,"C3"]
[85557119,"ACCESSOIRES COMPL. CV 19 EL.",null,847,null,null,"/","/","/",3661238024571,39,660,615,370,"C3"]
[85557120,"ACCESSOIRES COMPL. CV 20 EL.",null,674,null,null,"/","/","/",3661238024564,26,660,615,370,"C3"]
[85557121,"ACCESSOIRES COMPL. CV 21 EL.",null,884,null,null,"/","/","/",3661238024557,41,660,615,370,"C3"]
[85557122,"ACCESSOIRES COMPL. CV 22 EL.",null,894,null,null,"/","/","/",3661238024540,28,660,615,370,"C3"]
[85557123,"ACCESSOIRES COMPL. CV 23 EL.",null,968,null,null,"/","/","/",3661238024533,28,660,615,370,"C3"]
[85557124,"ACCESSOIRES COMPL. CV 24 EL.",null,1012,null,null,"/","/","/",3661238024526,41.5,660,615,370,"C3"]
[85557125,"ACCESSOIRES COMPL. CV 25 EL.",null,1092,null,null,"/","/","/",3661238024519,44.5,660,615,370,"C3"]
[82590523,"PORTE FOYERE PLEINE PEINTE",null,359,null,null,"/","/","/",3661238018778,39,610,490,140,"C3"]
[80080539,"PLAQUE RACCORD.EMB.D.300",null,201,null,null,"/","/","/",3661238001688,20,800,595,110,"C3"]
[80080535,"PLAQUE RACCORD.EMB.D.350",null,174,null,null,"/","/","/",3661238001701,19,800,595,110,"C3"]
[80080536,"PLAQUE RACCORD.EMB.D.400",null,178,null,null,"/","/","/",3661238001695,18.5,800,595,110,"C3"]
[80080534,"PLAQUE RACCORD.PLEINE",null,123,null,null,"/","/","/",3661238001718,20.5,800,595,50,"C3"]
[82088960,"DEPART DUMEE TOLE CDE 800",null,474,null,null,"/","/","/",3661238020863,27.5,960,950,245,"C3"]
[80087700,"TUBE REPARTITEUR 20-22",null,201,null,null,"/","/","/",3661238001671,6.5,1235,235,250,"C3"]
[80087701,"TUBE REPARTITEUR 23-24",null,247,null,null,"/","/","/",3661238001664,8,1235,235,250,"C3"]
[80087702,"TUBE REPARTITEUR 25",null,253,null,null,"/","/","/",3661238001657,8,1235,235,250,"C3"]
[82597761,"TURBULATEURS CM22",null,85,null,null,"/","/","/",3661238018747,12.5,610,470,190,"C3"]
[82597762,"TURBULATEURS CM23",null,150,null,null,"/","/","/",3661238018730,23.5,610,470,190,"C3"]
[85557031,"ISOLATION CORPS  8-9 ELEMENTS",null,200,null,null,"/","/","/",3661238025370,16,1615,1215,420,"C3"]
[85557032,"ISOLATION CORPS 10 ELEMENTS",null,222,null,null,"/","/","/",3661238025363,17.5,1615,1215,420,"C3"]
[85557033,"ISOLATION CORPS 11-12 ELEMENTS",null,242,null,null,"/","/","/",3661238025356,18.5,1615,1215,420,"C3"]
[85557034,"ISOLATION CORPS 13-14 ELEMENTS",null,243,null,null,"/","/","/",3661238025349,20,1615,1215,420,"C3"]
[85557035,"ISOLATION CORPS 15 ELEMENTS",null,266,null,null,"/","/","/",3661238025332,22,1615,1215,420,"C3"]
[85557036,"ISOLATION CORPS 16-17 ELEMENTS",null,300,null,null,"/","/","/",3661238025325,22.5,1615,1215,420,"C3"]
[85557037,"ISOLATION CORPS 18-19 ELEMENTS",null,349,null,null,"/","/","/",3661238025318,24,1670,1260,610,"C3"]
[85557038,"ISOLATION CORPS 20 ELEMENTS",null,311,null,null,"/","/","/",3661238025301,25,1670,1260,610,"C3"]
[85557039,"ISOLATION CORPS 21-22 ELEMENTS",null,398,null,null,"/","/","/",3661238025295,27,1670,1260,610,"C3"]
[85557040,"ISOLATION CORPS 23-24 ELEMENTS",null,423,null,null,"/","/","/",3661238025288,28,1670,1260,610,"C3"]
[85557041,"ISOLATION CORPS 25 ELEMENTS",null,435,null,null,"/","/","/",3661238025271,29.5,1670,1260,610,"C3"]
[100013745,"COLIS DOC. TECHN. PKX-PKR 550/09","MS3",256,null,null,"/","/","/",3661238365797,1.2,3210,230,120,"C3"]
[100013747,"COLIS DOC. TECHN. PKX-PKR 550/10","MS4",256,null,null,"/","/","/",3661238365810,1.2,3210,230,120,"C3"]
[100013748,"COLIS DOC. TECHN. PKX-PKR 550/11","MS5",256,null,null,"/","/","/",3661238365827,1.2,3210,230,120,"C3"]
[100013749,"COLIS DOC. TECHN. PKX-PKR 550/12","MS6",256,null,null,"/","/","/",3661238365834,1.2,3210,230,120,"C3"]
[100013750,"COLIS DOC. TECHN. PKX-PKR 550/13","MS7",256,null,null,"/","/","/",3661238365841,1.2,3210,230,120,"C3"]
[100013751,"COLIS DOC. TECHN. PKX-PKR 550/14","MS8",256,null,null,"/","/","/",3661238365858,1.2,3210,230,120,"C3"]
[100013752,"COLIS DOC. TECHN. PKX-PKR 550/15","MS9",256,null,null,"/","/","/",3661238365865,1.2,3210,230,120,"C3"]
[100013753,"COLIS DOC. TECHN. PKX-PKR 550/16","MS10",256,null,null,"/","/","/",3661238365872,1.2,3210,230,120,"C3"]
[100013757,"COLIS DOC. TECHN. PKX-PKR 550/17","MS11",256,null,null,"/","/","/",3661238365896,1.2,3210,230,120,"C3"]
[100013758,"COLIS DOC. TECHN. PKX-PKR 550/18","MS12",266,null,null,"/","/","/",3661238365902,1.2,3210,230,120,"C3"]
[100013759,"COLIS DOC. TECHN. PKX-PKR 550/19","MS13",266,null,null,"/","/","/",3661238365919,1.2,3210,230,120,"C3"]
[100013760,"COLIS DOC. TECHN. PKX-PKR 550/20","MS14",266,null,null,"/","/","/",3661238365926,1.2,3210,230,120,"C3"]
[100013761,"COLIS DOC. TECHN. PKX-PKR 550/21","MS15",266,null,null,"/","/","/",3661238365933,1.2,3210,230,120,"C3"]
[100013762,"COLIS DOC. TECHN. PKX-PKR 550/22","MS16",266,null,null,"/","/","/",3661238365940,1.2,3210,230,120,"C3"]
[100013763,"COLIS DOC. TECHN. PKX-PKR 550/23","MS17",266,null,null,"/","/","/",3661238365957,1.2,3210,230,120,"C3"]
[100013764,"COLIS DOC. TECHN. PKX-PKR 550/24","MS18",266,null,null,"/","/","/",3661238365964,1.2,3210,230,120,"C3"]
[100013765,"COLIS DOC. TECHN. PKX-PKR 550/25","MS19",266,null,null,"/","/","/",3661238365971,1.2,3210,230,120,"C3"]
[100013680,"COLIS PANNEAU AVANT 9 A 17 ELMTS","MS1",847,null,null,"/","/","/",3661238365520,77,750,1270,420,"C3"]
[100013681,"COLIS PANNEAU AVANT 18 A 25 ELMTS","MS2",1063,null,null,"/","/","/",3661238365537,77,750,1270,420,"C3"]
[100007220,"JAQUETTE LATERALE AVANT 800 GT530","MR3",245,null,null,"/","/","/",3661238092822,57.5,870,1550,220,"C3"]
[100007221,"JAQUETTE LATERALE AVANT 940 GT530","MR4",336,null,null,"/","/","/",3661238092815,76.5,1020,1550,220,"C3"]
[100007222,"JAQUETTE LATERALE AVANT 1050 GT530","MR5",359,null,null,"/","/","/",3661238092808,74,1020,1550,220,"C3"]
[85557010,"JAQUETTE LATERALE ARRIERE 400","FA10",167,null,null,"/","/","/",3661238025523,18.25,1510,430,80,"C3"]
[85557011,"JAQUETTE LATERALE ARRIERE 600","FA11",212,null,null,"/","/","/",3661238025516,25.5,1510,630,100,"C3"]
[85557016,"JAQUETTE PIECES VARIABLES COMPL.","FA16",282,null,null,"/","/","/",3661238025509,26.5,1290,450,80,"C3"]
[85557017,"JAQUETTE PIECES VARIABLES  7 ELTS","FA17",349,null,null,"/","/","/",3661238025493,26,1290,450,80,"C3"]
[85557018,"JAQUETTE PIECES VARIABLES 8 ELTS","FA18",403,null,null,"/","/","/",3661238025486,27.5,1430,450,80,"C3"]
[85557019,"JAQUETTE PIECES VARIABLES 9 ELTS","FA19",431,null,null,"/","/","/",3661238025479,31,1550,450,80,"C3"]
[85557020,"JAQUETTE PIECES VARIABLES 10 ELTS","FA20",431,null,null,"/","/","/",3661238025462,32.5,1700,450,80,"C3"]
[85557021,"JAQUETTE PIECES VARIABLES 11 ELTS","FA21",431,null,null,"/","/","/",3661238025455,33.5,1740,450,80,"C3"]
[85557022,"JAQUETTE PIECES VARIABLES 12 ELTS","FA22",431,null,null,"/","/","/",3661238025448,36.5,1840,450,80,"C3"]
[85557023,"JAQUETTE PIECES VARIABLES 13 ELTS","FA23",431,null,null,"/","/","/",3661238025431,38.5,1940,450,80,"C3"]
[85557024,"JAQUETTE PIECES VARIABLES 14 ELTS","FA24",432,null,null,"/","/","/",3661238025424,41.5,2100,450,80,"C3"]
[85557025,"JAQUETTE PIECES VARIABLES 15 ELTS","FA25",434,null,null,"/","/","/",3661238025417,46,2340,450,80,"C3"]
[85557026,"JAQUETTE PIECES VARIABLES 16 ELTS","FA26",434,null,null,"/","/","/",3661238025400,46,2330,450,80,"C3"]
[85557027,"JAQUETTE PIECES VARIABLES 17 ELTS","FA27",434,null,null,"/","/","/",3661238025394,47,2340,450,80,"C3"]
[85558529,"CORPS ASSEMBLE 09 EL.",null,11613,null,null,"/","/","/",3661238024311,1980,1870,1060,1480,"C3"]
[85558530,"CORPS ASSEMBLE 10 EL.",null,12363,null,null,"/","/","/",3661238024304,2193,1980,1060,1480,"C3"]
[85558531,"CORPS ASSEMBLE 11 EL.",null,13165,null,null,"/","/","/",3661238024298,2373,2090,1060,1480,"C3"]
[85558532,"CORPS ASSEMBLE 12 EL.",null,13866,null,null,"/","/","/",3661238024281,2520,2200,1060,1480,"C3"]
[85558533,"CORPS ASSEMBLE 13 EL.",null,14673,null,null,"/","/","/",3661238024274,2750,2310,1060,1480,"C3"]
[85558534,"CORPS ASSEMBLE 14 EL.",null,15496,null,null,"/","/","/",3661238024267,2937,2420,1060,1480,"C3"]
[85558535,"CORPS ASSEMBLE 15 EL.",null,16155,null,null,"/","/","/",3661238024250,3122,2530,1060,1480,"C3"]
[85558536,"CORPS ASSEMBLE 16 EL.",null,17145,null,null,"/","/","/",3661238024243,3180,2640,1060,1480,"C3"]
[85558537,"CORPS ASSEMBLE 17 EL.",null,18479,null,null,"/","/","/",3661238024236,3360,2750,1060,1480,"C3"]
[85558538,"CORPS ASSEMBLE 18 EL.",null,19007,null,null,"/","/","/",3661238024229,3540,2860,1060,1480,"C3"]
[85558539,"CORPS ASSEMBLE 19 EL.",null,19971,null,null,"/","/","/",3661238024212,3831,2970,1060,1480,"C3"]
[85558540,"CORPS ASSEMBLE 20 EL.",null,20544,null,null,"/","/","/",3661238024205,4046,3080,1060,1480,"C3"]
[85558541,"CORPS ASSEMBLE 21 EL.",null,21879,null,null,"/","/","/",3661238024199,4230,3190,1060,1480,"C3"]
[85558542,"CORPS ASSEMBLE 22 EL.",null,22783,null,null,"/","/","/",3661238024182,4415,3300,1060,1480,"C3"]
[85558543,"CORPS ASSEMBLE 23 EL.",null,23751,null,null,"/","/","/",3661238024175,4596,3410,1060,1480,"C3"]
[85558544,"CORPS ASSEMBLE 24 EL.",null,24790,null,null,"/","/","/",3661238024168,4784,3520,1060,1480,"C3"]
[85558545,"CORPS ASSEMBLE 25 EL.",null,25765,null,null,"/","/","/",3661238024151,4800,3630,1060,1480,"C3"]
[82287750,"OUTILS DE CHAUF 7 A 10 ELTS",null,45,null,null,"/","/","/",3661238019782,4,140,65,1840,"C3"]
[82287751,"OUTILS DE CHAUF 11 A 15 ELTS",null,47,null,null,"/","/","/",3661238019775,5,null,null,null,"C3"]
[82287752,"OUTILS DE CHAUF 16 A 21 ELTS",null,64,null,null,"/","/","/",3661238019768,5,null,null,null,"C3"]
[82287753,"OUTILS DE CHAUF 22 ELTS",null,64,null,null,"/","/","/",3661238019751,5,null,null,null,"C3"]
[82287757,"OUTILS DE CHAUF 23 A 25 ELTS",null,69,null,null,"/","/","/",3661238019744,3,130,160,60,"C3"]
[100004380,"TABLEAU STANDARD OERTLI","MG1",325,3.34,"11.14","/","/","/",3661238111332,5.0599999999999996,800,200,200,"C3"]
[100004381,"TABLEAU R OERTLI","MG2",501,3.34,"11.14","/","/","/",3661238111325,10.39,830,430,270,"C3"]
[]
["OPTIONS"]
[100012592,"REA 060B",null,235,0.12,95010,"/","/","/",null,null,null,null,null,"C0"]
[125400,"REA  232B : POUR 2 CIRCUITS VANNE",null,1151,0.12,95010,"/","/","/",3661238108448,null,null,null,null,"C0"]
[125355,"STATION D'AMBIANCE","RES11",352,0.12,95010,"/","/","/",3661238108493,0.5,null,null,null,"C0"]
[125403,"SONDE WWF/ECS ( POUR TABLEAU AVEC REA)",null,49,0.02,95020,"/","/","/",3661238108431,null,null,null,null,"C0"]
[126490,"CABLAGE POUR 2è VANNE MELANGEUSE",null,76,0.02,95020,"/","/","/",3661238107496,null,null,null,null,"C0"]
[126624,"COMMANDE A DISTANCE ","RFF60",153,0.12,95010,"/","/","/",3661238107472,null,null,null,null,"C0"]
[82197729,"THERMOMETRE FUMEES    ","BP28",103,0.02,95020,"/","/","/",3661238020733,0.33,195,150,125,"C0"]
[126589,"OUTIL DE MONTAGE JD-TE Plus",null,3202,null,null,"/","/","/",3661238107489]
[]
["FAMILLE:","REGULATION TEMPERATURE EXTERIEURE"]
[]
[100018255,"OE-TRONIC 4 MR","AD282",1053,0.12,95010,"/","/","/",3661238514454,2,360,280,140,"C0"]
[]
["OPTIONS"]
[100018920,"BOITIER MURAL INTERFACE OTH/MIDBUS","AD286",139,0.12,95010,"/","/","/",3661238544918,1,213,113,100,"C0"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.16,200,150,30,"C0"]
[88017017,"SONDE DEPART v3v","AD199",80,0.02,95020,"/","/","/",3661238049185,0.21,150,200,40,"C0"]
[100013477,"CDE A DISTANCE FILAIRE RS 400   ","AD257",177,0.12,95010,"/","/","/",3661238364257,0.253,175,122,60,"C0"]
[100013472,"CDE A DISTANCE RADIO RS 400R     ","AD255",238,0.12,95010,"/","/","/",3661238364233,0.253,175,122,60,"C0"]
[100013307,"MODULE CHAUDIERE RADIO (EMETTEUR)","AD252",123,0.12,95010,"/","/","/",3661238363601,0.32,260,160,130,"C0"]
[100002803,"COMMANDE A DISTANCE SIMPLIFIEE AD208","AD208",104,0.12,95010,"/","/","/",3661238554931,null,null,null,null,"C0"]
[88017851,"CABLE DE LIAISON BUS LG 12 M","AD134",110,0.12,95010,"/","/","/",3661238048850,0.37,350,260,30,"C0"]
[100013305,"COLIS SONDE SYSTÈME OE-TRONIC 4","AD250",46,0.02,95020,"/","/","/",3661238363588,0.13400000000000001,150,210,25,"C0"]
[100013306,"SONDE EXTERIEURE RADIO ","AD251",77,0.12,95010,"/","/","/",3661238363595,0.15,150,210,40,"C0"]
[100013307,"MODULE CHAUDIERE RADIO (EMETTEUR)","AD252",123,0.12,95010,"/","/","/",3661238363601,0.32,260,160,130,"C0"]
[88017878,"MODULE DE TELESURVEILLANCE VOCAL TELCOM 2","AD152",704,0.12,95010,"/","/","/",3661238048751,1.05,210,190,105,"C0"]
[88017836,"CABLE BUS RX11  LG 1,5 M","AD124",84,0.02,95020,"/","/","/",3661238048911,0.06,210,160,5,"C0"]
[81997720,"CABLE LIAIS.CDI 40M ","DB119",149,0.02,95020,"/","/","/",3661238001350,1.34,310,215,130,"C0"]
[85757741,"SONDE EXTERIEURE","FM46",41,0.02,95020,"/","/","/",3661238022751,0.12,200,150,40,"C0"]
[7618086,"INTERFACE MODBUS+MOD.INTERNET OE",null,417,0.12,95010,"/","/","/",null,1.6,315,310,115,"prix net"]
[]
[]
[88017904,"THERMOSTAT AMBIANCE PROGRAMMABLE","AD191",161,0.12,95010,"/","/","/",3661238102415,0.25,135,90,55,"C0"]
[88017010,"THERMOSTAT D'AMBIANCE PROGRAMMABLE (SANS FILS)","AD192",286,0.12,95010,"/","/","/",3661238102439,0.42499999999999999,180,150,90,"C0"]
[100000030,"COLIS OPTION SONDE ECS","AD212",49,0.02,95020,"/","/","/",3661238011168,0.16,200,150,30,"C0"]
[88017017,"SONDE DEPART v3v","AD199",80,0.02,95020,"/","/","/",3661238049185,0.21,150,200,40,"C0"]
[88017014," PLATINE + SONDE V3V","AD196",180,0.02,95020,"/","/","/",3661238102422,0.52,260,170,120,"C0"]
[161118," COMMANDE A DISTANCE INTERACTIVE  ","AD194",197,0.12,95010,"/","/","/",3661238106505,0.15,0,0,0,"C0"]
[100002803,"COMMANDE A DISTANCE SIMPLIFIEE AD208","AD208",104,0.12,95010,"/","/","/",3661238554931,0.2,120,85,40,"C0"]
[85757742,"SONDE FUMEES","FM47",72,0.02,95020,"/","/","/",3661238022744,0.17,210,160,40,"C0"]
[88017851,"CABLE DE LIAISON BUS LG 12 M","AD134",110,0.02,95020,"/","/","/",3661238048850,0.37,350,260,30,"C0"]
[88017887,"ENSEMBLE DE 2 SONDES SOLAIRES","AD160",97,0.02,95020,"/","/","/",3661238048720,0.21,210,170,40,"C7"]
[100012352,"COLIS OETRONIC 3 MR ","AD243",1605,0.12,95010,"/","/","/",3661238554955,2.52,null,null,null,"C0"]
[]
[]
[125392,"REA-130B POUR 1 CIRCUIT",null,665,0.12,95010,"/","/","/",3661238108486,null,null,null,null,"C0"]
[125394,"REA-131B POUR 2 CIRCUITS",null,856,0.12,95010,"/","/","/",3661238108479,null,null,null,null,"C0"]
[125400,"REA  232B : POUR 2 CIRCUITS VANNE",null,1151,0.12,95010,"/","/","/",3661238108448,null,null,null,null,"C0"]
[100012592,"REA 060B",null,235,0.12,95010,"/","/","/",null,null,null,null,null,"C0"]
[125355,"STATION D'AMBIANCE","RES11",352,0.12,95010,"/","/","/",3661238108493,0.5,null,null,null,"C0"]
[125403,"SONDE WWF/ECS ( POUR TABLEAU AVEC REA)",null,49,0.02,95020,"/","/","/",3661238108431,null,null,null,null,"C0"]
[126624,"COMMANDE A DISTANCE ","RFF60",153,0.12,95010,"/","/","/",3661238107472,null,null,null,null,"C0"]
[126490,"CABLAGE POUR 2è VANNE MELANGEUSE",null,76,0.02,95020,"/","/","/",3661238107496,null,null,null,null,"C0"]
[]
["FAMILLE:","EQUIPEMENTS  DE CHAUFFERIE"]
[]
[7650329,"PURGEUR RP 1/2","SA16",57,null,null,null,null,null,3661238657441,0.7,150,85,75,"C0"]
[7650330,"DEGAZEUR MICROBULLES RP 5/4 ","SA17",119,null,null,null,null,null,3661238657458,1.3,230,100,75,"C0"]
[7650333,"DEGAZEUR MICROBULLES RP 1_1/2 ","SA18",135,null,null,null,null,null,3661238657465,1.6,265,100,75,"C0"]
[7650334,"DEGAZEUR MICROBULLES RP 2","SA19",379,null,null,null,null,null,3661238657472,3.6,305,165,130,"C0"]
[7650336,"DEGAZEUR MICROBULLES DN50/PN16","SA20",960,null,null,null,null,null,3661238657489,14,570,376,223,"C0"]
[7650338,"DEGAZEUR MICROBULLES DN65/PN16","SA21",991,null,null,null,null,null,3661238657496,15,570,376,223,"C0"]
[7650339,"DEGAZEUR MICROBULLES DN80/PN16","SA22",1358,null,null,null,null,null,3661238657502,16,685,480,240,"C0"]
[7650340,"DEGAZEUR MICROBULLES DN100/PN16","SA23",1413,null,null,null,null,null,3661238657519,19,685,480,240,"C0"]
[7660261,"DEGAZEUR MICROBULLES DN125/PN16 S","SA42",3339,null,null,null,null,null,3661238667815,60,888,774,526,"C0"]
[]
["SEPARATEUR AVEC BARREAU MAGNETIQUE "]
[7650376,"SEPARATEUR BOUES A AIMANT RP 1_1/4","SA24",162,null,null,null,null,null,3661238657526,1.29,205,100,75,"C0"]
[7650377,"SEPARATEUR BOUES A AIMANT RP 1_1/2 ","SA25",171,null,null,null,null,null,3661238657533,1.45,240,100,75,"C0"]
[7650378,"SEPARATEUR BOUES A AIMANT RP 2 S","SA26",410,null,null,null,null,null,3661238657540,3.5,250,160,130,"C0"]
[]
[7651722,"SEPARATEUR AVEC BARREAU MAGNETIQUE DN65",null,{"$f":"D5055+D5059","v":1357},null,null,null,null,null,3661238659735,null,null,null,null,"C0"]
[7651730,"SEPARATEUR AVEC BARREAU MAGNETIQUE DN80",null,{"$f":"D5056+D5059","v":1728},null,null,null,null,null,3661238659742,null,null,null,null,"C0"]
[7651732,"SEPARATEUR AVEC BARREAU MAGNETIQUE DN100",null,{"$f":"D5057+D5059","v":1778},null,null,null,null,null,3661238659759,null,null,null,null,"C0"]
[7651733,"SEPARATEUR AVEC BARREAU MAGNETIQUE DN125",null,{"$f":"D5058+D5060","v":3055},null,null,null,null,null,3661238659766,null,null,null,null,"C0"]
[]
["COMPOSANTS"]
[7650381,"SEPARATEUR BOUES DN65/PN16","SA27",892,null,null,null,null,null,3661238657557,15,570,376,223,"C0"]
[7650382,"SEPARATEUR BOUES DN80/PN16 ","SA28",1263,null,null,null,null,null,3661238657564,16,685,490,240,"C0"]
[7650383,"SEPARATEUR BOUES DN100/PN16","SA29",1313,null,null,null,null,null,3661238657571,19,685,490,240,"C0"]
[7650384,"SEPARATEUR BOUES DN125/PN16","SA30",2531,null,null,null,null,null,3661238657588,60,888,774,526,"C0"]
[7650386,"BARREAU MAGNETIQUE POUR DN50 A 100","SA31",465,null,null,null,null,null,3661238657595,0.8,452,107,107,"C0"]
[7650387,"BARREAU MAGNETIQUE POUR DN125","SA32",524,null,null,null,null,null,3661238657601,0.8,452,107,107,"C0"]
[]
[7651695,"SEPAR.BOUES DERIV./CIRC.4M3_H DN32","SA33",2025,null,null,null,null,null,3661238659650,13,680,540,1100,"C0"]
[7651698,"SEPAR.BOUES DERIV./CIRC.9M3_H DN32","SA34",3509,null,null,null,null,null,3661238659667,50,1200,800,900,"C0"]
[]
[7651699,"POCHE 25 MICRON ","SA35",32,null,null,null,null,null,3661238659674,0.06,350,180,20,"C0"]
[7651700,"JOINT TORIQUE POUR SEPARATEUR SA33","SA36",11,null,null,null,null,null,3661238659681,0.02,150,150,3,"C0"]
[7651701,"POCHE 50 MICRON","SA37",16,null,null,null,null,null,3661238659698,7.0000000000000007E-2,250,150,150,"c0"]
[7651702,"JOINT TORIQUE POUR SEPARATEUR SA34","SA38",16,null,null,null,null,null,3661238659704,0.01,150,150,5,"C0"]
[]
[7651703,"SOLUTECH LESSIVAGE/DESEMBOUAGE","SA39",611,null,null,null,null,null,3660965332959,21,270,230,420,"C0"]
[7651705,"SOLUTECH PROTECTION INTEGRALE","SA40",611,null,null,null,null,null,3660965332942,21,270,230,420,"C0"]
[7651707,"KIT PRELEVEMT EAU CHAUF./EAU VILLE ","SA41",66,null,null,null,null,null,3661238659810,0.2,120,35,85,"C0"]
[]
["FAMILLE:","EAU CHAUDE SANITAIRE"]
[]
[]
[89529086,"PREPARATEUR OBD 150","GM29",1517,null,null,"/","/","/",3661238102408,101,695,910,1040,"C0"]
[89527720,"COLIS RENFORT","EA82",59,null,null,"/","/","/",3661238047839,1.79,615,170,120,"C0"]
[100002340,"BALLON OBC 162/TA + PANNEAU AVANT",null,{"$f":"+D5080+D5081","v":1673},null,null,"/","/","/",3661238111981,null,null,null,null,"C0"]
[100001610,"OBC 162 /TA","BH105",1517,null,null,"/","/","/",3661238112780,94.5,680,680,1110,"C0"]
[89557702,"PANNEAU AVANT","BH87",156,null,null,"/","/","/",3661238102361,3.85,680,640,100,"C0"]
[100002341,"BALLON OBC 252/TA + PANNEAU AVANT",null,{"$f":"+D5083+D5084","v":2016},null,null,"/","/","/",3661238111974,null,null,null,null,"C0"]
[100001611,"OBC 252 /TA","BH106",1860,null,null,"/","/","/",3661238112773,123,680,680,1480,"C0"]
[89557702,"PANNEAU AVANT","BH87",156,null,null,"/","/","/",3661238102361,3.85,680,640,100,"C0"]
[100009972,"BALLON OBA 150","EA84",1508,null,null,"/","/","/",3661238375239,106.5,700,900,1290,"C0"]
[]
["OPTIONS"]
[100000492,"KIT ANODE MAGNESIUM","EA103",66,null,null,"/","/","/",3661238011069,0.9,560,90,85,"C0"]
[89997049,"KIT DE LIAISION GS 140 - OBD 150","EA92",456,null,null,"/","/","/",3661238044463,7,575,505,140,"C0"]
[100006328,"KIT DE LIAISON GSR 140 P - OBD 150","EA113",444,null,null,"/","/","/",3661238100954,4.5,575,500,140,"C0"]
[89557001,"COLIS TUBULURE PK-PU-CU 150 / OBC 162/252","BH73",456,null,null,"/","/","/",3661238047600,6,575,500,135,"C0"]
[89557002,"COLIS TUBULURE PK-PU-CU 150 / OBC 162/252","BH75",456,null,null,"/","/","/",3661238047594,6,575,500,135,"C0"]
[89997045,"TUB. LIAISON OBC/PKR 250","BH93",456,null,null,"/","/","/",3661238044494,6.5,575,505,140,"C0"]
[89557010,"KIT ENSEMBLE CHAUFFANT 2400 W ","BH88",565,null,null,"/","/","/",3661238102378,3.2,660,215,215,"C0"]
[89557009,"KIT DE TRANSFORMATION G/R 3/4 '' ET 1 ''","BH84",32,null,null,"/","/","/",3661238047563,0.32500000000000001,200,140,45,"C0"]
[]
[]
["PREPARATEUR EMAILLE HAUTES \"PERFORMANCE\" OBPB"]
[100019196,"PREPARATEUR VERTICAL OBPB 150","EC624",1401,null,null,"/","C stockage \nECS",null,3661238551121,68,900,800,1093,"C0"]
[100019197,"PREPARATEUR VERTICAL OBPB 200","EC625",1556,null,null,"/","C stockage \nECS",null,3661238551138,85,900,800,1363,"C0"]
[100019198,"PREPARATEUR VERTICAL OBPB 300","EC626",1984,null,null,"/","C stockage \nECS",null,3661238551145,110,900,800,1883,"C0"]
[100019199,"PREPARATEUR VERTICAL OBPB 400","EC627",2902,null,null,"/","C stockage \nECS",null,3661238551152,146,980,850,1771,"C0"]
[100019200,"PREPARATEUR VERTICAL OBPB 500","EC628",3187,null,null,"/","C stockage \nECS",null,3661238551169,173,980,850,1889,"C0"]
[]
["PREPARATEUR  OBLC   (Oertli Priméa)"]
[100018187,"PREPARATEUR VERTICAL OBLC 150","EC614",1141,null,null,"/","C stockage \nECS",null,3661238548114,68,900,800,1110,"C0"]
[100018188,"PREPARATEUR VERTICAL OBLC 200","EC615",1310,null,null,"/","C stockage \nECS",null,3661238548121,85,900,800,1380,"C0"]
[100018189,"PREPARATEUR VERTICAL OBLC 300","EC616",1611,null,null,"/","C stockage \nECS",null,3661238548138,11,900,800,1900,"C0"]
[100018190,"PREPARATEUR VERTICAL OBLC 400","EC617",2417,null,null,"/","C stockage \nECS",null,3661238548145,146,380,860,1820,"C0"]
[100018191,"PREPARATEUR VERTICAL OBLC 500","EC618",2598,null,null,"/","C stockage \nECS",null,3661238548152,173,980,860,1910,"C0"]
[]
["OPTIONS"]
[100007832,"REGULATION POMPE DE CHARGE SLA 2","EC320",208,0.12,95010,"/","/","/",3661238101494,0.66,225,195,85,"C0"]
[100010652,"KIT OECOPROTEC avec OETRONIC, jusqu'à 300 L","EC431",123,null,null,"/","/","/",3661238364745,0.49,255,170,120,"C7"]
[126765,"ANODE ACI CORREX UP BALLON > 300 LITRES","AM7",532,0.02,95020,"/","/","/",3661238047440,0.44,425,100,55,"C0"]
[163179,"ANODE A COURANT IMPOSE (150 A 300L)","AJ38",306,0.02,95020,"/","/","/",3661238046849,0.35,250,95,50,"C0"]
[100020083,"KIT RESISTANCE ELECTRIQUE 3 KW","ER336",392,null,null,"/","/","/",3661238573314,2.8,1210,190,140,"C0"]
[]
["KITS DE LIAISON"]
[100007834,"KIT DE LIAISON PKR-PUR / OB (<=300 L)","EA116",525,null,null,"/","/","/",3661238113350,7,600,500,135,"C0"]
[100007835,"KIT LIAISON PK264-6","EA117",525,null,null,"/","/","/",3661238113312,6.5,600,500,135,"C0"]
[100007837,"KIT LIAISON CHAUDIERE / BALLON","EA119",602,null,null,"/","/","/",3661238113336,7,600,500,135,"C0"]
[100007836,"TUBULURE GSR 230 - PKR256 à 258/OB(<=300)  ","EA118",525,null,null,"/","/","/",3661238113343,6.5,600,500,135,"C0"]
[100007827,"KIT LIAISON CHAUDIERE / BALLON","EA121",602,null,null,"/","/","/",3661238116528,6.5,600,500,135,"C0"]
[100015479,"VANNE INVERSION CHAUFF/SANITAIRE + SONDE ECS","EH145",335,null,null,"/","/","/",3661238381605,4.2,410,210,125,"C6"]
[]
[]
["CUVE"]
[7650480,"BALLON B 650","AJ78",2961,null,null,"/","/","/",3661238351523,280,1200,1200,1940,"C0"]
[7650481,"BALLON B 800","AJ79",3961,null,null,"/","/","/",3661238166394,287,1000,990,2345,"C0"]
[7650482,"BALLON B 1000","AJ80",4390,null,null,"/","/","/",3661238166387,384,900,900,2400,"C0"]
[7650483,"BALLON B 1500","AJ81",4799,null,null,null,null,null,3661238657779,378,1970,1500,1023,"C0"]
[7650484,"BALLON B 2000","AJ82",5003,null,null,null,null,null,3661238657786,399,1780,1329,2162,"C0"]
[7650485,"BALLON B 2500","AJ83",6126,null,null,null,null,null,3661238657793,510,1590,2200,2019,"C0"]
[7650486,"BALLON B 3000","AJ84",6432,null,null,null,null,null,3661238657809,532,1590,2200,2186,"C0"]
[]
["HABILLAGE SEMI RIGIDE"]
[7650496,"JAQUETTE RIGIDE 650 TP B/RSB ","AJ94",613,null,null,null,null,null,3661238657908,34,1250,1120,1697,"C0"]
[7650497,"JAQUETTE RIGIDE 800 TP B/RSB","AJ95",633,null,null,null,null,null,3661238657915,36,1250,1120,2024,"C0"]
[7650499,"JAQUETTE RIGIDE 1000 TP B/RSB ","AJ97",715,null,null,null,null,null,3661238657939,39,1970,1500,2023,"C0"]
[7650502,"JAQUETTE RIGIDE 1500 TP B/RSB ","AJ99",1123,null,null,null,null,null,3661238657953,44,1590,2200,2019,"C0"]
[7650506,"JAQUETTE RIGIDE 2000 TP B/RSB ","AJ101",1327,null,null,null,null,null,3661238657977,49,1250,1120,2024,"C0"]
[7650508,"JAQUETTE RIGIDE 2500 TP B/RSB ","AJ103",1532,null,null,null,null,null,3661238657991,54,1970,1500,2023,"C0"]
[7650511,"JAQUETTE RIGIDE 3000 TP B/RSB ","AJ105",1736,null,null,null,null,null,3661238658219,61,1590,2200,2019,"C0"]
[]
["HABILLAGE RIGIDE (classement au feu MO)"]
[7650583,"JAQUETTE RIGIDE M0 800 TP B/RSB","AJ141",1378,null,null,null,null,null,3661238658653,41,1860,800,550,"C0"]
[7650584,"JAQUETTE RIGIDE M0 1000 TP B/RSB","AJ142",1532,null,null,null,null,null,3661238658660,44,2080,800,550,"C0"]
[7650585,"JAQUETTE RIGIDE M0 1500 TP B/RSB","AJ143",1991,null,null,null,null,null,3661238658677,70,2030,1040,570,"C0"]
[7650587,"JAQUETTE RIGIDE M0 2000 TP B/RSB","AJ144",2144,null,null,null,null,null,3661238658684,76,2250,1040,570,"C0"]
[7650589,"JAQUETTE RIGIDE M0 2500 TP B/RSB","AJ145",2553,null,null,null,null,null,3661238658691,80,2250,1040,570,"C0"]
[7650590,"JAQUETTE RIGIDE M0 2500 TP B/RSB","AJ146",2604,null,null,null,null,null,3661238658707,86,2250,1040,570,"C0"]
[]
["OPTIONS"]
[89757750,"RESISTANCE BLINDEE 6 KW/400V A VISSER 1''1/2","AJ36",628,null,null,"/","/","/",3661238046863,2.4700000000000002,695,170,180,"C0"]
[100019313,"KIT ELECTRIQUE 9 KW/400V 1 1/2 ( POUR RSB 1000 A 3000 )","AJ47",650,null,null,"/","/","/",3661238553316,4.5,695,170,180,"C7"]
[100019314,"KIT ELECTRIQUE 12 KW/400V  1 1/2  ( POUR RSB 1500 A 3000 )","ER335",728,null,null,"/","/","/",3661238553323,2.8,1210,190,140,"C7"]
[7651086,"RESIST. BLIND. 9 KW 400V  DN110 ","AJ164",500,null,null,null,null,null,3661238659179,7.1,760,493,190,"C0"]
[7651088,"RESIST. BLIND. 9 KW 400V  DN110 ","AJ165",582,null,null,null,null,null,3661238659179,7.1,760,493,190,"C0"]
[7651116,"RESIST.B.30KW400V DN110 SUP.800L ","AJ166",664,null,null,null,null,null,3661238659193,10.1,760,493,190,"C0"]
[89608920,"ANODE ACI CORREX UP BALLON > 300 LITRES","AM7",532,0.02,95020,"/","/","/",3661238047440,0.44,425,100,55,"C0"]
[89757746,"THERMOMETRE","AJ32",51,null,null,"/","/","/",3661238046887,0.18,145,190,125,"C0"]
[7651078,"DOIGT DE GANT 350 MM 1/2 ","AJ162",36,null,null,null,null,null,3661238659155,1.1000000000000001,54,54,560,"C0"]
[7651082,"BRIDE LATERALE 110 A EMBOUT 1_1/2","AJ163",286,null,null,null,null,null,3661238659162,3.6,315,315,190,"C0"]
[]
[]
["MODULES ECS INSTANTANEE FWM COMPLET"]
[7606029,"MODULE ECS INST 3 M3 FWM 50-170","EC682",3711,null,null,"/","/","/",3661238584860,45,880,650,300,"C7"]
[7606142,"MODULE ECS INST 4 M3 FWM 70-240","EC683",4240,null,null,"/","/","/",3661238584877,52,880,650,300,"C7"]
[]
[7606152,"GROUPE DE RECIRCULATION 2M3 DN20 FWM","EC689",478,null,null,"/","/","/",3661238584938,8,350,250,200,"C7"]
[7618250,"GROUPE DE RECIRCULATION 3M3 DN32 FWM","EC685",1113,null,null,"/","/","/",3661238604025,13,1200,300,200,"C7"]
[7618251,"KIT CASCADE DN 25 2 FWM 50","EC690",1272,null,null,"/","/","/",3661238604032,13,1200,300,200,"C7"]
[7618252,"KIT CASCADE DN 32 2 FWM 70","EC691",1802,null,null,"/","/","/",3661238604049,18,1200,300,200,"C7"]
[7606147,"VANNE 3 VOIES DN25 FWM50 ET SONDES ","EC686",372,null,null,"/","/","/",3661238584907,3,150,150,100,"C7"]
[7606150,"VANNE 3 VOIES DN32 FWM70 ET SONDES ","EC687",478,null,null,"/","/","/",3661238584914,4,150,150,100,"C7"]
[]
["FAMILLE:","STOCKAGE DE L'EAU DE CHAUFFAGE"]
[]
[]
["CUVE"]
[7650454,"BALLON PSB 600 ","AJ52",1021,null,null,null,null,null,3661238657311,109,1165,950,2033,"C0"]
[7650455,"BALLON PSB 800","AJ53",1103,null,null,null,null,null,3661238657328,141,1250,1120,1930,"C0"]
[7650456,"BALLON PSB 1000","AJ54",1225,null,null,null,null,null,3661238657335,162,1250,1120,2171,"C0"]
[7650457,"BALLON PSB 1500","AJ55",1634,null,null,null,null,null,3661238657342,323,1970,1500,2007,"C0"]
[7650458,"BALLON PSB 2000","AJ56",2144,null,null,null,null,null,3661238657359,348,1780,1329,2176,"C0"]
[7650459,"BALLON PSB 2500","AJ57",2348,null,null,null,null,null,3661238657366,427,1590,2200,2040,"C0"]
[7650460,"BALLON PSB 300","AJ58",2757,null,null,null,null,null,3661238657373,457,1590,2200,2198,"C0"]
[]
["HABILLAGE RIGIDE (HR)"]
[7650489,"JAQUETTE RIGIDE 600 PS/PSE ","AJ87",613,null,null,null,null,null,3661238657830,31,1165,950,2033,"C0"]
[7650490,"JAQUETTE RIGIDE 800 PS/PSE ","AJ88",633,null,null,null,null,null,3661238657847,35,1250,1120,1930,"C0"]
[7650491,"JAQUETTE RIGIDE 1000 PS/PSE ","AJ89",715,null,null,null,null,null,3661238657854,39,1250,1120,2171,"C0"]
[7650492,"JAQUETTE RIGIDE 1500 PS/PSE ","AJ90",1123,null,null,null,null,null,3661238657861,44,1950,1500,2037,"C0"]
[7650493,"JAQUETTE RIGIDE 2000 PS/PSE ","AJ91",1327,null,null,null,null,null,3661238657878,49,1780,1329,2176,"C0"]
[7650494,"JAQUETTE RIGIDE 2500 PS/PSE ","AJ92",1532,null,null,null,null,null,3661238657885,54,1590,2200,2035,"C0"]
[7650495,"JAQUETTE RIGIDE 3000 PS/PSE ","AJ93",1736,null,null,null,null,null,3661238657892,61,1590,2200,2197,"C0"]
[]
["HABILLAGE SOUPLE (HS)"]
[7650513,"JAQUETTE SOUPLE M1 600 PS/PSE","AJ107",306,null,null,null,null,null,3661238658233,33,1840,1260,210,"C0"]
[7650514,"JAQUETTE SOUPLE M1 800 PS/PSE","AJ108",306,null,null,null,null,null,3661238658240,37,1750,1230,230,"C0"]
[7650526,"JAQUETTE SOUPLE M1 1000 PS/PSE","AJ109",408,null,null,null,null,null,3661238658257,41,2090,1200,260,"C0"]
[7650527,"JAQUETTE SOUPLE M1 1500 PS/PSE","AJ110",715,null,null,null,null,null,3661238658264,47,1900,1180,350,"C0"]
[7650528,"JAQUETTE SOUPLE M1 2000 PS/PSE","AJ111",817,null,null,null,null,null,3661238658271,50,2110,1370,300,"C0"]
[7650529,"JAQUETTE SOUPLE M1 2500 PS/PSE","AJ112",919,null,null,null,null,null,3661238658288,57,1900,1200,420,"C0"]
[7650532,"JAQUETTE SOUPLE M1 3000 PS/PSE","AJ113",1021,null,null,null,null,null,3661238658295,62,2060,1270,420,"C0"]
[]
["FAMILLE:","BRULEUR  FIOUL"]
[]
[]
["107140FA","OES-151L EV",null,{"$f":"+D5217+D5221+D5223","v":1202},null,null,"Pas concerné par l'étiquettage",null,null,3661238109124,14,500,300,385,"B0"]
["107141FA","OES 151L E",null,{"$f":"+D5218+D5221+D5223","v":1047},null,null,"Pas concerné par l'étiquettage",null,null,3661238109100,14,500,300,385,"B0"]
["107300FA","OES-152L E",null,{"$f":"+D5219+D5221+D5223","v":1047},null,null,"Pas concerné par l'étiquettage",null,null,3661238109018,14,500,300,385,"B0"]
[100005322,"OES 153 LE",null,{"$f":"D5220+D5222","v":1134},null,null,"Pas concerné par l'étiquettage",null,null,null,14,500,300,385,"B1"]
[]
["COMPOSANTS"]
[107140,"OES-151L EV",null,1194,null,null,"/","/","/",3661238109131,14,500,300,385,"B0"]
[107141,"OES 151L E",null,1039,null,null,"/","/","/",3661238109117,14,500,300,385,"B0"]
[107300,"OES-152L E",null,1039,null,null,"/","/","/",3661238109025,14,500,300,385,"B0"]
[100005070,"OES 153 LE",null,1126,null,null,"/","/","/",3661238582613,14,500,300,385,"B1"]
[107177,"NOTICE BRULEUR OES 151/152",null,0,null,null,"/","/","/",3661238109070,null,null,null,null,"B2"]
[100006710,"NOTICE BRULEUR OES 153+ pse Wieland",null,8,null,null,"/","/","/",null,null,null,null,null,"B1"]
[83176,"PRISE WIELAND MALE 7P ",null,8,null,null,"/","/","/",3661238113114,null,null,null,null,"B1"]
[]
[]
["108786FA","OEN-151-1 LEV + Prise",null,{"$f":"D5230+D5232+D5233","v":1466},null,null,"Pas concerné par l'étiquettage",null,null,3661238108684,14,800,305,400,"B1"]
["107840FA","OEN-155 L EV + Prise",null,{"$f":"D5231+D5232+D5233","v":1594},null,null,"Pas concerné par l'étiquettage",null,null,3661238108905,14,800,305,400,"B1"]
[]
["COMPOSANTS"]
[108786,"OEN-151-1 LEV",null,1458,null,null,"/","/","/",3661238108691,14,800,305,400,"B1"]
[107840,"OEN-155 L EV ",null,1586,null,null,"/","/","/",3661238108912,14,800,305,400,"B1"]
[107331,"NOTICE BRULEUR",null,0,null,null,"/","/","/",3661238109001,null,null,null,null,"B1"]
[83176,"PRISE WIELAND MALE 7P ",null,8,null,null,null,null,null,3661238113114,null,null,null,null,"B1"]
[]
["OPTIONS"]
[602523,"CONTRE-PLAQUE PERCAGE 120/DIX.150",null,84,null,null,"/","/","/",3661238106208,1,null,null,null,"B1"]
[100012500,"FILTRE DEGAZEUR TIGERLOOP COMBI",null,135,null,null,"/","/","/",null,1.4,null,null,null,"B1"]
[]
[]
[100010370,"OECO FIRST OEX 4",null,{"$f":"SUM(D5243:D5245)","v":787},null,null,null,null,null,null,null,null,null,null,"B3"]
[]
["COMPOSANTS"]
[100009280,"OEX 4",null,766,null,null,null,null,null,3661238649026,14,null,null,null,"B3"]
[100010374,"SACHET NOTICE ",null,0,null,null,null,null,null,null,null,null,null,null,"B3"]
[7615461,"GICLEUR ",null,21,null,null,null,null,null,3661238601918,0.2,null,null,null,"B3"]
[]
[]
["107936FA","OES 255 LE ",null,{"$f":"D5255+D5259+D5261","v":1253},null,null,"Pas concerné par l'étiquettage",null,null,3661238108882,17,800,305,400,"B1"]
["107938FA","OES 255 LZ",null,{"$f":"D5256+D5259+D5261+D5260","v":1854},null,null,"Pas concerné par l'étiquettage",null,null,3661238108868,18,800,305,400,"B1"]
[]
[]
["107188FA","OEN 251 LE",null,{"$f":"D5257+D5259+D5261","v":2200},null,null,"Pas concerné par l'étiquettage",null,null,3661238109049,18,800,305,400,"B1"]
[]
["COMPOSANTS"]
[107936,"OES 255 LE",null,1245,null,null,"/","/","/",3661238108899,17,800,305,400,"B1"]
[107938,"OES 255 LZ",null,1839,null,null,"/","/","/",3661238108875,18,800,305,400,"B1"]
[100019686,"OEN 251 LE",null,2192,null,null,"/","/","/",3661238109056,18,800,305,400,"B1"]
[108481,"NOTICE OES 250",null,null,null,null,"/","/","/",3661238108769,null,null,null,null,"B2"]
[108494,"NOTICE OEN 250",null,null,null,null,"/","/","/",3661238108752,null,null,null,null,"B2"]
[83191,"PRISE WIELAND MALE 4P ",null,7,null,null,"/","/","/",3661238113107,null,null,null,null,"B1"]
[83176,"PRISE WIELAND MALE 7P ",null,8,null,null,"/","/","/",3661238113114,null,null,null,null,"B1"]
[]
[]
[100004980,"OES 352 LE",null,{"$f":"D5274+D5282","v":1295},null,null,"Pas concerné par l'étiquettage",null,null,3661238109858,24,780,370,420,"B1"]
[100004981,"OES 353 LE",null,{"$f":"D5275+D5282","v":1503},null,null,"Pas concerné par l'étiquettage",null,null,3661238109841,24,780,370,420,"B1"]
[100004982,"OES 354 LE",null,{"$f":"D5276+D5282","v":1568},null,null,"Pas concerné par l'étiquettage",null,null,3661238109834,24,780,370,420,"B1"]
[100004984,"OES 352 LZ",null,{"$f":"D5277+D5282","v":1844},null,null,"Pas concerné par l'étiquettage",null,null,3661238109827,25,780,370,420,"B1"]
[100004985,"OES 353 LZ",null,{"$f":"D5278+D5282","v":1912},null,null,"Pas concerné par l'étiquettage",null,null,3661238109810,25,780,370,420,"B1"]
[100004986,"OES 354 LZ",null,{"$f":"D5279+D5282","v":1980},null,null,"Pas concerné par l'étiquettage",null,null,3661238109803,25,780,370,420,"B1"]
[100004987,"OES 355 LZ",null,{"$f":"D5280+D5282","v":2116},null,null,"Pas concerné par l'étiquettage",null,null,3661238109797,33,900,370,500,"B1"]
[100004988,"OES 356 LZ",null,{"$f":"D5281+D5282","v":2390},null,null,"Pas concerné par l'étiquettage",null,null,3661238109780,33,900,370,500,"B1"]
[]
["COMPOSANTS"]
[100004070,"OES 352 LE",null,1282,null,null,"/","/","/",3661238111509,24,780,370,420,"B1"]
[100004071,"OES 353 LE",null,1490,null,null,"/","/","/",3661238111493,24,780,370,420,"B1"]
[100004072,"OES 354 LE",null,1555,null,null,"/","/","/",3661238111486,24,780,370,420,"B1"]
[100004074,"OES 352 LZ",null,1831,null,null,"/","/","/",3661238111479,25,780,370,420,"B1"]
[100004075,"OES 353 LZ",null,1899,null,null,"/","/","/",3661238111462,25,780,370,420,"B1"]
[100004076,"OES 354 LZ",null,1967,null,null,"/","/","/",3661238111455,25,780,370,420,"B1"]
[100004077,"OES 355 LZ",null,2103,null,null,"/","/","/",3661238111448,33,900,370,500,"B1"]
[100003700,"OES 356 LZ",null,2377,null,null,"/","/","/",3661238111660,33,900,370,500,"B1"]
[100004999,"Sachet DOCUMENTATION OES 350 L FR (notice + 2 prises W)",null,13,null,null,"/","/","/",3661238109681,0.2,null,null,null,"B2"]
[]
["OPTIONS"]
[602523,"CONTRE-PLAQUE PERCAGE 120/DIX.150",null,84,null,null,"/","/","/",3661238106208,1,200,200,5,"B1"]
[602519,"CONTRE-PLAQUE PERCAGE 130/DIX.170",null,78,null,null,"/","/","/",3661238001770,3,260,260,6,"B1"]
[88027180,"CAISSON INSONORISANT POUR 350",null,1573,null,null,"/","/","/",3661238048270,47,515,640,910,"B1"]
[]
[]
["105617FA","OES-441-1 LZ",null,{"$f":"D5297+D5298+D5308+D5309","v":2631},null,null,"Pas concerné par l'étiquettage",null,null,3661238109254,63,1190,550,535,"B1"]
["106124FA","OES-441-2 LZ",null,{"$f":"D5299+D5300+D5308+D5309","v":3181},null,null,"Pas concerné par l'étiquettage",null,null,3661238109223,63,1190,550,535,"B1"]
["105518FA","OES-441-3 LZ",null,{"$f":"D5301+D5302+D5308+D5309","v":3407},null,null,"Pas concerné par l'étiquettage",null,null,3661238109315,69,1190,550,535,"B1"]
["105519FA","OES-442 LZ",null,{"$f":"D5303+D5304+D5308+D5309","v":3682},null,null,"Pas concerné par l'étiquettage",null,null,3661238109292,69,1190,550,535,"B1"]
["105520FA","OES-443 LZ",null,{"$f":"D5305+D5306+D5307+D5308+D5309","v":3954},null,null,"Pas concerné par l'étiquettage",null,null,3661238109278,76,1190,550,535,"B1"]
[]
["COMPOSANTS"]
[105617,"OES-441-1 LZ",null,2606,null,null,"/","/","/",3661238109261,63,1190,550,535,"B1"]
[106284,"GICLEUR 6.50G 45° B",null,10,null,null,"/","/","/",3661238109209,0.03,null,null,null,"B1"]
[106124,"OES-441-2 LZ",null,3156,null,null,"/","/","/",3661238109230,63,1190,550,535,"B1"]
[106285,"GICLEUR 7.50G 45° B",null,10,null,null,"/","/","/",3661238109193,0.03,null,null,null,"B2"]
[105518,"OES-441-3 LZ",null,3382,null,null,"/","/","/",3661238109322,69,1190,550,535,"B1"]
[106287,"GICLEUR 10.00G 45° B",null,10,null,null,"/","/","/",3661238109186,0.03,null,null,null,"B2"]
[105519,"OES-442 LZ",null,3657,null,null,"/","/","/",3661238109308,69,1190,550,535,"B1"]
[106287,"GICLEUR 10.00G 45° B",null,10,null,null,"/","/","/",3661238109186,0.5,null,null,null,"B2"]
[105520,"OES-443 LZ",null,3919,null,null,"/","/","/",3661238109285,76,1190,550,535,"B1"]
[106291,"GICLEUR 10,00G 60° B",null,10,null,null,"/","/","/",3661238109179,0.03,null,null,null,"B1"]
[106282,"GICLEUR 5,00G 45° B",null,10,null,null,"/","/","/",3661238109216,0.03,null,null,null,"B1"]
[83176,"PRISE WIELAND MALE 7P ",null,8,null,null,"/","/","/",3661238113114,null,null,null,null,"B1"]
[83191,"PRISE WIELAND MALE 4P ",null,7,null,null,"/","/","/",3661238113107,null,null,null,null,"B1"]
[]
["OPTIONS"]
[88027182,"CAISSON INSONORISANT POUR  440L",null,2202,null,null,"/","/","/",3661238048263,98,1160,970,890,"B2"]
[]
[]
[108005,"OES 541 LZ (2 allures) ",null,4874,null,null,"/","/","/",3661238108851,65,1390,700,660,"B2"]
[]
["FAMILLE:","BRULEUR  GAZ"]
[]
[]
["107580FA","OES 151GE",null,{"$f":"D5324+D5327+D5326","v":1795},null,null,"Pas concerné par l'étiquettage",null,null,3661238108967,15,800,310,400,"B2"]
["107590FA","OES 155 GE",null,{"$f":"D5325+D5327+D5326","v":2084},null,null,"Pas concerné par l'étiquettage",null,null,3661238108943,16.5,800,310,400,"B2"]
[]
["COMPOSANTS"]
[107580,"OES 151GE",null,1787,null,null,"/","/","/",3661238108974,15,800,310,400,"B2"]
[107590,"OES 155 GE",null,2076,null,null,"/","/","/",3661238108950,16.5,800,310,400,"B2"]
[107558,"Notice",null,0,null,null,"/","/","/",3661238108981,null,null,null,null,"B2"]
[83176,"PRISE WIELAND MALE 7P       ",null,8,null,null,"/","/","/",3661238113114,null,null,null,null,"B1"]
[]
["OPTIONS"]
[88027289,"KIT GPL POUR BRUL G100 DD",null,147,null,null,"/","/","/",3661238048089,0.26,230,180,250,"B2"]
[88027290,"KIT GPL POUR BRUL G200/1",null,146,null,null,"/","/","/",3661238048072,0.25,340,190,35,"B2"]
[]
[]
["108534FA","OEN 255 GE",null,{"$f":"D5338+D5342+D5340","v":2376},null,null,"Pas concerné par l'étiquettage",null,null,3661238108738,20,800,305,400,"B2"]
["108535FA","OEN 255 GI",null,{"$f":"D5339+D5342+D5340+D5341","v":2830},null,null,"Pas concerné par l'étiquettage",null,null,3661238108714,21.5,800,305,400,"B2"]
[]
["COMPOSANTS"]
[108534,"OEN 255 GE",null,2368,null,null,"/","/","/",3661238108745,20,800,305,400,"B2"]
[108535,"OEN 255 GI",null,2815,null,null,"/","/","/",3661238108721,21.5,800,305,400,"B2"]
[83176,"PRISE WIELAND MALE 7P ",null,8,null,null,"/","/","/",3661238113114,0.05,null,null,null,"B1"]
[83191,"PRISE WIELAND MALE 4P ",null,7,null,null,"/","/","/",3661238113107,0.05,null,null,null,"B1"]
[108665,"NOTICE",null,0,null,null,"/","/","/",3661238108707,null,null,null,null,"B2"]
[]
["OPTIONS"]
[200001978,"KIT DE CONVERSION PROPANE",null,450,null,null,"/","/","/",3661238001794,0.6,430,180,80,"B2"]
[92089,"CONTROLEUR D'ETANCHEITE VPS 504",null,1153,null,null,"/","/","/",null,null,null,null,null,"P/R"]
[100002804,"SET CONTROLEUR ETANCHEITE TC116 W05-T",null,1118,null,null,"/","/","/",null,null,null,null,null,"B2"]
[]
[]
[100004989,"OES 352 GE",null,{"$f":"D5358+D5364","v":3006},null,null,"Pas concerné par l'étiquettage",null,null,3661238109773,32,900,365,490,"B2"]
[100004990,"OES 353 GE",null,{"$f":"D5359+D5364","v":3281},null,null,"Pas concerné par l'étiquettage",null,null,3661238109766,32,900,365,490,"B2"]
[100004991,"OES 352 GI",null,{"$f":"D5360+D5364","v":3209},null,null,"Pas concerné par l'étiquettage",null,null,3661238109759,32,900,365,490,"B2"]
[100004992,"OES 353 GI",null,{"$f":"D5361+D5364","v":3553},null,null,"Pas concerné par l'étiquettage",null,null,3661238109742,32,900,365,490,"B2"]
[100004993,"OES 355 GI - 20 mbar",null,{"$f":"D5362+D5364","v":4374},null,null,"Pas concerné par l'étiquettage",null,null,3661238109735,40,900,365,490,"B2"]
[100004994,"OES 355 GI - 300 mbar",null,{"$f":"D5363+D5364","v":4031},null,null,"Pas concerné par l'étiquettage",null,null,3661238109728,39,900,365,490,"B2"]
[]
["COMPOSANTS"]
[100004593,"OES 352 GE",null,2993,null,null,"/","/","/",3661238110403,32,900,365,490,"B2"]
[100004594,"OES 353 GE",null,3268,null,null,"/","/","/",3661238110397,32,900,365,490,"B2"]
[100004595,"OES 352 GI",null,3196,null,null,"/","/","/",3661238110380,32,900,365,490,"B2"]
[100004596,"OES 353 GI",null,3540,null,null,"/","/","/",3661238110373,32,900,365,490,"B2"]
[100004597,"OES 355 GI - 20 mbar",null,4361,null,null,"/","/","/",3661238110366,40,900,365,490,"B2"]
[100004598,"OES 355 GI - 300 mbar",null,4018,null,null,"/","/","/",3661238110359,39,900,365,490,"B2"]
[100005000,"SACHET DOCUMENTATION OES 350 G FR (notice + 2 prises W)",null,13,null,null,"/","/","/",3661238109674,0.2,null,null,null,"B2"]
[]
["OPTIONS"]
[602524,"CONTRE-PLAQUE PERCAGE 170/DIX. 200",null,119,null,null,"/","/","/",3661238106192,null,null,null,null,"B1"]
[200005840,"KIT DE CONVERSION PROPANE",null,435,null,null,"/","/","/",3661238166295,0.49,230,140,60,"B2"]
[200005841,"KIT DE CONVERSION PROPANE",null,435,null,null,"/","/","/",3661238166288,0.6,430,180,80,"B2"]
[88027180,"CAISSON INSONORISANT POUR 350",null,1573,null,null,"/","/","/",3661238048270,null,null,null,null,"B1"]
[130716,"INTERRUPTEUR +/- POUR GI (CPR)",null,"P/R",null,null,"/","/","/",null,null,null,null,null,"P/R"]
[]
[]
[100004995,"OEN 352 GI",null,{"$f":"D5379+D5382","v":3415},null,null,"Pas concerné par l'étiquettage",null,null,3661238109711,32,900,365,490,"B2"]
[100004996,"OEN 353 GI",null,{"$f":"D5380+D5382","v":3963},null,null,"Pas concerné par l'étiquettage",null,null,3661238109704,36,900,365,490,"B2"]
[100004997,"OEN 355 GI - 20 mbar",null,{"$f":"D5381+D5382","v":4507},null,null,"Pas concerné par l'étiquettage",null,null,3661238109698,42,900,365,490,"B2"]
[]
["COMPOSANTS"]
[100004599,"OEN 352 GI",null,3402,null,null,"/","/","/",3661238110342,32,900,365,490,"B2"]
[100004600,"OEN 353 GI",null,3950,null,null,"/","/","/",3661238110335,36,900,365,490,"B2"]
[100004601,"OEN 355 GI - 20 mbar",null,4494,null,null,"/","/","/",3661238110328,42,900,365,490,"B2"]
[100005001,"Sachet DOCUMENTATION OEN 350 G FR (notice + 2 prises W)",null,13,null,null,"/","/","/",3661238109667,0.2,null,null,null,"B2"]
[]
["OPTIONS"]
[602524,"CONTRE-PLAQUE PERCAGE 170/DIX. 200",null,119,null,null,"/","/","/",3661238106192,3.5,300,300,6,"B1"]
[7626036,"KIT REGULATEUR RWF55 ","MW1",1245,0.12,95010,"/","/","/",3661238048065,2.7,250,210,165,"B2"]
[200005580,"S/E POTENTIOMETRE DE RECOPIE",null,374,null,null,"/","/","/",null,null,null,null,null,"B2"]
[106446,"CAISSON INSONORISANT POUR 350",null,1573,null,null,"/","/","/",3661238048270,47,510,640,910,"B1"]
[130716,"INTERRUPTEUR +/- POUR GI (CPR)",null,"P/R",null,null,"/","/","/",3661238150539,null,null,null,null,"P/R"]
[]
[]
[106401,"OES 441.2 GI",null,3473,null,null,"/","/","/",3661238109162,61,1180,550,535,"B2"]
[106402,"OES 441.3 GI",null,4842,null,null,"/","/","/",3661238109155,60.5,1180,550,535,"B2"]
[106404,"OES 443 GI",null,5357,null,null,"/","/","/",3661238109148,67.5,1180,550,535,"B2"]
[]
["OPTIONS"]
[100019540,"RAMPE GAZ MB-VEF 415 S32",null,1430,null,null,"/","/","/",3661238564770,9,null,null,null,"B2"]
[100019542,"RAMPE GAZ MB-VEF 420 S12",null,1850,null,null,"/","/","/",3661238564794,9,null,null,null,"B2"]
[100019543,"RAMPE GAZ MB-VEF 425 S12",null,2688,null,null,"/","/","/",3661238564800,9,null,null,null,"B2"]
[88027177,"REGULATEUR PRESSION 300 mbar GDJ 50 RACCORDT. Ø 2''","GDJ50",432,null,null,"/","/","/",3661238048287,3.1,255,220,205,"B2"]
[88027182,"CAISSON INSONNORISANT",null,2202,null,null,"/","/","/",3661238048263,98,1160,970,890,"B2"]
[97955833,"SET RACCORDEMENT  RAMPE FOYER",null,34,null,null,"/","/","/",3661238102118,0.14000000000000001,null,null,null,"B2"]
[88027317,"KIT POUR FONCTIONNEMENT BRULEUR EN 2 ALLURES (THERMOSTAT  2 POINTS)",null,113,0.12,95010,"/","/","/",3661238047952,1,260,270,170,"B2"]
[105627,"CHARIOT BRULEUR OE 440",null,1107,null,null,"/","/","/",3661238109247,14,1200,800,500,"B2"]
[7626036,"KIT REGULATEUR RWF55 ","MW1",1245,0.12,95010,"/","/","/",3661238048065,2.7,250,210,165,"B2"]
[200005582,"KIT POTENTIOMETRE DE RECOPIE ",null,374,null,null,"/","/","/",null,0.52,180,420,80,"B2"]
[]
[]
[108286,"OES 541 GI (modulant)",null,6174,null,null,"/","/","/",3661238108844,70,1395,710,660,"B2"]
[108287,"OES 542 GI (modulant)",null,7938,null,null,"/","/","/",3661238108837,105,1400,1000,670,"B2"]
[]
["OPTIONS"]
[108055,"RAMPE MBD  420 CTD (100-300 mbar)",null,1840,null,null,"/","/","/",3661238048126,12.5,570,350,290,"B2"]
[88027298,"ADAPTATEUR FN 65 2\"",null,206,null,null,"/","/","/",3661238048034,6.2,320,240,240,"B2"]
[88027299,"ADAPTATEUR FN 80 FN 65",null,352,null,null,"/","/","/",3661238048027,11,470,380,390,"B2"]
[88027317,"KIT POUR FONCTIONNEMENT BRULEUR EN 2 ALLURES (THERMOSTAT  2 POINTS)",null,113,0.12,95010,"/","/","/",3661238047952,1,260,270,170,"B2"]
[130990,"RWD 40 POUR OEN 540 GI",null,null,null,null,"/","/","/",3661238321489,null,null,null,null,"P/R"]
[100006662,"SET POTENTIOMETRE DE RECOPIE",null,497,null,null,"/","/","/",3661238161740,0.2,170,90,70,"B2"]
[]
["FAMILLE:","CHAUDIERE A COMBUSTIBLE SOLIDE"]
[]
[]
[603464,"COMBUSTIBLE SOLIDE  ","CF124",{"$f":"D5431+D5437+D5443+D5449","v":3620},null,null,"Pas concerné par l'étiquettage",null,null,3661238106130,null,null,null,null,"C0"]
[603465,"COMBUSTIBLE SOLIDE  ","CF125",{"$f":"D5432+D5438+D5444+D5449","v":4117},null,null,"Pas concerné par l'étiquettage",null,null,3661238106123,null,null,null,null,"C0"]
[603466,"COMBUSTIBLE SOLIDE","CF126",{"$f":"D5433+D5439+D5445+D5449","v":4655},null,null,"Pas concerné par l'étiquettage",null,null,3661238106116,null,null,null,null,"C0"]
[603467,"COMBUSTIBLE SOLIDE  ","CF127",{"$f":"D5434+D5440+D5446+D5449","v":5102},null,null,"Pas concerné par l'étiquettage",null,null,3661238106109,null,null,null,null,"C0"]
[603468,"COMBUSTIBLE SOLIDE ","CF128",{"$f":"D5435+D5441+D5447+D5449","v":5521},null,null,"Pas concerné par l'étiquettage",null,null,3661238106093,null,null,null,null,"C0"]
[603469,"COMBUSTIBLE SOLIDE  ","CF129",{"$f":"D5436+D5442+D5448+D5449","v":6016},null,null,"Pas concerné par l'étiquettage",null,null,3661238106086,null,null,null,null,"C0"]
[]
["COMPOSANTS"]
[82627704,"CORPS CHAUDIERE CF 124CSE",null,2020,null,null,"/","/","/",3661238018723,176,1030,425,445,"C0"]
[82627705,"CORPS CHAUDIERE CF 125CSE",null,2485,null,null,"/","/","/",3661238018716,215.5,1035,540,445,"C0"]
[82627706,"CORPS CHAUDIERE CF 126CSE",null,2977,null,null,"/","/","/",3661238018709,255.5,1035,645,445,"C0"]
[82627707,"CORPS CHAUDIERE CF 127CSE",null,3401,null,null,"/","/","/",3661238018693,297,1040,755,445,"C0"]
[82627708,"CORPS CHAUDIERE CF 128CSE",null,3785,null,null,"/","/","/",3661238018686,335.5,1040,865,445,"C0"]
[82627709,"CORPS CHAUDIERE CF 129CSE",null,4248,null,null,"/","/","/",3661238018679,373.5,1040,975,445,"C0"]
[82627714,"ACCESSOIRES CF 124 CSE L2",null,889,null,null,"/","/","/",3661238018662,51,660,615,370,"C0"]
[82627715,"ACCESSOIRES CF 125 CSE L3",null,911,null,null,"/","/","/",3661238018655,55,660,615,370,"C0"]
[82627716,"ACCESSOIRES CF 126 CSE L4",null,950,null,null,"/","/","/",3661238018648,59.5,660,615,370,"C0"]
[82627717,"ACCESSOIRES CF 127 CSE L5",null,970,null,null,"/","/","/",3661238018631,61.5,660,615,370,"C0"]
[82627718,"ACCESSOIRES CF 128 CSE L6",null,994,null,null,"/","/","/",3661238018624,65,660,615,370,"C0"]
[82627719,"ACCESSOIRES CF 129 CSE L7",null,1024,null,null,"/","/","/",3661238018617,69,660,615,370,"C0"]
[82697704,"GARNITURE JAQUETTE 4 ELTS L34",null,670,null,null,"/","/","/",3661238018457,7.5,1070,680,140,"C0"]
[82697705,"GARNITURE JAQUETTE 5 ELTS L35",null,680,null,null,"/","/","/",3661238018440,22,1070,680,140,"C0"]
[82697706,"GARNITURE JAQUETTE 6 ELTS L36",null,687,null,null,"/","/","/",3661238018433,24,1070,680,140,"C0"]
[82697707,"GARNITURE JAQUETTE 7 ELTS L37",null,690,null,null,"/","/","/",3661238018426,27.5,1070,1010,140,"C0"]
[82697708,"GARNITURE JAQUETTE 8 ELTS L38",null,701,null,null,"/","/","/",3661238018419,29.5,1070,1020,150,"C0"]
[82697709,"GARNITURE JAQUETTE 9 ELTS L39",null,703,null,null,"/","/","/",3661238018402,35.5,1070,1020,150,"C0"]
[80018701,"OUTILS DE CHAUFFE COMPLET",null,41,null,null,"/","/","/",3661238001763,1.81,1070,105,50,"C0"]
[]
["OPTIONS"]
[82697720,"ECHANGEUR DE SECURITE S/VANNE ","CF124/5",641,null,null,"/","/","/",3661238018396,7,800,170,170,"C0"]
[82697721,"ECHANGEUR DE SECURITE S/VANNE ","CF126/7",641,null,null,"/","/","/",3661238018389,7.5,1170,130,180,"C0"]
[82697722,"ECHANGEUR DE SECURITE S/VANNE ","CF128/9",641,null,null,"/","/","/",3661238018372,8.3000000000000007,125,1160,14,"C0"]
[82697701,"VANNE DE COMMANDE DE L'ECHANGEUR DE SECURITE","L33",215,null,null,"/","/","/",3661238018464,0.63,215,130,40,"C0"]
[]
[]
[100013120,"CHAUDIÈRE BÛCHES 20 KW INVERSE  CBI-II 20","ML37",4933,null,null,"Pas concerné par l'étiquettage",null,null,3661238362024,329,770,590,1180,"C0"]
[100013121,"CHAUDIÈRE BÛCHES 30 KW INVERSE  CBI-II 30","ML38",6073,null,null,"Pas concerné par l'étiquettage",null,null,3661238362031,347,970,590,1180,"C0"]
[100013122,"CHAUDIÈRE BÛCHES 40 KW INVERSE  CBI-II 40","ML39",7531,null,null,"Pas concerné par l'étiquettage",null,null,3661238362017,398,970,670,1260,"C0"]
[100020114,"CHAUDIÈRE BÛCHES 30 KW INVERSE OCBI 30 C5","ML49",5930,null,null,"Pas concerné par l'étiquettage",null,null,null,null,null,null,null,"C0"]
[]
[]
[100004770,"CHAUDIERE BUCHES 20 KW A TIRAGE NATUREL  CBB 20 ","ML1",3961,null,null,"Pas concerné par l'étiquettage",null,null,3661238002340,288,700,1155,1430,"C0"]
[100004771,"CHAUDIERE BUCHES 30 KW A TIRAGE NATUREL CBB 30","ML2",4674,null,null,"Pas concerné par l'étiquettage",null,null,3661238002333,344,695,1150,1600,"C0"]
[100004772,"CHAUDIERE BUCHES 15 KW A TIRAGE NATUREL  OCBB 15 E","ML3",4439,null,null,"Pas concerné par l'étiquettage",null,null,3661238002326,302,685,1000,1365,"C0"]
[]
["OPTIONS"]
[100004803,"GROUPE DE RELEVE DU RETOUR  FRR L21","ML9",912,null,null,"/","/","/",3661238002197,9.5,370,190,230,"C0"]
[100020120,"MODULE DE TEMPERAURE RETOUR ","ML52",689,null,null,"/","/","/",3661238574403,5.2,null,null,null,"C0"]
[82697701,"VANNE DE COMMANDE DE L'ECHANGEUR DE SECURITE",null,215,null,null,"/","/","/",3661238018464,0.63,215,130,40,"C0"]
[]
["OPTIONS REGULATIONS CIRCUIT ECS-CHAUFFAGE"]
[125392,"REA-130B POUR 1 CIRCUIT",null,665,0.12,95010,"/","/","/",3661238108486,null,null,null,null,"C0"]
[125394,"REA-131B POUR 2 CIRCUITS",null,856,0.12,95010,"/","/","/",3661238108479,null,null,null,null,"C0"]
[125400,"REA  232B : POUR 2 CIRCUITS VANNE",null,1151,0.12,95010,"/","/","/",3661238108448,null,null,null,null,"C0"]
[84907702,"THERMOSTAT DE FUMEE (CDE Chaudière Fioul/gaz) ",null,486,null,null,"/","/","/",3661238033115,1,305,205,125,"C0"]
[100002330,"MODULE HYDRAULIQUE CH. BOIS ","EA108",832,null,null,"/","/","/",3661238007444,8,400,270,230,"C0"]
[]
["FAMILLE:","POÊLE A BOIS ET GRANULES"]
[]
[]
[100019281,"POÊLE A BOIS OPBE 7 T","LB6",1346,null,null,"Pas concerné par l'étiquettage",null,null,3661238550827,131,580,710,1210,"C2"]
[100019282,"POÊLE A BOIS OPBE 7 G","LB7",1346,null,null,"Pas concerné par l'étiquettage",null,null,3661238550834,152,715,580,1210,"C2"]
[100019283,"POÊLE A BOIS OPBA 6 T","LB8",2130,null,null,"Pas concerné par l'étiquettage",null,null,3661238550841,165,650,710,1350,"C2"]
[100019284,"POÊLE A BOIS OPBA 6 O    ","LB9",2130,null,null,"Pas concerné par l'étiquettage",null,null,3661238550858,168,650,710,1350,"C2"]
[]
[]
[7617764,"POÊLE OPBR 5 T   TÔLE NOIRE","LB44",2494,null,null,"Pas concerné par l'étiquettage",null,null,3661238602977,157,1500,714,637,"C2"]
[]
[]
[7618738,"POÊLE OPBR 5 CR   HABILLAGE CERAM ROUGE",null,{"$f":"D5497+D5498","v":3948},null,null,"Pas concerné par l'étiquettage",null,null,null,null,null,null,null,"C2"]
[7618737,"POÊLE OPBR 5 CB   HABILLAGE CERAM BLANC",null,{"$f":"D5497+D5499","v":3948},null,null,"Pas concerné par l'étiquettage",null,null,null,null,null,null,null,"C2"]
[7618736,"POÊLE OPBR 5 CN   HABILLAGE CERAM NOIR",null,{"$f":"D5497+D5500","v":3948},null,null,"Pas concerné par l'étiquettage",null,null,null,null,null,null,null,"C2"]
[]
["COMPOSANTS"]
[7617766,"POÊLE OPBR 5 C CORPS SEUL CERAM","LB46",2078,null,null,"/","/","/",3661238602991,125,1460,714,637,"C2"]
[7617767,"HABILLAGE OPBR CERAMIQUE BORDEAUX","LB47",1870,null,null,"/","/","/",3661238603004,82,572,1535,600,"C2"]
[7617769,"HABILLAGE OPBR CERAMIQUE BLANCHE","LB49",1870,null,null,"/","/","/",3661238603035,82,572,1535,600,"C2"]
[7617768,"HABILLAGE OPBR CERAMIQUE NOIR","LB48",1870,null,null,"/","/","/",3661238603028,82,572,1535,600,"C2"]
[]
[]
[7618739,"POÊLE OPBR 5 PG PIERRE DE GRES ",null,{"$f":"D5507+D5508","v":2701},null,null,"Pas concerné par l'étiquettage",null,null,null,null,null,null,null,"C2"]
[7618740,"POÊLE OPBR 5 PO PIERRE OLAIRE",null,{"$f":"D5507+D5509","v":2701},null,null,"Pas concerné par l'étiquettage",null,null,null,null,null,null,null,"C2"]
[]
["COMPOSANTS"]
[7617765,"CORPS SEUL PIERRE","LB45",2078,null,null,"/","/","/",3661238602984,132,1460,714,637,"C2"]
[7617770,"HABILLAGE OPBR PIERRE DE GRES","LB50",623,null,null,"/","/","/",3661238603042,86,500,1500,200,"C2"]
[7617773,"HABILLAGE OPBR PIERRE OLAIRE","LB51",623,null,null,"/","/","/",3661238603059,100,550,1535,300,"C2"]
[]
["OPTIONS"]
[7617774,"BLOC ACCUMULATION OPBR","LB52",255,null,null,"/","/","/",3661238603066,84,265,1080,360,"C2"]
[100019287,"PROTECTION DE SOL ARROND 1000X100","LB17",112,null,null,"/","/","/",3661238550889,15,1060,1025,20,"C2"]
[]
[]
[7651027,"POELE A BOIS OPBE 8 T","LB81",1276,null,null,null,null,null,3661238659148,133,920,670,556,"C2"]
[]
["OPTIONS"]
[100019286,"PROTECTION DE SOL RECT 900X750  ","LB16",95,null,null,"/","/","/",3661238550872,11.3,940,810,20,"C2"]
[]
[]
[7651164,"POELE PELLETS 8KW BLANC",null,{"$f":"D5529+D5530","v":3267},null,null,"/","/","/",3661238659377,null,null,null,null,"C2"]
[7651165,"POELE PELLETS 8KW PERLE",null,{"$f":"D5529+D5531","v":3267},null,null,"/","/","/",3661238659384,null,null,null,null,"C2"]
[7651167,"POELE PELLETS 8KW GRIS",null,{"$f":"D5529+D5532","v":3267},null,null,"/","/","/",3661238659391,null,null,null,null,"C2"]
[7651168,"POELE PELLETS 8KW NOIR",null,{"$f":"D5529+D5533","v":3267},null,null,"/","/","/",3661238659407,null,null,null,null,"C2"]
[7651170,"POELE PELLETS 8KW INOX",null,{"$f":"D5529+D5534","v":3267},null,null,"/","/","/",3661238659414,null,null,null,null,"C2"]
[]
["COMPOSANTS"]
[7651024,"CORPS DE CHAUFFE OPPA 8 CS ","LB80",3012,1.67,14080,"/","/","/",3661238659131,114,1202,714,637,"C2"]
[7650999,"HABILLAGE BLANC ","LB73",255,null,null,"/","/","/",3661238659063,14.9,90,950,360,"C2"]
[7651001,"HABILLAGE PERLE","LB74",255,null,null,"/","/","/",3661238659070,14.9,90,950,360,"C2"]
[7651002,"HABILLAGE GRIS","LB75",255,null,null,"/","/","/",3661238659087,14.9,90,950,360,"C2"]
[7651004,"HABILLAGE NOIR","LB76",255,null,null,"/","/","/",3661238659094,14.9,90,950,360,"C2"]
[7651005,"HABILLAGE INOX","LB77",255,null,null,"/","/","/",3661238659100,14.9,90,950,360,"C2"]
[]
[]
[7648370,"OMPA 6 R-NO",null,{"$f":"D5549+D5551","v":3574},null,null,"/","/","/",3661238655751,null,null,null,null,"C2"]
[7648372,"OMPA 6 R-NB",null,{"$f":"D5549+D5552","v":3574},null,null,"/","/","/",3661238655775,null,null,null,null,"C2"]
[7648374,"OMPA 6 RC-BA",null,{"$f":"D5549+D5556+D5554","v":3931},null,null,"/","/","/",3661238655799,null,null,null,null,"C2"]
[7648376,"OMPA 6 RC-NO",null,{"$f":"D5549+D5556+D5555","v":3931},null,null,"/","/","/",3661238655812,null,null,null,null,"C2"]
[7648378,"OMPA 6 RC-RO",null,{"$f":"D5549+D5556+D5553","v":3931},null,null,"/","/","/",3661238655836,null,null,null,null,"C2"]
[7648371,"OMPA 9 R-NO",null,{"$f":"D5550+D5551","v":3676},null,null,"/","/","/",3661238655768,null,null,null,null,"C2"]
[7648373,"OMPA 9 R-NB",null,{"$f":"D5550+D5552","v":3676},null,null,"/","/","/",3661238655782,null,null,null,null,"C2"]
[7648375,"OMPA 9 RC-BA",null,{"$f":"D5550+D5556+D5554","v":4033},null,null,"/","/","/",3661238655805,null,null,null,null,"C2"]
[7648377,"OMPA 9 RC-NO",null,{"$f":"D5550+D5556+D5555","v":4033},null,null,"/","/","/",3661238655829,null,null,null,null,"C2"]
[7648379,"OMPA 9 RC-RO",null,{"$f":"D5550+D5556+D5553","v":4033},null,null,"/","/","/",3661238655843,null,null,null,null,"C2"]
[]
["COMPOSANTS"]
[7647780,"OMPA 6 CORPS PELLETS 6KW ","LB64",2042,1.67,14080,"/","/","/",3661238654891,87.5,660,600,1300,"C2"]
[7647782,"OMPA 9 CORPS PELLETS 9KW","LB65",2144,1.67,14080,"/","/","/",3661238654907,87.5,660,600,1300,"C2"]
[7647773,"HABILLAGE ROND ACIER NOIR ","LB59",1532,null,null,"/","/","/",3661238654846,58.5,1200,600,700,"C2"]
[7647774,"HABILLAGE ROND ACIER N-B","LB60",1532,null,null,"/","/","/",3661238654853,42,1200,400,700,"C2"]
[7647775,"HABILLAGE ROND CERAM. BORDEAUX ","LB61",715,null,null,"/","/","/",3661238654860,33.5,600,400,600,"C2"]
[7647777,"HABILLAGE ROND CERAM. BLANC ","LB62",715,null,null,"/","/","/",3661238654877,33.5,600,400,600,"C2"]
[7647778,"HABILLAGE ROND CERAM. NOIR","LB63",715,null,null,"/","/","/",3661238654884,33.5,600,400,600,"C2"]
[7648984,"PORTE POUR HABIL. CERAM.","LB66",1174,null,null,"/","/","/",3661238656024,43,1200,400,700,"C2"]
[]
[]
[7651162,"POELE PELLETS 8KW BLANC",null,{"$f":"D5563+D5564","v":2553},null,null,"/","/","/",3661238659377,null,null,null,null,"C2"]
[7651163,"POELE PELLETS 8KW PERLE",null,{"$f":"D5563+D5565","v":2553},null,null,"/","/","/",3661238659384,null,null,null,null,"C2"]
[]
["COMPOSANTS"]
[7651023,"CORPS DE CHAUFFE OPPE 8 F","LB79",2369,1.67,14080,"/","/","/",3661238659124,105,1026,710,677,"C2"]
[7650967,"HABILLAGE BLANC ","LB70",184,null,null,"/","/","/",3661238659032,6.2,960,370,120,"C2"]
[7650971,"HABILLAGE PERLE","LB71",184,null,null,"/","/","/",3661238659049,6.2,960,370,120,"c2"]
[]
["OPTIONS"]
[100019287,"PROTECTION DE SOL ARROND 1000X100","LB17",112,null,null,"/","/","/",3661238550889,15,1060,1025,20,"C2"]
[7650953,"MODULE WIFI POELE PELLET ","LB68",153,null,null,"/","/","/",3661238659018,0.2,50,50,20,"C2"]
[]
[]
[7617755,"POÊLE A PELLETS OPPA 8 V","LB38",3473,1.67,14080,"Pas concerné par l'étiquettage",null,null,3661238603011,119,1202,714,637,"C2"]
[7617756,"POÊLE A PELLETS OPPA 8 PVI","LB39",3654,1.67,14080,"Pas concerné par l'étiquettage",null,null,3661238602922,119,1202,714,637,"C2"]
[7617757,"POÊLE A PELLETS OPPA 8 GVI","LB40",4183,1.67,14080,"Pas concerné par l'étiquettage",null,null,3661238602939,138,1417,714,637,"C2"]
[null,null,null,null,null,null,null,null,null,3661238602977,157,1500,714,637,"C2"]
["OPTIONS VENTOUSE HORIZONTALE POUR POELE A PELLETS BBC"]
[7607218,"KIT VENTOUSE H 80-130 PGI","LB25",974,null,null,"/","/","/",3661238585713,14.8,1030,530,535,"C2"]
[7607219,"ELEMENT DROIT L1000 80-130 PGI ","LB26",154,null,null,"/","/","/",3661238585720,2.6,1030,105,105,"C2"]
[7607220,"ELEMENT DROIT L450 80-130 PGI","LB27",106,null,null,"/","/","/",3661238585737,1.4,510,105,105,"C2"]
[7607221,"ELEMENT DROIT L250 80-130 PGI","LB28",90,null,null,"/","/","/",3661238585744,1,330,105,105,"C2"]
[7607222,"ELEMENT REGLABLE 80-130 PGI","LB29",134,null,null,"/","/","/",3661238585751,2,510,105,105,"C2"]
[7607223,"KIT TRAVERSEE MUR STH 80-130 PGI","LB30",364,null,null,"/","/","/",3661238585768,10.6,500,500,510,"C2"]
[7607224,"COLLIER MURAL D130","LB31",30,null,null,"/","/","/",3661238585775,0.2,400,270,30,"C2"]
[]
["OPTIONS"]
[100019286,"PROTECTION DE SOL RECT 900X750  ","LB16",95,null,null,"/","/","/",3661238550872,11.3,940,810,20,"C2"]
[100019287,"PROTECTION DE SOL ARROND 1000X100","LB17",112,null,null,"/","/","/",3661238550889,15,1060,1025,20,"C2"]
[]
["FAMILLE:","CHAUDIERE  ELECTRIQUE"]
[]
[100013409,"CER 8M",null,2732,5,14070,"D","/","/",3661238572959,22,310,495,260,"C8"]
[100013450,"CER 12M",null,2815,5,14070,"D","/","/",3661238572911,22,310,495,260,"C8"]
[100013452,"CER 12TR",null,2985,5,14070,"D","/","/",3661238572966,22,310,495,260,"C8"]
[]
["OPTIONS"]
[100013456,"SONDE EXTERIEURE CER","JE7",75,0.02,95020,"/","/","/",3661238573215,0.1,46,64,30,"C8"]
[100003690,"SONDE PT 1000 CER SUR CABLE SILICONE (sonde départ V3V)","EC171",62,0.02,95020,"/","/","/",3661238573239,0.112,0,0,0,"C8"]
[100013562,"RELAIS STATIQUE SIP 8A/230 V (2 pces)","JE8",26,0.12,95010,"/","/","/",3661238572942,0.01,23,23,4,"C8"]
[89997002,"KIT DE SECURITE ","EA47",129,null,null,"/","/","/",3661238044654,6.1,635,195,170,"C0"]
[100020073,"THERMOSTAT SIMPLIFIE CER T87 OPEN THERM FILAIRE","JE5",157,0.12,95010,"/","/","/",3661238102156,6.55,405,270,240,"C8"]
[100020074,"THERMOSTAT SIMPLIFIE CER Y87 OPEN THERM RADIO FREQUENCE","JE6",426,0.12,95010,"/","/","/",3661238102149,8.1999999999999993,405,270,240,"C8"]
[100020075,"THERMOSTAT PROGRAMMABLE CER 850-2 OPEN THERM FILAIRE","JE4",438,0.12,95010,"/","/","/",3661238044739,1.56,400,230,130,"C8"]
[]
[100013563,"PRESSE ETOUPE COMPLET M25",null,6,null,null,"/","/","/",null,null,null,null,null,"C8"]
["COMPOSANTS"]
[100013568,"PRESSE ETOUPE M25",null,3,null,null,"/","/","/",null,0.02,48,30,0,"C8"]
[100013569,"ECROU POUR PRESSE ETOUPE M25",null,3,null,null,"/","/","/",null,0.02,9,32," ","C8"]
[]
[100013564,"PRESSE ETOUPE COMPLET M16",null,4,null,null,"/","/","/",null,null,null,null,null,"C8"]
["COMPOSANTS"]
[100013570,"PRESSE ETOUPE M16",null,2,null,null,"/","/","/",null,7.0000000000000007E-2,42,19,0,"C8"]
[100013571,"ECROU POUR PRESSE ETOUPE M16",null,2,null,null,"/","/","/",null,5.0000000000000001E-3,9,22,0,"C8"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C8"]
[100013565,"PRESSE ETOUPE COMPLET M12",null,4,null,null,"/","/","/",null,null,null,null,null,"C8"]
["COMPOSANTS"]
[100013572,"PRESSE ETOUPE M12",null,2,null,null,"/","/","/",null,0.05,35,12,0,"C8"]
[100013573,"ECROU POUR PRESSE ETOUPE M12",null,2,null,null,"/","/","/",null,3.0000000000000001E-3,9,15,0,"C8"]
[100020165,"CONSOLE MUR COLLECTEUR ","EA141",44,null,null,"/","/","/",3661238108653,1.2,220,125,70,"C0"]
[100020166,"CONSOLE MUR 1 MODULE ","EA142",116,null,null,"/","/","/",3661238108646,1.6,220,125,70,"C0"]
[100020167,"CIRCUIT DIRECT P.ELEC CLASSE A  ","EA143",644,0.83,14050,"/","/","/",3661238108639,5.0999999999999996,460,270,235,"C0"]
[100020168,"CIRCUIT V3V P.ELEC","EA144",916,0.83,14050,"/","/","/",3661238575059,6,460,270,235,"C0"]
[100020169,"MODULE HYDR COMPACT 2 CIRCUITS HEE","EA145",1146,0.83,14050,"/","/","/",3661238108622,9,525,415,210,"C0"]
[]
[null,"TARIF INDICATIF DES MISES  EN SERVICE "]
[]
[null,"MISE EN SERVICE CHAUDIERE ELECTRIQUE "]
[null,"MISE EN SERVICE OENOVIAPAC (tous modèles)"]
[null,"MISE EN SERVICE PAC HYBRIDES"]
[null,"MISE EN SERVICE OTWH SPLIT "]
[null,"MISE EN SERVICE OTWH"]
[null,"MISE EN SERVICE CESI BASICSUN/POWERSUN/PERFECTSUN"]
[null,"MISE EN SERVICE SSC OECOSUN "]
[null,"MISE EN SERVICE SSC OECOSUN AVEC PAC"]
[null,"MISE EN SERVICE GMR 1000/3000 CONDENS GMX - GMR 1000/2000"]
[null,"MISE EN SERVICE GMR 5000 CONDENS"]
[null,"MISE EN SERVICE 2 X GMR 5000 CONDENS"]
[null,"MISE EN SERVICE 3 X GMR 5000 CONDENS"]
[null,"MISE EN SERVICE 4 X GMR 5000 CONDENS"]
[null,"MISE EN SERVICE POELE A PELLETS  OPPA"]
[null,"MISE EN SERVICE GSR 140-45 A 115 CONDENS"]
[null,"MISE EN SERVICE GSR 230 CONDENS"]
[null,"MISE EN SERVICE GSR 330 DUO CONDENS "]
[null,"MISE EN SERVICE GSR 330 CONDENS VD/VG"]
[null,"MISE EN SERVICE OECOIL TOUS MODELES"]
[null,"MISE EN SERVICE PU 260 CONDENS"]
[null,"MISE EN SERVICE OENOVIAFIOUL CONFORT"]
[null,"MISE EN SERVICE OENOVIAGAZ TOUS MODELES"]
[null,"MISE EN SERVICE OEX"]
[null,"MISE EN SERVICE OES/OEN 150L EV"]
[null,"MISE EN SERVICE OES/OEN 250L "]
[null,"MISE EN SERVICE OES 350-1 ALL"]
[null,"MISE EN SERVICE OES 350-2 ALL"]
[null,"MISE EN SERVICE 440 LZ"]
[null,"MISE EN SERVICE OES 540 L"]
[null,"MISE EN SERVICE OES 150 G"]
[null,"MISE EN SERVICE OES 350 GE"]
[null,"MISE EN SERVICE OES 350 GI"]
[null,"MISE EN SERVICE OEN-350 GI"]
[null,"MISE EN SERVICE  OES 440 GI"]
[null,"MISE EN SERVICE OES 540 GM/GI "]

{"sheet":"Feuille Power OPC","index":9,"n_rows":121,"n_cols":13,"rows_kept":121,"cut":false,"hidden":true,"merged":[[44,0,47,0],[86,0,87,0],[53,0,59,0],[10,0,30,0],[78,2,78,3],[84,2,84,3],[91,1,91,2],[7,1,7,3],[10,1,10,4],[37,1,38,1],[72,2,72,3]]}
[]
[null,"DESIGNATION","COLIS            ","PPHT unit.        ","Nbre capteur par rangée       ","Nbre rangée     "]
[null,null,null,null,null,null,null,"listePower7","listePower10","listePower15"]
[null,"►CAPTEURS TUBULAIRES",null,null,null,null,null,0,0,0]
[null,"1 capteur plan POWER 7",{"$f":"'Sun 3000'!#REF!","v":{"$error":"#REF!"}},0,0,0,null,1,1,1]
[null,"1 capteur plan POWER 10",{"$f":"'Sun 3000'!F19","v":"ER40"},{"$f":"'Sun 3000'!G19","v":1656},{"$f":"'Sun 3000'!H19","v":0},{"$f":"'Sun 3000'!I19","v":0},null,2,2,2]
[null,"1 capteur plan POWER 15",{"$f":"'Sun 3000'!F20","v":"ER41"},{"$f":"'Sun 3000'!G20","v":1974},{"$f":"'Sun 3000'!H20","v":0},{"$f":"'Sun 3000'!I20","v":0},null,3,3,3]
[null,{"$f":"IF(E8>6,\"--Attention plus de 6 capteurs par rangée--\",\"\")","v":""},null,null,null,null,null,4,4,4]
[null,"►ACCESSOIRES POUR RACCORDEMENT HYDRAULIQUE",null,null,null,null,null,5,5,5]
[null,null,null,null,null,null,null,6,6,6]
[null,"• Raccordement des capteurs en montage   vertical  juxtaposés ou  horizontal  superposés ",null,null,null,null,null,7,7,7]
[null,"juxtaposés ou horizontal superposés",null,null,null,null,null,8,8,8]
[null,"Kit de raccordement hydraulique (extémité+bouchon) Tichelmann","EG 394",null,"nbre colis/rangée","nbre colis final par type capteur ",null,9,9,9]
[null,"                               Power7",null,null,1,0,null,10,10,10]
[null,"                               Power10",null,null,1,{"$f":"E15*F6","v":0},null,11,11]
[null,"                               Power15",null,null,1,{"$f":"E16*F7","v":0},null,12,12]
[null,null,null,{"$f":"'Sun 3000'!G27","v":112},"somme colis EG394",{"$f":"F14+F15+F16","v":0},null,13,13]
[null,null,null,null,null,null,null,14,14]
[null,"Kit de liaison entre 2 capteurs","EG 393",null,null,null,null,15]
[null,"                               Power7",null,null,{"$f":"IF(E5=0,0,E5-1)","v":0},0,null,16]
[null,"                               Power10",null,null,{"$f":"IF(E6=0,0,E6-1)","v":0},{"$f":"E21*F6","v":0}]
[null,"                               Power15",null,null,{"$f":"IF(E7=0,0,E7-1)","v":0},{"$f":"E22*F7","v":0}]
[null,null,null,{"$f":"'Sun 3000'!G28","v":150},"somme colis EG393",{"$f":"F20+F21+F22","v":0}]
[]
[null,"Kit raccordement flexibles capteur tubulaire + sonde capteur","EG 355"]
[null,"                               Power7",null,null,1,0]
[null,"                               Power10",null,null,1,{"$f":"E27*F6","v":0}]
[null,"                               Power15",null,null,1,{"$f":"E28*F7","v":0}]
[null,null,null,{"$f":"'Sun 3000'!G29","v":197},"somme colis EG355",{"$f":"F26+F27+F28","v":0}]
[]
[null,"Kit fixation 1 capteur tubulaire","EG 392"]
[null,"                               Power7",null,null,{"$f":"E5","v":0},0]
[null,"                               Power10",null,null,{"$f":"E6","v":0},{"$f":"E33*F6","v":0}]
[null,"                               Power15",null,null,{"$f":"E7","v":0},{"$f":"E34*F7","v":0}]
[null,null,null,{"$f":"'Sun 3000'!G30","v":78},"somme colis EG392",{"$f":"F32+F33+F34","v":0}]
[]
[]
[null,"►ELEMENTS DE POSE SUR TOIT OU TERRASSE  "]
[]
[]
[null,"A choisir parmi les types de montage suivants :"]
[null,"SUR TOIT OU EN TERRASSE"]
[null,"• Profilés à choisir en fonction du montage capteurs souhaité"]
[null,null,null,null,"nbre colis/rangée","nbre colis final"]
[null,"Montage vertical  sur profilés de ER "]
[null,"Kit de montage 1 capteur POWER 7","ER 30",{"$f":"'Sun 3000'!#REF!","v":{"$error":"#REF!"}},{"$f":"E5","v":0},0,null,{"$f":"G46*D46","v":{"$error":"#REF!"}}]
[null,"Kit de montage 1 capteur POWER 10","ER 31",{"$f":"'Sun 3000'!G39","v":158},{"$f":"E6","v":0},{"$f":"E47*F6","v":0},null,{"$f":"D47*G47","v":0}]
[null,"Kit de montage 1 capteur POWER 15","ER 32",{"$f":"'Sun 3000'!G40","v":166},{"$f":"E7","v":0},{"$f":"E48*F7","v":0},null,{"$f":"D48*G48","v":0}]
[]
[]
[]
[null,"• Supports inclinables pour TERRASSE (ou au sol) "]
[null,"à choisir selon la disposition des capteurs en + des profilés"]
[null,"3 supports avec croix stabilisatrices pour 2 capt. Montage    vertical    ","EG 358",{"$f":"'Sun 3000'!G46","v":287},"nbre colis/rangée","nbre colis final"]
[null,"                               Power7",null,null,0,"PAS montage en terrasse "]
[null,"                               Power10",null,null,1,{"$f":"E56*F6","v":0}]
[null,"                               Power15",null,null,1,{"$f":"E57*F7","v":0}]
[null,null,null,null,"somme colis EG 358",{"$f":"F56+F57","v":0}]
[]
[null,"3 supports (sans croix stabilisatrices) pour 2 capt. Montage    vertical","EG 359",{"$f":"'Sun 3000'!G47","v":245},"nbre colis/rangée","nbre colis final"]
[null,"                               Power7",null,null,0,"PAS montage en terrasse "]
[null,null,"pr un nbre de capteurs compris entre 0 et 7","nbre capteur compris entre 8 et 14"]
[null,"                               Power10",{"$f":"IF(E6=0,0,IF(E6=1,0,IF(E6=2,0,IF(E6=3,1,IF(E6=4,1,IF(E6=5,1,IF(E6=6,2,IF(E6=7,2,0))))))))","v":0},{"$f":"IF(E6=8,2,IF(E6=9,3,IF(E6=10,3,IF(E6=11,3,IF(E6=12,4,IF(E6=13,4,IF(E6=14,4,0)))))))","v":0},{"$f":"IF(D63=0,C63,D63)","v":0},{"$f":"E63*F6","v":0}]
[null,"                               Power15",{"$f":"IF(E7=0,0,IF(E7=1,0,IF(E7=2,0,IF(E7=3,1,IF(E7=4,1,IF(E7=5,1,IF(E7=6,2,IF(E7=7,2,0))))))))","v":0},{"$f":"IF(E7=8,2,IF(E7=9,3,IF(E7=10,3,IF(E7=11,3,IF(E7=12,4,IF(E7=13,4,IF(E7=14,4,0)))))))","v":0},{"$f":"IF(D64=0,C64,D64)","v":0},{"$f":"E64*F7","v":0}]
[null,null,null,null,"somme colis EG 359",{"$f":"F63+F64","v":0}]
[]
[]
[null,"• Ferrures d’ancrage pour montage SUR TOITURE   "]
[null," à choisir selon le type de couverture en + des profilés",null,null,null,null,null,"listechevrons"]
[null,{"$f":"'Sun 3000'!D52","v":"montage indépendant des chevrons en alu pour tuiles mécaniques"},{"$f":"H78","v":89807311},{"$f":"'Sun 3000'!G52","v":98},{"$f":"E75+E81+E87","v":0},null,null,"montage indépendant des chevrons en alu pour tuiles mécaniques",1,89807311,"4 pces EG 311",89807312,"6 pces EG 312"]
[null,null,{"$f":"H79","v":89807312},{"$f":"'Sun 3000'!G53","v":141},{"$f":"E76+E82+E88","v":0},null,null,"montage sur chevrons en inox pour tuiles mécaniques",2,89807313,"4 pces EG 313",89807314,"6 pces EG 314"]
[null,null,null,null,null,null,null,"montage sur chevrons en inox pour tuiles plates",3,89807315,"4 pces EG315",89807316,"6 pces EG 316"]
[null,null,"nbre colis par rangée",null,null,null,null,"montage sur chevrons en inox sur toit éternit",4,89807317,"4 pces EG 317",89807318,"6 pces EG 318"]
[null,null,"pr un nbre de capteurs compris entre 2 et 9","nbre capteur compris entre 10 et 16","nbre colis final",null,null,"montage sur chevrons en inox sur toit d'ardoises",5,89807319,"4 pces EG 319",89807320,"6 pces EG 320"]
[null,"Power7 /colis 4pces",null,{"$f":"VLOOKUP(E5,C111:E121,2)","v":0},0]
[null," Power7 /colis 6pces",null,{"$f":"VLOOKUP(E5,C111:E121,3)","v":0},0,null,null,{"$f":"VLOOKUP('Sun 3000'!D52,H70:I74,2,FALSE)","v":1}]
[]
[null,null,null,null,null,null,null,{"$f":"VLOOKUP(H76,I70:K74,2,FALSE)","v":89807311}]
[null,null,"nbre colis par rangée",null,null,null,null,{"$f":"VLOOKUP(H76,I70:M74,4,FALSE)","v":89807312}]
[null,null,"pr un nbre de capteurs compris entre 2 et 9","nbre capteur compris entre 10 et 16","nbre colis final"]
[null,"                               Power10 4 pces",null,{"$f":"VLOOKUP(E6,C111:E121,2)","v":0},{"$f":"(D81)*F6","v":0}]
[null,"                               Power10 6 pces",null,{"$f":"VLOOKUP(E6,C111:E121,3)","v":0},{"$f":"(D82)*F6","v":0}]
[]
[]
[null,null,"nbre colis par rangée"]
[null,null,"pr un nbre de capteurs compris entre 2 et 9","nbre capteur compris entre 10 et 16","nbre colis final"]
[null,"                               Power15 4 pces",null,{"$f":"VLOOKUP(E7,C111:E121,2)","v":0},{"$f":"(D87)*F7","v":0}]
[null,"                               Power15 6 pces",null,{"$f":"VLOOKUP(E7,C111:E121,3)","v":0},{"$f":"D88*F7","v":0}]
[]
[]
[]
[null,"• Montage sur tuiles canal "]
[null,"Kit tire-fonds pour montage sur tuiles canal","6 pces EG 94",{"$f":"'Sun 3000'!G57","v":287},null,{"$f":"E100+E103+E106","v":0}]
[null,null,"8 pces EG 95",{"$f":"'Sun 3000'!G58","v":245},null,{"$f":"E101+E104+E107","v":0}]
[]
[]
[]
[]
[null,null,null,null,"nbre colis final"]
[null,"Power  7  colis 6 pces EG94",null,{"$f":"VLOOKUP(E5,C111:E121,2)","v":0},0]
[null,"Power7  colis 8 pces EG95",null,{"$f":"VLOOKUP(E5,C111:E121,3)","v":0},0]
[]
[null,"                               Power10 6 pces EG 94",null,{"$f":"VLOOKUP(E6,C111:E121,2)","v":0},{"$f":"D103*F6","v":0}]
[null,"                               Power10 EG 95",null,{"$f":"VLOOKUP(E6,C111:E121,3)","v":0},{"$f":"D104*F6","v":0}]
[]
[null,"                               Power15 4 pces ER 136",null,{"$f":"VLOOKUP(E7,C111:E121,2)","v":0},{"$f":"D106*F7","v":0}]
[null,"                               Power15 6 pces ER 137",null,{"$f":"VLOOKUP(E7,C111:E121,3)","v":0},{"$f":"D107*F7","v":0}]
[]
[]
[null,null,"Nombre","kit 4 pces","kit 6 pces"]
[null,null,0,0,0]
[null,null,1,1,0]
[null,null,2,0,1]
[null,null,3,2,0]
[null,null,4,1,1]
[null,null,5,0,2]
[null,null,6,2,1]
[null,null,7,1,2]
[null,null,8,0,3]
[null,null,9,2,2]
[null,null,10,2,3]

{"sheet":"Mise à jour","index":10,"n_rows":5,"n_cols":4,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
[]
["Date : ","2017-01-18","Auteur :","Alexandre Diebold"]
[]
[null,"Modifications :"]
[null,null,"Actualisation des tarifs à partir de la version de 01/2017"]